(kicad_pcb (version 4) (host pcbnew 4.0.3-stable)
  (general
    (links 89)
    (no_connects 0)
    (area 53.899999 36.754999 111.200001 87.070001)
    (thickness 1.6)
    (drawings 38)
    (tracks 1030)
    (zones 0)
    (modules 37)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.2032)
    (user_trace_width 0.635)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.635)
    (via_min_drill 0.381)
    (user_via 0.635 0.381)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0635)
    (pad_to_paste_clearance -0.127)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x0b0e8_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory PDFs/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /VIN)
  (net 4 "Net-(C6-Pad2)")
  (net 5 "Net-(C7-Pad2)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D2-Pad1)")
  (net 8 /PB0)
  (net 9 /PB1)
  (net 10 /PB2)
  (net 11 /PB3)
  (net 12 /PB4)
  (net 13 /PB5)
  (net 14 /PB6)
  (net 15 /PB7)
  (net 16 /PC0)
  (net 17 /PC1)
  (net 18 /PC4)
  (net 19 /PC5)
  (net 20 /PC6)
  (net 21 /PC7)
  (net 22 /PD0)
  (net 23 /PD1)
  (net 24 AVR_MISO)
  (net 25 /PD3)
  (net 26 /PD4)
  (net 27 /PD5)
  (net 28 /PD6)
  (net 29 /PD7)
  (net 30 AVR_TX)
  (net 31 AVR_MOSI)
  (net 32 AVR_RX)
  (net 33 AVR_SCK)
  (net 34 "Net-(P7-Pad1)")
  (net 35 /CAN-)
  (net 36 ~AVR_RST)
  (net 37 /CAN+)
  (net 38 TXCAN)
  (net 39 RXCAN)
  (net 40 "Net-(U2-Pad4)")
  (net 41 /AREF)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1778)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /AREF)
    (add_net /CAN+)
    (add_net /CAN-)
    (add_net /PB0)
    (add_net /PB1)
    (add_net /PB2)
    (add_net /PB3)
    (add_net /PB4)
    (add_net /PB5)
    (add_net /PB6)
    (add_net /PB7)
    (add_net /PC0)
    (add_net /PC1)
    (add_net /PC4)
    (add_net /PC5)
    (add_net /PC6)
    (add_net /PC7)
    (add_net /PD0)
    (add_net /PD1)
    (add_net /PD3)
    (add_net /PD4)
    (add_net /PD5)
    (add_net /PD6)
    (add_net /PD7)
    (add_net /VIN)
    (add_net AVR_MISO)
    (add_net AVR_MOSI)
    (add_net AVR_RX)
    (add_net AVR_SCK)
    (add_net AVR_TX)
    (add_net GND)
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(U2-Pad4)")
    (add_net RXCAN)
    (add_net TXCAN)
    (add_net ~AVR_RST)
  )
  (module Graphics:oshw (layer F.Cu) (tedit 0)
    (at 66.04 82.55)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Graphics:purdue (layer F.Cu) (tedit 0)
    (at 95.885 82.55)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57F87A9F)
    (at 96.52 73.66 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value ATA6560 (at 0 3.5 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 TXCAN))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 RXCAN))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /CAN-))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /CAN+))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 57F87C4F)
    (at 100.965 53.34 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P11 (at -12.7 14.605 270) (layer F.SilkS) hide)
    (fp_text value AREF (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /AREF))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Crystals:Crystal_HC49-SD_SMD (layer F.Cu) (tedit 0)
    (at 88.9 71.755 90)
    (descr "Crystal Quarz HC49-SD SMD")
    (tags "Crystal Quarz HC49-SD SMD")
    (attr smd)
    (fp_text reference Y1 (at -5.207 -3.429 90) (layer F.SilkS))
    (fp_text value 16MHz (at 2.54 5.08 90) (layer F.Fab))
    (pad 1 smd rect (at -4.84886 0 90) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 4.84886 0 90) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad2)"))
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 57F86142)
    (at 71.12 66.04 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at -4.318 -5.715 270) (layer F.SilkS))
    (fp_text value ATMEGA32M1-A (at 0 6.05 90) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 AVR_MISO))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 /PD3))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 /PC1))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 TXCAN))
    (pad 7 smd rect (at -4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 RXCAN))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 /PB0))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 /PB1))
    (pad 10 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad2)"))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 /PD4))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 /PD5))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 /PD6))
    (pad 15 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 /PD7))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 /PB2))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 /PC4))
    (pad 18 smd rect (at 4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 /PC5))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 /AREF))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /PC6))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /PB3))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /PB4))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 /PC7))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 /PB5))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /PB6))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 /PB7))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 /PD0))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /PC0))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 ~AVR_RST))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 /PD1))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 71.12 73.025)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -2.413 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 73.66 58.42 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 69.85 58.42)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -2.667 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 41 /AREF))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 66.04 76.835 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 1.778 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 80.01 76.835 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.778 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 81.915 70.485 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.651 90) (layer F.SilkS))
    (fp_text value 18pF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 84.455 68.58 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0.889 -1.778 90) (layer F.SilkS))
    (fp_text value 18pF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 95.25 67.31 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 1.778 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 75.565 75.565 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value POWER_LED (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 59.69 56.515)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at -2.667 0) (layer F.SilkS))
    (fp_text value STATUS_LED (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FritzLib:2x01_ScrewTerm (layer F.Cu) (tedit 57F87CA7)
    (at 58.42 77.47 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.762 -2.413 90) (layer F.SilkS))
    (fp_text value VIN (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 /VIN))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 57F87C87)
    (at 83.185 49.53 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 10.795 -9.525 90) (layer F.SilkS) hide)
    (fp_text value PORTB (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /PB0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /PB1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /PB2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /PB3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /PB4))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /PB5))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /PB6))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /PB7))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07 (layer F.Cu) (tedit 57F87C53)
    (at 83.185 53.34 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 13.335 -1.27 90) (layer F.SilkS) hide)
    (fp_text value PORTC (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /PC0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /PC1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /PC4))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /PC5))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PC6))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /PC7))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x07.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 57F87C8F)
    (at 83.185 45.72 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 8.255 -4.445 90) (layer F.SilkS) hide)
    (fp_text value PORTD (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /PD0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /PD1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 AVR_MISO))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /PD3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /PD4))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /PD5))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /PD6))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /PD7))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02 (layer F.Cu) (tedit 57F87C67)
    (at 73.66 52.07)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value PD3 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /PD3))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 AVR_TX))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /PD3))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 AVR_MOSI))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x02.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02 (layer F.Cu) (tedit 57F87C8C)
    (at 73.66 45.72)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 2.54 -8.255) (layer F.SilkS) hide)
    (fp_text value PD4 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /PD4))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 AVR_RX))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /PD4))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 AVR_SCK))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x02.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57F87D01)
    (at 106.045 69.85 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 -2.54 270) (layer F.SilkS) hide)
    (fp_text value CAN_R (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /CAN-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 57F87C93)
    (at 58.42 45.72)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 5.08 -8.89) (layer F.SilkS) hide)
    (fp_text value ISP (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 AVR_MISO))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 AVR_SCK))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 AVR_MOSI))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 ~AVR_RST))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module FritzLib:2x01_ScrewTerm (layer F.Cu) (tedit 57C657BE)
    (at 106.68 60.96 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at -0.508 -2.54 270) (layer F.SilkS))
    (fp_text value CAN (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 37 /CAN+))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 35 /CAN-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57F87C96)
    (at 58.42 60.96)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P10 (at 1.905 -22.225) (layer F.SilkS) hide)
    (fp_text value UART (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 AVR_TX))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 AVR_RX))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 55DB43C0)
    (at 67.31 48.26 270)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 0 270) (layer F.SilkS))
    (fp_text value ~RESET (at -0.635 1.27 270) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 36 ~AVR_RST))
    (pad 1 smd rect (at -2.7 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 55360473)
    (at 70.485 76.835)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at -1.524 -2.286) (layer F.SilkS))
    (fp_text value MIC5235 (at -0.05 2.35) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 75.565 78.105)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.667 0) (layer F.SilkS))
    (fp_text value 470 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 64.135 53.975 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.778 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 36 ~AVR_RST))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 59.69 53.975 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R3 (at 2.667 -0.127 180) (layer F.SilkS))
    (fp_text value 470 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 /PC7))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 97.79 67.31 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.905 270) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 38 TXCAN))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5415D7BD)
    (at 104.775 73.66)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 1.905) (layer F.SilkS))
    (fp_text value 120 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(P7-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /CAN+))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_Pad_Via (layer F.Cu) (tedit 57F885EB)
    (at 58.42 40.64)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (fp_text reference P12 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad "" thru_hole circle (at 2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_Pad_Via (layer F.Cu) (tedit 57F885EF)
    (at 105.41 40.64)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (fp_text reference P13 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad "" thru_hole circle (at 2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_Pad_Via (layer F.Cu) (tedit 57F885E7)
    (at 58.42 83.185)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (fp_text reference P14 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad "" thru_hole circle (at 2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_Pad_Via (layer F.Cu) (tedit 57F885E4)
    (at 105.41 83.185)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (fp_text reference P15 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad "" thru_hole circle (at 2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.025 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.025) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.431891 -1.431891) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (dimension 57.15 (width 0.3) (layer Margin)
    (gr_text "2.2500 in" (at 82.55 95.965) (layer Margin))
    (feature1 (pts (xy 111.125 90.805) (xy 111.125 97.315)))
    (feature2 (pts (xy 53.975 90.805) (xy 53.975 97.315)))
    (crossbar (pts (xy 53.975 94.615) (xy 111.125 94.615)))
    (arrow1a (pts (xy 111.125 94.615) (xy 109.998496 95.201421)))
    (arrow1b (pts (xy 111.125 94.615) (xy 109.998496 94.028579)))
    (arrow2a (pts (xy 53.975 94.615) (xy 55.101504 95.201421)))
    (arrow2b (pts (xy 53.975 94.615) (xy 55.101504 94.028579)))
  )
  (dimension 50.165 (width 0.3) (layer Margin)
    (gr_text "1.9750 in" (at 122 61.9125 90) (layer Margin))
    (feature1 (pts (xy 114.3 36.83) (xy 123.35 36.83)))
    (feature2 (pts (xy 114.3 86.995) (xy 123.35 86.995)))
    (crossbar (pts (xy 120.65 86.995) (xy 120.65 36.83)))
    (arrow1a (pts (xy 120.65 36.83) (xy 121.236421 37.956504)))
    (arrow1b (pts (xy 120.65 36.83) (xy 120.063579 37.956504)))
    (arrow2a (pts (xy 120.65 86.995) (xy 121.236421 85.868496)))
    (arrow2b (pts (xy 120.65 86.995) (xy 120.063579 85.868496)))
  )
  (gr_text PWR (at 58.42 71.755) (layer F.SilkS))
  (gr_line (start 111.125 36.83) (end 53.975 36.83) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.125 86.995) (end 111.125 36.83) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 53.975 86.995) (end 111.125 86.995) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 53.975 36.83) (end 53.975 86.995) (layer Edge.Cuts) (width 0.15))
  (gr_text github.com/jfri2 (at 79.5655 84.0105) (layer F.SilkS))
  (gr_text "Design by John Fritz" (at 79.5655 81.7245) (layer F.SilkS))
  (gr_text "ATmegaXXM1 CAN BREAKOUT" (at 82.042 40.767) (layer F.SilkS))
  (gr_text 120Ω (at 108.585 69.85 90) (layer F.SilkS))
  (gr_text PD3 (at 71.12 53.34 90) (layer F.SilkS))
  (gr_text PD4 (at 71.12 46.99 90) (layer F.SilkS))
  (gr_text ISP (at 55.245 48.26) (layer F.SilkS))
  (gr_text ~RST (at 64.135 48.26 90) (layer F.SilkS))
  (gr_text CANL (at 106.68 66.675) (layer F.SilkS))
  (gr_text CANH (at 106.68 57.785) (layer F.SilkS))
  (gr_text GND (at 61.722 66.04) (layer F.SilkS))
  (gr_text RX (at 61.341 63.5) (layer F.SilkS))
  (gr_text TX (at 61.341 60.96) (layer F.SilkS))
  (gr_text PORTC (at 104.775 53.34) (layer F.SilkS))
  (gr_text PORTB (at 104.775 49.53) (layer F.SilkS))
  (gr_text PORTD (at 104.775 45.72) (layer F.SilkS))
  (gr_text RX (at 78.74 45.72) (layer F.SilkS))
  (gr_text SCK (at 79.121 48.26) (layer F.SilkS))
  (gr_text TX (at 78.74 52.07) (layer F.SilkS))
  (gr_text MOSI (at 79.375 54.61) (layer F.SilkS))
  (gr_text AREF|PB7|PD7 (at 100.965 59.9186 90) (layer F.SilkS))
  (gr_text GND|PB6|PD6 (at 98.425 59.69 90) (layer F.SilkS))
  (gr_text PC7|PB5|PD5 (at 95.885 59.69 90) (layer F.SilkS))
  (gr_text PC6|PB4|PD4 (at 93.345 59.69 90) (layer F.SilkS))
  (gr_text PC5|PB3|PD3 (at 90.805 59.69 90) (layer F.SilkS))
  (gr_text PC4|PB2|PD2 (at 88.265 59.69 90) (layer F.SilkS))
  (gr_text PC1|PB1|PD1 (at 85.725 59.69 90) (layer F.SilkS))
  (gr_text PC0|PB0|PD0 (at 83.185 59.69 90) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.61 37.465) (xy 54.61 86.36) (xy 110.49 86.36) (xy 110.49 37.465)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.61 37.465) (xy 54.61 86.36) (xy 110.49 86.36) (xy 110.49 37.465)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.0254))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.6 37.465) (xy 101.6 44.45) (xy 109.22 44.45) (xy 109.22 37.465)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.0254))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.6 37.465) (xy 101.6 44.45) (xy 109.22 44.45) (xy 109.22 37.465)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.0254))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.6 79.375) (xy 101.6 86.36) (xy 109.22 86.36) (xy 109.22 79.375)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.0254))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.61 37.465) (xy 54.61 44.45) (xy 62.23 44.45) (xy 62.23 37.465)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.0254))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.61 79.375) (xy 54.61 86.36) (xy 62.23 86.36) (xy 62.23 79.375)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.0254))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.6 79.375) (xy 101.6 86.36) (xy 109.22 86.36) (xy 109.22 79.375)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.0254))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.61 79.375) (xy 54.61 86.36) (xy 62.23 86.36) (xy 62.23 79.375)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.61 37.465) (xy 54.61 44.45) (xy 62.865 44.45) (xy 62.865 37.465)
      )
    )
  )
)
