(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 41)
    (no_connects 0)
    (area 122.368057 84.5184 197.590343 153.360001)
    (thickness 1.6002)
    (drawings 2)
    (tracks 155)
    (zones 0)
    (modules 26)
    (nets 37)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 159.9792 119.2974)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /Anode)
  (net 4 /Din)
  (net 5 /HV6)
  (net 6 /HV5)
  (net 7 /HV10)
  (net 8 /HV4)
  (net 9 /HV9)
  (net 10 /HV3)
  (net 11 /HV8)
  (net 12 /HV2)
  (net 13 /HV7)
  (net 14 /HV1)
  (net 15 "Net-(LED1-Pad2-DO)")
  (net 16 "Net-(LED2-Pad2-DO)")
  (net 17 /HV15)
  (net 18 /HV12)
  (net 19 /HV11)
  (net 20 /HV14)
  (net 21 /HV13)
  (net 22 "Net-(NX1-PadP$1)")
  (net 23 "Net-(NX1-PadP$2)")
  (net 24 "Net-(NX1-PadP$3)")
  (net 25 "Net-(NX1-PadP$4)")
  (net 26 "Net-(NX1-PadP$5)")
  (net 27 "Net-(NX1-PadP$6)")
  (net 28 "Net-(NX1-PadP$7)")
  (net 29 "Net-(NX1-PadP$8)")
  (net 30 "Net-(NX1-PadP$9)")
  (net 31 "Net-(NX1-PadP$10)")
  (net 32 "Net-(NX1-PadP$12)")
  (net 33 "Net-(NX1-PadP$14)")
  (net 34 "Net-(NX1-PadP$15)")
  (net 35 "Net-(NX1-PadP$16)")
  (net 36 "Net-(NX1-PadP$17)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /Anode)
    (add_net /Din)
    (add_net /HV1)
    (add_net /HV10)
    (add_net /HV11)
    (add_net /HV12)
    (add_net /HV13)
    (add_net /HV14)
    (add_net /HV15)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /HV9)
    (add_net GND)
    (add_net "Net-(LED1-Pad2-DO)")
    (add_net "Net-(LED2-Pad2-DO)")
    (add_net "Net-(NX1-PadP$1)")
    (add_net "Net-(NX1-PadP$10)")
    (add_net "Net-(NX1-PadP$12)")
    (add_net "Net-(NX1-PadP$14)")
    (add_net "Net-(NX1-PadP$15)")
    (add_net "Net-(NX1-PadP$16)")
    (add_net "Net-(NX1-PadP$17)")
    (add_net "Net-(NX1-PadP$2)")
    (add_net "Net-(NX1-PadP$3)")
    (add_net "Net-(NX1-PadP$4)")
    (add_net "Net-(NX1-PadP$5)")
    (add_net "Net-(NX1-PadP$6)")
    (add_net "Net-(NX1-PadP$7)")
    (add_net "Net-(NX1-PadP$8)")
    (add_net "Net-(NX1-PadP$9)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 162.9792 142.3774 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AA1E063)
    (at 159.9792 112.9474 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.4 0.05 270) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at -3.81 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AA1E05B)
    (at 159.9792 125.6474 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.25 180) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at -3.81 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5AD289DB)
    (at 149.86 101.92 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value PWR (at 0 2.33 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer F.Cu) (tedit 5AD289E4)
    (at 170.18 96.84 270)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33 270) (layer F.SilkS) hide)
    (fp_text value NL7037 (at 1.27 22.65 270) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV9))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /HV11))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV10))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /HV15))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV1))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV8))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV4))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /HV13))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /HV12))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV7))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV3))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV6))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV2))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV5))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Din))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /HV14))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:adafruit-WS2812B (layer F.Cu) (tedit 5AA1D6C0)
    (at 160.07064 129.4574)
    (attr smd)
    (fp_text reference LED1 (at 3.8989 0.4445 270) (layer F.SilkS))
    (fp_text value WS2812B5050 (at 0 0) (layer F.SilkS) hide)
    (pad 1-VD smd rect (at 2.44856 1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2-DO smd rect (at 2.44856 -1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(LED1-Pad2-DO)"))
    (pad 3-GN smd rect (at -2.44856 -1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4-DI smd rect (at -2.44856 1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 4 /Din))
  )
  (module adafruit:adafruit-WS2812B (layer F.Cu) (tedit 5AA1D6C8)
    (at 159.9792 109.1374)
    (attr smd)
    (fp_text reference LED2 (at 3.8989 0.4445 270) (layer F.SilkS))
    (fp_text value WS2812B5050 (at 0 0) (layer F.SilkS) hide)
    (pad 1-VD smd rect (at 2.44856 1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2-DO smd rect (at 2.44856 -1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(LED2-Pad2-DO)"))
    (pad 3-GN smd rect (at -2.44856 -1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4-DI smd rect (at -2.44856 1.64846 180) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(LED1-Pad2-DO)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580 (layer F.Cu) (tedit 5AA1E084)
    (at 159.9792 89.2974)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO14580")
    (tags "mounting hole 3.2mm no annular m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580 (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580 (layer F.Cu) (tedit 5AA1E076)
    (at 135.9792 137.2974)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO14580")
    (tags "mounting hole 3.2mm no annular m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580 (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580 (layer F.Cu) (tedit 5AA1E06E)
    (at 183.9792 137.2974)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO14580")
    (tags "mounting hole 3.2mm no annular m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580 (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 181.5692 123.1074)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 27K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(NX1-PadP$5)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /HV2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 181.5692 116.7574)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 27K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(NX1-PadP$6)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /HV3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 170.1392 102.7874)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.175 0) (layer F.SilkS))
    (fp_text value 22K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(NX1-PadP$9)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /HV4))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 138.3892 116.7574 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 27K (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(NX1-PadP$14)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /HV5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 138.3892 123.1074 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 27K (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(NX1-PadP$15)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /HV6))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 140.9292 129.4574 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 24K (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(NX1-PadP$16)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /HV7))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 159.9792 140.8874)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 27K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(NX1-PadP$1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /HV8))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 179.0292 129.4574)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 24K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(NX1-PadP$4)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /HV9))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 179.0292 109.1374)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 33K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(NX1-PadP$7)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /HV10))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 172.6792 135.8074)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 24K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(NX1-PadP$3)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /HV11))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 159.9792 104.6924)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at -3.81 0) (layer F.SilkS))
    (fp_text value 27K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(NX1-PadP$10)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /HV12))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 147.2792 135.8074 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 24K (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(NX1-PadP$17)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /HV13))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 144.7392 104.0574 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 33K (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(NX1-PadP$12)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /HV14))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 167.5992 139.6174)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 22K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(NX1-PadP$2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /HV15))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 176.4892 105.3274)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 22K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(NX1-PadP$8)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /HV1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mynixies:mynixies-RTS-5-DSUB-ALLPINS (layer F.Cu) (tedit 5AD2974E)
    (at 159.9792 119.2974)
    (attr virtual)
    (fp_text reference NX1 (at 0 -21.59) (layer F.SilkS) hide)
    (fp_text value B7971 (at 0.127 14.605) (layer F.SilkS))
    (pad P$1 thru_hole circle (at 0 17.4625) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 22 "Net-(NX1-PadP$1)"))
    (pad P$2 thru_hole circle (at 5.97154 16.4084) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 23 "Net-(NX1-PadP$2)"))
    (pad P$3 thru_hole circle (at 11.22426 13.37564) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 24 "Net-(NX1-PadP$3)"))
    (pad P$4 thru_hole circle (at 15.12062 8.72998) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 25 "Net-(NX1-PadP$4)"))
    (pad P$5 thru_hole circle (at 17.1958 3.03022) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 26 "Net-(NX1-PadP$5)"))
    (pad P$6 thru_hole circle (at 17.1958 -3.03022) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 27 "Net-(NX1-PadP$6)"))
    (pad P$7 thru_hole circle (at 15.12062 -8.72998) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 28 "Net-(NX1-PadP$7)"))
    (pad P$8 thru_hole circle (at 11.22426 -13.37564) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 29 "Net-(NX1-PadP$8)"))
    (pad P$9 thru_hole circle (at 5.97154 -16.4084) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 30 "Net-(NX1-PadP$9)"))
    (pad P$10 thru_hole circle (at 0 -17.4625) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 31 "Net-(NX1-PadP$10)"))
    (pad P$11 thru_hole circle (at -5.97154 -16.4084) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask))
    (pad P$12 thru_hole circle (at -11.22426 -13.37564) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 32 "Net-(NX1-PadP$12)"))
    (pad P$13 thru_hole circle (at -15.12062 -8.72998) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 3 /Anode))
    (pad P$14 thru_hole circle (at -17.1958 -3.03022) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 33 "Net-(NX1-PadP$14)"))
    (pad P$15 thru_hole circle (at -17.1958 3.03022) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 34 "Net-(NX1-PadP$15)"))
    (pad P$16 thru_hole circle (at -15.12062 8.72998) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 35 "Net-(NX1-PadP$16)"))
    (pad P$17 thru_hole circle (at -11.22426 13.37564) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 36 "Net-(NX1-PadP$17)"))
    (pad "" np_thru_hole circle (at 0 0) (size 10.16 10.16) (drill 10.16) (layers *.Cu *.Mask))
  )
  (gr_circle (center 160.02 119.38) (end 192.52 119.38) (layer Edge.Cuts) (width 0.127))
  (gr_text "nixies.us\nB7971" (at 161.92 142.66) (layer B.Mask))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 193.04 86.36) (xy 127 85.4) (xy 127 152.4) (xy 193.04 153.36)
      )
    )
  )
)
