<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="31.496" y2="0" width="0" layer="20"/>
<wire x1="31.496" y1="0" x2="31.496" y2="28.575" width="0" layer="20"/>
<wire x1="31.496" y1="28.575" x2="0" y2="28.575" width="0" layer="20"/>
<wire x1="0" y1="28.575" x2="0" y2="0" width="0" layer="20"/>
<text>HV Rescue 26</text>
<text>KO4XL  Aug '15
Rev 1</text>
</plain>
<libraries>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="DIL20">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PLUG" library="avr-7" package="DIL20" value="TINY2313-*P*">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SOCKET" library="avr-7" package="DIL20" value="TINY26P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="RESET">
<contactref element="PLUG" pad="1"/>
<contactref element="SOCKET" pad="10"/>
</signal>
<signal name="XTAL1">
<contactref element="PLUG" pad="5"/>
<contactref element="SOCKET" pad="7"/>
</signal>
<signal name="VCC">
<contactref element="PLUG" pad="20"/>
<contactref element="SOCKET" pad="5"/>
<contactref element="SOCKET" pad="15"/>
</signal>
<signal name="GND">
<contactref element="PLUG" pad="10"/>
<contactref element="SOCKET" pad="16"/>
<contactref element="SOCKET" pad="6"/>
</signal>
<signal name="RDY/!BSY">
<contactref element="PLUG" pad="3"/>
<contactref element="SOCKET" pad="9"/>
</signal>
<signal name="!OE">
<contactref element="PLUG" pad="6"/>
<contactref element="SOCKET" pad="8"/>
</signal>
<signal name="!WR">
<contactref element="PLUG" pad="7"/>
<contactref element="SOCKET" pad="1"/>
</signal>
<signal name="BS1/PAGEL">
<contactref element="PLUG" pad="8"/>
<contactref element="SOCKET" pad="4"/>
</signal>
<signal name="XA0">
<contactref element="PLUG" pad="9"/>
<contactref element="SOCKET" pad="2"/>
</signal>
<signal name="XA1/BS2">
<contactref element="PLUG" pad="11"/>
<contactref element="SOCKET" pad="3"/>
</signal>
<signal name="DATA0">
<contactref element="PLUG" pad="12"/>
<contactref element="SOCKET" pad="20"/>
</signal>
<signal name="DATA1">
<contactref element="PLUG" pad="13"/>
<contactref element="SOCKET" pad="19"/>
</signal>
<signal name="DATA2">
<contactref element="PLUG" pad="14"/>
<contactref element="SOCKET" pad="18"/>
</signal>
<signal name="DATA3">
<contactref element="PLUG" pad="15"/>
<contactref element="SOCKET" pad="17"/>
</signal>
<signal name="DATA4">
<contactref element="PLUG" pad="16"/>
<contactref element="SOCKET" pad="14"/>
</signal>
<signal name="DATA5">
<contactref element="PLUG" pad="17"/>
<contactref element="SOCKET" pad="13"/>
</signal>
<signal name="DATA6">
<contactref element="PLUG" pad="18"/>
<contactref element="SOCKET" pad="12"/>
</signal>
<signal name="DATA7">
<contactref element="PLUG" pad="19"/>
<contactref element="SOCKET" pad="11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
