(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 170)
    (tracks 762)
    (zones 0)
    (modules 37)
    (nets 93)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 /ADDR23)
  (net 4 /ADDR22)
  (net 5 /ADDR21)
  (net 6 /ADDR20)
  (net 7 /ADDR19)
  (net 8 /ADDR18)
  (net 9 /ADDR17)
  (net 10 /ADDR16)
  (net 11 /ADDR15)
  (net 12 /ADDR14)
  (net 13 /ADDR13)
  (net 14 /ADDR12)
  (net 15 /ADDR11)
  (net 16 /ADDR10)
  (net 17 /ADDR9)
  (net 18 /ADDR8)
  (net 19 /ADDR7)
  (net 20 /ADDR6)
  (net 21 /ADDR5)
  (net 22 /ADDR4)
  (net 23 /ADDR3)
  (net 24 /ADDR2)
  (net 25 /ADDR1)
  (net 26 /ADDR0)
  (net 27 /SDA)
  (net 28 /SCL)
  (net 29 /RTC_XOUT)
  (net 30 /RTC_XIN)
  (net 31 /XOUT)
  (net 32 /XIN)
  (net 33 /~RESET)
  (net 34 /DATA7)
  (net 35 /DATA6)
  (net 36 /DATA5)
  (net 37 /DATA4)
  (net 38 /DATA3)
  (net 39 /DATA2)
  (net 40 /DATA1)
  (net 41 /DATA0)
  (net 42 /~CS3)
  (net 43 /~CS2)
  (net 44 /~CS1)
  (net 45 /~CS0)
  (net 46 /~WR)
  (net 47 /~RD)
  (net 48 /~MREQ)
  (net 49 /~IORQ)
  (net 50 /~INSTRD)
  (net 51 /~HALT_SLP)
  (net 52 /~WAIT)
  (net 53 /~BUSACK)
  (net 54 /~BUSREQ)
  (net 55 /~NMI)
  (net 56 /TDO)
  (net 57 /TDI)
  (net 58 /TCK)
  (net 59 /TMS)
  (net 60 /TRIGOUT)
  (net 61 /PHI)
  (net 62 +BATT)
  (net 63 /PD7)
  (net 64 /PD6)
  (net 65 /PD5)
  (net 66 /PD4)
  (net 67 /PD3)
  (net 68 /PD2)
  (net 69 /PD1)
  (net 70 /PD0)
  (net 71 /PC7)
  (net 72 /PC6)
  (net 73 /PC5)
  (net 74 /PC4)
  (net 75 /PC3)
  (net 76 /PC2)
  (net 77 /PC1)
  (net 78 /PC0)
  (net 79 /PB7)
  (net 80 /PB6)
  (net 81 /PB5)
  (net 82 /PB4)
  (net 83 /PB3)
  (net 84 /PB2)
  (net 85 /PB1)
  (net 86 /PB0)
  (net 87 /FTDI_GND)
  (net 88 /FTDI_VCC)
  (net 89 /~FTDI_RTS)
  (net 90 /FTDI_RX)
  (net 91 /FTDI_TX)
  (net 92 /~FTDI_CTS)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +BATT)
    (add_net /ADDR0)
    (add_net /ADDR1)
    (add_net /ADDR10)
    (add_net /ADDR11)
    (add_net /ADDR12)
    (add_net /ADDR13)
    (add_net /ADDR14)
    (add_net /ADDR15)
    (add_net /ADDR16)
    (add_net /ADDR17)
    (add_net /ADDR18)
    (add_net /ADDR19)
    (add_net /ADDR2)
    (add_net /ADDR20)
    (add_net /ADDR21)
    (add_net /ADDR22)
    (add_net /ADDR23)
    (add_net /ADDR3)
    (add_net /ADDR4)
    (add_net /ADDR5)
    (add_net /ADDR6)
    (add_net /ADDR7)
    (add_net /ADDR8)
    (add_net /ADDR9)
    (add_net /DATA0)
    (add_net /DATA1)
    (add_net /DATA2)
    (add_net /DATA3)
    (add_net /DATA4)
    (add_net /DATA5)
    (add_net /DATA6)
    (add_net /DATA7)
    (add_net /FTDI_GND)
    (add_net /FTDI_RX)
    (add_net /FTDI_TX)
    (add_net /FTDI_VCC)
    (add_net /PB0)
    (add_net /PB1)
    (add_net /PB2)
    (add_net /PB3)
    (add_net /PB4)
    (add_net /PB5)
    (add_net /PB6)
    (add_net /PB7)
    (add_net /PC0)
    (add_net /PC1)
    (add_net /PC2)
    (add_net /PC3)
    (add_net /PC4)
    (add_net /PC5)
    (add_net /PC6)
    (add_net /PC7)
    (add_net /PD0)
    (add_net /PD1)
    (add_net /PD2)
    (add_net /PD3)
    (add_net /PD4)
    (add_net /PD5)
    (add_net /PD6)
    (add_net /PD7)
    (add_net /PHI)
    (add_net /RTC_XIN)
    (add_net /RTC_XOUT)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TCK)
    (add_net /TDI)
    (add_net /TDO)
    (add_net /TMS)
    (add_net /TRIGOUT)
    (add_net /XIN)
    (add_net /XOUT)
    (add_net /~BUSACK)
    (add_net /~BUSREQ)
    (add_net /~CS0)
    (add_net /~CS1)
    (add_net /~CS2)
    (add_net /~CS3)
    (add_net /~FTDI_CTS)
    (add_net /~FTDI_RTS)
    (add_net /~HALT_SLP)
    (add_net /~INSTRD)
    (add_net /~IORQ)
    (add_net /~MREQ)
    (add_net /~NMI)
    (add_net /~RD)
    (add_net /~RESET)
    (add_net /~WAIT)
    (add_net /~WR)
    (add_net GND)
  )
  (module footprints:oshw_small (layer B.Cu) (tedit 0)
    (at 118.6688 62.1792 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module footprints:SO-8 (layer F.Cu) (tedit 5DBF573B)
    (at 209.55 60.96)
    (tags "Avago HCPL-0530")
    (attr smd)
    (fp_text reference U3 (at 0.635 0 180) (layer F.SilkS))
    (fp_text value "PC Powered" (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at 1.905 2.795) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 89 /~FTDI_RTS))
    (pad 5 smd rect (at 1.905 -2.795) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 87 /FTDI_GND))
    (pad 3 smd rect (at 0.635 2.795) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 87 /FTDI_GND))
    (pad 6 smd rect (at 0.635 -2.795) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 67 /PD3))
    (pad 2 smd rect (at -0.635 2.795) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 87 /FTDI_GND))
    (pad 7 smd rect (at -0.635 -2.795) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 69 /PD1))
    (pad 1 smd rect (at -1.905 2.795) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 91 /FTDI_TX))
    (pad 8 smd rect (at -1.905 -2.795) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 88 /FTDI_VCC))
  )
  (module footprints:SO-8 (layer F.Cu) (tedit 5DBF573B)
    (at 203.835 60.96 180)
    (tags "Avago HCPL-0530")
    (attr smd)
    (fp_text reference U2 (at 0.635 0 180) (layer F.SilkS))
    (fp_text value "BB Powered" (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at 1.905 2.795 180) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 70 /PD0))
    (pad 5 smd rect (at 1.905 -2.795 180) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.635 2.795 180) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.635 -2.795 180) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 90 /FTDI_RX))
    (pad 2 smd rect (at -0.635 2.795 180) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.635 -2.795 180) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 92 /~FTDI_CTS))
    (pad 1 smd rect (at -1.905 2.795 180) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 68 /PD2))
    (pad 8 smd rect (at -1.905 -2.795 180) (size 0.64 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 212.979 61.073 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 /FTDI_GND))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 /FTDI_VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 200.42 60.946 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 167.64 88.9 180)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference J18 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value PORTB (at 5.08 8.89 90) (layer F.SilkS))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 /PB7))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 /PB6))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 /PB5))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 /PB4))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 /PB3))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 /PB2))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 /PB1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 /PB0))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 144.78 91.44 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference J2 (at 0 -2.77 90) (layer F.SilkS) hide)
    (fp_text value PORTC (at 5.08 8.89 180) (layer F.SilkS))
    (fp_text user %R (at 0 8.89) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 /PC7))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 /PC6))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 /PC5))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 /PC4))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 /PC3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 /PC2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 /PC1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 /PC0))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EZ80L92AZ050SG:QFP50P1600X1600X160-100N (layer F.Cu) (tedit 0)
    (at 147.32 73.66 225)
    (attr smd)
    (fp_text reference U1 (at -5.46132 -9.83136 45) (layer F.SilkS))
    (fp_text value EZ80L92AZ050SG (at 0.449013 9.429269 45) (layer F.SilkS))
    (pad 75 smd rect (at 7.725 -6 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 63 /PD7))
    (pad 74 smd rect (at 7.725 -5.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 64 /PD6))
    (pad 73 smd rect (at 7.725 -5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 65 /PD5))
    (pad 72 smd rect (at 7.725 -4.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 66 /PD4))
    (pad 71 smd rect (at 7.725 -4 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 67 /PD3))
    (pad 70 smd rect (at 7.725 -3.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 68 /PD2))
    (pad 69 smd rect (at 7.725 -3 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 69 /PD1))
    (pad 68 smd rect (at 7.725 -2.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 70 /PD0))
    (pad 67 smd rect (at 7.725 -2 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 66 smd rect (at 7.725 -1.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 56 /TDO))
    (pad 65 smd rect (at 7.725 -1 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 57 /TDI))
    (pad 64 smd rect (at 7.725 -0.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 60 /TRIGOUT))
    (pad 63 smd rect (at 7.725 0 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 58 /TCK))
    (pad 62 smd rect (at 7.725 0.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 59 /TMS))
    (pad 61 smd rect (at 7.725 1 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 60 smd rect (at 7.725 1.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 62 +BATT))
    (pad 59 smd rect (at 7.725 2 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 29 /RTC_XOUT))
    (pad 58 smd rect (at 7.725 2.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 30 /RTC_XIN))
    (pad 57 smd rect (at 7.725 3 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 56 smd rect (at 7.725 3.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 55 smd rect (at 7.725 4 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 51 /~HALT_SLP))
    (pad 54 smd rect (at 7.725 4.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 53 /~BUSACK))
    (pad 53 smd rect (at 7.725 5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 54 /~BUSREQ))
    (pad 52 smd rect (at 7.725 5.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 55 /~NMI))
    (pad 51 smd rect (at 7.725 6 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 33 /~RESET))
    (pad 25 smd rect (at -7.725 6 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 6 /ADDR20))
    (pad 24 smd rect (at -7.725 5.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 7 /ADDR19))
    (pad 23 smd rect (at -7.725 5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 8 /ADDR18))
    (pad 22 smd rect (at -7.725 4.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 9 /ADDR17))
    (pad 21 smd rect (at -7.725 4 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 10 /ADDR16))
    (pad 20 smd rect (at -7.725 3.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 11 /ADDR15))
    (pad 19 smd rect (at -7.725 3 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 18 smd rect (at -7.725 2.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 17 smd rect (at -7.725 2 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 12 /ADDR14))
    (pad 16 smd rect (at -7.725 1.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 13 /ADDR13))
    (pad 15 smd rect (at -7.725 1 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 14 /ADDR12))
    (pad 14 smd rect (at -7.725 0.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 15 /ADDR11))
    (pad 13 smd rect (at -7.725 0 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 16 /ADDR10))
    (pad 12 smd rect (at -7.725 -0.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 17 /ADDR9))
    (pad 11 smd rect (at -7.725 -1 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 18 /ADDR8))
    (pad 10 smd rect (at -7.725 -1.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 19 /ADDR7))
    (pad 9 smd rect (at -7.725 -2 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 20 /ADDR6))
    (pad 8 smd rect (at -7.725 -2.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -7.725 -3 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 6 smd rect (at -7.725 -3.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 21 /ADDR5))
    (pad 5 smd rect (at -7.725 -4 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 22 /ADDR4))
    (pad 4 smd rect (at -7.725 -4.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 23 /ADDR3))
    (pad 3 smd rect (at -7.725 -5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 24 /ADDR2))
    (pad 2 smd rect (at -7.725 -5.5 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 25 /ADDR1))
    (pad 1 smd rect (at -7.725 -6 225) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 26 /ADDR0))
    (pad 100 smd rect (at -6 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 61 /PHI))
    (pad 99 smd rect (at -5.5 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 28 /SCL))
    (pad 98 smd rect (at -5 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 27 /SDA))
    (pad 97 smd rect (at -4.5 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 96 smd rect (at -4 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 95 smd rect (at -3.5 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 79 /PB7))
    (pad 94 smd rect (at -3 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 80 /PB6))
    (pad 93 smd rect (at -2.5 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 81 /PB5))
    (pad 92 smd rect (at -2 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 82 /PB4))
    (pad 91 smd rect (at -1.5 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 83 /PB3))
    (pad 90 smd rect (at -1 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 84 /PB2))
    (pad 89 smd rect (at -0.5 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 85 /PB1))
    (pad 88 smd rect (at 0 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 86 /PB0))
    (pad 87 smd rect (at 0.5 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 86 smd rect (at 1 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 31 /XOUT))
    (pad 85 smd rect (at 1.5 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 32 /XIN))
    (pad 84 smd rect (at 2 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 83 smd rect (at 2.5 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 71 /PC7))
    (pad 82 smd rect (at 3 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 72 /PC6))
    (pad 81 smd rect (at 3.5 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 73 /PC5))
    (pad 80 smd rect (at 4 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 74 /PC4))
    (pad 79 smd rect (at 4.5 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 75 /PC3))
    (pad 78 smd rect (at 5 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 76 /PC2))
    (pad 77 smd rect (at 5.5 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 77 /PC1))
    (pad 76 smd rect (at 6 -7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 78 /PC0))
    (pad 50 smd rect (at 6 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 52 /~WAIT))
    (pad 49 smd rect (at 5.5 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 50 /~INSTRD))
    (pad 48 smd rect (at 5 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 46 /~WR))
    (pad 47 smd rect (at 4.5 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 47 /~RD))
    (pad 46 smd rect (at 4 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 48 /~MREQ))
    (pad 45 smd rect (at 3.5 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 49 /~IORQ))
    (pad 44 smd rect (at 3 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 43 smd rect (at 2.5 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 42 smd rect (at 2 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 34 /DATA7))
    (pad 41 smd rect (at 1.5 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 35 /DATA6))
    (pad 40 smd rect (at 1 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 36 /DATA5))
    (pad 39 smd rect (at 0.5 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 37 /DATA4))
    (pad 38 smd rect (at 0 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 38 /DATA3))
    (pad 37 smd rect (at -0.5 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 39 /DATA2))
    (pad 36 smd rect (at -1 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 40 /DATA1))
    (pad 35 smd rect (at -1.5 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 41 /DATA0))
    (pad 34 smd rect (at -2 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 33 smd rect (at -2.5 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 32 smd rect (at -3 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 42 /~CS3))
    (pad 31 smd rect (at -3.5 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 43 /~CS2))
    (pad 30 smd rect (at -4 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 44 /~CS1))
    (pad 29 smd rect (at -4.5 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 45 /~CS0))
    (pad 28 smd rect (at -5 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 3 /ADDR23))
    (pad 27 smd rect (at -5.5 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 4 /ADDR22))
    (pad 26 smd rect (at -6 7.725 315) (size 1.42 0.27) (layers F.Cu F.Paste F.Mask)
      (net 5 /ADDR21))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 213.36 68.58 270)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J22 (at 4.385 -2.27 90) (layer F.SilkS) hide)
    (fp_text value TTY (at 4.385 14.97 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.77 6.35) (layer F.Fab) hide)
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 /~FTDI_RTS))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 /FTDI_RX))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 /FTDI_TX))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 /FTDI_VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 /~FTDI_CTS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 /FTDI_GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 195.58 68.58 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J21 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value GND (at -1.27 0 225) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 114.3 53.34 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J20 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value RTC_VDD (at 0 -2.33 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 +BATT))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 81.28 53.34 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J19 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value VDD (at 1.27 0 -45) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 175.26 68.58 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J17 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value PHI (at 0 -2.33 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 /PHI))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 106.68 68.58 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J16 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value TRIGOUT (at 0 -2.33 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 /TRIGOUT))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A429)
    (at 132.08 91.44 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J15 (at 0 -2.77 90) (layer F.SilkS) hide)
    (fp_text value ZDI (at 0 10.39 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 /TDO))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 /TDI))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 /TCK))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 /TMS))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 86.36 68.58 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J14 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value ~NMI (at 0 -2.33 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 /~NMI))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 91.44 68.58 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J13 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value ~BUSREQACK (at 0 -4.87 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -1.27) (layer B.Fab))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /~BUSACK))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /~BUSREQ))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 91.44 53.34 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J12 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value ~WAIT (at 0 -4.87 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -1.27) (layer B.Fab))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /~HALT_SLP))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 /~WAIT))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 96.52 53.34 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J11 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value ~INSTRD (at 0 -2.33 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /~INSTRD))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 109.22 53.34 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J10 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value "IRQ & Mem" (at 0 -9.95 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -3.81) (layer B.Fab))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /~WR))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /~RD))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /~MREQ))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /~IORQ))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 149.86 53.34 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J9 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value ~CS[0..3] (at 0 -9.95 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -3.81) (layer B.Fab))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /~CS3))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /~CS2))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /~CS1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /~CS0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 137.16 53.34 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J8 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value DATA[0..7] (at 0 -20.11 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -8.89) (layer B.Fab))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /DATA7))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /DATA6))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /DATA5))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /DATA4))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /DATA3))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /DATA2))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /DATA1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /DATA0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 81.28 68.58 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J7 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value ~RESET (at 0 -2.33 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /~RESET))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 180.34 68.58 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J6 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value XINOUT (at 0 -4.87 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -1.27) (layer B.Fab))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /XOUT))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /XIN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 99.06 68.58 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J5 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value RTC_XINOUT (at 0 -4.87 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -1.27) (layer B.Fab))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /RTC_XOUT))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /RTC_XIN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 187.96 68.58 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value I2C (at 0 -4.87 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -1.27) (layer B.Fab))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /SDA))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /SCL))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x24_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 213.36 53.34 90)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (fp_text reference J3 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value ADDR[0..23] (at 0 -60.75 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -29.21) (layer B.Fab))
    (pad 24 thru_hole oval (at 0 -58.42 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /ADDR23))
    (pad 23 thru_hole oval (at 0 -55.88 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /ADDR22))
    (pad 22 thru_hole oval (at 0 -53.34 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /ADDR21))
    (pad 21 thru_hole oval (at 0 -50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /ADDR20))
    (pad 20 thru_hole oval (at 0 -48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /ADDR19))
    (pad 19 thru_hole oval (at 0 -45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /ADDR18))
    (pad 18 thru_hole oval (at 0 -43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /ADDR17))
    (pad 17 thru_hole oval (at 0 -40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /ADDR16))
    (pad 16 thru_hole oval (at 0 -38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /ADDR15))
    (pad 15 thru_hole oval (at 0 -35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /ADDR14))
    (pad 14 thru_hole oval (at 0 -33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /ADDR13))
    (pad 13 thru_hole oval (at 0 -30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /ADDR12))
    (pad 12 thru_hole oval (at 0 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /ADDR11))
    (pad 11 thru_hole oval (at 0 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /ADDR10))
    (pad 10 thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /ADDR9))
    (pad 9 thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /ADDR8))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /ADDR7))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /ADDR6))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /ADDR5))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /ADDR4))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /ADDR3))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /ADDR2))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /ADDR1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /ADDR0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 127 71.12)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference J1 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value PORTD (at 5.08 8.89 90) (layer F.SilkS))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 /PD7))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 /PD6))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 /PD5))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 /PD4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 /PD3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 /PD2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 /PD1))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 /PD0))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_4x4.5 (layer F.Cu) (tedit 5BCA39CF)
    (at 86.36 60.706)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 4.0x4.5mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C9 (at -4.445 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.8 0) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.8 0) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x4.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 145.398718 68.596282 45)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 0 1.43 45) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 45) (layer B.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 45) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.875 0 45) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 152.035282 72.025282 315)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0 1.43 135) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 135) (layer B.Fab))
    (fp_text user %R (at 0 0 135) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 315) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.875 0 315) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 149.716718 77.867282 45)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 1.43 45) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 45) (layer B.Fab))
    (fp_text user %R (at 0 0 45) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 45) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.875 0 45) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 144.415282 77.613282 315)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 1.43 135) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 135) (layer B.Fab))
    (fp_text user %R (at 0 0 135) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 315) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.875 0 315) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 141.875282 75.040718 135)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 1.43 315) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 315) (layer B.Fab))
    (fp_text user %R (at 0 0 315) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 135) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.875 0 135) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 142.129282 71.738718 45)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 1.43 225) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 225) (layer B.Fab))
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 45) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.875 0 45) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 153.526718 74.057282 225)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 1.43 45) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 45) (layer B.Fab))
    (fp_text user %R (at 0 0 45) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 225) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.875 0 225) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 148.733282 68.469282 315)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 1.43 135) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 135) (layer B.Fab))
    (fp_text user %R (at 0 0 135) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 315) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.875 0 315) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 171.45 72.39) (end 171.45 71.12) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 123.19 72.39) (end 124.46 72.39) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_text "eZ80 Breadboard Breakout\nVersion 1.0\nJune Tate-Gans\nhttp://github.com/jtgans/zippy" (at 119.38 62.0776) (layer F.SilkS))
  (gr_text TDX0/IR_TXD (at 128.905 71.12 45) (layer F.SilkS))
  (gr_text RXD0/IR_RXD (at 128.905 73.66 45) (layer F.SilkS))
  (gr_text ~CTS0 (at 128.905 78.74 45) (layer F.SilkS))
  (gr_text ~RTS0 (at 128.905 76.2 45) (layer F.SilkS))
  (gr_text ~DTR0 (at 128.905 81.28 45) (layer F.SilkS))
  (gr_text ~DSR0 (at 128.905 83.82 45) (layer F.SilkS))
  (gr_text ~DCD0 (at 128.905 86.36 45) (layer F.SilkS))
  (gr_text ~RI0 (at 128.905 88.9 45) (layer F.SilkS))
  (gr_text MOSI (at 165.735 71.12 315) (layer F.SilkS))
  (gr_text MISO (at 165.735 73.66 315) (layer F.SilkS))
  (gr_text T5_OUT (at 165.735 76.2 315) (layer F.SilkS))
  (gr_text T4_OUT (at 165.735 78.74 315) (layer F.SilkS))
  (gr_text SCK (at 165.735 81.28 315) (layer F.SilkS))
  (gr_text SS (at 165.735 83.82 315) (layer F.SilkS))
  (gr_text T1_IN (at 165.735 86.36 315) (layer F.SilkS))
  (gr_text T0_IN (at 165.735 88.9 315) (layer F.SilkS))
  (gr_text ~RI1 (at 162.56 89.535 45) (layer F.SilkS))
  (gr_text ~DCD1 (at 160.02 89.535 45) (layer F.SilkS))
  (gr_text ~DSR1 (at 157.48 89.535 45) (layer F.SilkS))
  (gr_text ~DTR1 (at 154.94 89.535 45) (layer F.SilkS))
  (gr_text ~CTS1 (at 152.4 89.535 45) (layer F.SilkS))
  (gr_text ~RTS1 (at 149.86 89.535 45) (layer F.SilkS))
  (gr_text RXD1 (at 147.32 89.535 45) (layer F.SilkS))
  (gr_text TXD1 (at 144.78 89.535 45) (layer F.SilkS))
  (gr_text TDO (at 139.7 89.535 45) (layer F.SilkS))
  (gr_text TDI (at 137.16 89.535 45) (layer F.SilkS))
  (gr_text TCK (at 134.62 89.535 45) (layer F.SilkS))
  (gr_text TMS (at 132.08 89.535 45) (layer F.SilkS))
  (gr_text A0 (at 213.36 54.991 315) (layer F.SilkS))
  (gr_text A1 (at 210.82 54.991 315) (layer F.SilkS))
  (gr_text A2 (at 208.28 54.991 315) (layer F.SilkS))
  (gr_text A3 (at 205.74 54.991 315) (layer F.SilkS))
  (gr_text A4 (at 203.2 54.991 315) (layer F.SilkS))
  (gr_text A5 (at 200.66 54.991 315) (layer F.SilkS))
  (gr_text A6 (at 198.12 54.991 315) (layer F.SilkS))
  (gr_text A7 (at 195.58 54.991 315) (layer F.SilkS))
  (gr_text A8 (at 193.04 54.991 315) (layer F.SilkS))
  (gr_text A9 (at 190.5 54.991 315) (layer F.SilkS))
  (gr_text A10 (at 187.96 54.991 315) (layer F.SilkS))
  (gr_text A11 (at 185.42 54.991 315) (layer F.SilkS))
  (gr_text A12 (at 182.88 54.991 315) (layer F.SilkS))
  (gr_text A13 (at 180.34 54.991 315) (layer F.SilkS))
  (gr_text A14 (at 177.8 54.991 315) (layer F.SilkS))
  (gr_text A15 (at 175.26 54.991 315) (layer F.SilkS))
  (gr_text A16 (at 172.72 54.991 315) (layer F.SilkS))
  (gr_text A17 (at 170.18 54.991 315) (layer F.SilkS))
  (gr_text A18 (at 167.64 54.991 315) (layer F.SilkS))
  (gr_text A19 (at 165.1 54.991 315) (layer F.SilkS))
  (gr_text A20 (at 162.56 54.991 315) (layer F.SilkS))
  (gr_text A21 (at 160.02 54.991 315) (layer F.SilkS))
  (gr_text A22 (at 157.48 54.991 315) (layer F.SilkS))
  (gr_text A23 (at 154.94 54.991 315) (layer F.SilkS))
  (gr_text ~CS0 (at 149.86 54.991 315) (layer F.SilkS))
  (gr_text ~CS1 (at 147.32 54.991 315) (layer F.SilkS))
  (gr_text ~CS2 (at 144.78 54.991 315) (layer F.SilkS))
  (gr_text ~CS3 (at 142.24 54.991 315) (layer F.SilkS))
  (gr_text D0 (at 137.16 54.991 315) (layer F.SilkS))
  (gr_text D1 (at 134.62 54.991 315) (layer F.SilkS))
  (gr_text D2 (at 132.08 54.991 315) (layer F.SilkS))
  (gr_text D3 (at 129.54 54.991 315) (layer F.SilkS))
  (gr_text D4 (at 127 54.991 315) (layer F.SilkS))
  (gr_text D5 (at 124.46 54.991 315) (layer F.SilkS))
  (gr_text D6 (at 121.92 54.991 315) (layer F.SilkS))
  (gr_text D7 (at 119.38 54.991 315) (layer F.SilkS))
  (gr_text +BATT (at 114.3 54.991 315) (layer F.SilkS))
  (gr_text ~IORQ (at 109.22 54.991 315) (layer F.SilkS))
  (gr_text ~MREQ (at 106.68 54.991 315) (layer F.SilkS))
  (gr_text ~RD (at 104.14 54.991 315) (layer F.SilkS))
  (gr_text ~WR (at 101.6 54.991 315) (layer F.SilkS))
  (gr_text ~INSTRD (at 96.52 54.991 315) (layer F.SilkS))
  (gr_text ~WAIT (at 91.44 54.991 315) (layer F.SilkS))
  (gr_text ~HALT_SLP (at 88.9 54.991 315) (layer F.SilkS))
  (gr_text ~RESET (at 81.28 67.31 45) (layer F.SilkS))
  (gr_text ~NMI (at 86.36 67.31 45) (layer F.SilkS))
  (gr_text ~BUSREQ (at 91.44 67.31 45) (layer F.SilkS))
  (gr_text ~BUSACK (at 93.98 67.31 45) (layer F.SilkS))
  (gr_text RTC_XOUT (at 101.6 67.31 45) (layer F.SilkS))
  (gr_text RTC_XIN (at 99.06 67.31 45) (layer F.SilkS))
  (gr_text TRIGOUT (at 106.68 67.31 45) (layer F.SilkS))
  (gr_text PHI (at 175.26 67.31 45) (layer F.SilkS))
  (gr_text XOUT (at 180.34 67.31 45) (layer F.SilkS))
  (gr_text XIN (at 182.88 67.31 45) (layer F.SilkS))
  (gr_text SCL (at 187.96 67.31 45) (layer F.SilkS))
  (gr_text SDA (at 190.5 67.183 45) (layer F.SilkS))
  (gr_text ~RTS (at 200.66 67.183 45) (layer F.SilkS))
  (gr_text RX (at 203.2 67.183 45) (layer F.SilkS))
  (gr_text TX (at 205.74 67.183 45) (layer F.SilkS))
  (gr_text VCC (at 208.28 67.183 45) (layer F.SilkS))
  (gr_text ~CTS (at 210.82 67.183 45) (layer F.SilkS))
  (gr_text GND (at 213.36 67.183 45) (layer F.SilkS))
  (gr_arc (start 213.36 68.58) (end 213.36 71.12) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 167.64 91.44) (end 167.64 93.98) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 127 91.44) (end 124.46 91.44) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 81.28 68.58) (end 78.74 68.58) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 81.28 53.34) (end 81.28 50.8) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 213.36 53.34) (end 215.9 53.34) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 170.18 91.44) (end 170.18 72.39) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 127 93.98) (end 167.64 93.98) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 124.46 72.39) (end 124.46 91.44) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 81.28 71.12) (end 123.19 71.12) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 78.74 53.34) (end 78.74 68.58) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 213.36 71.12) (end 171.45 71.12) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 215.9 53.34) (end 215.9 68.58) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 81.28 50.8) (end 213.36 50.8) (layer Edge.Cuts) (width 0.127))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 214.63 52.07) (xy 214.63 56.642) (xy 214.63 69.85) (xy 198.12 69.85) (xy 168.91 69.85)
        (xy 168.91 92.71) (xy 125.73 92.71) (xy 125.73 69.85) (xy 80.01 69.85) (xy 80.01 52.07)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 214.63 52.07) (xy 214.63 69.85) (xy 168.91 69.85) (xy 168.91 92.71) (xy 125.73 92.71)
        (xy 125.73 69.85) (xy 80.01 69.85) (xy 80.01 52.07)
      )
    )
  )
  (zone (net 1) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.73 92.71) (xy 125.73 69.85) (xy 80.01 69.85) (xy 80.01 52.07) (xy 214.63 52.07)
        (xy 214.63 69.85) (xy 168.91 69.85) (xy 168.91 92.71)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.73 92.71) (xy 125.73 69.85) (xy 80.01 69.85) (xy 80.01 52.07) (xy 214.63 52.07)
        (xy 214.63 69.85) (xy 168.91 69.85) (xy 168.91 92.71)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.12 69.85) (xy 198.12 65.024) (xy 202.438 65.024) (xy 202.438 62.23) (xy 205.232 62.23)
        (xy 205.232 65.024) (xy 206.502 65.024) (xy 206.502 56.642) (xy 208.407 56.642) (xy 208.407 59.309)
        (xy 210.693 59.309) (xy 210.693 56.642) (xy 214.63 56.642) (xy 214.63 56.896) (xy 214.63 69.85)
        (xy 198.501 69.85)
      )
    )
  )
)
