(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "DripDrop")
    (date "2022-07-04")
    (rev "1")
    (company "Marcin Kucharczyk")
    (comment 1 "github.com/quhar/dripdrop")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.1016)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J1-Pad6)")
  (net 6 "Net-(J1-Pad8)")
  (net 7 "Net-(J2-Pad1)")
  (net 8 "Net-(J2-Pad2)")
  (net 9 "+5V")
  (net 10 "GND")
  (net 11 "Net-(J7-Pad3)")
  (net 12 "3.3V")
  (net 13 "Net-(J6-Pad1)")
  (net 14 "Net-(Q1-Pad1)")
  (net 15 "Net-(Q2-Pad1)")
  (net 16 "SCL")
  (net 17 "GPIO17")
  (net 18 "SDA")
  (net 19 "GPIO16")
  (net 20 "unconnected-(U1-Pad2)")
  (net 21 "unconnected-(U1-Pad16)")
  (net 22 "unconnected-(U1-Pad17)")
  (net 23 "unconnected-(U1-Pad18)")
  (net 24 "unconnected-(U1-Pad20)")
  (net 25 "unconnected-(U1-Pad21)")
  (net 26 "unconnected-(U1-Pad22)")
  (net 27 "unconnected-(U1-Pad24)")
  (net 28 "unconnected-(U1-Pad25)")
  (net 29 "unconnected-(U1-Pad29)")
  (net 30 "unconnected-(U1-Pad34)")
  (net 31 "unconnected-(U1-Pad35)")
  (net 32 "unconnected-(U2-Pad7)")
  (net 33 "unconnected-(U2-Pad8)")
  (net 34 "Net-(J1-Pad4)")
  (net 35 "Net-(J1-Pad7)")
  (net 36 "Net-(J7-Pad1)")
  (net 37 "Net-(J8-Pad2)")
  (net 38 "Net-(J8-Pad3)")
  (net 39 "Net-(J8-Pad4)")
  (net 40 "Net-(J8-Pad5)")
  (net 41 "Net-(J8-Pad6)")
  (net 42 "Net-(J8-Pad7)")
  (net 43 "Net-(J8-Pad8)")
  (net 44 "Net-(J8-Pad9)")
  (net 45 "Net-(J9-Pad3)")
  (net 46 "Net-(J9-Pad2)")
  (net 47 "Net-(J3-Pad2)")
  (net 48 "Net-(J3-Pad3)")
  (net 49 "Net-(U1-Pad5)")
  (net 50 "Net-(U1-Pad10)")
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 97.282 104.1654)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 123.19 75.184 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -2.54 0 180) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 9 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 18 "SDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-323_SC-70_Handsoldering" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 134.4653 93.3552 90)
    (descr "SOT-323, SC-70 Handsoldering")
    (tags "SOT-323 SC-70 Handsoldering")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q2" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "2N7002" (at 0 2.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -1.33 -0.65) (size 0.45 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(Q2-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at -1.33 0.65) (size 0.45 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect (at 1.33 0) (size 0.45 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(J9-Pad3)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A429)
    (at 130.9266 88.5956 90)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 2.4134 2.4234 180) (layer "F.SilkS"))
    (fp_text value "Garage remote" (at 0 7.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "3.3V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J9-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J9-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-2-2.54_1x02_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5B294F98)
    (at 93.5228 66.421 -90)
    (descr "Terminal Block Phoenix MPT-0,5-2-2.54, 2 pins, pitch 2.54mm, size 5.54x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-2-2.54 pitch 2.54mm size 5.54x6.2mm^2 drill 1.1mm pad 2.2mm")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 3.8608 -4.064) (layer "F.SilkS"))
    (fp_text value "WH Termistor" (at 1.27 4.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 2.54 2.54 270) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 2.54 270) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-2-2.54_1x02_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 134.4418 96.2508)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0.9656 1.6662) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 15 "Net-(Q2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 10 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 130.5385 96.2367)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0.955 1.6995) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 14 "Net-(Q1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 10 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 97.282 60.96)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 98.7806 67.3608 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -0.0254 -1.905 180) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 7 "Net-(J2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 10 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 91.6786 98.8618 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 -2.3468 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x08_Male" (at 1.27 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 3.81) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-2-2.54_1x02_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5B294F98)
    (at 132.5626 72.263 90)
    (descr "Terminal Block Phoenix MPT-0,5-2-2.54, 2 pins, pitch 2.54mm, size 5.54x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-2-2.54 pitch 2.54mm size 5.54x6.2mm^2 drill 1.1mm pad 2.2mm")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at 5.08 0 180) (layer "F.SilkS"))
    (fp_text value "Door open reed" (at 1.27 4.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 2.54 2.54 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 2.54 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(J6-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-2-2.54_1x02_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 123.19 68.834 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at -2.3622 0.0254 180) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 16 "SCL") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 9 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.794 98.933 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -2.3876 0.0508 180) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 17 "GPIO17") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 14 "Net-(Q1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "qhr:NodeMCU 32S" (layer "F.Cu")
    (tedit 0)
    (at 114.8888 82.436)
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -5.4148 -14.618 unlocked) (layer "F.SilkS"))
    (fp_text value "NodeMCU_32s" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -11.43 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "3.3V") (pinfunction "3.3V") (pintype "power_in"))
    (pad "2" thru_hole circle (at -11.43 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "unconnected-(U1-Pad2)") (pinfunction "EN") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at -11.43 -17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)") (pinfunction "SVP") (pintype "passive"))
    (pad "4" thru_hole circle (at -11.43 -15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)") (pinfunction "SVN") (pintype "passive"))
    (pad "5" thru_hole circle (at -11.43 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 49 "Net-(U1-Pad5)") (pinfunction "P34") (pintype "passive"))
    (pad "6" thru_hole circle (at -11.43 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 47 "Net-(J3-Pad2)") (pinfunction "P35") (pintype "passive"))
    (pad "7" thru_hole circle (at -11.43 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)") (pinfunction "P32") (pintype "passive"))
    (pad "8" thru_hole circle (at -11.43 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad4)") (pinfunction "P33") (pintype "passive"))
    (pad "9" thru_hole circle (at -11.43 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)") (pinfunction "P25") (pintype "passive"))
    (pad "10" thru_hole circle (at -11.43 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 50 "Net-(U1-Pad10)") (pinfunction "P26") (pintype "passive"))
    (pad "11" thru_hole circle (at -11.43 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 48 "Net-(J3-Pad3)") (pinfunction "P27") (pintype "passive"))
    (pad "12" thru_hole circle (at -11.43 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad6)") (pinfunction "P14") (pintype "passive"))
    (pad "13" thru_hole circle (at -11.43 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad5)") (pinfunction "P12") (pintype "passive"))
    (pad "14" thru_hole circle (at -11.43 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "15" thru_hole circle (at -11.43 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad2)") (pinfunction "P13") (pintype "passive"))
    (pad "16" thru_hole circle (at -11.43 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 "unconnected-(U1-Pad16)") (pinfunction "SD2") (pintype "passive+no_connect"))
    (pad "17" thru_hole circle (at -11.43 17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 "unconnected-(U1-Pad17)") (pinfunction "SD3") (pintype "passive+no_connect"))
    (pad "18" thru_hole circle (at -11.43 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "unconnected-(U1-Pad18)") (pinfunction "CMD") (pintype "passive+no_connect"))
    (pad "19" thru_hole circle (at -11.43 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "+5V") (pinfunction "5V") (pintype "power_in"))
    (pad "20" thru_hole circle (at 11.43 22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "unconnected-(U1-Pad20)") (pinfunction "CLK") (pintype "passive+no_connect"))
    (pad "21" thru_hole circle (at 11.43 20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "unconnected-(U1-Pad21)") (pinfunction "SD0") (pintype "passive+no_connect"))
    (pad "22" thru_hole circle (at 11.43 17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 "unconnected-(U1-Pad22)") (pinfunction "SD1") (pintype "passive+no_connect"))
    (pad "23" thru_hole circle (at 11.43 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(J1-Pad7)") (pinfunction "P15") (pintype "passive"))
    (pad "24" thru_hole circle (at 11.43 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "unconnected-(U1-Pad24)") (pinfunction "P2") (pintype "passive+no_connect"))
    (pad "25" thru_hole circle (at 11.43 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "unconnected-(U1-Pad25)") (pinfunction "P0") (pintype "passive+no_connect"))
    (pad "26" thru_hole circle (at 11.43 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad8)") (pinfunction "P4") (pintype "passive"))
    (pad "27" thru_hole circle (at 11.43 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "GPIO16") (pinfunction "P16") (pintype "passive"))
    (pad "28" thru_hole circle (at 11.43 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "GPIO17") (pinfunction "P17") (pintype "passive"))
    (pad "29" thru_hole circle (at 11.43 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "unconnected-(U1-Pad29)") (pinfunction "P5") (pintype "passive+no_connect"))
    (pad "30" thru_hole circle (at 11.43 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(J7-Pad1)") (pinfunction "P18") (pintype "passive"))
    (pad "31" thru_hole circle (at 11.43 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(J7-Pad3)") (pinfunction "P19") (pintype "passive"))
    (pad "32" thru_hole circle (at 11.43 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "33" thru_hole circle (at 11.43 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "SDA") (pinfunction "P21") (pintype "passive"))
    (pad "34" thru_hole circle (at 11.43 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "unconnected-(U1-Pad34)") (pinfunction "RX") (pintype "passive+no_connect"))
    (pad "35" thru_hole circle (at 11.43 -15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "unconnected-(U1-Pad35)") (pinfunction "TX") (pintype "passive+no_connect"))
    (pad "36" thru_hole circle (at 11.43 -17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "SCL") (pinfunction "P22") (pintype "passive"))
    (pad "37" thru_hole circle (at 11.43 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(J6-Pad1)") (pinfunction "P23") (pintype "passive"))
    (pad "38" thru_hole circle (at 11.43 -22.86) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "GND") (pinfunction "GND") (pintype "power_in"))
  )
  (footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-4-2.54_1x04_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5B294F98)
    (at 93.4974 73.0708 -90)
    (descr "Terminal Block Phoenix MPT-0,5-4-2.54, 4 pins, pitch 2.54mm, size 10.6x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-4-2.54 pitch 2.54mm size 10.6x6.2mm^2 drill 1.1mm pad 2.2mm")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 3.81 -4.16) (layer "F.SilkS"))
    (fp_text value "Ultrasonic Sensor" (at 3.81 4.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 2 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 49 "Net-(U1-Pad5)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 50 "Net-(U1-Pad10)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole rect (at 7.62 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "+5V") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-4-2.54_1x04_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 118.872 98.298 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 9 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 10 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 116.078 71.628)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 9 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 10 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-323_SC-70_Handsoldering" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 130.5385 93.3411 90)
    (descr "SOT-323, SC-70 Handsoldering")
    (tags "SOT-323 SC-70 Handsoldering")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "2N7002" (at 0 2.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -1.33 -0.65) (size 0.45 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(Q1-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at -1.33 0.65) (size 0.45 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect (at 1.33 0) (size 0.45 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(J9-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5B294F98)
    (at 132.6388 82.8548 90)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J7" (at 7.6962 -0.0254 180) (layer "F.SilkS"))
    (fp_text value "Door closed reed" (at 2.54 4.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 2 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 5.08 2.54 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 2.54 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 2.54 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 "Net-(J7-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(J7-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-4-2.54_1x04_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5B294F98)
    (at 93.4974 84.7802 -90)
    (descr "Terminal Block Phoenix MPT-0,5-4-2.54, 4 pins, pitch 2.54mm, size 10.6x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-4-2.54 pitch 2.54mm size 10.6x6.2mm^2 drill 1.1mm pad 2.2mm")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 3.81 -4.16 180) (layer "F.SilkS"))
    (fp_text value "Ultrasonic Sensor" (at 3.81 4.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 2 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 "Net-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 48 "Net-(J3-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole rect (at 7.62 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "+5V") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-4-2.54_1x04_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 133.7056 98.9584 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at -2.3368 0.0254) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 19 "GPIO16") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 15 "Net-(Q2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 132.5372 104.1654)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "" (at 0.4826 -13.1064) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 132.5372 62.103)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "" (at 0.4826 -13.1064) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "digikey-footprints:Barrel_Jack_5.5mmODx2.1mmID_PJ-102A" (layer "B.Cu")
    (tedit 5CAD146F)
    (at 115.824 99.774)
    (property "Category" "Connectors, Interconnects")
    (property "DK_Datasheet_Link" "https://www.cui.com/product/resource/digikeypdf/pj-202a.pdf")
    (property "DK_Detail_Page" "/product-detail/en/cui-inc/PJ-202A/CP-202A-ND/252007")
    (property "Description" "CONN PWR JACK 2X5.5MM KINKED PIN")
    (property "Digi-Key_PN" "CP-202A-ND")
    (property "Family" "Barrel - Power Connectors")
    (property "MPN" "PJ-202A")
    (property "Manufacturer" "CUI Inc.")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "J4" (at 0 12.1 180) (layer "B.SilkS"))
    (fp_text value "PJ-202A" (at 0 -5.8 180) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 -3) (size 2.6 2) (drill oval 1.6 1) (layers *.Cu *.Mask)
      (net 9 "+5V") (pintype "passive"))
    (pad "2" thru_hole rect locked (at 0 3) (size 2.6 2) (drill oval 1.6 1) (layers *.Cu *.Mask)
      (net 10 "GND") (pintype "passive"))
    (pad "3" thru_hole rect locked (at -4.7 0) (size 2 2.6) (drill oval 1 1.6) (layers *.Cu *.Mask)
      (net 10 "GND") (pintype "passive"))
  )
  (footprint "Package_DIP:DIP-18_W7.62mm" (layer "B.Cu")
    (tedit 5A02E8C5)
    (at 119.878 71.638 180)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 2.33) (layer "B.SilkS"))
    (fp_text value "MCP23008-xP" (at 3.81 -22.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 -10.16) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "SCL") (pinfunction "SCL") (pintype "input"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "GND") (pinfunction "A2") (pintype "input"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "GND") (pinfunction "A1") (pintype "input"))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "GND") (pinfunction "A0") (pintype "input"))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "+5V") (pinfunction "~{RESET}") (pintype "input"))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "unconnected-(U2-Pad7)") (pinfunction "NC") (pintype "no_connect"))
    (pad "8" thru_hole oval (at 0 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "unconnected-(U2-Pad8)") (pinfunction "INT") (pintype "output+no_connect"))
    (pad "9" thru_hole oval (at 0 -20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "10" thru_hole oval (at 7.62 -20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(J8-Pad2)") (pinfunction "GP0") (pintype "bidirectional"))
    (pad "11" thru_hole oval (at 7.62 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(J8-Pad3)") (pinfunction "GP1") (pintype "bidirectional"))
    (pad "12" thru_hole oval (at 7.62 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(J8-Pad4)") (pinfunction "GP2") (pintype "bidirectional"))
    (pad "13" thru_hole oval (at 7.62 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(J8-Pad5)") (pinfunction "GP3") (pintype "bidirectional"))
    (pad "14" thru_hole oval (at 7.62 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(J8-Pad6)") (pinfunction "GP4") (pintype "bidirectional"))
    (pad "15" thru_hole oval (at 7.62 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(J8-Pad7)") (pinfunction "GP5") (pintype "bidirectional"))
    (pad "16" thru_hole oval (at 7.62 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(J8-Pad8)") (pinfunction "GP6") (pintype "bidirectional"))
    (pad "17" thru_hole oval (at 7.62 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(J8-Pad9)") (pinfunction "GP7") (pintype "bidirectional"))
    (pad "18" thru_hole rect (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-18_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 107.696 94.488)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (property "Sheetfile" "dripdrop.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at 0 2.33 180) (layer "B.SilkS"))
    (fp_text value "Relay module" (at 0 -25.19 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -11.43 270) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J8-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J8-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J8-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J8-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J8-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J8-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J8-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J8-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole rect (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "+5V") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 137.922 57.3024) (end 137.922 108.204) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 88.13 108.204) (end 88.13 57.3024) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 123.952 66.04) (end 105.6894 66.04) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 105.6894 57.3024) (end 88.13 57.3024) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 137.922 108.204) (end 88.13 108.204) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 123.952 57.3024) (end 123.952 66.04) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 123.952 57.3024) (end 137.922 57.3024) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 105.6894 66.04) (end 105.6894 57.3024) (layer "Edge.Cuts") (width 0.1))
  (gr_text "1" (at 110.236 89.408) (layer "B.SilkS"))
  (gr_text "2" (at 110.236 86.868) (layer "B.SilkS"))
  (gr_text "7" (at 110.236 74.168) (layer "B.SilkS"))
  (gr_text "5" (at 110.236 79.248) (layer "B.SilkS"))
  (gr_text "github.com/quhar/dripdrop\nMarcin Kucharczyk" (at 90.424 81.534 -90) (layer "B.SilkS"))
  (gr_text "6" (at 110.236 76.708) (layer "B.SilkS"))
  (gr_text "0" (at 110.236 91.948) (layer "B.SilkS"))
  (gr_text "5V" (at 110.236 71.628) (layer "B.SilkS"))
  (gr_text "4" (at 110.236 81.788) (layer "B.SilkS"))
  (gr_text "3" (at 110.236 84.328) (layer "B.SilkS"))
  (gr_text "GND" (at 110.744 94.488) (layer "B.SilkS"))
  (gr_text "E" (at 89.3064 75.5904 90) (layer "F.SilkS"))
  (gr_text "NO" (at 128.524 82.804) (layer "F.SilkS"))
  (gr_text "3.3V" (at 131.064 90.678) (layer "F.SilkS"))
  (gr_text "GND" (at 89.3064 72.9488 90) (layer "F.SilkS"))
  (gr_text "NC" (at 128.524 77.724) (layer "F.SilkS"))
  (gr_text "T" (at 89.3064 89.8906 90) (layer "F.SilkS"))
  (gr_text "33" (at 94.234 94.488) (layer "F.SilkS"))
  (gr_text "39" (at 91.694 94.488) (layer "F.SilkS"))
  (gr_text "5V" (at 89.3064 92.4052 90) (layer "F.SilkS"))
  (gr_text "36" (at 91.694 100.838) (layer "F.SilkS"))
  (gr_text "14" (at 96.774 94.488) (layer "F.SilkS"))
  (gr_text "4" (at 99.314 94.488) (layer "F.SilkS"))
  (gr_text "C" (at 128.524 80.264) (layer "F.SilkS"))
  (gr_text "5V" (at 89.3064 80.6704 90) (layer "F.SilkS"))
  (gr_text "B" (at 133.604 90.678) (layer "F.SilkS"))
  (gr_text "12" (at 96.7886 100.838) (layer "F.SilkS"))
  (gr_text "GND" (at 135.89 90.678) (layer "F.SilkS"))
  (gr_text "GND" (at 89.281 84.6582 90) (layer "F.SilkS"))
  (gr_text "T" (at 89.3064 78.1558 90) (layer "F.SilkS"))
  (gr_text "25" (at 94.234 100.838) (layer "F.SilkS"))
  (gr_text "15" (at 99.314 100.838) (layer "F.SilkS"))
  (gr_text "E" (at 89.3064 87.4776 90) (layer "F.SilkS"))
  (zone (net 10) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 145.542 115.57)
        (xy 84.074 115.062)
        (xy 86.868 55.118)
        (xy 144.272 54.864)
      )
    )
  )
  (zone (net 10) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.67 125.73)
        (xy 77.47 125.73)
        (xy 83.82 52.07)
        (xy 154.94 52.07)
      )
    )
  )
)
