<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="15.23" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="30.404" y2="0" width="0" layer="20"/>
<wire x1="30.404" y1="0" x2="30.404" y2="15.23" width="0" layer="20"/>
<wire x1="30.404" y1="15.23" x2="0" y2="15.23" width="0" layer="20"/>
<text>12v</text>
<text>RV-Project.Com 
PWM LED Dimmer
</text>
<text>V3.1    4/21/2019</text>
<text>GND</text>
<text>12v</text>
<text>GND</text>
<text>LED-</text>
<text>LED+</text>
<text>Order 2Oz Copper</text>
<hole x="1.905" y="1.905" drill="2.286"/>
<hole x="28.575" y="13.335" drill="2.286"/>
<text>12v</text>
<text>GND</text>
<text>LED-</text>
<text>LED+</text>
<text>12v</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="1206-RES">
</package>
</packages>
</library>
<library name="a-lib_SMD">
<description>All SMD Devices; Actives, Passives, Connectors</description>
<packages>
<package name="SOIC-8(.150MM)">
</package>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;SMA diode.&lt;br&gt;
Pad Size: 0.225"x0.07"</description>
</package>
<package name="SOT23-3">
<description>SMD MMBT2222, BAV90, etc.</description>
</package>
<package name="1206-CAP">
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="RVPROJECT_NEWLOGO_XSMALL">
</package>
</packages>
</library>
<library name="a-lib_Connectors">
<description>Thru-Hole Connectors (Connectors, Terminals)</description>
<packages>
<package name="1X01_HEADER">
<description>Drill: 0.039" dia</description>
</package>
</packages>
</library>
<library name="a-lib_Passives">
<description>Thru-Hole Passives (Resistors, Capacitors)</description>
<packages>
<package name="CT6EP">
<description>Copal CT6-6EP Trimmer Potentiometer</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R4" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="a-lib_SMD" package="SOIC-8(.150MM)" value=""/>
<element name="D2" library="a-lib_SMD" package="SMA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="a-lib_SMD" package="SMA-DIODE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="a-lib_SMD" package="SOT23-3" value="">
<attribute name="PARTNO" value="MBT2222"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="a-lib_SMD" package="1206-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="a-lib_SMD" package="1206-CAP" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TB1" library="a-lib_Connectors" package="1X01_HEADER" value="">
<attribute name="VALUE"/>
</element>
<element name="TB2" library="a-lib_Connectors" package="1X01_HEADER" value="">
<attribute name="VALUE"/>
</element>
<element name="TB4" library="a-lib_Connectors" package="1X01_HEADER" value="">
<attribute name="VALUE"/>
</element>
<element name="TB5" library="a-lib_Connectors" package="1X01_HEADER" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="a-lib_Passives" package="CT6EP" value="">
<attribute name="NAME"/>
</element>
<element name="TB3" library="a-lib_Connectors" package="1X01_HEADER" value="">
<attribute name="VALUE"/>
</element>
<element name="TB6" library="a-lib_Connectors" package="1X01_HEADER" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="a-lib_Asthetics" package="RVPROJECT_NEWLOGO_XSMALL" value=""/>
<element name="C3" library="a-lib_SMD" package="1206-CAP" value="1nF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="P$1"/>
<contactref element="Q1" pad="2"/>
<contactref element="TB2" pad="1"/>
<contactref element="TB3" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="P$8"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="P$4"/>
<contactref element="TB4" pad="1"/>
<contactref element="TB1" pad="1"/>
<contactref element="TB6" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="A"/>
<contactref element="R1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="D3" pad="C"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="P$6"/>
<contactref element="U1" pad="P$2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="P$5"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="P$3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R4" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="Q1" pad="3"/>
<contactref element="TB5" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="D3" pad="A"/>
<contactref element="D2" pad="C"/>
<contactref element="U1" pad="P$7"/>
<contactref element="R3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
