(kicad_pcb (version 20171130) (host pcbnew 5.0.2-4.fc29)
  (general
    (thickness 1.6)
    (drawings 28)
    (tracks 14)
    (zones 0)
    (modules 10)
    (nets 8)
  )
  (page A4)
  (layers
    (0 Top signal hide)
    (31 Bottom signal hide)
    (33 F.Adhes user hide)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.781)
    (user_trace_width 0.1524)
    (user_trace_width 0.3)
    (user_trace_width 0.781)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.1)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.6 2.6)
    (pad_drill 1.3)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 78.74 66.04)
    (grid_origin 78.74 66.04)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /D0)
  (net 2 /D1)
  (net 3 GND)
  (net 4 VCC)
  (net 5 "Net-(J2-Pad2)")
  (net 6 "Net-(D0-R1-Pad1)")
  (net 7 "Net-(D1-R1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_gap 0.2286)
    (diff_pair_width 0.1524)
    (add_net /D0)
    (add_net /D1)
    (add_net "Net-(D0-R1-Pad1)")
    (add_net "Net-(D1-R1-Pad1)")
    (add_net "Net-(J2-Pad2)")
  )
  (net_class PWR ""
    (clearance 0.254)
    (trace_width 0.3)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_gap 0.2286)
    (diff_pair_width 0.1524)
    (add_net GND)
    (add_net VCC)
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer Top) (tedit 5C5DB83C)
    (at 87.376 64.516)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.Fab))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer Top) (tedit 5C5DB812)
    (at 87.376 50.546)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.81) (layer F.Fab))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer Top) (tedit 5C5DB826)
    (at 97.282 50.546)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.Fab))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module OPL_Resistor:PR-D1.8_L3.3MM (layer Top) (tedit 5C54D99E)
    (at 92.075 62.738 180)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr virtual)
    (fp_text reference D0-R1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 1.5K (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.775 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 /D0))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 6 "Net-(D0-R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (offset (xyz -2.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OPL_Resistor:PR-D1.8_L3.3MM (layer Top) (tedit 5C54D9AD)
    (at 92.075 59.436)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr virtual)
    (fp_text reference D0-R2 (at 0 0) (layer F.SilkS))
    (fp_text value 560 (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 -1.775) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 /D0))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (offset (xyz -2.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OPL_Resistor:PR-D1.8_L3.3MM (layer Top) (tedit 5C54D9CD)
    (at 92.075 52.578 180)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr virtual)
    (fp_text reference D1-R1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 1.5K (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.775 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-R1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 /D1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (offset (xyz -2.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OPL_Resistor:PR-D1.8_L3.3MM (layer Top) (tedit 5C54D9B5)
    (at 92.075 55.626)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr virtual)
    (fp_text reference D1-R2 (at 0 0) (layer F.SilkS))
    (fp_text value 560 (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 -1.775) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 /D1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (offset (xyz -2.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-05A_1x05_P2.54mm_Vertical (layer Top) (tedit 5B78013E)
    (at 82.042 62.738 90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-05A example for new part number: 22-27-2051, 5 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J2 (at 9.398 4.826 90) (layer F.SilkS))
    (fp_text value Conn_01x05_Female (at 5.08 4.08 90) (layer F.Fab))
    (fp_text user %R (at 5.08 -2.22 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 1 /D0))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 5 thru_hole oval (at 10.16 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 /D1))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-05A_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer Top) (tedit 5C5DB833)
    (at 97.282 64.516)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.Fab))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type086_RT03404HBLC_1x04_P3.81mm_Horizontal (layer Top) (tedit 5C5DC1EE)
    (at 102.616 63.246 90)
    (descr "terminal block Metz Connect Type086_RT03404HBLC, 4 pins, pitch 3.81mm, size 15.1x7.3mm^2, drill diamater 0.7mm, pad diameter 1.4mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_310861_RT034xxHBLC_OFF-026114K.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type086_RT03404HBLC pitch 3.81mm size 15.1x7.3mm^2 drill 0.7mm pad 1.4mm")
    (fp_text reference J1 (at 9.906 -4.572 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x04 (at 5.715 4.66 90) (layer F.Fab))
    (fp_text user %R (at 5.715 2.4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(D0-R1-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-R1-Pad1)"))
    (pad 3 thru_hole circle (at 7.62 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole circle (at 11.43 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type086_RT03404HBLC_1x04_P3.81mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /usr/share/kicad/modules/TerminalBlock_MetzConnect.pretty/TerminalBlock_MetzConnect_Type086_RT03404HBLC_1x04_P3.81mm_Horizontal.kicad_mod
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MC_1,5_4-G-3.81_1x04_P3.81mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 80.01 57.658 270) (layer B.SilkS))
  (gr_text D0 (at 80.01 62.738 270) (layer B.SilkS))
  (gr_text D1 (at 80.01 52.705 270) (layer B.SilkS))
  (gr_text VCC (at 80.01 55.118 270) (layer B.SilkS))
  (gr_text GND (at 100.33 55.626 270) (layer B.SilkS))
  (gr_text D1 (at 100.33 59.436 270) (layer B.SilkS))
  (gr_text D0 (at 100.33 63.246 270) (layer B.SilkS))
  (gr_text VCC (at 100.33 51.816 270) (layer B.SilkS))
  (gr_text GND (at 85.598 57.658 90) (layer F.SilkS))
  (gr_text VCC (at 85.598 55.118 90) (layer F.SilkS))
  (gr_text D1 (at 85.598 52.705 90) (layer F.SilkS))
  (gr_text D0 (at 85.598 62.738 90) (layer F.SilkS))
  (gr_text VCC (at 100.33 51.816 90) (layer F.SilkS))
  (gr_text GND (at 100.33 55.626 90) (layer F.SilkS))
  (gr_text D1 (at 100.33 59.436 90) (layer F.SilkS))
  (gr_text D0 (at 100.33 63.246 90) (layer F.SilkS))
  (gr_text INPUT (at 98.044 58.166 90) (layer F.SilkS))
  (gr_text OUTPUT (at 86.868 58.166 90) (layer F.SilkS))
  (gr_line (start 78.74 66.04) (end 78.74 50.8) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 106.68 49.022) (end 106.68 50.8) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 78.74 49.022) (end 106.68 49.022) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 106.68 66.04) (end 78.74 66.04) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 78.74 49.022) (end 78.74 50.8) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 106.68 50.8) (end 106.68 66.04) (layer Edge.Cuts) (width 0.2))
  (gr_text "5v -> 3.3v\nR1: 680Ω R2:1.2KΩ" (at 86.106 57.912 270) (layer B.SilkS))
  (gr_text "12v -> 5v\nR1: 1.2KΩ R2:820Ω" (at 91.948 57.912 270) (layer B.SilkS))
  (gr_text "12v -> 3.3v\nR1: 1.5KΩ R2:560Ω" (at 96.774 57.658 270) (layer B.SilkS))
  (gr_text "makerspace auth\nvoltage divider" (at 105.41 57.15 270) (layer B.SilkS))
  (zone (net 3) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.994 49.276) (xy 78.994 65.786) (xy 106.426 65.786) (xy 106.426 49.276)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.994 49.276) (xy 78.994 65.786) (xy 106.426 65.786) (xy 106.426 49.276)
      )
    )
  )
)
