(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 273)
    (zones 0)
    (modules 74)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.4)
    (user_trace_width 0.609)
    (user_trace_width 0.8)
    (user_trace_width 1.5)
    (user_trace_width 2.5)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 1.3)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 110.04 93.02)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C13-Pad2)")
  (net 3 "Net-(J3-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad2)")
  (net 6 "Net-(C12-Pad1)")
  (net 7 "Net-(C1-Pad2)")
  (net 8 "Net-(C3-Pad2)")
  (net 9 "Net-(C4-Pad1)")
  (net 10 "Net-(C5-Pad1)")
  (net 11 "Net-(J1-Pad1)")
  (net 12 "Net-(J2-Pad1)")
  (net 13 "Net-(J4-Pad1)")
  (net 14 "Net-(JP1-Pad2)")
  (net 15 "Net-(JP2-Pad2)")
  (net 16 "Net-(JP3-Pad2)")
  (net 17 "Net-(JP4-Pad2)")
  (net 18 "Net-(JP5-Pad2)")
  (net 19 "Net-(JP6-Pad2)")
  (net 20 "Net-(J6-Pad1)")
  (net 21 "Net-(J10-Pad1)")
  (net 22 "Net-(J11-Pad1)")
  (net 23 "Net-(J6-Pad3)")
  (net 24 "Net-(J9-Pad1)")
  (net 25 "Net-(J12-Pad1)")
  (net 26 "Net-(R11-Pad2)")
  (net 27 "Net-(R10-Pad1)")
  (net 28 "Net-(R15-Pad1)")
  (net 29 "Net-(R16-Pad1)")
  (net 30 "Net-(R19-Pad2)")
  (net 31 "Net-(R20-Pad2)")
  (net 32 "Net-(C2-Pad2)")
  (net 33 "Net-(C5-Pad2)")
  (net 34 "Net-(C6-Pad1)")
  (net 35 "Net-(C6-Pad2)")
  (net 36 "Net-(C11-Pad1)")
  (net 37 "Net-(C10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R20-Pad2)")
  )
  (net_class SMD ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (net_class grounds ""
    (clearance 0.254)
    (trace_width 1)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
  )
  (net_class power ""
    (clearance 0.254)
    (trace_width 1)
    (via_dia 0.762)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (net_class signal ""
    (clearance 0.2)
    (trace_width 0.6096)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(JP3-Pad2)")
    (add_net "Net-(JP4-Pad2)")
    (add_net "Net-(JP5-Pad2)")
    (add_net "Net-(JP6-Pad2)")
  )
  (net_class soic ""
    (clearance 0.1524)
    (trace_width 0.4)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (module SMC_generic:DIPSO_Socket_LOMC (layer F.Cu) (tedit 5F6BBF75)
    (at 109.79 82.02 270)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U1 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value OPA1656 (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user 1 (at 5.71 -0.44 180 unlocked) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 1.905 3.3 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 2 "Net-(C13-Pad2)"))
    (pad 8 thru_hole circle (at 5.715 4.3 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 36 "Net-(C11-Pad1)"))
    (pad 6 thru_hole circle (at 3.5 5.08 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 10 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 4 2.54 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 4 "Net-(C3-Pad1)"))
    (pad 8 smd roundrect (at 5.715 6.535 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C11-Pad1)"))
    (pad 7 smd roundrect (at 4.445 6.535 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(C5-Pad2)"))
    (pad 6 smd roundrect (at 3.175 6.535 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C5-Pad1)"))
    (pad 5 smd roundrect (at 1.905 6.535 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(R15-Pad1)"))
    (pad 4 smd roundrect (at 1.905 1.085 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C13-Pad2)"))
    (pad 3 smd roundrect (at 3.175 1.085 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C1-Pad2)"))
    (pad 2 smd roundrect (at 4.445 1.085 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C3-Pad1)"))
    (pad 1 smd roundrect (at 5.715 1.085 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C3-Pad2)"))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(C11-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C13-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(C5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C1-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R15-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:DIPSO_Socket_LOMC (layer F.Cu) (tedit 5F6BBF75)
    (at 69.39 82.07 270)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U2 (at 3.81 9.8 90) (layer F.SilkS))
    (fp_text value OPA1656 (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user 1 (at 5.71 -0.44 180 unlocked) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 1.905 3.3 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 37 "Net-(C10-Pad1)"))
    (pad 8 thru_hole circle (at 5.715 4.3 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 6 "Net-(C12-Pad1)"))
    (pad 6 thru_hole circle (at 3.5 5.08 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 34 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 4 2.54 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 9 "Net-(C4-Pad1)"))
    (pad 8 smd roundrect (at 5.715 6.535 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C12-Pad1)"))
    (pad 7 smd roundrect (at 4.445 6.535 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(C6-Pad2)"))
    (pad 6 smd roundrect (at 3.175 6.535 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(C6-Pad1)"))
    (pad 5 smd roundrect (at 1.905 6.535 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(R16-Pad1)"))
    (pad 4 smd roundrect (at 1.905 1.085 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(C10-Pad1)"))
    (pad 3 smd roundrect (at 3.175 1.085 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C2-Pad2)"))
    (pad 2 smd roundrect (at 4.445 1.085 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C4-Pad1)"))
    (pad 1 smd roundrect (at 5.715 1.085 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C4-Pad2)"))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C12-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C10-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(C2-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C4-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R16-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 129.79 105.77 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J13 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value gnd (at 0 2.25 90) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 47.09 112.37 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP6 (at -0.2 -2.4 180) (layer F.Fab))
    (fp_text value 0dB (at 0 -2.3) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(JP6-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W4.5mm_P5.00mm_Wima (layer F.Cu) (tedit 5D533F69)
    (at 61.59 94.57)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (fp_text reference C6 (at -2 0 270) (layer F.SilkS))
    (fp_text value 100p (at 2.5 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.7))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 124.99 80.17 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5 2 180) (layer F.SilkS))
    (fp_text value 75k (at 5.25 -0.05) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 59.99 104.27 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 11.7 0) (layer F.SilkS))
    (fp_text value 3k9 (at 5 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C6-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 111.59 104.17 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 11.8 0) (layer F.SilkS))
    (fp_text value 3k9 (at 5.08 -0.1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 104.99 94.57)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C7 (at 7 0 270) (layer F.SilkS))
    (fp_text value 100n (at 2.3 0 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(C11-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 89.79 101.77 180)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C11 (at 2.9 -2.8 270) (layer F.SilkS))
    (fp_text value 10u (at -1.6 -0.1 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(C11-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 104.99 77.17)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C3 (at 7 0.2 270) (layer F.SilkS))
    (fp_text value 15n (at 2.5 0.1 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 95.79 83.27 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C15 (at 2.4 -3.4 90) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C13-Pad2)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(C11-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 89.79 95.52)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C17 (at -3 2.65 270) (layer F.SilkS))
    (fp_text value 10u (at 1.7 0.1 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 -1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C13-Pad2)"))
    (pad 1 thru_hole rect (at 0 1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(C11-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 122.39 74.37 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C1 (at 7.1 -0.05 270) (layer F.SilkS))
    (fp_text value 15n (at 2.35 -0.05 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C1-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 101.89 77.17 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C9 (at 7.1 0 270) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C13-Pad2)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 89.79 89.02 180)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C13 (at 3 -2.65 90) (layer F.SilkS))
    (fp_text value 10u (at -1.65 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 -1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C13-Pad2)"))
    (pad 1 thru_hole rect (at 0 1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 74.69 94.57 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C8 (at -2.1 0 270) (layer F.SilkS))
    (fp_text value 100n (at 2.3 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C12-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 81.79 101.77 180)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C12 (at -2.9 -2.8 90) (layer F.SilkS))
    (fp_text value 10u (at -1.7 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 -1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C12-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 69.69 77.17)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C4 (at 7.1 0 270) (layer F.SilkS))
    (fp_text value 15n (at 2.35 0.1 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C4-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 75.79 83.27 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C16 (at 2.5 3.5 90) (layer F.SilkS))
    (fp_text value 100n (at 2.4 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C12-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C10-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 81.79 95.52)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C18 (at 2.9 2.65 270) (layer F.SilkS))
    (fp_text value 10u (at 1.8 0.1 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C12-Pad1)"))
    (pad 2 thru_hole circle (at 0 -1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(C10-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 49.19 74.27)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C2 (at 7.1 0 270) (layer F.SilkS))
    (fp_text value 15n (at 2.6 -0.05 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 61.59 77.17)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C10 (at -2.05 0 270) (layer F.SilkS))
    (fp_text value 100n (at 2.45 0.1 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C10-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_5x11mm_Silmic (layer F.Cu) (tedit 5D587B39)
    (at 81.79 89.02 180)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C14 (at -2.9 -2.65 90) (layer F.SilkS))
    (fp_text value 10u (at 1.7 0.2 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(C10-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/cp_5x11mm_Silmic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 131.29 73.27 270)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 40.29 73.27 270)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 131.29 112.27 270)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 40.29 112.27 270)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 129.79 85.77)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J1 (at 0 -2.148) (layer F.Fab))
    (fp_text value In (at 2.3 0.9 90 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 41.79 85.77)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J9 (at 0 -2.148) (layer F.Fab))
    (fp_text value In (at -2.6 0.7 -90 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 "Net-(J9-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 129.79 101.02 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J2 (at 0 -2.148) (layer F.Fab))
    (fp_text value To (at -2.4 0 90 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 41.79 101.02 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J11 (at 0 -2.148) (layer F.Fab))
    (fp_text value To (at 2.5 0 -90 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "Net-(J11-Pad1)"))
  )
  (module SMC_generic:mkds_1,5-3 (layer F.Cu) (tedit 5F6753A1)
    (at 85.79 111.77)
    (descr "3-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J6 (at 0 -5.4) (layer F.Fab))
    (fp_text value Power (at 0 3.5) (layer F.SilkS))
    (pad 3 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J6-Pad3)"))
    (pad 1 thru_hole circle (at -5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J6-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (thermal_width 1))
    (model ${KIPRJMOD}/Lib/3D/pxc_1935174_03_PT-1-5-3-5-0-H_3D.stp
      (offset (xyz -30.09899954795837 -44.70399932861328 -38.86199941635132))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 90))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 95.09 114.37 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R29 (at 11.85 0) (layer F.SilkS))
    (fp_text value 10 (at 5.1 0.15 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J6-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 110.29 99.47 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R23 (at 11.9 0 270) (layer F.SilkS))
    (fp_text value 3k9 (at 4.9 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(C5-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 110.29 72.27 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 4.9 2.2) (layer F.SilkS))
    (fp_text value 75k (at 5.08 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 124.99 98.67 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R25 (at 5 2 180) (layer F.SilkS))
    (fp_text value 47 (at 5.05 -0.05) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(C5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 90.87 83.97 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.1 -2.2) (layer F.SilkS))
    (fp_text value 75k (at 5.1 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J9-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 114.83 84.87)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.16 -2 180) (layer F.SilkS))
    (fp_text value 75k (at 5 0.1) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 98.39 114.37 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R27 (at -1.6 0) (layer F.SilkS))
    (fp_text value 10 (at 5.2 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C13-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 114.83 89.57)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R17 (at 5.16 -2 180) (layer F.SilkS))
    (fp_text value 3k9 (at 5 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 76.49 114.37 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R28 (at 11.9 -0.1) (layer F.SilkS))
    (fp_text value 10 (at 5.3 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J6-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 71.49 99.47 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R24 (at -1.7 0 270) (layer F.SilkS))
    (fp_text value 3k9 (at 5.1 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C6-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 71.49 72.27 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 5.3 2.3) (layer F.SilkS))
    (fp_text value 75k (at 5 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C4-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 46.59 98.77)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R26 (at 5.1 -2) (layer F.SilkS))
    (fp_text value 47 (at 5.1 0.1) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 80.71 79.57)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5 2.1) (layer F.SilkS))
    (fp_text value 75k (at 4.8 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C4-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 56.79 84.87 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.1 2) (layer F.SilkS))
    (fp_text value 75k (at 5.2 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(C2-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 46.63 80.17)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.1 -2) (layer F.SilkS))
    (fp_text value 75k (at 4.86 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 73.19 114.37 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R30 (at -1.6 0) (layer F.SilkS))
    (fp_text value 10 (at 5.3 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C10-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 56.79 89.77 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R18 (at 5.1 2) (layer F.SilkS))
    (fp_text value 3k9 (at 5.2 0.1) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R16-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 124.49 104.37 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at 2.2 2.5 180) (layer F.Fab))
    (fp_text value "In | Out" (at 2.2 2) (layer F.SilkS))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(JP1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 47.09 104.57 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP4 (at -2.2 2.45 180) (layer F.Fab))
    (fp_text value "Out | In" (at -2.3 2) (layer F.SilkS))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(JP4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 119.49 109.87)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at 0 4.9 180) (layer F.Fab))
    (fp_text value 10dB (at 0 4.87) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(JP2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(JP1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 124.49 112.37 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP3 (at 0 -2.4) (layer F.Fab))
    (fp_text value 0dB (at 0 -2.4) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(JP3-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 52.09 109.87)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP5 (at -0.3 4.9 180) (layer F.Fab))
    (fp_text value 10dB (at 0 4.87) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(JP5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(JP4-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 114.89 114.37 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 11.9 0.05) (layer F.SilkS))
    (fp_text value 3k9 (at 5.25 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(JP1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 104.99 104.17 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R19 (at 11.8 0) (layer F.SilkS))
    (fp_text value 3k9 (at 4.95 0 270) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R19-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 108.29 104.17 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at -1.7 0.1) (layer F.SilkS))
    (fp_text value 3k9 (at 5 0.1 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(JP2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 101.69 114.37 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R21 (at 11.85 0.05) (layer F.SilkS))
    (fp_text value 3k9 (at 5.1 0.05 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R19-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 114.79 93.97)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R15 (at 5.2 -2 180) (layer F.SilkS))
    (fp_text value 3k9 (at 5.3 0.1) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R15-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(JP3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 56.69 114.47 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 11.9 0.1) (layer F.SilkS))
    (fp_text value 3k9 (at 5 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R10-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(JP4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 63.29 104.27 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R14 (at -1.7 0.1) (layer F.SilkS))
    (fp_text value 3k9 (at 5 0.1 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(JP5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 69.89 114.37 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R22 (at 11.9 0.1) (layer F.SilkS))
    (fp_text value 3k9 (at 4.95 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R20-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 56.79 94.37 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R16 (at 5.1 2) (layer F.SilkS))
    (fp_text value 3k9 (at 5.2 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R16-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(JP6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W4.5mm_P5.00mm_Wima (layer F.Cu) (tedit 5D533F69)
    (at 96.89 94.57)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (fp_text reference C5 (at -2.1 0.1 270) (layer F.SilkS))
    (fp_text value 100p (at 2.6 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(C5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.7))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 129.79 78.77 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J3 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value Rn/c (at 0 2.5 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(J3-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 41.79 78.77 270)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J12 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value Ln/c (at 0 2.5 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 "Net-(J12-Pad1)"))
  )
  (module SMC_generic:mkds_1,5-3 (layer F.Cu) (tedit 5F674A74)
    (at 85.79 73.77 180)
    (descr "3-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J7 (at 0 -5.4) (layer F.Fab))
    (fp_text value Power (at 0 3.5 180 unlocked) (layer F.SilkS))
    (pad 3 thru_hole circle (at 5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J6-Pad1)"))
    (pad 1 thru_hole circle (at -5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J6-Pad3)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/pxc_1935174_03_PT-1-5-3-5-0-H_3D.stp
      (offset (xyz -30.09899954795837 -44.70399932861328 -38.86199941635132))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 90))
    )
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 129.79 96.27 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J4 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value From (at 0 2.4 90) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 129.79 92.77 90)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J5 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value Out (at 1.3 2.3 90) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 41.79 92.77 270)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J8 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value Out (at -1.3 2.6 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 21 "Net-(J10-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 41.79 96.27 270)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J10 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value From (at 0.1 2.5 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 21 "Net-(J10-Pad1)"))
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 66.59 104.27 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R20 (at 11.7 0) (layer F.SilkS))
    (fp_text value 3k9 (at 5.2 -0.1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C6-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R20-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 41.79 105.77 270)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J14 (at 0 -2.148 90) (layer F.Fab))
    (fp_text value gnd (at 0 2.25 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_text -V (at 80.79 115.27) (layer B.SilkS))
  (gr_text -V (at 80.79 70.27 180) (layer B.SilkS))
  (gr_text +V (at 90.69 70.27 180) (layer B.SilkS))
  (gr_text +V (at 90.89 115.27) (layer B.SilkS))
  (gr_text "v1.1, Nov. 2020" (at 104.89 109.17 180) (layer B.SilkS))
  (gr_text "LOMC v1 Warp Filter" (at 66.69 109.27 180) (layer B.SilkS))
  (gr_text Left (at 37.69 89.07 270) (layer F.SilkS))
  (gr_text Right (at 133.69 88.97 90) (layer F.SilkS))
  (gr_text Switch (at 37.79 98.67 270) (layer F.SilkS))
  (gr_text Switch (at 133.69 98.67 90) (layer F.SilkS))
  (gr_text Filter (at 121.99 102.07) (layer F.SilkS))
  (gr_text Filter (at 49.59 102.27) (layer F.SilkS))
  (gr_text Gain (at 49.59 111.27 270) (layer F.SilkS))
  (gr_text Gain (at 121.99 111.37 270) (layer F.SilkS))
  (gr_text +V (at 90.79 106.77) (layer F.SilkS))
  (gr_text -V (at 80.89 106.77) (layer F.SilkS))
  (gr_text -V (at 76.54 72.02 180) (layer F.SilkS))
  (gr_text +V (at 95.29 71.77 180) (layer F.SilkS))
  (gr_line (start 35.79 116.77) (end 35.79 68.77) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.79 116.77) (end 35.79 116.77) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.79 68.77) (end 135.79 116.77) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 35.79 68.77) (end 135.79 68.77) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.29 69.27) (xy 95.29 69.27) (xy 87.39 77.27) (xy 87.39 107.77) (xy 84.19 107.77)
        (xy 84.19 77.27) (xy 76.29 69.27) (xy 36.29 69.27) (xy 36.29 116.27) (xy 135.29 116.27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35.79 76.77) (xy 41.79 76.77) (xy 43.79 74.77) (xy 43.79 68.77) (xy 35.79 68.77)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35.79 108.77) (xy 41.79 108.77) (xy 43.79 110.77) (xy 43.79 116.77) (xy 35.79 116.77)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.79 108.77) (xy 129.79 108.77) (xy 127.79 110.77) (xy 127.79 116.77) (xy 135.79 116.77)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.79 68.77) (xy 127.79 74.77) (xy 129.79 76.77) (xy 135.79 76.77) (xy 135.79 68.77)
      )
    )
  )
)
