(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A3")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x0001000_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "GND")
  (net 3 "Net-(C5-Pad1)")
  (net 4 "Net-(C6-Pad2)")
  (net 5 "/V_CAP")
  (net 6 "Net-(C9-Pad1)")
  (net 7 "Net-(C8-Pad1)")
  (net 8 "Net-(C10-Pad1)")
  (net 9 "/trigger_coil(+)")
  (net 10 "Net-(D1-Pad1)")
  (net 11 "Net-(D10-Pad3)")
  (net 12 "Net-(D11-Pad3)")
  (net 13 "Net-(D12-Pad3)")
  (net 14 "Net-(D13-Pad3)")
  (net 15 "Net-(D14-Pad3)")
  (net 16 "Net-(D15-Pad3)")
  (net 17 "Net-(D16-Pad3)")
  (net 18 "/HV_INPUT")
  (net 19 "Net-(D21-Pad1)")
  (net 20 "Net-(Q2-Pad1)")
  (net 21 "/trigger_coil(-)")
  (net 22 "Net-(R1-Pad1)")
  (net 23 "Net-(R2-Pad1)")
  (net 24 "Net-(R3-Pad1)")
  (net 25 "Net-(R4-Pad1)")
  (net 26 "Net-(R5-Pad1)")
  (net 27 "Net-(R6-Pad1)")
  (net 28 "Net-(R7-Pad1)")
  (net 29 "Net-(R8-Pad1)")
  (net 30 "Net-(D18-Pad1)")
  (net 31 "Net-(R30-Pad2)")
  (net 32 "/CAP_DISABLE")
  (net 33 "Net-(Q1-Pad2)")
  (net 34 "Net-(R39-Pad1)")
  (net 35 "Net-(R28-Pad2)")
  (net 36 "Net-(R29-Pad2)")
  (net 37 "Net-(R40-Pad2)")
  (net 38 "Net-(R45-Pad1)")
  (net 39 "Net-(J1-Pad1)")
  (net 40 "unconnected-(U4-Pad4)")
  (net 41 "unconnected-(U5-Pad3)")
  (net 42 "Net-(U6-Pad3)")
  (net 43 "Net-(U6-Pad5)")
  (net 44 "/K1")
  (net 45 "/K2")
  (net 46 "/K3")
  (net 47 "/K4")
  (net 48 "/K5")
  (net 49 "/K6")
  (net 50 "/K7")
  (net 51 "/K8")
  (net 52 "Net-(C10-Pad2)")
  (net 53 "Net-(C11-Pad1)")
  (net 54 "Net-(C13-Pad1)")
  (net 55 "/CAP_RDY")
  (net 56 "Net-(C14-Pad1)")
  (net 57 "Net-(R27-Pad1)")
  (net 58 "Net-(R33-Pad2)")
  (net 59 "Net-(R41-Pad1)")
  (net 60 "Net-(R42-Pad2)")
  (net 61 "Net-(R44-Pad2)")
  (net 62 "Net-(R46-Pad1)")
  (net 63 "Net-(R48-Pad1)")
  (footprint "Diode_THT:D_A-405_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 227.33 78.74)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D22" (at 3.81 -2.47) (layer "F.SilkS"))
    (fp_text value "10V" (at 3.81 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.2 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 56 "Net-(C14-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 135.89 91.44)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP6" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "K3" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 46 "/K3") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Package_DIP:DIP-8_W7.62mm_Socket" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 212.09 87.63)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at -0.254 -2.54) (layer "F.SilkS"))
    (fp_text value "TC4420" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(C14-Pad1)") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(C13-Pad1)") (pinfunction "INPUT") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "unconnected-(U5-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(R44-Pad2)") (pinfunction "OUTPUT") (pintype "output"))
    (pad "7" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(R44-Pad2)") (pinfunction "OUTPUT") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(C14-Pad1)") (pinfunction "VDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 63CA0401)
    (at 140.97 71.12)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at 0 -3.198) (layer "F.SilkS") hide)
    (fp_text value "G2" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.2) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "Net-(R2-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_THT:TO-247-3_Vertical" (layer "F.Cu")
    (tedit 63ACD78A)
    (at 83.82 135.89)
    (descr "TO-247-3, Vertical, RM 5.45mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html")
    (tags "TO-247-3 Vertical RM 5.45mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D14" (at 5.45 -3.45) (layer "F.SilkS"))
    (fp_text value "1.2kV SCR" (at 5.45 3.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.45 -3.45) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 49 "/K6") (pinfunction "K") (pintype "passive") (zone_connect 2))
    (pad "2" thru_hole oval locked (at 5.45 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 48 "/K5") (pinfunction "A") (pintype "passive") (clearance 1.8))
    (pad "3" thru_hole oval locked (at 10.9 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 15 "Net-(D14-Pad3)") (pinfunction "G") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-247-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 243.84 119.38 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C6" (at 2.5 -2.2 90) (layer "F.SilkS"))
    (fp_text value "1u" (at 2.5 2.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 101.6 152.4)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R15" (at 10.652 -3.08) (layer "F.SilkS"))
    (fp_text value "RP" (at 6.35 2.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 50 "/K7") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(D15-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 53.34 120.65)
    (descr "Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=22.86mm, 4W, length*diameter=18*9mm^2")
    (tags "Resistor Axial_DIN0918 series Axial Horizontal pin pitch 22.86mm 4W length 18mm diameter 9mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R22" (at 11.43 -5.62) (layer "F.SilkS"))
    (fp_text value "R_SHARE" (at 11.43 5.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.43 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 47 "/K4") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 22.86 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 48 "/K5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-247-3_Vertical" (layer "F.Cu")
    (tedit 63ACD790)
    (at 83.82 151.13)
    (descr "TO-247-3, Vertical, RM 5.45mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html")
    (tags "TO-247-3 Vertical RM 5.45mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D15" (at 5.45 -3.45) (layer "F.SilkS"))
    (fp_text value "1.2kV SCR" (at 5.45 3.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.45 -3.45) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 50 "/K7") (pinfunction "K") (pintype "passive") (zone_connect 2))
    (pad "2" thru_hole oval locked (at 5.45 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 49 "/K6") (pinfunction "A") (pintype "passive") (clearance 1.8))
    (pad "3" thru_hole oval locked (at 10.9 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 16 "Net-(D15-Pad3)") (pinfunction "G") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-247-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W6.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 255.27 68.58 -90)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 6mm Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C10" (at 7.5 -4.25 90) (layer "F.SilkS"))
    (fp_text value "0.47" (at 7.5 4.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 15 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 52 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W6.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3299W_Vertical" (layer "F.Cu")
    (tedit 5A3D4994)
    (at 228.6 69.85 180)
    (descr "Potentiometer, vertical, Bourns 3299W, https://www.bourns.com/pdfs/3299.pdf")
    (tags "Potentiometer vertical Bourns 3299W")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV2" (at -2.54 -3.16) (layer "F.SilkS"))
    (fp_text value "20k" (at -2.54 5.44) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 1.14) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(R48-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "/V_CAP") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3299W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Radial_D8.7mm_P5.00mm_Fastron_07HCP" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 252.73 93.98)
    (descr "Inductor, Radial series, Radial, pin pitch=5.00mm, , diameter=8.7mm, Fastron, 07HCP, http://cdn-reichelt.de/documents/datenblatt/B400/DS_07HCP.pdf")
    (tags "Inductor Radial series Radial pin pitch 5.00mm  diameter 8.7mm Fastron 07HCP")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L2" (at 2.5 -5.6) (layer "F.SilkS"))
    (fp_text value "47u" (at 2.5 5.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "+5V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(C10-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Radial_D8.7mm_P5.00mm_Fastron_07HCP.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tedit 63AC7B6D)
    (at 196.85 93.98 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Category" "Discrete Semiconductor Products")
    (property "DK_Datasheet_Link" "https://www.onsemi.com/pub/Collateral/FQP30N06L-D.pdf")
    (property "DK_Detail_Page" "/product-detail/en/on-semiconductor/FQP30N06L/FQP30N06L-ND/1055122")
    (property "Description" "MOSFET N-CH 60V 32A TO-220")
    (property "Digi-Key_PN" "FQP30N06L-ND")
    (property "Family" "Transistors - FETs, MOSFETs - Single")
    (property "MPN" "FQP30N06L")
    (property "Manufacturer" "ON Semiconductor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "Q2" (at 2.54 -4.27 90) (layer "F.SilkS"))
    (fp_text value "IRFB260NPbF" (at 2.54 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(Q2-Pad1)") (pinfunction "G") (pintype "bidirectional"))
    (pad "2" thru_hole oval locked (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "/trigger_coil(-)") (pinfunction "D") (pintype "bidirectional") (zone_connect 2))
    (pad "3" thru_hole oval locked (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "S") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L26.5mm_W11.5mm_P22.50mm_MKS4" (layer "F.Cu")
    (tedit 63CA047D)
    (at 201.93 55.88 -90)
    (descr "C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*11.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 22.50mm  length 26.5mm width 11.5mm Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C19" (at 11.25 -7 90) (layer "F.SilkS"))
    (fp_text value "2u2 Film" (at 11.25 7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "/trigger_coil(+)") (pintype "passive") (zone_connect 2))
    (pad "2" thru_hole circle locked (at 22.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L26.5mm_W11.5mm_P22.50mm_MKS4.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 207.391 94.742 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R41" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "100" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(R41-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(C13-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 130.81 106.68 180)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 6.35 -2.92 180) (layer "F.SilkS"))
    (fp_text value "RS" (at 6.35 2.92 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(D12-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 227.33 60.96)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R43" (at 10.414 0) (layer "F.SilkS"))
    (fp_text value "33k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(D21-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-247-3_Vertical" (layer "F.Cu")
    (tedit 63ACD76E)
    (at 83.82 90.17)
    (descr "TO-247-3, Vertical, RM 5.45mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html")
    (tags "TO-247-3 Vertical RM 5.45mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D11" (at 5.45 -3.45) (layer "F.SilkS"))
    (fp_text value "1.2kV SCR" (at 5.45 3.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.45 -3.45) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 46 "/K3") (pinfunction "K") (pintype "passive") (zone_connect 2))
    (pad "2" thru_hole oval locked (at 5.45 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 45 "/K2") (pinfunction "A") (pintype "passive") (clearance 1.8))
    (pad "3" thru_hole oval locked (at 10.9 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 12 "Net-(D11-Pad3)") (pinfunction "G") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-247-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 243.84 130.81 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R46" (at 3.81 0.105 90) (layer "F.SilkS"))
    (fp_text value "47" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(R46-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L26.5mm_W11.5mm_P22.50mm_MKS4" (layer "F.Cu")
    (tedit 63CA0484)
    (at 217.17 55.88 -90)
    (descr "C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*11.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 22.50mm  length 26.5mm width 11.5mm Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C18" (at 11.25 -7 90) (layer "F.SilkS"))
    (fp_text value "2u2 Film" (at 11.25 7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "/trigger_coil(+)") (pintype "passive") (zone_connect 2))
    (pad "2" thru_hole circle locked (at 22.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L26.5mm_W11.5mm_P22.50mm_MKS4.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 6351EF95)
    (at 109.22 57.15 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 10.16 1.524) (layer "F.SilkS"))
    (fp_text value "FW" (at 3.81 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 2.71) (layer "F.SilkS") hide)
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.2 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 "/K1") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 229.87 104.14 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R26" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(D18-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF1)
    (at 214.63 163.83 -90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 9.398 0.254 -180) (layer "F.SilkS"))
    (fp_text value "330u" (at 2.5 6.25 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -270) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 140.97 76.2)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP4" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "K2" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 45 "/K2") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 140.97 137.16)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP12" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "K6" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 49 "/K6") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 151.13 40.64)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R31" (at 7.62 -3.37) (layer "F.SilkS"))
    (fp_text value "24M" (at 7.62 3.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 "Net-(R30-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 149 59)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (clearance 1)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF5" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.5mm" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 53.34 105.41)
    (descr "Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=22.86mm, 4W, length*diameter=18*9mm^2")
    (tags "Resistor Axial_DIN0918 series Axial Horizontal pin pitch 22.86mm 4W length 18mm diameter 9mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R21" (at 11.43 -5.62) (layer "F.SilkS"))
    (fp_text value "R_SHARE" (at 11.43 5.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.43 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 46 "/K3") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 22.86 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 47 "/K4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3299W_Vertical" (layer "F.Cu")
    (tedit 5A3D4994)
    (at 219.71 127)
    (descr "Potentiometer, vertical, Bourns 3299W, https://www.bourns.com/pdfs/3299.pdf")
    (tags "Potentiometer vertical Bourns 3299W")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV1" (at 4.318 3.048) (layer "F.SilkS"))
    (fp_text value "100k" (at -2.54 5.44) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 1.14) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C9-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3299W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 101.6 76.2)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R10" (at 10.452 -3.28) (layer "F.SilkS"))
    (fp_text value "RP" (at 6.35 2.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 45 "/K2") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(D10-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 257.81 173.99 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at 2.5 -2.2 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 2.5 2.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 234.91 134.62 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C15" (at 2.5 2.032) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 2.5 2.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 130.81 137.16 180)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R6" (at 6.35 -2.92 180) (layer "F.SilkS"))
    (fp_text value "RS" (at 6.35 2.92 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 "Net-(R6-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(D14-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 234.95 55.88 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R48" (at -2.794 0) (layer "F.SilkS"))
    (fp_text value "360k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(R48-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "/trigger_coil(+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 63CA0410)
    (at 140.97 101.6)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP7" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "G4" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 "Net-(R4-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 53.34 59.69)
    (descr "Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=22.86mm, 4W, length*diameter=18*9mm^2")
    (tags "Resistor Axial_DIN0918 series Axial Horizontal pin pitch 22.86mm 4W length 18mm diameter 9mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R18" (at 11.43 -5.62) (layer "F.SilkS"))
    (fp_text value "R_SHARE" (at 11.43 5.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.43 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "/HV_INPUT") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 22.86 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 44 "/K1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 198.12 138.43)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R32" (at -4.064 0) (layer "F.SilkS"))
    (fp_text value "100k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "my_library:Keystone_PC_screw_terminal" (layer "F.Cu")
    (tedit 62606593)
    (at 86.238 35.185)
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at -0.513 2.026 unlocked) (layer "F.SilkS"))
    (fp_text value "HV_IN" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3 12) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 18 "/HV_INPUT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle (at 2 5) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 18 "/HV_INPUT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle (at 2 12) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 18 "/HV_INPUT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle (at -3 5) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 18 "/HV_INPUT") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 109.22 163.83 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D8" (at 7.368 2.73) (layer "F.SilkS"))
    (fp_text value "FW" (at 3.81 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 2.73) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 4.2 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(D16-Pad3)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 "/K8") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 101.6 106.68)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R12" (at 12.052 -3.48) (layer "F.SilkS"))
    (fp_text value "RP" (at 6.35 2.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 47 "/K4") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(D12-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 636BCDBE)
    (at 259 190)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF3" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3 3) (drill 3) (layers F&B.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 227.33 152.4)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R42" (at 3.556 2.794) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(R42-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-18-3" (layer "F.Cu")
    (tedit 5A02FF81)
    (at 233.045 93.98 -90)
    (descr "TO-18-3")
    (tags "TO-18-3")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q1" (at 1.27 4.318 90) (layer "F.SilkS"))
    (fp_text value "2N2222" (at 1.27 4.02 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -4.02 90) (layer "F.Fab"))
    (pad "1" thru_hole oval locked (at 0 0 270) (size 1.6 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 1.27 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 33 "Net-(Q1-Pad2)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 2.54 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 56 "Net-(C14-Pad1)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-18-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 109.22 87.63 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at 10.16 1.524) (layer "F.SilkS"))
    (fp_text value "FW" (at 3.81 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 2.45) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 4.2 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(D11-Pad3)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 46 "/K3") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 130.81 91.44 180)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 6.35 -2.92 180) (layer "F.SilkS"))
    (fp_text value "RS" (at 6.35 2.92 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 "Net-(R3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(D11-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 224.79 111.76 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C16" (at -3.81 0 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 2.5 2.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 246.38 62.23)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D19" (at -3.2 0) (layer "F.SilkS"))
    (fp_text value "MUR120" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 53 "Net-(C11-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(C10-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 63CA0407)
    (at 135.89 86.36)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP5" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "G3" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 "Net-(R3-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 243.84 169.164 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R39" (at -3.048 0 90) (layer "F.SilkS"))
    (fp_text value "2.7" (at 3.81 -2.645 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R39-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "my_library:Versatile_Link" (layer "F.Cu")
    (tedit 62C884E6)
    (at 255.27 139.7)
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U7" (at 0 6.35) (layer "F.SilkS"))
    (fp_text value "HFBR-1528Z" (at 0 -2.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5.08 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R45-Pad1)") (pinfunction "ANODE") (pintype "input"))
    (pad "2" thru_hole circle (at -5.08 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U6-Pad3)") (pinfunction "CATHODE") (pintype "input"))
    (pad "3" thru_hole circle (at -5.08 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "4" thru_hole circle (at -5.08 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "5" thru_hole circle (at 2.54 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "6" thru_hole circle (at 2.54 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 234.95 104.14 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R33" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "100" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(R33-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 234.696 87.376 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C14" (at -2.032 3.048 180) (layer "F.SilkS"))
    (fp_text value "33u" (at 1 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 636BCDB6)
    (at 259 40)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF2" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3 3) (drill 3) (layers F&B.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 234.95 115.062 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R34" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(R33-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 113.03 40.64)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R29" (at 7.62 -3.37) (layer "F.SilkS"))
    (fp_text value "24M" (at 7.62 3.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 35 "Net-(R28-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 "Net-(R29-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm_Socket" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 212.09 104.15)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at 0.254 -3.058) (layer "F.SilkS"))
    (fp_text value "MCP6002-xP" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "/CAP_RDY") (pintype "output"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(D18-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(R33-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(D18-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(R33-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "/CAP_DISABLE") (pintype "output"))
    (pad "8" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "my_library:Versatile_Link" (layer "F.Cu")
    (tedit 62C884E6)
    (at 255.27 123.19)
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U8" (at 0 6.35) (layer "F.SilkS"))
    (fp_text value "HFBR-1528Z" (at 0 -2.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5.08 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(R46-Pad1)") (pinfunction "ANODE") (pintype "input"))
    (pad "2" thru_hole circle (at -5.08 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U6-Pad5)") (pinfunction "CATHODE") (pintype "input"))
    (pad "3" thru_hole circle (at -5.08 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "4" thru_hole circle (at -5.08 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "5" thru_hole circle (at 2.54 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "6" thru_hole circle (at 2.54 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
  )
  (footprint "Package_TO_SOT_THT:TO-247-3_Vertical" (layer "F.Cu")
    (tedit 63ACD769)
    (at 83.82 74.93)
    (descr "TO-247-3, Vertical, RM 5.45mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html")
    (tags "TO-247-3 Vertical RM 5.45mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D10" (at 5.45 -3.45) (layer "F.SilkS"))
    (fp_text value "1.2kV SCR" (at 5.45 3.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.45 -3.45) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 45 "/K2") (pinfunction "K") (pintype "passive") (zone_connect 2))
    (pad "2" thru_hole oval locked (at 5.45 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 44 "/K1") (pinfunction "A") (pintype "passive") (clearance 1.8))
    (pad "3" thru_hole oval locked (at 10.9 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 11 "Net-(D10-Pad3)") (pinfunction "G") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-247-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 63CA0423)
    (at 140.97 132.08)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP11" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "G6" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 "Net-(R6-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 130.81 121.92 180)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R5" (at 6.35 -2.92) (layer "F.SilkS"))
    (fp_text value "RS" (at 6.35 2.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(D13-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 93.98 40.64)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R28" (at 7.62 -3.37) (layer "F.SilkS"))
    (fp_text value "24M" (at 7.62 3.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "/HV_INPUT") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 35 "Net-(R28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-247-3_Vertical" (layer "F.Cu")
    (tedit 63ACD784)
    (at 83.82 120.65)
    (descr "TO-247-3, Vertical, RM 5.45mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html")
    (tags "TO-247-3 Vertical RM 5.45mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D13" (at 5.45 -3.45) (layer "F.SilkS"))
    (fp_text value "1.2kV SCR" (at 5.45 3.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.45 -3.45) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 48 "/K5") (pinfunction "K") (pintype "passive") (zone_connect 2))
    (pad "2" thru_hole oval locked (at 5.45 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 47 "/K4") (pinfunction "A") (pintype "passive") (clearance 1.8))
    (pad "3" thru_hole oval locked (at 10.9 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 14 "Net-(D13-Pad3)") (pinfunction "G") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-247-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 63CA042B)
    (at 135.89 147.32)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP13" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "G7" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 "Net-(R7-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "my_library:Keystone_PC_screw_terminal" (layer "F.Cu")
    (tedit 62606593)
    (at 219.71 173.99)
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -6.35 8.89 unlocked) (layer "F.SilkS"))
    (fp_text value "GND_input" (at 0 1 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2 5) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle (at 2 12) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle (at -3 5) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle (at -3 12) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_THT:TO-247-3_Vertical" (layer "F.Cu")
    (tedit 63ACD7AE)
    (at 83.82 166.37)
    (descr "TO-247-3, Vertical, RM 5.45mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html")
    (tags "TO-247-3 Vertical RM 5.45mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D16" (at 5.45 -3.45) (layer "F.SilkS"))
    (fp_text value "1.2kV SCR" (at 5.45 3.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.45 -3.45) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 51 "/K8") (pinfunction "K") (pintype "passive") (zone_connect 2))
    (pad "2" thru_hole oval locked (at 5.45 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 50 "/K7") (pinfunction "A") (pintype "passive") (clearance 1.8))
    (pad "3" thru_hole oval locked (at 10.9 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 17 "Net-(D16-Pad3)") (pinfunction "G") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-247-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 191 179)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (clearance 1)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF7" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.5mm" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 130.81 167.64 180)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R8" (at 6.35 -2.92 180) (layer "F.SilkS"))
    (fp_text value "RS" (at 6.35 2.92 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 "Net-(R8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(D16-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 6351EFBB)
    (at 135.89 60.96)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "K1" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 44 "/K1") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 132.08 40.64)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R30" (at 7.62 -3.37) (layer "F.SilkS"))
    (fp_text value "24M" (at 7.62 3.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 "Net-(R29-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 "Net-(R30-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-15_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 234.95 161.29 -90)
    (descr "Diode, DO-15 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "Diode DO-15 series Axial Horizontal pin pitch 10.16mm  length 7.6mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D17" (at -3.81 0 90) (layer "F.SilkS"))
    (fp_text value "5V TVS" (at 5.08 2.92 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.2 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.65 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "+5V") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-15_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 256.54 56.515 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D20" (at 13.36 0.05) (layer "F.SilkS"))
    (fp_text value "MUR120" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 52 "Net-(C10-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 53 "Net-(C11-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 198.12 143.51)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R35" (at -4.064 0) (layer "F.SilkS"))
    (fp_text value "100k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 140.97 106.68)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP8" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "K4" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 47 "/K4") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 198.12 128.778)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R37" (at -4.064 0) (layer "F.SilkS"))
    (fp_text value "4k7" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 101.6 137.16)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R14" (at 11.652 -3.08) (layer "F.SilkS"))
    (fp_text value "RP" (at 6.35 2.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 49 "/K6") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(D14-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 207.732 99.187 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C13" (at 2.5 -2.2) (layer "F.SilkS"))
    (fp_text value "100p" (at 2.5 2.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 135.89 152.4)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP14" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "K7" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 50 "/K7") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 135.89 121.92)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP10" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "K5" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 48 "/K5") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Package_DIP:DIP-8_W7.62mm_Socket" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 248.92 104.15)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "LT1172" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(R27-Pad1)") (pinfunction "V_C") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "/V_CAP") (pinfunction "FEED") (pintype "input"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "5" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pinfunction "V_IN") (pintype "input"))
    (pad "6" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "E1") (pintype "input"))
    (pad "7" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C10-Pad1)") (pinfunction "V_SW") (pintype "input"))
    (pad "8" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "E2") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-247-3_Vertical" (layer "F.Cu")
    (tedit 63ACD77A)
    (at 83.82 105.41)
    (descr "TO-247-3, Vertical, RM 5.45mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html")
    (tags "TO-247-3 Vertical RM 5.45mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D12" (at 5.45 -3.45) (layer "F.SilkS"))
    (fp_text value "1.2kV SCR" (at 5.45 3.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.45 -3.45) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 47 "/K4") (pinfunction "K") (pintype "passive") (zone_connect 2))
    (pad "2" thru_hole oval locked (at 5.45 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 46 "/K3") (pinfunction "A") (pintype "passive") (clearance 1.8))
    (pad "3" thru_hole oval locked (at 10.9 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 13 "Net-(D12-Pad3)") (pinfunction "G") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-247-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 109.22 118.11 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D5" (at 10.16 1.524) (layer "F.SilkS"))
    (fp_text value "FW" (at 3.81 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 2.67) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 4.2 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(D13-Pad3)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 48 "/K5") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 240.03 161.544 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C12" (at 8.128 0.254 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 2.5 2.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 198.12 124.206)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C8" (at -3.58781 0) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 2.5 2.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 243.84 108.6 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C7" (at 7.85 0.125 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 2.5 2.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "/V_CAP") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-247-3_Vertical" (layer "F.Cu")
    (tedit 63ACD720)
    (at 83.82 59.69)
    (descr "TO-247-3, Vertical, RM 5.45mm, see https://toshiba.semicon-storage.com/us/product/mosfet/to-247-4l.html")
    (tags "TO-247-3 Vertical RM 5.45mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D9" (at 5.45 -3.45) (layer "F.SilkS"))
    (fp_text value "1.2kV SCR" (at 5.45 3.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.45 -3.45) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 44 "/K1") (pinfunction "K") (pintype "passive") (zone_connect 2))
    (pad "2" thru_hole oval locked (at 5.45 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 18 "/HV_INPUT") (pinfunction "A") (pintype "passive") (clearance 1.8))
    (pad "3" thru_hole oval locked (at 10.9 0) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 10 "Net-(D1-Pad1)") (pinfunction "G") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-247-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 53.34 90.17)
    (descr "Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=22.86mm, 4W, length*diameter=18*9mm^2")
    (tags "Resistor Axial_DIN0918 series Axial Horizontal pin pitch 22.86mm 4W length 18mm diameter 9mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R20" (at 11.43 -5.62) (layer "F.SilkS"))
    (fp_text value "R_SHARE" (at 11.43 5.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.43 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 45 "/K2") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 22.86 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 46 "/K3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 217.17 44.704)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R47" (at 6.35 -2.92) (layer "F.SilkS"))
    (fp_text value "100 / 1W" (at 6.35 2.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "/trigger_coil(+)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(D21-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 242.57 137.16)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C17" (at 1 -3.75) (layer "F.SilkS"))
    (fp_text value "1u" (at 1 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 636BCDAC)
    (at 49 40)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF1" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3 3) (drill 3) (layers F&B.Cu *.Mask))
  )
  (footprint "my_library:Keystone_PC_screw_terminal" (layer "F.Cu")
    (tedit 636BCDD4)
    (at 86.238 174.588)
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "0V" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3 12) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle (at 2 5) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle (at -3 5) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle (at 2 12) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Package_DIP:DIP-8_W7.62mm_Socket" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 212.09 138.43)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -0.254 -2.794) (layer "F.SilkS"))
    (fp_text value "LM393" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(R40-Pad2)") (pintype "open_collector"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "/V_CAP") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C5-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C9-Pad1)") (pinfunction "_") (pintype "input"))
    (pad "7" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(R42-Pad2)") (pintype "open_collector"))
    (pad "8" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 109.22 133.35 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D6" (at 10.16 1.524) (layer "F.SilkS"))
    (fp_text value "FW" (at 3.81 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0.068 2.47) (layer "F.SilkS") hide)
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.2 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(D14-Pad3)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 49 "/K6") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 101.6 167.64)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R16" (at 11.652 -3.29) (layer "F.SilkS"))
    (fp_text value "RP" (at 6.35 2.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 51 "/K8") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(D16-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 109.22 148.59 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D7" (at 9.906 1.524) (layer "F.SilkS"))
    (fp_text value "FW" (at 3.81 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 2.47) (layer "F.SilkS") hide)
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.2 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(D15-Pad3)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 50 "/K7") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 205.74 133.604 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R36" (at 11.684 0) (layer "F.SilkS"))
    (fp_text value "15k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 53.34 135.89)
    (descr "Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=22.86mm, 4W, length*diameter=18*9mm^2")
    (tags "Resistor Axial_DIN0918 series Axial Horizontal pin pitch 22.86mm 4W length 18mm diameter 9mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R23" (at 11.43 -5.62) (layer "F.SilkS"))
    (fp_text value "R_SHARE" (at 11.43 5.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.43 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 48 "/K5") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 22.86 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 49 "/K6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 130.81 152.4 180)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R7" (at 6.35 -2.92 180) (layer "F.SilkS"))
    (fp_text value "RS" (at 6.35 2.92 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(D15-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 53.34 151.13)
    (descr "Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=22.86mm, 4W, length*diameter=18*9mm^2")
    (tags "Resistor Axial_DIN0918 series Axial Horizontal pin pitch 22.86mm 4W length 18mm diameter 9mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R24" (at 11.43 -5.62) (layer "F.SilkS"))
    (fp_text value "R_SHARE" (at 11.43 18) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.43 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 49 "/K6") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 22.86 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 50 "/K7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 202.692 94.869 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R44" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "10" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(Q2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(R44-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W6.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 246.38 68.58 -90)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 6mm Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C11" (at 7.5 -4.25 90) (layer "F.SilkS"))
    (fp_text value "0.47" (at 7.5 4.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 53 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 15 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W6.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 63CA041A)
    (at 135.89 116.84)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP9" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "G5" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "Net-(R5-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 219.71 152.4 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R40" (at 3.81 -2.794) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(R40-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 198.12 148.59)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at -3.58781 -0.254) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 2.5 2.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "my_library:Keystone_PC_screw_terminal" (layer "F.Cu")
    (tedit 62606593)
    (at 234.95 173.99)
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -6.35 8.89 unlocked) (layer "F.SilkS"))
    (fp_text value "5V_input" (at 0 1 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3 5) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle (at -3 12) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle (at 2 5) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle (at 2 12) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 101.6 60.96)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R9" (at 12.252 -3.52) (layer "F.SilkS"))
    (fp_text value "RP" (at 6.35 2.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 44 "/K1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(D1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 101.6 121.92)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R13" (at 12.052 -3.48) (layer "F.SilkS"))
    (fp_text value "RP" (at 6.35 2.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 48 "/K5") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(D13-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 246.38 50.8)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D21" (at -3.2 0) (layer "F.SilkS"))
    (fp_text value "MUR120" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 "Net-(D21-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 52 "Net-(C10-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF1)
    (at 226.06 163.83 -90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 9.398 0 -180) (layer "F.SilkS"))
    (fp_text value "330u" (at 2.5 6.25 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -270) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 218.44 121.92 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C9" (at -2.95 0.05) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 2.5 2.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 63CA0437)
    (at 140.97 162.56)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP15" (at 0 -3.81) (layer "F.SilkS") hide)
    (fp_text value "G8" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.81) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 "Net-(R8-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "my_library:Keystone_PC_screw_terminal" (layer "F.Cu")
    (tedit 63CEB607)
    (at 204.47 173.99)
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at -6.35 8.89 unlocked) (layer "F.SilkS"))
    (fp_text value "T_-" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3 12) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 21 "/trigger_coil(-)") (pinfunction "Pin_1") (pintype "passive") (clearance 1) (zone_connect 2))
    (pad "1" thru_hole circle (at -3 5) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 21 "/trigger_coil(-)") (pinfunction "Pin_1") (pintype "passive") (clearance 1) (zone_connect 2))
    (pad "1" thru_hole circle (at 2 5) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 21 "/trigger_coil(-)") (pinfunction "Pin_1") (pintype "passive") (clearance 1))
    (pad "1" thru_hole circle (at 2 12) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 21 "/trigger_coil(-)") (pinfunction "Pin_1") (pintype "passive") (clearance 1))
  )
  (footprint "my_library:Keystone_PC_screw_terminal" (layer "F.Cu")
    (tedit 63CA0498)
    (at 205.74 36.455)
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 5.588 7.995 unlocked) (layer "F.SilkS"))
    (fp_text value "T_+" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2 12) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 9 "/trigger_coil(+)") (pinfunction "Pin_1") (pintype "passive") (zone_connect 2))
    (pad "1" thru_hole circle (at 2 5) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 9 "/trigger_coil(+)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" thru_hole circle (at -3 12) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 9 "/trigger_coil(+)") (pinfunction "Pin_1") (pintype "passive") (zone_connect 2))
    (pad "1" thru_hole circle (at -3 5) (size 3.4 3.4) (drill 2) (layers *.Cu *.Mask)
      (net 9 "/trigger_coil(+)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Diode_THT:D_A-405_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 229.87 115.062 -90)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D18" (at 3.81 -2.47 -90) (layer "F.SilkS"))
    (fp_text value "4.7V" (at 3.81 2.47 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9 -90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.2 0 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "Net-(D18-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 109.22 102.87 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D4" (at 10.16 1.524) (layer "F.SilkS"))
    (fp_text value "FW" (at 3.81 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 2.47) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 4.2 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(D12-Pad3)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 "/K4") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 247.65 93.98 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at 2.5 -5.25) (layer "F.SilkS"))
    (fp_text value "100u" (at 2.5 5.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 130.81 60.96 180)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 6.35 -2.92 180) (layer "F.SilkS"))
    (fp_text value "RS" (at 6.35 2.92 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(D1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 256.54 118.11 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R27" (at -3.1 0.103) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(R27-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm_Socket" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 227.33 138.43)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U6" (at -0.254 -2.74) (layer "F.SilkS"))
    (fp_text value "SN7545x" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "/CAP_RDY") (pinfunction "1A") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(R40-Pad2)") (pinfunction "1B") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U6-Pad3)") (pinfunction "1Y") (pintype "output"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "5" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U6-Pad5)") (pinfunction "2Y") (pintype "output"))
    (pad "6" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(R42-Pad2)") (pinfunction "2A") (pintype "input"))
    (pad "7" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pinfunction "2B") (pintype "input"))
    (pad "8" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pinfunction "VCC") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Radial_D8.7mm_P5.00mm_Fastron_07HCP" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 248.92 179.07 90)
    (descr "Inductor, Radial series, Radial, pin pitch=5.00mm, , diameter=8.7mm, Fastron, 07HCP, http://cdn-reichelt.de/documents/datenblatt/B400/DS_07HCP.pdf")
    (tags "Inductor Radial series Radial pin pitch 5.00mm  diameter 8.7mm Fastron 07HCP")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L1" (at -3.556 0 180) (layer "F.SilkS"))
    (fp_text value "100u" (at 2.5 5.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "+5V") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Radial_D8.7mm_P5.00mm_Fastron_07HCP.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 101.6 91.44)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R11" (at 11.052 -3.26) (layer "F.SilkS"))
    (fp_text value "RP" (at 6.35 2.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 46 "/K3") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(D11-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 243.84 143.51 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R45" (at 3.585 0.105 90) (layer "F.SilkS"))
    (fp_text value "47" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R45-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 636BCDA2)
    (at 49 190)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF4" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3 3) (drill 3) (layers F&B.Cu *.Mask))
  )
  (footprint "my_library:Versatile_Link" (layer "F.Cu")
    (tedit 62C884E6)
    (at 255.27 156.21)
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 0 6.35) (layer "F.SilkS"))
    (fp_text value "HFBR-2528Z" (at 0 -2.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5.08 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(R41-Pad1)") (pinfunction "DATA") (pintype "output"))
    (pad "2" thru_hole circle (at -5.08 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "3" thru_hole circle (at -5.08 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R39-Pad1)") (pinfunction "VCC") (pintype "input"))
    (pad "4" thru_hole circle (at -5.08 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "unconnected-(U4-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" thru_hole circle (at 2.54 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "6" thru_hole circle (at 2.54 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 224.8154 95.2754 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R38" (at 10.795 0 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "/CAP_DISABLE") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(Q1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 140.97 167.64)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP16" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "K8" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 51 "/K8") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm" (layer "F.Cu")
    (tedit 63CA03F6)
    (at 135.89 55.88)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "G1" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "Net-(R1-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 53.34 166.37)
    (descr "Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=22.86mm, 4W, length*diameter=18*9mm^2")
    (tags "Resistor Axial_DIN0918 series Axial Horizontal pin pitch 22.86mm 4W length 18mm diameter 9mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R25" (at 11.43 -5.62) (layer "F.SilkS"))
    (fp_text value "R_SHARE" (at 11.43 5.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.43 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 50 "/K7") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 22.86 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 51 "/K8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 6351DB57)
    (at 109.22 72.39 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at 10.414 1.27) (layer "F.SilkS"))
    (fp_text value "FW" (at 3.81 2.47) (layer "F.Fab"))
    (fp_text user "K" (at -0.132 2.47) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 4.2 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D10-Pad3)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 "/K2") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 149 179)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (clearance 1)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF8" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.5mm" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 130.81 76.2 180)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 6.35 -2.92 180) (layer "F.SilkS"))
    (fp_text value "RS" (at 6.35 2.92 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(D10-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 191 59)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (clearance 1)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF6" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.5mm" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 53.34 74.93)
    (descr "Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=22.86mm, 4W, length*diameter=18*9mm^2")
    (tags "Resistor Axial_DIN0918 series Axial Horizontal pin pitch 22.86mm 4W length 18mm diameter 9mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R19" (at 11.43 -5.62) (layer "F.SilkS"))
    (fp_text value "R_SHARE" (at 11.43 5.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.43 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 44 "/K1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 22.86 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 45 "/K2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal" (layer "F.Cu")
    (tedit 63AC7F15)
    (at 124.25 183.5 180)
    (descr "Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=22.86mm, 4W, length*diameter=18*9mm^2")
    (tags "Resistor Axial_DIN0918 series Axial Horizontal pin pitch 22.86mm 4W length 18mm diameter 9mm")
    (property "Sheetfile" "46_SCR_TH_stack_complete_V3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R17" (at 11.43 -5.62) (layer "F.SilkS"))
    (fp_text value "10mOhm" (at 11.43 5.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.43 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 51 "/K8") (pintype "passive") (clearance 1))
    (pad "2" thru_hole oval locked (at 22.86 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect locked (start 44 35) (end 264 195) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "HV SOLID STATE SWITCH\naz 12/22" (at 56.388 190.5) (layer "F.SilkS"))
  (gr_text "GND" (at 219.456 190.5) (layer "F.SilkS"))
  (gr_text "HV OK" (at 262.128 135.89 90) (layer "F.SilkS"))
  (gr_text "RDY" (at 262.128 151.638 90) (layer "F.SilkS"))
  (gr_text "5V INPUT" (at 234.696 190.5) (layer "F.SilkS"))
  (gr_text "HV IN" (at 77.724 43.18) (layer "F.SilkS"))
  (gr_text "TRIG.COIL(-)" (at 204.47 190.5) (layer "F.SilkS"))
  (gr_text "TRIG.COIL(+)" (at 205.74 37.465) (layer "F.SilkS"))
  (gr_text "TRIGGER" (at 262.382 168.402 90) (layer "F.SilkS"))
  (gr_text "HV RTN" (at 77.651267 183.102858) (layer "F.SilkS"))
  (zone (net 50) (net_name "/K7") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 1.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 3))
    (polygon
      (pts
        (xy 138.43 147.32)
        (xy 138.43 154.94)
        (xy 138.43 156.21)
        (xy 73.66 156.21)
        (xy 72.39 156.21)
        (xy 72.39 146.05)
        (xy 73.66 146.05)
        (xy 138.43 146.05)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.43 177.8)
        (xy 138.43 204.47)
        (xy 39.37 204.47)
        (xy 39.37 176.53)
        (xy 137.16 176.53)
      )
    )
  )
  (zone (net 45) (net_name "/K2") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 1.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 3))
    (polygon
      (pts
        (xy 143.51 71.12)
        (xy 143.51 80.01)
        (xy 142.24 80.01)
        (xy 73.66 80.01)
        (xy 72.644 80.01)
        (xy 72.644 69.85)
        (xy 73.66 69.85)
        (xy 143.51 69.85)
      )
    )
  )
  (zone (net 18) (net_name "/HV_INPUT") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 1.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 3))
    (polygon
      (pts
        (xy 96.52 49.53)
        (xy 80.01 49.53)
        (xy 80.01 36.83)
        (xy 96.52 36.83)
      )
    )
  )
  (zone (net 46) (net_name "/K3") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 1.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 3))
    (polygon
      (pts
        (xy 138.43 86.36)
        (xy 138.43 93.98)
        (xy 138.43 95.25)
        (xy 73.66 95.25)
        (xy 72.39 95.25)
        (xy 72.39 86.36)
        (xy 72.39 85.09)
        (xy 138.43 85.09)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.7 190.5)
        (xy 168.91 190.5)
        (xy 168.91 204.47)
        (xy 137.16 204.47)
        (xy 137.16 189.23)
        (xy 138.43 189.23)
      )
    )
  )
  (zone (net 49) (net_name "/K6") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 1.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 3))
    (polygon
      (pts
        (xy 143.51 132.08)
        (xy 143.51 140.97)
        (xy 142.24 140.97)
        (xy 73.66 140.97)
        (xy 72.39 140.97)
        (xy 72.39 130.81)
        (xy 73.66 130.81)
        (xy 143.51 130.81)
      )
    )
  )
  (zone (net 47) (net_name "/K4") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 1.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 3))
    (polygon
      (pts
        (xy 143.51 101.6)
        (xy 143.51 109.22)
        (xy 143.51 110.49)
        (xy 73.66 110.49)
        (xy 72.39 110.49)
        (xy 72.39 100.33)
        (xy 73.66 100.33)
        (xy 143.51 100.33)
      )
    )
  )
  (zone (net 51) (net_name "/K8") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 1.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 3))
    (polygon
      (pts
        (xy 143.51 162.56)
        (xy 143.51 170.18)
        (xy 143.51 171.45)
        (xy 72.39 171.45)
        (xy 72.39 170.18)
        (xy 72.39 162.56)
        (xy 72.39 161.29)
        (xy 143.51 161.29)
      )
    )
  )
  (zone (net 48) (net_name "/K5") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 1.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 3))
    (polygon
      (pts
        (xy 138.43 116.84)
        (xy 138.43 124.46)
        (xy 138.43 125.73)
        (xy 73.66 125.73)
        (xy 72.39 125.73)
        (xy 72.39 115.57)
        (xy 73.66 115.57)
        (xy 138.43 115.57)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 278.13 204.47)
        (xy 168.91 204.47)
        (xy 168.91 22.86)
        (xy 198.12 22.86)
        (xy 198.12 58.42)
        (xy 199.39 59.69)
        (xy 219.71 59.69)
        (xy 220.98 58.42)
        (xy 220.98 22.86)
        (xy 222.885 22.86)
        (xy 276.86 22.86)
      )
    )
  )
  (zone (net 44) (net_name "/K1") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 1.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 3))
    (polygon
      (pts
        (xy 138.43 54.61)
        (xy 138.43 64.77)
        (xy 137.16 64.77)
        (xy 74.93 64.77)
        (xy 73.66 64.77)
        (xy 73.66 54.61)
        (xy 74.93 54.61)
        (xy 137.16 54.61)
      )
    )
  )
  (zone (net 9) (net_name "/trigger_coil(+)") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219.71 57.15)
        (xy 218.44 58.42)
        (xy 200.66 58.42)
        (xy 199.39 57.15)
        (xy 199.39 30.48)
        (xy 219.71 30.48)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 269.24 204.47)
        (xy 168.91 204.47)
        (xy 168.91 190.5)
        (xy 170.18 190.5)
        (xy 209.55 190.5)
        (xy 210.82 189.23)
        (xy 210.82 175.26)
        (xy 209.55 173.99)
        (xy 190.5 173.99)
        (xy 189.23 172.72)
        (xy 189.23 101.6)
        (xy 190.5 100.33)
        (xy 198.12 100.33)
        (xy 199.39 99.06)
        (xy 199.39 85.09)
        (xy 198.12 83.82)
        (xy 170.18 83.82)
        (xy 168.91 82.55)
        (xy 168.91 30.48)
        (xy 196.85 30.48)
        (xy 198.12 31.75)
        (xy 198.12 58.42)
        (xy 199.39 59.69)
        (xy 219.71 59.69)
        (xy 220.98 58.42)
        (xy 220.98 30.48)
        (xy 224.79 30.48)
        (xy 269.24 30.48)
      )
    )
  )
  (zone (net 21) (net_name "/trigger_coil(-)") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.75))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.12 86.36)
        (xy 198.12 97.79)
        (xy 196.85 99.06)
        (xy 189.23 99.06)
        (xy 187.96 100.33)
        (xy 187.96 173.99)
        (xy 189.23 175.26)
        (xy 208.28 175.26)
        (xy 209.55 176.53)
        (xy 209.55 187.96)
        (xy 208.28 189.23)
        (xy 168.91 189.23)
        (xy 168.91 186.69)
        (xy 168.91 86.36)
        (xy 170.18 85.09)
        (xy 196.85 85.09)
      )
    )
  )
)
