(kicad_pcb (version 20170123) (host pcbnew "(2017-07-06 revision 885a4c1bc)-makepkg")
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 249)
    (zones 0)
    (modules 63)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 5)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFDFF)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 "Net-(C7-Pad1)")
  (net 9 +15V)
  (net 10 "Net-(J2-Pad2)")
  (net 11 "Net-(J3-Pad1)")
  (net 12 "Net-(J3-Pad2)")
  (net 13 "Net-(J4-Pad2)")
  (net 14 "Net-(J4-Pad1)")
  (net 15 "Net-(J5-Pad1)")
  (net 16 "Net-(J5-Pad2)")
  (net 17 "Net-(RV1-Pad2)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +15V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(RV1-Pad2)")
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 56.458 28.961)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59627161)
    (at 43.18 22.225 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15k (at -0.127 0 90) (layer F.SilkS))
    (fp_text user %R (at -1.397 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 35.581 26.081)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 57.228 21.584)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 28.45 21.85)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 28.45 19.85)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 28.45 17.85)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 28.4 16)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 28.4 23.8)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 26.4 23.8)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 24.4 23.8)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 22.4 23.8)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 20.4 23.8)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 42.05 40.25)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 42.05 38.25)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 42.05 36.25)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 28.85 40.05)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 28.85 34.05)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 28.85 32.05)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 28.85 30.05)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 42.05 34.25)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 52.85 33.65)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 52.85 40.25)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 55.45 16.25)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 50.25 16.25)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 18.4 23.8)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 59627686)
    (at 21.2 37.2)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (fp_text reference REF** (at 0.136 -0.116) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580_Pad (at -0.499 5.853) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 70.75 40.25)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 70.75 16.25)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 18.25 16.25)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 18.25 40.25)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Connectors_Molex:Molex_KK-6410-03_03x2.54mm_Straight (layer F.Cu) (tedit 59626CFE)
    (at 25.4 19.685 180)
    (descr "Connector Headers with Friction Lock, 22-27-2031, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2031")
    (fp_text reference J1 (at -3.048 -1.143 270) (layer F.SilkS))
    (fp_text value CONN_01X03_MALE (at 3.683 6.477 180) (layer F.Fab))
    (fp_text user %R (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 +15V))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-03_03x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-03_03x2.54mm_Straight (layer F.Cu) (tedit 59626E32)
    (at 50.165 36.83 180)
    (descr "Connector Headers with Friction Lock, 22-27-2031, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2031")
    (fp_text reference J2 (at 7.493 0.889 270) (layer F.SilkS))
    (fp_text value CONN_01X03_MALE (at 1.397 -8.636 180) (layer F.Fab))
    (fp_text user %R (at 2.54 0 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-03_03x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 59626D01)
    (at 67.31 28.575 270)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference J3 (at -1.27 3.81 270) (layer F.SilkS))
    (fp_text value CONN_01X02_MALE (at 0.381 -7.112 270) (layer F.Fab))
    (fp_text user %R (at 1.27 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 59626D06)
    (at 67.31 23.495 270)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference J4 (at -1.27 3.81 270) (layer F.SilkS))
    (fp_text value CONN_01X02_MALE (at 5.334 -8.89 270) (layer F.Fab))
    (fp_text user %R (at 1.27 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 59626D09)
    (at 67.31 18.415 270)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference J5 (at -1.905 3.81 270) (layer F.SilkS))
    (fp_text value CONN_01X02_MALE (at 10.922 -10.795 270) (layer F.Fab))
    (fp_text user %R (at 1.27 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Suntan_TSR-3386H_Vertical (layer F.Cu) (tedit 59626D23)
    (at 38.1 17.78 270)
    (descr "Potentiometer, vertically mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, Bourns 3339H Single, Vishay T7YA Single, Suntan TSR-3386H Single, http://www.Suntan.com/docs/51016/TSR-3386.pdf")
    (tags "Potentiometer vertical  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single  Bourns 3339H Single  Vishay T7YA Single  Suntan TSR-3386H Single")
    (fp_text reference RV1 (at 0 8.89 270) (layer F.SilkS))
    (fp_text value 10k (at 0.381 2.667 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 2.54 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(RV1-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Suntan_TSR-3386H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 59626D9D)
    (at 26.67 27.94 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C1 (at 5.715 2.54 270) (layer F.SilkS))
    (fp_text value 100µ (at 0.254 -1.778 270) (layer F.SilkS))
    (fp_text user %R (at 1.1 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5962734F)
    (at 20.32 29.21 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 100n (at -0.127 0 90) (layer F.SilkS))
    (fp_text user %R (at -1.397 0.127 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 59626DB4)
    (at 45.085 17.78 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value 33n (at -0.127 -0.127 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 59626DEE)
    (at 46.99 22.225 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 10n (at 0 0 90) (layer F.SilkS))
    (fp_text user %R (at -1.27 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 59627334)
    (at 49.53 31.75)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at -0.762 -1.778 90) (layer F.SilkS))
    (fp_text value 220n (at 0 0.127) (layer F.SilkS))
    (fp_text user %R (at -1.27 0.127) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 59627323)
    (at 60.96 25.4)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at -3.048 -0.254 90) (layer F.SilkS))
    (fp_text value 220n (at 0 0.127) (layer F.SilkS))
    (fp_text user %R (at -1.524 0.127) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 59627347)
    (at 60.96 17.78)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at -3.048 -0.762 270) (layer F.SilkS))
    (fp_text value 220n (at 0 0.381) (layer F.SilkS))
    (fp_text user %R (at -1.397 0) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59626E05)
    (at 43.18 27.305 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15k (at -0.127 0 90) (layer F.SilkS))
    (fp_text user %R (at -1.27 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59627282)
    (at 44.45 31.75 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 2.794 1.524 270) (layer F.SilkS))
    (fp_text value 1k (at 0.127 0 180) (layer F.SilkS))
    (fp_text user %R (at 1.397 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59626E19)
    (at 46.99 27.305 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 15 (at -0.127 0 90) (layer F.SilkS))
    (fp_text user %R (at -1.27 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59626E8E)
    (at 51.435 29.21)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0.127 -2.032 90) (layer F.SilkS))
    (fp_text value 100k (at 0 0) (layer F.SilkS))
    (fp_text user %R (at -1.397 0) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59626E85)
    (at 54.61 31.75 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at -3.175 0 270) (layer F.SilkS))
    (fp_text value 1k (at 0 -0.127 180) (layer F.SilkS))
    (fp_text user %R (at 1.397 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59626EA9)
    (at 60.96 30.48 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at -2.54 -1.27 270) (layer F.SilkS))
    (fp_text value 15 (at 0 0 180) (layer F.SilkS))
    (fp_text user %R (at 1.397 -0.127 180) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 596272FC)
    (at 60.96 27.94 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 3.048 0.762 270) (layer F.SilkS))
    (fp_text value 100k (at 0 0 180) (layer F.SilkS))
    (fp_text user %R (at 1.397 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J4-Pad2)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59626ED2)
    (at 56.515 29.21 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 1.143 2.032 90) (layer F.SilkS))
    (fp_text value 1k (at 0 -0.127 180) (layer F.SilkS))
    (fp_text user %R (at 1.397 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59626EFB)
    (at 60.96 22.86 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 3.048 0.254 270) (layer F.SilkS))
    (fp_text value 15 (at 0 2.413 180) (layer F.SilkS))
    (fp_text user %R (at 1.143 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J5-Pad2)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59626F04)
    (at 60.96 20.32)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at -3.048 -0.762 90) (layer F.SilkS))
    (fp_text value 100k (at 0.127 2.54) (layer F.SilkS))
    (fp_text user %R (at -1.143 0) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J5-Pad1)"))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-263-2 (layer F.Cu) (tedit 59627216)
    (at 35.56 31.75 270)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (zone_connect 0)
    (attr smd)
    (fp_text reference U1 (at -0.762 6.35 270) (layer F.SilkS))
    (fp_text value LM7812 (at 4.318 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.95 2.775 270) (size 4.55 5.25) (layers F.Cu F.Paste)
      (net 1 GND) (zone_connect 0))
    (pad 2 smd rect (at 5.8 -2.775 270) (size 4.55 5.25) (layers F.Cu F.Paste)
      (net 1 GND) (zone_connect 0))
    (pad 2 smd rect (at 0.95 -2.775 270) (size 4.55 5.25) (layers F.Cu F.Paste)
      (net 1 GND) (zone_connect 0))
    (pad 2 smd rect (at 5.8 2.775 270) (size 4.55 5.25) (layers F.Cu F.Paste)
      (net 1 GND) (zone_connect 0))
    (pad 2 smd rect (at 3.375 0 270) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 0))
    (pad 3 smd rect (at -5.775 2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)") (zone_connect 0))
    (pad 1 smd rect (at -5.775 -2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 9 +15V) (zone_connect 0))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-263-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 59626E28)
    (at 52.705 21.59)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at -4.445 -3.81 90) (layer F.SilkS))
    (fp_text value LM324 (at -1.016 0.254 90) (layer F.Fab))
    (fp_text user %R (at 0.127 -2.921) (layer F.Fab))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J5-Pad1)"))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(RV1-Pad2)"))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(RV1-Pad2)"))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J4-Pad1)"))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(RV1-Pad2)"))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F6)
    (at 56.515 26.543)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module ViaStitching:Via_06 (layer F.Cu) (tedit 596252F0)
    (at 57.658 30.861)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value V (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 59627699)
    (at 67.7 37.2)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (fp_text reference REF** (at 0.118 -0.116) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580_Pad (at 0.245 5.599) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Symbols:OSHW-Symbol_8.9x8mm_SilkScreen (layer F.Cu) (tedit 59627291)
    (at 35.56 25.654)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at -0.508 -11.938) (layer F.SilkS) hide)
    (fp_text value OSHW-Symbol_8.9x8mm_SilkScreen (at -22.733 2.159 90) (layer F.Fab) hide)
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 59627663)
    (at 27.94 36.83 180)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference 12V_AUX (at 3.302 4.064 180) (layer F.SilkS))
    (fp_text value Molex_KK-6410-02_02x2.54mm_Straight (at 2.794 -8.636 180) (layer F.Fab))
    (fp_text user %R (at 1.524 -7.747 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module IRFP250:irfp250_scaled_loresw (layer B.Cu) (tedit 0)
    (at 56.4515 27.4955)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module IRFP250:to247_scaled_lowres (layer B.Cu) (tedit 0)
    (at 36.83 35.814)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (gr_text wanhunglo.com (at 58.166 37.592) (layer B.SilkS))
  (gr_text "G D S" (at 32.893 38.735 -48) (layer B.SilkS))
  (gr_text "IRFP250 Ratings\nVDSS = 200V\nRDSon = 75mΩ @ 10Vgs\nID = 21A @ 100°C Tc\nP = 109W @ 100°C Tc\nRjc = 0.7 K/W" (at 46.736 26.67) (layer B.SilkS))
  (gr_text "Wan Hung Lo Brand" (at 52.324 17.907) (layer B.SilkS))
  (gr_text "S    G" (at 71.2 19.7 90) (layer F.SilkS))
  (gr_text "S    G" (at 71.2 24.7 90) (layer F.SilkS))
  (gr_text "VCC  GND" (at 26.67 40.64) (layer F.SilkS))
  (gr_text "GND Sens VCC" (at 47.625 40.513) (layer F.SilkS))
  (gr_text "S    G" (at 71.2 29.8 90) (layer F.SilkS))
  (gr_text "GND GND_DUT +15VDC" (at 23.495 16.002) (layer F.SilkS))
  (gr_text "Rev. 1.0" (at 58.674 34.036) (layer F.SilkS))
  (gr_text "Triple MOSFET\nelectronic load" (at 58.42 37.846) (layer F.SilkS))
  (gr_line (start 71.755 15.24) (end 17.145 15.24) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.755 41.275) (end 71.755 15.24) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 17.145 41.275) (end 71.755 41.275) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 17.145 15.24) (end 17.145 41.275) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing chamfer))
    (polygon
      (pts
        (xy 17.145 41.275) (xy 17.145 15.24) (xy 71.755 15.24) (xy 71.755 41.275)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing chamfer))
    (polygon
      (pts
        (xy 17.145 15.24) (xy 71.755 15.24) (xy 71.755 41.275) (xy 17.145 41.275)
      )
    )
  )
)
