<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="48.26" x2="35.23" y2="48.26" width="0" layer="20"/>
<wire x1="35.23" y1="48.26" x2="35.23" y2="81.27" width="0" layer="20"/>
<wire x1="35.23" y1="81.27" x2="0" y2="81.27" width="0" layer="20"/>
<wire x1="0" y1="81.27" x2="0" y2="48.26" width="0" layer="20"/>
<text>Dactyl R v0.2
@joedevivo</text>
<text>GND</text>
<text>Row5</text>
<text>D</text>
<text>7</text>
<text>SCL</text>
<text>SDA</text>
<text>C</text>
<text>B</text>
<text>A</text>
<text>9</text>
<text>8</text>
<text>Row4</text>
<text>Row3</text>
<text>Row2</text>
<text>Row1</text>
<text>Row0</text>
<text>Dactyl R v0.2
@joedevivo</text>
<text>Vcc</text>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_3MM">
<description>&lt;h3&gt;LED 3MM PTH&lt;/h3&gt;

3 mm, round.

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 3mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X07">
<description>&lt;h3&gt;Plated Through Hole -7 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="my_parts">
<packages>
<package name="SJ-43514_HEADPHONES-3.5MM_X4">
</package>
</packages>
</library>
<library name="teensy">
<packages>
<package name="TEENSY">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="SparkFun-LED" package="LED_3MM" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun-LED" package="LED_3MM" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="SparkFun-LED" package="LED_3MM" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06" value="Rows">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X07" value="Columns">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="220">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="220">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="220">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3" value="2.2k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value="2.2k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="my_parts" package="SJ-43514_HEADPHONES-3.5MM_X4" value="SJ-43514_HEADPHONES_3.5MM_X4"/>
<element name="_1" library="teensy" package="TEENSY" value="TEENSY"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="LED1" pad="K"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="K"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="LED3" pad="K"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="_1" pad="B5"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="_1" pad="B6"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="_1" pad="B7"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="_1" pad="+5V"/>
<contactref element="U$2" pad="4"/>
<contactref element="R4" pad="P$2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="_1" pad="B4"/>
</signal>
<signal name="N$8">
<contactref element="R4" pad="P$1"/>
<contactref element="U$2" pad="2"/>
<contactref element="_1" pad="D0"/>
</signal>
<signal name="N$9">
<contactref element="R5" pad="P$1"/>
<contactref element="U$2" pad="3"/>
<contactref element="_1" pad="D1"/>
</signal>
<signal name="N$11">
<contactref element="R3" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="_1" pad="GND"/>
<contactref element="U$2" pad="1"/>
<contactref element="_1" pad="D6"/>
</signal>
<signal name="N$14">
<contactref element="_1" pad="C6"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="_1" pad="D3"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="_1" pad="D2"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="ROW0">
<contactref element="_1" pad="F0"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="_1" pad="F1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="_1" pad="F4"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="_1" pad="F5"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$18">
<contactref element="_1" pad="F6"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$19">
<contactref element="_1" pad="F7"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="COL7">
<contactref element="_1" pad="B0"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="N$21">
<contactref element="_1" pad="B1"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$22">
<contactref element="_1" pad="B2"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$23">
<contactref element="_1" pad="B3"/>
<contactref element="J2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
