(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 7)
    (no_connects 0)
    (area 140.894999 98.984999 160.730001 116.915001)
    (thickness 1.6)
    (drawings 16)
    (tracks 24)
    (zones 0)
    (modules 4)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.508)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(IC1-Pad1)")
  (net 2 SD)
  (net 3 "Net-(IC1-Pad2)")
  (net 4 "Net-(IC1-Pad6)")
  (net 5 "Net-(IC1-Pad3)")
  (net 6 SCL)
  (net 7 GND)
  (net 8 VCC)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net GND)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad6)")
    (add_net SCL)
    (add_net SD)
    (add_net VCC)
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket (layer F.Cu) (tedit 5A06519A)
    (at 149.86 102.235)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), Socket")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference ATTiny85 (at 3.81 -2.286) (layer F.SilkS))
    (fp_text value ATTINY85-P (at 3.81 10.01) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(IC1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 SD))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad3)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 SCL))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 VCC))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5A06517D)
    (at 144.78 102.235)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference PPM (at 0 -2.286) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5A0611B6)
    (at 157.48 113.411 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference I2C (at 0 -2.413 270) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 SCL))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 SD))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A0F1AF7)
    (at 144.78 112.395)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference " " (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (gr_text "Rev. A" (at 144.78 115.697) (layer F.SilkS))
  (gr_text C (at 154.94 115.824) (layer F.SilkS))
  (gr_text D (at 152.527 115.824) (layer F.SilkS))
  (gr_text + (at 157.48 115.697) (layer F.SilkS))
  (gr_text - (at 149.86 115.697) (layer F.SilkS))
  (gr_text S (at 142.24 102.235) (layer F.SilkS))
  (gr_text + (at 142.24 104.775) (layer F.SilkS))
  (gr_text - (at 142.24 107.315) (layer F.SilkS))
  (gr_line (start 159.385 116.84) (end 142.24 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.655 115.57) (end 160.655 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.385 99.06) (end 142.24 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.97 115.57) (end 140.97 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 142.24 100.33) (end 140.97 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 159.385 100.33) (end 159.385 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 142.24 115.57) (end 142.24 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 159.385 115.57) (end 160.655 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.782 116.967) (xy 140.843 116.967) (xy 140.843 99.06) (xy 160.782 99.06)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.782 116.967) (xy 140.843 116.967) (xy 140.843 99.06) (xy 160.782 99.06)
      )
    )
  )
)
