(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 137)
    (no_connects 0)
    (area 55.924999 61.924999 136.075001 134.075001)
    (thickness 1.6)
    (drawings 67)
    (tracks 587)
    (zones 0)
    (modules 57)
    (nets 52)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VCC0)
  (net 2 /VCC1)
  (net 3 /3V)
  (net 4 /VCC3)
  (net 5 /5V)
  (net 6 /VCC2)
  (net 7 /GND)
  (net 8 /SCL0)
  (net 9 /~INT0)
  (net 10 /SDA0)
  (net 11 /SCL1)
  (net 12 /SDA1)
  (net 13 /SCL)
  (net 14 /SDA)
  (net 15 /~INT1)
  (net 16 /SCL2)
  (net 17 /~INT2)
  (net 18 /SDA2)
  (net 19 /SCL3)
  (net 20 /~INT3)
  (net 21 /SDA3)
  (net 22 /~INT)
  (net 23 /ALT-3V)
  (net 24 /RESET)
  (net 25 /3V-OUT)
  (net 26 /5V-OUT)
  (net 27 /ALT-5V)
  (net 28 /5GND)
  (net 29 /~RESET)
  (net 30 /~RESET0)
  (net 31 /~RESET1)
  (net 32 /~RESET2)
  (net 33 /~RESET3)
  (net 34 "Net-(P2-Pad2)")
  (net 35 "Net-(P2-Pad4)")
  (net 36 "Net-(P2-Pad6)")
  (net 37 "Net-(P2-Pad8)")
  (net 38 "Net-(P3-Pad2)")
  (net 39 "Net-(P3-Pad4)")
  (net 40 "Net-(P3-Pad6)")
  (net 41 "Net-(P3-Pad8)")
  (net 42 "Net-(JP104-Pad1)")
  (net 43 "Net-(D101-Pad1)")
  (net 44 "Net-(C2-Pad1)")
  (net 45 "Net-(JP5-Pad2)")
  (net 46 "Net-(JP6-Pad2)")
  (net 47 "Net-(JP7-Pad1)")
  (net 48 "Net-(P2-Pad10)")
  (net 49 "Net-(P2-Pad12)")
  (net 50 "Net-(P3-Pad10)")
  (net 51 "Net-(P3-Pad12)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /3V)
    (add_net /3V-OUT)
    (add_net /5GND)
    (add_net /5V)
    (add_net /5V-OUT)
    (add_net /ALT-3V)
    (add_net /ALT-5V)
    (add_net /GND)
    (add_net /RESET)
    (add_net /SCL)
    (add_net /SCL0)
    (add_net /SCL1)
    (add_net /SCL2)
    (add_net /SCL3)
    (add_net /SDA)
    (add_net /SDA0)
    (add_net /SDA1)
    (add_net /SDA2)
    (add_net /SDA3)
    (add_net /VCC0)
    (add_net /VCC1)
    (add_net /VCC2)
    (add_net /VCC3)
    (add_net /~INT)
    (add_net /~INT0)
    (add_net /~INT1)
    (add_net /~INT2)
    (add_net /~INT3)
    (add_net /~RESET)
    (add_net /~RESET0)
    (add_net /~RESET1)
    (add_net /~RESET2)
    (add_net /~RESET3)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D101-Pad1)")
    (add_net "Net-(JP104-Pad1)")
    (add_net "Net-(JP5-Pad2)")
    (add_net "Net-(JP6-Pad2)")
    (add_net "Net-(JP7-Pad1)")
    (add_net "Net-(P2-Pad10)")
    (add_net "Net-(P2-Pad12)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad8)")
    (add_net "Net-(P3-Pad10)")
    (add_net "Net-(P3-Pad12)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad6)")
    (add_net "Net-(P3-Pad8)")
  )
  (module Pin_Headers:Pin_Header_Straight_2x06_Pitch2.54mm (layer F.Cu) (tedit 5A985BBD)
    (at 85.09 120.65 90)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference P2 (at 3.175 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_6X2 (at 1.27 15.03 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 6.35 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VCC0))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VCC0))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VCC0))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(P2-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VCC1))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(P2-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VCC1))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(P2-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VCC1))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(P2-Pad12)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_logo:Logo_silk_CC-BY-NC-SA_10x3.6mm (layer F.Cu) (tedit 0)
    (at 115.57 116.205)
    (descr "CC BY-NC-SA logo, 10x3.6mm")
    (fp_text reference LIC1 (at 0.3 -1.4) (layer F.SilkS) hide)
    (fp_text value CC-BY-NC-SA-icon (at 0.3 0.5) (layer F.SilkS) hide)
  )
  (module Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 90.17 97.79 90)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -4.3 90) (layer F.SilkS))
    (fp_text value TCA9545A (at 0 4.3 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(JP5-Pad2)"))
    (pad 2 smd rect (at -2.95 -2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(JP6-Pad2)"))
    (pad 3 smd rect (at -2.95 -1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at -2.95 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 /~INT0))
    (pad 5 smd rect (at -2.95 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 /SDA0))
    (pad 6 smd rect (at -2.95 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 /SCL0))
    (pad 7 smd rect (at -2.95 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 /~INT1))
    (pad 8 smd rect (at -2.95 1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 /SDA1))
    (pad 9 smd rect (at -2.95 2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCL1))
    (pad 10 smd rect (at -2.95 2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 /GND))
    (pad 11 smd rect (at 2.95 2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 /~INT2))
    (pad 12 smd rect (at 2.95 2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 /SDA2))
    (pad 13 smd rect (at 2.95 1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 16 /SCL2))
    (pad 14 smd rect (at 2.95 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /~INT3))
    (pad 15 smd rect (at 2.95 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 /SDA3))
    (pad 16 smd rect (at 2.95 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 /SCL3))
    (pad 17 smd rect (at 2.95 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 /~INT))
    (pad 18 smd rect (at 2.95 -1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 /SCL))
    (pad 19 smd rect (at 2.95 -2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 14 /SDA))
    (pad 20 smd rect (at 2.95 -2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A8B40B4)
    (at 88.9 125.095 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at 0.635 -3.175 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /3V-OUT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VCC1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /5V-OUT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A8B40B3)
    (at 88.9 127.635 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP2 (at -0.635 -3.175 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /3V-OUT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VCC0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /5V-OUT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A8B3CE7)
    (at 88.9 71.12 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP3 (at -0.635 -2.54 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /3V-OUT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /VCC2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /5V-OUT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A8B3CE9)
    (at 88.9 68.58 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP4 (at 0.635 -2.54 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /3V-OUT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VCC3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /5V-OUT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_4x2 (layer F.Cu) (tedit 5A9C5B07)
    (at 115.57 124.46 180)
    (descr "Box header 4x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P4 (at -7.62 5.715 180) (layer F.SilkS))
    (fp_text value MY_CONN_I2C (at 0 5.7 180) (layer F.SilkS) hide)
    (pad 8 thru_hole oval (at 3.81 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 28 /5GND))
    (pad 7 thru_hole oval (at 3.81 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 7 /GND))
    (pad 1 thru_hole rect (at -3.81 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 25 /3V-OUT))
    (pad 2 thru_hole oval (at -3.81 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 26 /5V-OUT))
    (pad 3 thru_hole oval (at -1.27 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SCL0))
    (pad 4 thru_hole oval (at -1.27 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 9 /~INT0))
    (pad 5 thru_hole oval (at 1.27 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SDA0))
    (pad 6 thru_hole oval (at 1.27 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 30 /~RESET0))
    (model walter/conn_strip/vasch_strip_4x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_4x2 (layer F.Cu) (tedit 5A9C5B11)
    (at 115.57 88.9 180)
    (descr "Box header 4x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P6 (at -7.62 5.715 180) (layer F.SilkS))
    (fp_text value MY_CONN_I2C (at 0 5.7 180) (layer F.SilkS) hide)
    (pad 8 thru_hole oval (at 3.81 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 28 /5GND))
    (pad 7 thru_hole oval (at 3.81 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 7 /GND))
    (pad 1 thru_hole rect (at -3.81 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 25 /3V-OUT))
    (pad 2 thru_hole oval (at -3.81 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 26 /5V-OUT))
    (pad 3 thru_hole oval (at -1.27 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 16 /SCL2))
    (pad 4 thru_hole oval (at -1.27 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 17 /~INT2))
    (pad 5 thru_hole oval (at 1.27 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 18 /SDA2))
    (pad 6 thru_hole oval (at 1.27 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 32 /~RESET2))
    (model walter/conn_strip/vasch_strip_4x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Main:MECH_NPTH_M3 (layer F.Cu) (tedit 579B0774)
    (at 61 68)
    (fp_text reference MP1 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 -2.8) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.6) (layers *.Cu *.Mask F.SilkS))
  )
  (module Main:MECH_NPTH_M3 (layer F.Cu) (tedit 579B0774)
    (at 131 68)
    (fp_text reference MP2 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 -2.8) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.6) (layers *.Cu *.Mask F.SilkS))
  )
  (module Main:MECH_NPTH_M3 (layer F.Cu) (tedit 579B0774)
    (at 131 128)
    (fp_text reference MP3 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 -2.8) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.6) (layers *.Cu *.Mask F.SilkS))
  )
  (module Main:MECH_NPTH_M3 (layer F.Cu) (tedit 579B0774)
    (at 61 128)
    (fp_text reference MP4 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 -2.8) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.6) (layers *.Cu *.Mask F.SilkS))
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A611D0D)
    (at 76.2 98.425 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -3.81 0 360) (layer F.SilkS))
    (fp_text value IRLML2502 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 /RESET))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /GND))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 102.87 124.46 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value IRLML2502 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 /RESET))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /GND))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 30 /~RESET0))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 102.87 106.68 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value IRLML2502 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 /RESET))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /GND))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 31 /~RESET1))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A9C5AF9)
    (at 102.87 88.9 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 -2.54 450) (layer F.SilkS))
    (fp_text value IRLML2502 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 /RESET))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /GND))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 /~RESET2))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 102.87 71.12 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value IRLML2502 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 /RESET))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /GND))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 33 /~RESET3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A5FCB8F)
    (at 78.74 127 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP101 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 7.41 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /ALT-3V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /3V-OUT))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /3V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A985A6B)
    (at 74.295 83.185)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP102 (at 0 7.62) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 7.41) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /ALT-5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /5V-OUT))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 5A5FCB94)
    (at 129.54 99.06 90)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference JP103 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Jumper (at 1.27 2.33 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /5GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 98.425 97.79)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q101 (at 0 -2.5) (layer F.SilkS))
    (fp_text value IRLML2244 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 29 /~RESET))
    (pad 2 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 /RESET))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_4x2 (layer F.Cu) (tedit 0)
    (at 65 98 270)
    (descr "Box header 4x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P1 (at 0 -5.7 270) (layer F.SilkS))
    (fp_text value MY_CONN_I2C (at 0 5.7 270) (layer F.SilkS) hide)
    (pad 8 thru_hole oval (at 3.81 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 28 /5GND))
    (pad 7 thru_hole oval (at 3.81 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 7 /GND))
    (pad 1 thru_hole rect (at -3.81 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 3 /3V))
    (pad 2 thru_hole oval (at -3.81 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 5 /5V))
    (pad 3 thru_hole oval (at -1.27 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SCL))
    (pad 4 thru_hole oval (at -1.27 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 22 /~INT))
    (pad 5 thru_hole oval (at 1.27 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 14 /SDA))
    (pad 6 thru_hole oval (at 1.27 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 29 /~RESET))
    (model walter/conn_strip/vasch_strip_4x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_4x2 (layer F.Cu) (tedit 5A9C5B0E)
    (at 115.57 106.68 180)
    (descr "Box header 4x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P5 (at -7.62 5.715 180) (layer F.SilkS))
    (fp_text value MY_CONN_I2C (at 0 5.7 180) (layer F.SilkS) hide)
    (pad 8 thru_hole oval (at 3.81 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 28 /5GND))
    (pad 7 thru_hole oval (at 3.81 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 7 /GND))
    (pad 1 thru_hole rect (at -3.81 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 25 /3V-OUT))
    (pad 2 thru_hole oval (at -3.81 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 26 /5V-OUT))
    (pad 3 thru_hole oval (at -1.27 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SCL1))
    (pad 4 thru_hole oval (at -1.27 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 15 /~INT1))
    (pad 5 thru_hole oval (at 1.27 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 12 /SDA1))
    (pad 6 thru_hole oval (at 1.27 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 31 /~RESET1))
    (model walter/conn_strip/vasch_strip_4x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_4x2 (layer F.Cu) (tedit 5A9C5B14)
    (at 115.57 71.12 180)
    (descr "Box header 4x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P7 (at -7.62 5.715 180) (layer F.SilkS))
    (fp_text value MY_CONN_I2C (at 0 5.7 180) (layer F.SilkS) hide)
    (pad 8 thru_hole oval (at 3.81 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 28 /5GND))
    (pad 7 thru_hole oval (at 3.81 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 7 /GND))
    (pad 1 thru_hole rect (at -3.81 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 25 /3V-OUT))
    (pad 2 thru_hole oval (at -3.81 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 26 /5V-OUT))
    (pad 3 thru_hole oval (at -1.27 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 19 /SCL3))
    (pad 4 thru_hole oval (at -1.27 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 20 /~INT3))
    (pad 5 thru_hole oval (at 1.27 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 21 /SDA3))
    (pad 6 thru_hole oval (at 1.27 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 33 /~RESET3))
    (model walter/conn_strip/vasch_strip_4x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "0 My Pins:KF141V-02P" (layer F.Cu) (tedit 5A985996)
    (at 70.739 71.12)
    (fp_text reference P8 (at 4.826 -0.635 90) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 /5GND))
    (pad 1 thru_hole circle (at 0 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 /5GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 /ALT-5V))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 /ALT-5V))
  )
  (module w_conn_pt-1,5:pt_1,5-2-3,5-h (layer F.Cu) (tedit 5A985991)
    (at 71.12 75.565 180)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P9 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 -5 180) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at -1.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 27 /ALT-5V))
    (pad 1 thru_hole rect (at 1.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 28 /5GND))
    (model walter/conn_pt-1_5/pt_1,5-2-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "0 My Pins:KF141V-02P" (layer F.Cu) (tedit 5A9859AA)
    (at 70.358 124.46 180)
    (fp_text reference P10 (at 4.318 -3.81 270) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 2.54 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 /ALT-3V))
    (pad 1 thru_hole circle (at 0 -2.54 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 /ALT-3V))
    (pad 2 thru_hole circle (at 2.54 2.54 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 /GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 /GND))
  )
  (module w_conn_pt-1,5:pt_1,5-2-3,5-h (layer F.Cu) (tedit 5A9859B0)
    (at 70.993 120.015)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P11 (at 0.127 -5.08 180) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 -5) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at -1.75 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 7 /GND))
    (pad 1 thru_hole rect (at 1.75 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 23 /ALT-3V))
    (model walter/conn_pt-1_5/pt_1,5-2-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 5A8B3ECD)
    (at 82.55 78.105 90)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference JP104 (at 6.985 0 90) (layer F.SilkS))
    (fp_text value Jumper (at 1.27 2.33 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(JP104-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /3V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A98596B)
    (at 60.325 120.015 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D101 (at 0 -1.905 450) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D101-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A64AD93)
    (at 83.82 97.79 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -3.81 0 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A8B466D)
    (at 71.755 107.95 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 4.445 0 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64AD9F)
    (at 80.01 86.36 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(JP7-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64ADA3)
    (at 82.55 86.36 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -5.08 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /SCL))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(JP104-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64AD86)
    (at 80.01 97.79 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 3.81 0 360) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64AEF5)
    (at 97.79 109.22 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCL1))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(P2-Pad12)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64AEF0)
    (at 95.25 109.22 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /SDA1))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(P2-Pad10)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64AEEC)
    (at 92.71 109.22 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 /~INT1))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(P2-Pad8)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64AEE8)
    (at 90.17 109.22 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /SCL0))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(P2-Pad6)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64AEE3)
    (at 87.63 109.22 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /SDA0))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(P2-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64AEDE)
    (at 85.09 109.22 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /~INT0))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(P2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64ADC6)
    (at 97.79 86.36 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at -5.08 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /~INT2))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(P3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64ADC2)
    (at 95.25 86.36 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R12 (at -5.08 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /SDA2))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(P3-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64ADBE)
    (at 92.71 86.36 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R13 (at -5.08 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /SCL2))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(P3-Pad6)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64ADB7)
    (at 90.17 86.36 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R14 (at -5.08 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 /~INT3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(P3-Pad8)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64ADAC)
    (at 87.63 86.36 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R15 (at -5.08 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 /SDA3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(P3-Pad10)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A64ADA7)
    (at 85.09 86.36 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R16 (at -5.08 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /SCL3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(P3-Pad12)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 104.14 97.79 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R101 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 /~RESET))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 108.585 97.79 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R102 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /GND))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 /RESET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A98596F)
    (at 62.23 114.3)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R103 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D101-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A8B404C)
    (at 77.47 104.775)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP5 (at -0.635 -2.54) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 7.41) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /3V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(JP5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A8B404F)
    (at 80.01 104.775)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP6 (at 0.635 -2.54) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 7.41) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /3V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(JP6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 5A8B3ECF)
    (at 80.01 78.105 90)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference JP7 (at 6.35 0 90) (layer F.SilkS))
    (fp_text value Jumper (at -0.635 3.81 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(JP7-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /3V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x06_Pitch2.54mm (layer F.Cu) (tedit 5A985BC3)
    (at 97.79 75.565 270)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference P3 (at 3.175 20.32 270) (layer F.SilkS))
    (fp_text value CONN_6X2 (at 1.27 15.03 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 6.35 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /VCC2))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /VCC2))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(P3-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /VCC2))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P3-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VCC3))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P3-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VCC3))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(P3-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VCC3))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P3-Pad12)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 66.04 83.82 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C3 (at 1.25 -4.46 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 1.25 4.46 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /3V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:KiCad-Logo2_8mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 129.54 114.3 270)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_8mm_SilkScreen (at 0.75 0 270) (layer B.Fab) hide)
  )
  (gr_text SDA0 (at 87.63 114.3 90) (layer F.SilkS))
  (gr_text SCL1 (at 97.79 114.3 90) (layer F.SilkS))
  (gr_text SDA2 (at 95.25 81.28 90) (layer F.SilkS))
  (gr_text SCL3 (at 85.09 81.28 90) (layer F.SilkS))
  (gr_text SDA (at 80.01 81.28 90) (layer F.SilkS))
  (gr_text Addr (at 78.74 114.935) (layer F.SilkS))
  (gr_text Alt (at 76.835 83.185 90) (layer F.SilkS))
  (gr_text Bus (at 76.835 87.63 90) (layer F.SilkS))
  (gr_text "5V Out" (at 71.755 85.725 90) (layer F.SilkS))
  (gr_text Bus (at 81.28 122.555 90) (layer F.SilkS))
  (gr_text "3V Out" (at 76.2 124.46 90) (layer F.SilkS))
  (gr_text Alt (at 81.28 127 90) (layer F.SilkS))
  (gr_text SCL (at 82.55 81.28 90) (layer F.SilkS))
  (gr_text "GND TIE" (at 132.08 97.79 90) (layer F.SilkS))
  (gr_line (start 57 134) (end 135 134) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 57 62) (end 135 62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 80 (width 0.3) (layer Cmts.User)
    (gr_text "80.000 mm" (at 96 43.65) (layer Cmts.User))
    (feature1 (pts (xy 56 60) (xy 56 42.3)))
    (feature2 (pts (xy 136 60) (xy 136 42.3)))
    (crossbar (pts (xy 136 45) (xy 56 45)))
    (arrow1a (pts (xy 56 45) (xy 57.126504 44.413579)))
    (arrow1b (pts (xy 56 45) (xy 57.126504 45.586421)))
    (arrow2a (pts (xy 136 45) (xy 134.873496 44.413579)))
    (arrow2b (pts (xy 136 45) (xy 134.873496 45.586421)))
  )
  (gr_text A1 (at 80.645 113.03) (layer F.SilkS))
  (gr_text 0 (at 74.93 108.585) (layer F.SilkS))
  (gr_text 0 (at 96.52 127.635) (layer F.SilkS))
  (gr_text 3V (at 89.535 130.81) (layer F.SilkS))
  (gr_text 5V (at 93.345 130.81) (layer F.SilkS))
  (gr_text 1 (at 96.52 125.095) (layer F.SilkS))
  (gr_text 2 (at 96.52 71.12) (layer F.SilkS))
  (gr_text "I2C Multiplexer 4" (at 130.175 113.03 90) (layer F.SilkS))
  (gr_text v2 (at 130.175 91.44 90) (layer F.SilkS))
  (gr_text by (at 130.175 86.995 90) (layer F.SilkS))
  (gr_text jeditekunum (at 130.175 80.01 90) (layer F.SilkS))
  (gr_text "Alt\n3V" (at 64.77 123.19) (layer F.SilkS))
  (gr_text + (at 73.66 64.516) (layer F.SilkS))
  (gr_text - (at 70.612 64.516) (layer F.SilkS))
  (gr_text "Pull\nUps" (at 102.87 118.11) (layer F.SilkS))
  (gr_text "Pull\nUps" (at 102.87 77.47) (layer F.SilkS))
  (gr_text SDA3 (at 87.63 81.28 90) (layer F.SilkS))
  (gr_text ~INT3 (at 90.17 81.28 90) (layer F.SilkS))
  (gr_text SCL2 (at 92.71 81.28 90) (layer F.SilkS))
  (gr_text ~INT2 (at 97.79 81.28 90) (layer F.SilkS))
  (gr_text ~INT1 (at 92.71 114.3 90) (layer F.SilkS))
  (gr_text SDA1 (at 95.25 114.3 90) (layer F.SilkS))
  (gr_text SCL0 (at 90.17 114.3 90) (layer F.SilkS))
  (gr_text ~INT0 (at 85.09 114.3 90) (layer F.SilkS))
  (gr_text A0 (at 76.835 113.03) (layer F.SilkS))
  (gr_text 1 (at 74.93 106.045) (layer F.SilkS))
  (gr_text "Alt\n5V" (at 64.77 73.025) (layer F.SilkS))
  (gr_text + (at 71.12 131.064) (layer F.SilkS))
  (gr_text - (at 68.58 131.064) (layer F.SilkS))
  (gr_text 3 (at 115.57 77.47) (layer F.SilkS))
  (gr_text 2 (at 115.57 95.25) (layer F.SilkS))
  (gr_text 1 (at 115.57 113.03) (layer F.SilkS))
  (gr_text 0 (at 115.57 130.81) (layer F.SilkS))
  (gr_text 3 (at 96.52 68.58) (layer F.SilkS))
  (gr_text 3V (at 89.535 65.405) (layer F.SilkS))
  (gr_text 5V (at 93.345 65.405) (layer F.SilkS))
  (gr_arc (start 135 133) (end 136 133) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 135 63) (end 135 62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136 133) (end 136 63) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 57 63) (end 56 63) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 57 133) (end 57 134) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 60 (width 0.3) (layer Cmts.User)
    (gr_text "60.000 mm" (at 31 98 90) (layer Cmts.User))
    (feature1 (pts (xy 40 68) (xy 29.3 68)))
    (feature2 (pts (xy 40 128) (xy 29.3 128)))
    (crossbar (pts (xy 32 128) (xy 32 68)))
    (arrow1a (pts (xy 32 68) (xy 32.586421 69.126504)))
    (arrow1b (pts (xy 32 68) (xy 31.413579 69.126504)))
    (arrow2a (pts (xy 32 128) (xy 32.586421 126.873496)))
    (arrow2b (pts (xy 32 128) (xy 31.413579 126.873496)))
  )
  (gr_line (start 56 63) (end 56 133) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 72 (width 0.3) (layer Cmts.User)
    (gr_text "72.000 mm" (at 26.65 98 90) (layer Cmts.User))
    (feature1 (pts (xy 33 62) (xy 25.3 62)))
    (feature2 (pts (xy 33 134) (xy 25.3 134)))
    (crossbar (pts (xy 28 134) (xy 28 62)))
    (arrow1a (pts (xy 28 62) (xy 28.586421 63.126504)))
    (arrow1b (pts (xy 28 62) (xy 27.413579 63.126504)))
    (arrow2a (pts (xy 28 134) (xy 28.586421 132.873496)))
    (arrow2b (pts (xy 28 134) (xy 27.413579 132.873496)))
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55.93 134) (xy 55.93 62) (xy 135.93 62) (xy 135.93 134) (xy 133.93 134)
      )
    )
    (polygon
      (pts        (xy 58 133) (xy 134 133) (xy 134 63) (xy 58 63)
      )
    )
  )
)
