<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="105.0925" x2="0" y2="1.5875" width="0" layer="20"/>
<wire x1="0" y1="1.5875" x2="1.5875" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.5875" y1="0" x2="106.3625" y2="0" width="0" layer="20"/>
<wire x1="106.3625" y1="0" x2="107.95" y2="1.5875" width="0" layer="20" curve="90"/>
<wire x1="107.95" y1="1.5875" x2="107.95" y2="105.0925" width="0" layer="20"/>
<wire x1="107.95" y1="105.0925" x2="106.3625" y2="106.68" width="0" layer="20" curve="90"/>
<wire x1="106.3625" y1="106.68" x2="1.5875" y2="106.68" width="0" layer="20"/>
<wire x1="1.5875" y1="106.68" x2="0" y2="105.0925" width="0" layer="20" curve="90"/>
<text>IOREF</text>
<text>MOSI</text>
<text>0V</text>
<text>!RESET</text>
<text>SCK</text>
<text>MISO</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>SDA</text>
<text>SCL</text>
<text>13</text>
<text>14</text>
<text>22</text>
<text>0V</text>
<text>VIN</text>
<text>0V</text>
<text>0V</text>
<text>3V3</text>
<text>!RESET</text>
<text>IOREF</text>
<text>A6</text>
<text>A7</text>
<text>0V</text>
<text>A5</text>
<text>A4</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>AREF</text>
<text>PulseDAQ</text>
<text>EPCCS.ORG</text>
<text>15063^0</text>
<text>JMP NONE: 9V
  JMP 1-2: 24V
     JMP 2-3: 12V
</text>
<text>SPI</text>
<text>JTAG</text>
<text>TCK</text>
<text>TDO</text>
<text>TMS</text>
<text>NC</text>
<text>TDI</text>
<text>GND</text>
<text>GND</text>
<text>5V</text>
<text>!RESET</text>
<text>NC</text>
<text>ADJ
AREF</text>
<text>D0 RX0</text>
<text>D1 TX0</text>
<text>B2 INT2</text>
<text>B5 ICP3/MOSI</text>
<text>D2 INT0/RX1</text>
<text>D3 INT1/TX1</text>
<text>B0 T0</text>
<text>B4 OC0B</text>
<text>B3 OC0A</text>
<text>C7</text>
<text>D6 
OC2B/ICP1</text>
<text>D5 OC1A</text>
<text>D4 OC1B</text>
<text>D7 OC2A</text>
<text>B6 OC2B</text>
<text>B7 OC3B</text>
<text>0V</text>
<text>AREF</text>
<text>C1 SDA</text>
<text>C0 SCL</text>
<text>5V</text>
<text>NC</text>
<text>NC</text>
<text>VIN</text>
<text>GND</text>
<text>GND</text>
<text>5V</text>
<text>3V3</text>
<text>!RESET</text>
<text>IOREF 5V</text>
<text>NC</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>A6</text>
<text>A7</text>
<text>0V</text>
<text>NC</text>
<text>PV+</text>
<text>PV-</text>
<text>B=4250
  100K</text>
<text>+BAT</text>
<text>-BAT</text>
<text>B=4250
  100K</text>
<text>CHARGE RATE IS FUNCTION 
OF PV POWER UP TO MAX, 
ABOUT 0.11A PER WATT.</text>
<text>POWER SEQUENCE CONTROL
PROVIDES SINGLE EVENT 
AT 6.58V AND DISCONNECT 
AT 5.88V.</text>
<text>6.71V:50.7k@40ºC
6.8365V:100k@25ºC
7.048V:357k@0ºC</text>
<text>MPP IDEAL:ACTUAL
13.8:14.5V-15.2k@70ºC
15.8:15.7V-50.7k@40ºC
17:16.8V-100k@25ºC
19:18.7V-357k@0ºC</text>
<text>S2: FORCE
CONNECT</text>
<text>S1: FORCE
LOAD</text>
<text>PROTECTED DIO</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>0V</text>
<text>0V</text>
<text>INPUTS</text>
<text>15mA</text>
<text>A</text>
<text>K</text>
<text>K</text>
<text>A</text>
<text>ANALOG (OR OC OUT)</text>
<text>0V</text>
<text>5V</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>FLOW PULSE</text>
<text>A</text>
<text>K</text>
<text>FLOW COMPUTER</text>
<text>OC</text>
<text>E</text>
<text>LAUNCH</text>
<text>A</text>
<text>K</text>
<text>LATCHING SOLENOID DRIVERS</text>
<text>-RESET+
+ SET -</text>
<text>-RESET+
+ SET -</text>
<text>-RESET+
+ SET -</text>
<text>K3</text>
<text>K2</text>
<text>K1</text>
<text>ADS1220 CH4</text>
<text>IDAC2</text>
<text>0V</text>
<text>A3</text>
<text>A2</text>
<text> A1
IDAC1</text>
<text>A0</text>
<text>ADS1220 CH3</text>
<text>IDAC2</text>
<text>0V</text>
<text>A3</text>
<text>A2</text>
<text> A1
IDAC1</text>
<text>A0</text>
<text>ADS1220 CH2</text>
<text>IDAC2</text>
<text>0V</text>
<text>A3</text>
<text>A2</text>
<text> A1
IDAC1</text>
<text>A0</text>
<text>ADS1220 CH1</text>
<text>IDAC2</text>
<text>0V</text>
<text>A3</text>
<text>A2</text>
<text> A1
IDAC1</text>
<text>A0</text>
<text>FT</text>
<text>S2</text>
<text>S1</text>
<text>&amp;</text>
<text>FT</text>
<text>OC</text>
<text>E</text>
<text>S1</text>
<text>OC</text>
<text>E</text>
<text>S2</text>
</plain>
<libraries>
<library name="R-C">
<description>&lt;pre&gt;CHIP RESISTOR
NOTE: rounded pads... http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf
See section on Tombstoneing. Lead free solder may not wet edges, and IPC does not allow exposed copper. 
My (rsutherland@epccs) experience suggest highly rounded pads reduce solder beads that can be extruded along edges of larger capacitors (0805).

USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="C0805(2012)">
<description>&lt;pre&gt;EIA 0805 (Metric Code Size 2012) Ceramic Chip
rounded pads are added in IPC 782 rev A
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
<package name="C1210(3225)">
<description>&lt;pre&gt;EIA 1210 (Metric Code Size 3225) Ceramic Chip
rounded pads are added in IPC 782 rev A.
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
</packages>
</library>
<library name="C-C">
<description>&lt;pre&gt; MULTILAYER CERAMIC CHIP CAPACITORS

Type: C1005 [EIA CC0402], C1608 [EIA CC0603], C2012 [EIA CC0805],
C3216 [EIA CC1206], C3225 [EIA CC1210], C4532 [EIA CC1812], C5750 [EIA CC2220]

CH 0±60 ppm/°C -25 to +85°C
C0G 0±30 ppm/°C -55 to +125°C
JB ±10% -25 to +85°C
X5R ±15% -55 to +85°C
X6S ±22% -55 to +105°C
X7R ±15% -55 to +125°C
X7S ±22% -55 to +125°C
X7T +22/-33% -55 to +125°C

TDK voltage cods
0G 4V
0J 6.3V
1A 10V
1C 16V
1E 25V
1V 35V
1H 50V
2A 100V
2E 250V
2V 350V
2W 450V
2J 630V

NOTE: rounded pads... http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf
See section on Tombstoneing. Lead free solder may not wet edges, and IPC does not allow exposed copper. 
My (rsutherland@epccs) experience suggest highly rounded pads reduce solder beads that can be extruded along edges of larger capacitors (0805).

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="C0603(1608)">
<description>&lt;pre&gt;EIA 0603 (Metric Code Size 1608) Ceramic Chip Capacitor
rounded pads are added in IPC 782 rev A, this pad was on Arduino Due and may have originated from Sparkfun.
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
<package name="C1206(3216)">
<description>&lt;pre&gt;EIA 1206 (Metric Code Size 3216) Ceramic Chip Capacitor
rounded pads are added in IPC 782 rev A.
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
<package name="C0805(2012)">
<description>&lt;pre&gt;EIA 0805 (Metric Code Size 2012) Ceramic Chip Capacitor
rounded pads are added in IPC 782 rev A, this pad was on Arduino and may have originated from Sparkfun.
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
</packages>
</library>
<library name="J-HDR3.5mm">
<description>&lt;pre&gt;HEADER 3.5MM center to center
USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="MCV4">
<description>&lt;pre&gt;MCV 1,5/4-G-3,5-RN [PHOENIX CONTACT,1843622] CONN HEADER SHROUDED 4POS 3.5MM
PST 1,0/4-3,5 [PHOENIX CONTACT,1945119] CONN HEADER STRIP PIN 4POS 3.5MM

Drill Size 3/64": .0469" (1.2mm)</description>
</package>
<package name="MCV6">
<description>&lt;pre&gt;MCV 1,5/6-G-3,5 [PHOENIX CONTACT,1843648] CONN HEADER SHROUDED 6POS 3.5MM
MCVR 1,5/6-ST-3,5 [PHOENIX CONTACT,1863194] CONN PLUG 6POS SCREW 3.5MM
PST 1,0/6-3,5 [PHOENIX CONTACT,1945135] CONN HEADER STRIP PIN 6POS 3.5MM
PT 1,5/6-PVH-3,5 [PHOENIX CONTACT,1984057] CONN PLUG STRIP 6POS 3.5MM

Drill Size 3/64": .0469" (1.2mm)</description>
</package>
<package name="MCV8">
<description>&lt;pre&gt;PHOENIX CONTACT 1843664
MCV 1,5/ 8-G-3,5
Drill Size 3/64": .0469" (1.2mm)</description>
</package>
<package name="MCV2">
<description>&lt;pre&gt;MCV 1,5/2-G-3,5-RN [PHOENIX CONTACT,1731471] CONN HEADER SHROUDED 2POS 3.5MM
PST 1,0/2-3,5 [PHOENIX CONTACT,1945096] CONN HEADER STRIP PIN 2POS 3.5MM

Drill Size 3/64": .0469" (1.2mm)</description>
</package>
</packages>
</library>
<library name="F-RST">
<description>&lt;pre&gt;Resettable Fuses
 
USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="C1206(3216)">
<description>&lt;pre&gt;EIA 1206 (Metric Code Size 3216) Ceramic Chip Capacitor
rounded pads are added in IPC 782 rev A.
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
<package name="GRID20BDY50DRL32">
<description>&lt;pre&gt;grid .2in (5.08mm), body .5in (13mm)
Drill .032in, Note: 20AWG is 0.032 and will not fit</description>
</package>
</packages>
</library>
<library name="D-GP">
<description>&lt;pre&gt;GEN PURPOSE DIODE
USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SMA">
<description>&lt;pre&gt;SMB 
http://www.diodes.com/datasheets/ap02001.pdf
center to center 4 mm
pad 2.5X x 1.7Y mm</description>
</package>
<package name="SOD123">
<description>&lt;pre&gt;SOD123
http://www.diodes.com/datasheets/ap02001.pdf</description>
</package>
</packages>
</library>
<library name="Q-NCH">
<description>&lt;pre&gt;N-CHANNEL MOSFET
ENHANCEMENT MODE is shown with a open/broken channel
DEPLETION MODE is shown with a closed/complete channel thus the idea of being on with zero gate voltage.

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOT23">
<description>&lt;pre&gt;SOT23 (based on SOT23-6) pin 3 is alone
http://www.diodes.com/_files/zetex_files/pack/SOT23-6.pdf
center(1) to center(2,3) 2.2 mm
center(2) to center(3) 1.9mm
pad .65X x 1.06Y mm</description>
</package>
</packages>
</library>
<library name="Q-NPN">
<description>&lt;pre&gt;NPN Bipolar junction transistor

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOT23">
<description>&lt;pre&gt;SOT23 (based on SOT23-6) pin 1 is alone (Cathode)
http://www.diodes.com/_files/zetex_files/pack/SOT23-6.pdf
center(1) to center(2,3) 2.2 mm
center(2) to center(3) 1.9mm
pad .65X x 1.06Y mm</description>
</package>
</packages>
</library>
<library name="HW-DINMnt">
<description>&lt;pre&gt;DIN Rail Adapters

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="USA10">
<description>&lt;pre&gt;USA10-4.6 [PhxCont,1202713] DINRAIL ADAPTER UNIVERSAL 10MM 4.6MM
with #6 screw size mounting holes</description>
</package>
</packages>
</library>
<library name="K-OPT">
<description>&lt;pre&gt;  Optocoupler, Photo Sensor, Optical Switch
http://en.wikipedia.org/wiki/Light-emitting_diode

USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SMD4">
<description>&lt;pre&gt;FODM121 [FAIRCHILD,FODM121AR2] OPTOCOUPLER TRANSISTOR 3750VRMS 4SMD
PC452 [FAIRCHILD,PC452J00000F] OPTOCOUPLER DARL 3750VRMS 4SMD</description>
</package>
</packages>
</library>
<library name="U-7400">
<description>&lt;pre&gt;Logic

USE AT YOUR OWN RISK...
This was form cadsoft libraian, but much of it is not valid, I have only 
looked at parts I'm using so far...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="14SOIC">
<description>&lt;pre&gt;14POS SMALL OUTLINE (14SO[IC])
pitch 1.27
pad .6mm X1.8mm
body-Center to pad-Center 2.7mm

referance TI's SOIC package, but pads are little larger and rounded</description>
</package>
<package name="SOT23-6,SOT26">
<description>&lt;pre&gt;Small Outline SOT23-6, SOT26, SC-74A</description>
</package>
<package name="16SOIC">
<description>&lt;pre&gt;Small Outline (SO/SOIC) package 1.27mm [50 mil] pitch, 4mm wide body, 6.2mm wide pin-pin, 10mm long
e.g. 74HC151 [TI,SN74HC151D] LOGIC 8TO1 MUX 16SOIC</description>
</package>
</packages>
</library>
<library name="H-Fiducial">
<description>&lt;pre&gt;Fiducianl Mark
USE AT YOUR OWN RISK...
Copyright (C) 2013 Ronald Steven Sutherland
Permission is granted to copy, distribute and/or modify this document 
under the terms of the GNU Free Documentation License, Version 1.2 or 
any later version published by the Free Software Foundation; with no 
Invariant Sections, no Front-Cover Texts, and no Back-Cover Texts. A 
copy of the license is included in the section entitled "GNU Free 
Documentation License".</description>
<packages>
<package name="FIDUCIAL-1.27">
<description>&lt;pre&gt;Fiducian R=1.27mm 
STOP=2.54mm
It is up to designer to not put traces under Fiducial (i.e. Void or sold plane only)
Autorouter restricted areas are defined as RECTangles, POLYGONs, or CIRCLEs on the 
tRestrict, bRestrict, or vRestrict layers.</description>
</package>
</packages>
</library>
<library name="J-BoardHDR">
<description>&lt;pre&gt;Arduino Footprint
Standard Interface
USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="ARDUINO_UNO">
<description>&lt;pre&gt;UNO R3 board footprint</description>
</package>
</packages>
</library>
<library name="C-T">
<description>&lt;pre&gt;Tantalum Electrolytic Capacitors
EIA Code 	Case Code 	L 	W 	H 	W1 	A
Tolerance 	±0.2 	+0.2/–0.1 	+0.2/–0.1 	+0.2 	+0.3/–0.2
3216-10 	I, K 	3.2 	1.6 	1.0 (max) 	1.2 	0.8
3216-12 	S 	3.2 	1.6 	1.2 (max) 	1.2 	0.8
3216-18 	A 	3.2 	1.6 	1.6 	1.2 	0.8
3528-12 	T 	3.5 	2.8 	1.2 (max) 	2.2 	0.8
3528-15 	M, H 	3.5 	2.8 	1.5 (max) 	2.2 	0.8
3528-21 	B 	3.5 	2.8 	1.9 	2.2 	0.8
6032-15 	U, W 	6.0 	3.2 	1.5 (max) 	2.2 	1.3
6032-28 	C 	6.0 	3.2 	2.6 	2.2 	1.3
7343-20 	V, Y 	7.3 	4.3 	2.0 (max) 	2.4 	1.3
7343-31 	D 	7.3 	4.3 	2.9 	2.4 	1.3
7343-43 	X, E 	7.3 	4.3 	4.1 	2.4 	1.3

Metric	[inch]
2013 	[0805]
3216 	[1206]
3528 	[1411]
6032 	[2413]
7343 	[2917]

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="3216">
<description>&lt;pre&gt;3.2mm x 1.6mm
Surface mount dimensions (EIA standard package sizes)
EIA Code 	Case Code 	L 	W 	H 	W1 	A
Tolerance 	±0.2 	+0.2/–0.1 	+0.2/–0.1 	+0.2 	+0.3/–0.2
3216-10 	I, K 	3.2 	1.6 	1.0 (max) 	1.2 	0.8
3216-12 	S, P 	3.2 	1.6 	1.2 (max) 	1.2 	0.8
3216-18 	A 	3.2 	1.6 	1.6 	1.2 	0.8

Note 3.2mm x 1.6mm is about 1206 (or .012 x .006 in)</description>
</package>
</packages>
</library>
<library name="L-FB">
<description>&lt;pre&gt;CHIP FERRITE BEADS
NOTE: rounded pads... http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf
See section on Tombstoneing. Lead free solder may not wet edges, and IPC does not allow exposed copper. 
My (rsutherland@epccs) experience suggest rounded pads reduce solder beads that can be extruded along edges of larger capacitors (0805) and similar devices.

USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="C0805(2012)">
<description>&lt;pre&gt;EIA 0805 (Metric Code Size 2012) Ferrite Chip
rounded pads are added in IPC 782 rev A
http://www.kemet.com/kemet/web/homepage/kfbk3.nsf/vaFeedbackFAQ/2209BDBA03843BBF85256BCD004EBC11/$file/f2100e.pdf</description>
</package>
</packages>
</library>
<library name="U-AVR">
<description>&lt;pre&gt;MCU's 8bit AVR 

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="ISP">
</package>
<package name="TQFP44">
<description>&lt;b&gt;44-lead Thin Quad Flat Package&lt;/b&gt;</description>
</package>
<package name="JTAG">
</package>
</packages>
</library>
<library name="Y-XTL">
<description>&lt;pre&gt;CRYSTAL
i.e. NDK NX3225SA-12.000000MHZ-STD-CSR-1

USE AT YOUR OWN RISK...

Copyright (C) 2014 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="CRYSTAL5X3.2MM">
<description>&lt;pre&gt; 16MHZ10 [ABRACON,ABM3B-16.000MHZ-10-1-U-T] CRYSTAL 16MHZ 10PF 10PPM SMD3.2X5MM</description>
</package>
</packages>
</library>
<library name="P-DCDC">
<description>&lt;pre&gt;POWER SUPPLIE DC 2 DC
some units are for schmatics only

USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOT223">
<description>&lt;pre&gt;SOT223
http://www.diodes.com/datasheets/ap02001.pdf</description>
</package>
<package name="SOT23-5,SOT25">
<description>&lt;pre&gt;Small Outline SOT23-5,SOT25,SC-74A</description>
</package>
</packages>
</library>
<library name="U-BUCK">
<description>&lt;pre&gt;BUCK Control and ilk

USE AT YOUR OWN RISK...

Copyright (C) 2015 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="12MSOP-EDP-HAND">
<description>&lt;pre&gt;12 Micro-SMALL OUTLINE PACKAGE (MSOP) with Exposed Die Pad
Warning: This Exposed Die Pad is setup for hand solder, not PnP.</description>
</package>
</packages>
</library>
<library name="L-PSMD">
<description>&lt;pre&gt;Inductor Power SMD

USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="L3939">
<description>&lt;pre&gt;Dimension (mm): 0.39 x 0.39 (10.1 x 10.1)
15UH2A2 [TDK,SLF10145T-150M2R2-PF] INDUCTOR POWER SHIELDED 15UH 2A2 SMD</description>
</package>
</packages>
</library>
<library name="S-Tactile">
<description>&lt;pre&gt;Switch Tactile/Snap-acting

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="C0805(2012)">
<description>&lt;pre&gt;EIA 0805 (Metric Code Size 2012) Ceramic Chip
rounded pads are added in IPC 782 rev A</description>
</package>
</packages>
</library>
<library name="U-Linear">
<description>&lt;pre&gt;Linear Amplifiers, Sensor Interfaces

USE AT YOUR OWN RISK...

Copyright (C) 2014 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOT23-6">
<description>&lt;pre&gt; Based on TI drawing 4204403-3/E which falls within JEDEC MO-193 variation AA (6p in)</description>
</package>
<package name="SOT23">
<description>&lt;pre&gt;SOT23 (based on SOT23-6) pin 1 is alone (Cathode)
http://www.diodes.com/_files/zetex_files/pack/SOT23-6.pdf
center(1) to center(2,3) 2.2 mm
center(2) to center(3) 1.9mm
pad .65X x 1.06Y mm</description>
</package>
</packages>
</library>
<library name="Q-PCH">
<description>&lt;pre&gt;N-CHANNEL MOSFET
ENHANCEMENT MODE is shown with a open/broken channel
DEPLETION MODE is shown with a closed/complete channel thus the idea of being on with zero gate voltage.

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOT23">
<description>&lt;pre&gt;SOT23 (based on SOT23-6) pin 3 is alone
http://www.diodes.com/_files/zetex_files/pack/SOT23-6.pdf
center(1) to center(2,3) 2.2 mm
center(2) to center(3) 1.9mm
pad .65X x 1.06Y mm</description>
</package>
</packages>
</library>
<library name="D-SBR">
<description>&lt;pre&gt;Super Barrier Rectifier
Super barrier diodes are rectifier diodes that incorporate the low forward voltage
drop of the Schottky diode with the surge-handling capability and low reverse 
leakage current of a normal p–n junction diode.

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SMA">
<description>&lt;pre&gt;SMB 
http://www.diodes.com/datasheets/ap02001.pdf
center to center 4 mm
pad 2.5X x 1.7Y mm</description>
</package>
</packages>
</library>
<library name="R-Trim">
<description>&lt;pre&gt;TRIMMER RESISTOR

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="3006P">
<description>&lt;pre&gt;3006P103 [BOURNS,3006P-1-103LF] TRIMMER 10K 0.75W 15TURN SIDE-ADJ</description>
</package>
</packages>
</library>
<library name="J-HDR2.54mm">
<description>&lt;pre&gt;HEADER 2.54MM center to center

USE AT YOUR OWN RISK...
 
Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="F1X10">
<description>&lt;pre&gt;FEMALE HEADER 10POS</description>
</package>
<package name="F1X8">
<description>&lt;pre&gt;FEMALE HEADER 8POS</description>
</package>
<package name="1X3">
<description>&lt;pre&gt;4 PIN 
.1" CENTER 
0.040" DRILL
auto PAD

http://www.sullinscorp.com/catalogs/78_Page80-81_HEADER_.100_2.54mm_FEMALE.pdf</description>
</package>
</packages>
</library>
<library name="C-Al">
<description>&lt;pre&gt;Aluminum Electrolytic Capacitors

USE AT YOUR OWN RISK...

Copyright (C) 2013 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="E7,5-18">
<description>&lt;pre&gt;ELECTROLYTIC CAPACITOR
pin spacing 7.5 mm, body diameter 18 mm
PW1J222 [NICHICON,UPW1J222MHD] CAP ALUM 63V 2200UF 20% RADIAL</description>
</package>
<package name="E5-10">
<description>&lt;pre&gt;ELECTROLYTIC CAPACITOR
pin spacing 5 mm, body diameter 10 mm
PW1J101 [NICHICON,UPW1J101MPD] CAP ALUM 63V 100UF 20% RADIAL</description>
</package>
</packages>
</library>
<library name="U-Boost">
<description>&lt;pre&gt;Boost Regulator
For step-up DC-DC

USE AT YOUR OWN RISK...

Copyright (C) 2014 Ronald Steven Sutherland
Released under the Creative Commons 
Attribution Share-Alike 3.0 License
http://creativecommons.org/licenses/by-sa/3.0</description>
<packages>
<package name="SOIC8">
<description>&lt;pre&gt;8POS Standard SMALLl OUTLINE Package (SO/SOIC) Narrow Body</description>
</package>
</packages>
</library>
<library name="L-PWR">
<description>&lt;pre&gt;Inductor Power

USE AT YOUR OWN RISK...
 
    Copyright (C) 2015 Ronald Sutherland
    Released under the Creative Commons 
    Attribution-ShareAlike 4.0 International
    http://creativecommons.org/licenses/by-sa/4.0</description>
<packages>
<package name="L2626">
<description>&lt;pre&gt;Dimension (mm): .26 x .26 (6.5 x 6.5)

SRR0604-101 [Bourns,SRR0604-101KL] INDUCTOR POWER SHIELDED 100UH SMD</description>
</package>
</packages>
</library>
<library name="U-ADC">
<description>&lt;pre&gt;Analog-to-Digital Converters

USE AT YOUR OWN RISK...

    Copyright (C) 2015 Ronald Sutherland
    Released under the Creative Commons 
    Attribution-ShareAlike 4.0 International
    http://creativecommons.org/licenses/by-sa/4.0</description>
<packages>
<package name="16TSSOP">
<description>&lt;pre&gt;16POS THIN SHRINK SMALL OUTLINE PACKAGE (16-TSSOP)


I (R Sutherland) based this on TI's drawing (4040064-4/G) for package type PW (R-PDSO-G16) ... PLASTIC SMALL OUTLINE</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="HW1" library="HW-DINMnt" package="USA10" value="USA10-4,6">
<attribute name="NAME"/>
</element>
<element name="HW2" library="HW-DINMnt" package="USA10" value="USA10-4,6">
<attribute name="NAME"/>
</element>
<element name="R153" library="R-C" package="C0805(2012)" value="49.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R156" library="R-C" package="C0805(2012)" value="49.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q127" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R148" library="R-C" package="C0805(2012)" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D108" library="D-GP" package="SMA" value="S1A">
<attribute name="NAME"/>
</element>
<element name="Q128" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R149" library="R-C" package="C0805(2012)" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D109" library="D-GP" package="SMA" value="S1A">
<attribute name="NAME"/>
</element>
<element name="R145" library="R-C" package="C0805(2012)" value="49.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R146" library="R-C" package="C0805(2012)" value="49.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K106" library="K-OPT" package="SMD4" value="FODM121SMD4">
<attribute name="NAME"/>
</element>
<element name="R152" library="R-C" package="C0805(2012)" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U106" library="U-7400" package="14SOIC" value="74HC00">
<attribute name="NAME"/>
</element>
<element name="U107" library="U-7400" package="14SOIC" value="74HC00">
<attribute name="NAME"/>
</element>
<element name="K103" library="K-OPT" package="SMD4" value="FODM121SMD4">
<attribute name="NAME"/>
</element>
<element name="K104" library="K-OPT" package="SMD4" value="FODM121SMD4">
<attribute name="NAME"/>
</element>
<element name="R147" library="R-C" package="C0805(2012)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R150" library="R-C" package="C0805(2012)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K105" library="K-OPT" package="SMD4" value="FODM121SMD4">
<attribute name="NAME"/>
</element>
<element name="R151" library="R-C" package="C0805(2012)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R120" library="R-C" package="C0805(2012)" value="249">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R117" library="R-C" package="C0805(2012)" value="1.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R134" library="R-C" package="C0805(2012)" value="249">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R118" library="R-C" package="C0805(2012)" value="1.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R135" library="R-C" package="C0805(2012)" value="249">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R133" library="R-C" package="C0805(2012)" value="1.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R157" library="R-C" package="C0805(2012)" value="1.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q129" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R158" library="R-C" package="C0805(2012)" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F102" library="F-RST" package="C1206(3216)" value="bD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F103" library="F-RST" package="C1206(3216)" value="bD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="H-Fiducial" package="FIDUCIAL-1.27" value="FIDUCIAL1.27"/>
<element name="U$2" library="H-Fiducial" package="FIDUCIAL-1.27" value="FIDUCIAL1.27"/>
<element name="U$3" library="H-Fiducial" package="FIDUCIAL-1.27" value="FIDUCIAL1.27"/>
<element name="U104" library="U-7400" package="SOT23-6,SOT26" value="74LVC1G97">
<attribute name="NAME"/>
</element>
<element name="C109" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C111" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C112" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="WH3" library="J-BoardHDR" package="ARDUINO_UNO" value="ARDUINO-UNO"/>
<element name="C14" library="C-T" package="3216" value="106A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="C-C" package="C0603(1608)" value="10pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="C-C" package="C0603(1608)" value="10pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="L-FB" package="C0805(2012)" value="JMP">
<attribute name="NAME"/>
</element>
<element name="C17" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J14" library="U-AVR" package="ISP" value="ISP-SPI"/>
<element name="R35" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="Y1" library="Y-XTL" package="CRYSTAL5X3.2MM" value="16MHZ">
<attribute name="NAME"/>
</element>
<element name="U4" library="U-AVR" package="TQFP44" value="ATMEGA1284P-AU">
<attribute name="NAME"/>
</element>
<element name="J13" library="U-AVR" package="JTAG" value="ISP-JTAG"/>
<element name="U5" library="P-DCDC" package="SOT223" value="MIC2920A-5">
<attribute name="NAME"/>
</element>
<element name="R15" library="R-C" package="C1210(3225)" value="OPEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="R-C" package="C0805(2012)" value="80.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="R-C" package="C0805(2012)" value="330k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="R-C" package="C0805(2012)" value="309k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="U-BUCK" package="12MSOP-EDP-HAND" value="LT3652"/>
<element name="R29" library="R-C" package="C0805(2012)" value="80.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="R-C" package="C1210(3225)" value="0R068">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="L-PSMD" package="L3939" value="15uH 2A2"/>
<element name="D2" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="C1" library="C-C" package="C0805(2012)" value="1uF"/>
<element name="C5" library="C-C" package="C0805(2012)" value="1uF"/>
<element name="R13" library="R-C" package="C0805(2012)" value="121k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="R-C" package="C0805(2012)" value="49.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="F-RST" package="GRID20BDY50DRL32" value="U250">
<attribute name="NAME"/>
</element>
<element name="R26" library="R-C" package="C0805(2012)" value="**10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="R-C" package="C0805(2012)" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="R-C" package="C0805(2012)" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="S-Tactile" package="C0805(2012)" value="PAD"/>
<element name="C4" library="C-C" package="C0805(2012)" value=".1uF"/>
<element name="D3" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="R2" library="R-C" package="C0805(2012)" value="205k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="R-C" package="C0805(2012)" value="*100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="R-C" package="C0805(2012)" value="20k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="R-C" package="C0805(2012)" value="309k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="R-C" package="C0805(2012)" value="20k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="R-C" package="C0805(2012)" value="274k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="U-Linear" package="SOT23-6" value="TPS3700">
<attribute name="NAME"/>
</element>
<element name="Q6" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="R-C" package="C0805(2012)" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="S2" library="S-Tactile" package="C0805(2012)" value="PAD">
<attribute name="NAME"/>
</element>
<element name="C2" library="C-C" package="C0603(1608)" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="R-C" package="C0805(2012)" value="5.62k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="D-SBR" package="SMA" value="SQ4"/>
<element name="D1" library="D-SBR" package="SMA" value="SQ4">
<attribute name="NAME"/>
</element>
<element name="R22" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="R-C" package="C0805(2012)" value="18.0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="R-C" package="C0805(2012)" value="49.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="R-C" package="C0805(2012)" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="U-Linear" package="SOT23" value="TLVH431">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="R-C" package="C0805(2012)" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="R-Trim" package="3006P" value="10k"/>
<element name="R19" library="R-C" package="C0805(2012)" value="JMP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="R-C" package="C0805(2012)" value="OPEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J17" library="J-HDR2.54mm" package="F1X10" value="PPPC101LFBN">
<attribute name="NAME"/>
</element>
<element name="J18" library="J-HDR2.54mm" package="F1X8" value="PPPC081LFBN">
<attribute name="NAME"/>
</element>
<element name="J16" library="J-HDR2.54mm" package="F1X10" value="PPPC101LFBN">
<attribute name="NAME"/>
</element>
<element name="J15" library="J-HDR2.54mm" package="F1X10" value="PPPC101LFBN"/>
<element name="R5" library="R-C" package="C0805(2012)" value="OPEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="R-C" package="C0805(2012)" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="R-C" package="C0805(2012)" value="432k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="R-C" package="C0805(2012)" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="R-C" package="C0805(2012)" value="200k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R119" library="R-C" package="C0805(2012)" value="249">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R116" library="R-C" package="C0805(2012)" value="1.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U102" library="U-7400" package="16SOIC" value="74HC238">
<attribute name="NAME"/>
</element>
<element name="C105" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q105" library="Q-NCH" package="SOT23" value="34N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q104" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R104" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R105" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q106" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R106" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q103" library="Q-NCH" package="SOT23" value="34N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q102" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R103" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R102" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q101" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R101" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C101" library="C-Al" package="E7,5-18" value="PW1J222">
<attribute name="NAME"/>
</element>
<element name="D101" library="D-SBR" package="SMA" value="SQ4">
<attribute name="NAME"/>
</element>
<element name="Q117" library="Q-NCH" package="SOT23" value="34N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q116" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R127" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R128" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q118" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R129" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q115" library="Q-NCH" package="SOT23" value="34N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q114" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R126" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R125" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q113" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R124" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C104" library="C-Al" package="E7,5-18" value="PW1J222"/>
<element name="D104" library="D-SBR" package="SMA" value="SQ4">
<attribute name="NAME"/>
</element>
<element name="Q125" library="Q-NCH" package="SOT23" value="34N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q124" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R140" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R141" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q126" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R142" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q123" library="Q-NCH" package="SOT23" value="34N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q122" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R139" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R138" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q121" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R137" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C108" library="C-Al" package="E7,5-18" value="PW1J222"/>
<element name="D105" library="D-SBR" package="SMA" value="SQ4">
<attribute name="NAME"/>
</element>
<element name="U101" library="U-Boost" package="SOIC8" value="MC34063A">
<attribute name="NAME"/>
</element>
<element name="Q119" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R112" library="R-C" package="C0805(2012)" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C103" library="C-C" package="C0603(1608)" value="330pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R109" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R130" library="R-C" package="C0805(2012)" value="15.8k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D102" library="D-SBR" package="SMA" value="SQ4">
<attribute name="NAME"/>
</element>
<element name="C107" library="C-Al" package="E5-10" value="PW1J101"/>
<element name="R113" library="R-C" package="C1210(3225)" value="1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q109" library="Q-PCH" package="SOT23" value="DMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q107" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q108" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R114" library="R-C" package="C0805(2012)" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R115" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R107" library="R-C" package="C0805(2012)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R108" library="R-C" package="C0805(2012)" value="5.62K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C106" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L101" library="L-PWR" package="L2626" value="150UH 0A3">
<attribute name="NAME"/>
</element>
<element name="R111" library="R-C" package="C0805(2012)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J19" library="J-HDR2.54mm" package="1X3" value="PBC03SAA"/>
<element name="R110" library="R-C" package="C0805(2012)" value="43.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R131" library="R-C" package="C0805(2012)" value="8.45k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C102" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D103" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="U103" library="P-DCDC" package="SOT223" value="LM317">
<attribute name="NAME"/>
</element>
<element name="R132" library="R-C" package="C0805(2012)" value="82.5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K101" library="K-OPT" package="SMD4" value="FODM121SMD4">
<attribute name="NAME"/>
</element>
<element name="K102" library="K-OPT" package="SMD4" value="FODM121SMD4">
<attribute name="NAME"/>
</element>
<element name="C22" library="C-T" package="3216" value="106A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="P-DCDC" package="SOT23-5,SOT25" value="KB33">
<attribute name="NAME"/>
</element>
<element name="C23" library="C-C" package="C0603(1608)" value="470pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R155" library="R-C" package="C0805(2012)" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K107" library="K-OPT" package="SMD4" value="FODM121SMD4">
<attribute name="NAME"/>
</element>
<element name="U108" library="U-7400" package="SOT23-6,SOT26" value="74LVC1G97">
<attribute name="NAME"/>
</element>
<element name="C113" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q131" library="Q-NCH" package="SOT23" value="K38">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R154" library="R-C" package="C0805(2012)" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D111" library="D-GP" package="SMA" value="S1A">
<attribute name="NAME"/>
</element>
<element name="F104" library="F-RST" package="C1206(3216)" value="bD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C210" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U202" library="U-7400" package="16SOIC" value="74HC138">
<attribute name="NAME"/>
</element>
<element name="U201" library="U-7400" package="14SOIC" value="74LVC07A">
<attribute name="NAME"/>
</element>
<element name="R202" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R203" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C216" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R214" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U204" library="U-7400" package="14SOIC" value="74LVC07A">
<attribute name="NAME"/>
</element>
<element name="C232" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R201" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R206" library="R-C" package="C0805(2012)" value="3.74k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U105" library="U-7400" package="14SOIC" value="">
<attribute name="NAME"/>
</element>
<element name="R207" library="R-C" package="C0805(2012)" value="2.49k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R204" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R205" library="R-C" package="C0805(2012)" value="4.99k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R144" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R143" library="R-C" package="C0805(2012)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q110" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R121" library="R-C" package="C0805(2012)" value="OPEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q111" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R122" library="R-C" package="C0805(2012)" value="OPEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q112" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R123" library="R-C" package="C0805(2012)" value="OPEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q120" library="Q-NPN" package="SOT23" value="K1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R136" library="R-C" package="C0805(2012)" value="OPEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C110" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="J-HDR3.5mm" package="MCV4" value="PST1,0/4-3,5">
<attribute name="NAME"/>
</element>
<element name="J2" library="J-HDR3.5mm" package="MCV4" value="PST1,0/4-3,5">
<attribute name="NAME"/>
</element>
<element name="J4" library="J-HDR3.5mm" package="MCV6" value="PST1,0/6-3,5">
<attribute name="NAME"/>
</element>
<element name="J7" library="J-HDR3.5mm" package="MCV8" value="PST1,0/8-3,5">
<attribute name="NAME"/>
</element>
<element name="J8" library="J-HDR3.5mm" package="MCV6" value="PST1,0/6-3,5">
<attribute name="NAME"/>
</element>
<element name="F101" library="F-RST" package="C1206(3216)" value="bD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="J-HDR3.5mm" package="MCV4" value="PST1,0/4-3,5">
<attribute name="NAME"/>
</element>
<element name="D112" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="D106" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="D107" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="D110" library="D-GP" package="SOD123" value="T4">
<attribute name="NAME"/>
</element>
<element name="C201" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C204" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C207" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R213" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R210" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R208" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R209" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C205" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C215" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C214" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C203" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C202" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U203" library="U-ADC" package="16TSSOP" value="ADS1220">
<attribute name="NAME"/>
</element>
<element name="C206" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C209" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C208" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J11" library="J-HDR3.5mm" package="MCV6" value="PST1,0/6-3,5">
<attribute name="NAME"/>
</element>
<element name="C217" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C219" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C222" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R217" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R216" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R212" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R215" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C212" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C223" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C220" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C218" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C211" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C221" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C213" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U205" library="U-ADC" package="16TSSOP" value="ADS1220">
<attribute name="NAME"/>
</element>
<element name="C224" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="J-HDR3.5mm" package="MCV6" value="PST1,0/6-3,5">
<attribute name="NAME"/>
</element>
<element name="C233" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C244" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C246" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R225" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R224" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R220" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R221" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C236" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C247" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C245" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C235" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C234" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C237" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C238" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U206" library="U-ADC" package="16TSSOP" value="ADS1220">
<attribute name="NAME"/>
</element>
<element name="C239" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J10" library="J-HDR3.5mm" package="MCV6" value="PST1,0/6-3,5">
<attribute name="NAME"/>
</element>
<element name="C225" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C240" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C242" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R223" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R222" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R218" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R219" library="R-C" package="C0805(2012)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C228" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C243" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C241" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C227" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C226" library="C-C" package="C0805(2012)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C229" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C230" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U207" library="U-ADC" package="16TSSOP" value="ADS1220">
<attribute name="NAME"/>
</element>
<element name="C231" library="C-C" package="C1206(3216)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J12" library="J-HDR3.5mm" package="MCV6" value="PST1,0/6-3,5">
<attribute name="NAME"/>
</element>
<element name="R211" library="R-C" package="C0805(2012)" value="1.24k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="C-C" package="C0603(1608)" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="J-HDR3.5mm" package="MCV6" value="PST1,0/6-3,5">
<attribute name="NAME"/>
</element>
<element name="J6" library="J-HDR3.5mm" package="MCV2" value="PST1,0/2-3,5">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="0V">
<contactref element="D108" pad="A"/>
<contactref element="D109" pad="A"/>
<contactref element="K106" pad="3"/>
<contactref element="Q129" pad="2(S)"/>
<contactref element="U106" pad="7"/>
<contactref element="C111" pad="2"/>
<contactref element="U107" pad="7"/>
<contactref element="C112" pad="2"/>
<contactref element="C109" pad="2"/>
<contactref element="U104" pad="2"/>
<contactref element="C20" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C18" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="Y1" pad="4"/>
<contactref element="Y1" pad="2"/>
<contactref element="U4" pad="6"/>
<contactref element="U4" pad="18"/>
<contactref element="U4" pad="39"/>
<contactref element="U4" pad="28"/>
<contactref element="C16" pad="2"/>
<contactref element="J14" pad="6"/>
<contactref element="J13" pad="10"/>
<contactref element="J13" pad="2"/>
<contactref element="C14" pad="-"/>
<contactref element="C15" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="R30" pad="1"/>
<contactref element="R26" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="D4" pad="A"/>
<contactref element="U1" pad="SNK6"/>
<contactref element="C5" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="U1" pad="SNK5"/>
<contactref element="U1" pad="SNK7"/>
<contactref element="U1" pad="SNK0"/>
<contactref element="U1" pad="SNK1"/>
<contactref element="U1" pad="SNK3"/>
<contactref element="U1" pad="SNK4"/>
<contactref element="C4" pad="2"/>
<contactref element="Q3" pad="E"/>
<contactref element="Q4" pad="E"/>
<contactref element="R34" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="R33" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="S2" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="C8" pad="2"/>
<contactref element="J16" pad="4"/>
<contactref element="J18" pad="2"/>
<contactref element="J18" pad="3"/>
<contactref element="J17" pad="9"/>
<contactref element="R32" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="R37" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="Q101" pad="E"/>
<contactref element="Q103" pad="2(S)"/>
<contactref element="Q106" pad="E"/>
<contactref element="Q105" pad="2(S)"/>
<contactref element="C101" pad="-"/>
<contactref element="Q113" pad="E"/>
<contactref element="Q115" pad="2(S)"/>
<contactref element="Q118" pad="E"/>
<contactref element="Q117" pad="2(S)"/>
<contactref element="C104" pad="-"/>
<contactref element="Q121" pad="E"/>
<contactref element="Q123" pad="2(S)"/>
<contactref element="Q126" pad="E"/>
<contactref element="Q125" pad="2(S)"/>
<contactref element="C108" pad="-"/>
<contactref element="U101" pad="4"/>
<contactref element="C103" pad="2"/>
<contactref element="C106" pad="2"/>
<contactref element="C107" pad="-"/>
<contactref element="R108" pad="1"/>
<contactref element="C102" pad="2"/>
<contactref element="R130" pad="1"/>
<contactref element="R110" pad="2"/>
<contactref element="R131" pad="2"/>
<contactref element="U101" pad="2"/>
<contactref element="D103" pad="C"/>
<contactref element="K101" pad="3"/>
<contactref element="K102" pad="3"/>
<contactref element="U6" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C22" pad="-"/>
<contactref element="K107" pad="3"/>
<contactref element="U102" pad="5"/>
<contactref element="U102" pad="8"/>
<contactref element="U102" pad="4"/>
<contactref element="C105" pad="2"/>
<contactref element="U108" pad="3"/>
<contactref element="U108" pad="2"/>
<contactref element="C113" pad="2"/>
<contactref element="D111" pad="A"/>
<contactref element="U202" pad="8"/>
<contactref element="U202" pad="5"/>
<contactref element="U105" pad="7"/>
<contactref element="C110" pad="2"/>
<contactref element="R119" pad="1"/>
<contactref element="Q110" pad="E"/>
<contactref element="R120" pad="1"/>
<contactref element="Q111" pad="E"/>
<contactref element="R134" pad="1"/>
<contactref element="Q112" pad="E"/>
<contactref element="R135" pad="1"/>
<contactref element="Q120" pad="E"/>
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="2"/>
<contactref element="J4" pad="6"/>
<contactref element="U201" pad="7"/>
<contactref element="C216" pad="2"/>
<contactref element="C210" pad="2"/>
<contactref element="U202" pad="4"/>
<contactref element="J3" pad="4"/>
<contactref element="U204" pad="7"/>
<contactref element="C232" pad="2"/>
<contactref element="C201" pad="2"/>
<contactref element="C214" pad="2"/>
<contactref element="C215" pad="2"/>
<contactref element="C202" pad="2"/>
<contactref element="C205" pad="2"/>
<contactref element="C203" pad="2"/>
<contactref element="C204" pad="2"/>
<contactref element="C207" pad="2"/>
<contactref element="U203" pad="5"/>
<contactref element="U203" pad="4"/>
<contactref element="C206" pad="2"/>
<contactref element="U201" pad="13"/>
<contactref element="U204" pad="13"/>
<contactref element="C217" pad="2"/>
<contactref element="C220" pad="2"/>
<contactref element="C223" pad="2"/>
<contactref element="C211" pad="2"/>
<contactref element="C212" pad="2"/>
<contactref element="C218" pad="2"/>
<contactref element="C219" pad="2"/>
<contactref element="C222" pad="2"/>
<contactref element="U205" pad="5"/>
<contactref element="U205" pad="4"/>
<contactref element="C221" pad="2"/>
<contactref element="J9" pad="5"/>
<contactref element="J11" pad="5"/>
<contactref element="C233" pad="2"/>
<contactref element="C245" pad="2"/>
<contactref element="C247" pad="2"/>
<contactref element="C234" pad="2"/>
<contactref element="C236" pad="2"/>
<contactref element="C235" pad="2"/>
<contactref element="C244" pad="2"/>
<contactref element="C246" pad="2"/>
<contactref element="C237" pad="2"/>
<contactref element="U206" pad="5"/>
<contactref element="U206" pad="4"/>
<contactref element="J10" pad="5"/>
<contactref element="C225" pad="2"/>
<contactref element="C241" pad="2"/>
<contactref element="C243" pad="2"/>
<contactref element="C226" pad="2"/>
<contactref element="C228" pad="2"/>
<contactref element="C227" pad="2"/>
<contactref element="C240" pad="2"/>
<contactref element="C242" pad="2"/>
<contactref element="C229" pad="2"/>
<contactref element="U207" pad="5"/>
<contactref element="U207" pad="4"/>
<contactref element="J12" pad="5"/>
<contactref element="U5" pad="TAB"/>
<contactref element="C21" pad="2"/>
<contactref element="J5" pad="6"/>
<contactref element="R38" pad="1"/>
</signal>
<signal name="PWR">
<contactref element="R4" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="U1" pad="9"/>
<contactref element="C7" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="C6" pad="1"/>
<contactref element="F1" pad="1"/>
<contactref element="R28" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="C11" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="Q1" pad="2(S)"/>
<contactref element="R36" pad="2"/>
</signal>
<signal name="PV_IN">
<contactref element="C3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="D1" pad="K"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="R153" pad="1"/>
<contactref element="K103" pad="1"/>
<contactref element="K104" pad="1"/>
<contactref element="R158" pad="1"/>
<contactref element="C109" pad="1"/>
<contactref element="U104" pad="5"/>
<contactref element="U106" pad="14"/>
<contactref element="C111" pad="1"/>
<contactref element="C112" pad="1"/>
<contactref element="U107" pad="14"/>
<contactref element="U104" pad="3"/>
<contactref element="Q128" pad="1(G)"/>
<contactref element="Q127" pad="1(G)"/>
<contactref element="L2" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="R35" pad="2"/>
<contactref element="D6" pad="C"/>
<contactref element="U4" pad="17"/>
<contactref element="U4" pad="38"/>
<contactref element="U4" pad="5"/>
<contactref element="J14" pad="2"/>
<contactref element="J13" pad="4"/>
<contactref element="C14" pad="+"/>
<contactref element="U5" pad="3"/>
<contactref element="J18" pad="7"/>
<contactref element="R5" pad="1"/>
<contactref element="Q119" pad="2(S)"/>
<contactref element="R145" pad="1"/>
<contactref element="R146" pad="1"/>
<contactref element="U102" pad="6"/>
<contactref element="U102" pad="16"/>
<contactref element="C105" pad="1"/>
<contactref element="R156" pad="1"/>
<contactref element="U108" pad="1"/>
<contactref element="C113" pad="1"/>
<contactref element="U108" pad="5"/>
<contactref element="Q131" pad="1(G)"/>
<contactref element="R214" pad="2"/>
<contactref element="K105" pad="1"/>
<contactref element="F101" pad="2"/>
<contactref element="L2" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="U4" pad="27"/>
<contactref element="J18" pad="4"/>
</signal>
<signal name="IO2">
<contactref element="U107" pad="10"/>
<contactref element="U4" pad="11"/>
<contactref element="J15" pad="5"/>
<contactref element="K102" pad="4"/>
<contactref element="R146" pad="2"/>
</signal>
<signal name="IO3">
<contactref element="U106" pad="10"/>
<contactref element="U4" pad="12"/>
<contactref element="J15" pad="6"/>
<contactref element="K101" pad="4"/>
<contactref element="R145" pad="2"/>
</signal>
<signal name="IO5">
<contactref element="R149" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="J15" pad="8"/>
<contactref element="U4" pad="44"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="IO6">
<contactref element="U4" pad="43"/>
<contactref element="J15" pad="9"/>
<contactref element="R154" pad="2"/>
</signal>
<signal name="IO7">
<contactref element="U4" pad="26"/>
<contactref element="J15" pad="10"/>
<contactref element="U102" pad="1"/>
</signal>
<signal name="N$48">
<contactref element="R155" pad="1"/>
<contactref element="K107" pad="1"/>
<contactref element="D112" pad="C"/>
</signal>
<signal name="N$51">
<contactref element="Q127" pad="2(S)"/>
<contactref element="R148" pad="1"/>
</signal>
<signal name="N$52">
<contactref element="Q127" pad="3(D)"/>
<contactref element="D108" pad="K"/>
<contactref element="F102" pad="1"/>
</signal>
<signal name="N$53">
<contactref element="Q128" pad="2(S)"/>
<contactref element="R149" pad="1"/>
</signal>
<signal name="N$54">
<contactref element="Q128" pad="3(D)"/>
<contactref element="D109" pad="K"/>
<contactref element="F103" pad="1"/>
</signal>
<signal name="IO6_">
<contactref element="F104" pad="2"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="IO5_">
<contactref element="F103" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$39">
<contactref element="K106" pad="2"/>
<contactref element="D110" pad="A"/>
<contactref element="J7" pad="7"/>
</signal>
<signal name="N$59">
<contactref element="K106" pad="1"/>
<contactref element="R152" pad="2"/>
<contactref element="D110" pad="C"/>
</signal>
<signal name="STOP">
<contactref element="U106" pad="3"/>
<contactref element="R147" pad="2"/>
<contactref element="U106" pad="4"/>
<contactref element="U104" pad="6"/>
</signal>
<signal name="N$63">
<contactref element="K103" pad="4"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="N$64">
<contactref element="K103" pad="3"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="N$65">
<contactref element="K104" pad="4"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="N$66">
<contactref element="K104" pad="3"/>
<contactref element="J7" pad="4"/>
</signal>
<signal name="START">
<contactref element="R150" pad="2"/>
<contactref element="U107" pad="3"/>
<contactref element="U107" pad="4"/>
<contactref element="U104" pad="1"/>
</signal>
<signal name="N$68">
<contactref element="U106" pad="6"/>
<contactref element="U106" pad="1"/>
</signal>
<signal name="N$69">
<contactref element="U106" pad="8"/>
<contactref element="U106" pad="2"/>
</signal>
<signal name="N$70">
<contactref element="U107" pad="6"/>
<contactref element="U107" pad="1"/>
</signal>
<signal name="N$71">
<contactref element="U107" pad="8"/>
<contactref element="U107" pad="2"/>
</signal>
<signal name="N$73">
<contactref element="K105" pad="3"/>
<contactref element="J7" pad="6"/>
</signal>
<signal name="N$74">
<contactref element="K105" pad="4"/>
<contactref element="J7" pad="5"/>
</signal>
<signal name="N$75">
<contactref element="R117" pad="1"/>
<contactref element="R120" pad="2"/>
<contactref element="Q111" pad="C"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="N$77">
<contactref element="R118" pad="1"/>
<contactref element="R134" pad="2"/>
<contactref element="Q112" pad="C"/>
<contactref element="J5" pad="4"/>
</signal>
<signal name="N$79">
<contactref element="R133" pad="1"/>
<contactref element="R135" pad="2"/>
<contactref element="Q120" pad="C"/>
<contactref element="J5" pad="5"/>
</signal>
<signal name="N$49">
<contactref element="U106" pad="11"/>
<contactref element="U106" pad="9"/>
</signal>
<signal name="N$50">
<contactref element="U107" pad="11"/>
<contactref element="U107" pad="9"/>
</signal>
<signal name="N$61">
<contactref element="R147" pad="1"/>
<contactref element="K103" pad="2"/>
</signal>
<signal name="N$62">
<contactref element="R150" pad="1"/>
<contactref element="K104" pad="2"/>
</signal>
<signal name="N$72">
<contactref element="Q129" pad="3(D)"/>
<contactref element="R151" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U106" pad="12"/>
<contactref element="U106" pad="13"/>
<contactref element="U107" pad="12"/>
<contactref element="U107" pad="13"/>
<contactref element="U106" pad="5"/>
<contactref element="U107" pad="5"/>
<contactref element="R158" pad="2"/>
<contactref element="U105" pad="12"/>
</signal>
<signal name="ADC2">
<contactref element="R118" pad="2"/>
<contactref element="U4" pad="35"/>
<contactref element="J17" pad="3"/>
<contactref element="R123" pad="2"/>
</signal>
<signal name="ADC3">
<contactref element="R133" pad="2"/>
<contactref element="U4" pad="34"/>
<contactref element="J17" pad="4"/>
<contactref element="R136" pad="2"/>
</signal>
<signal name="ADC4">
<contactref element="R157" pad="2"/>
<contactref element="U4" pad="33"/>
<contactref element="J17" pad="5"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="IO8">
<contactref element="U4" pad="15"/>
<contactref element="J16" pad="10"/>
<contactref element="U108" pad="4"/>
</signal>
<signal name="INT2">
<contactref element="R153" pad="2"/>
<contactref element="K106" pad="4"/>
<contactref element="U4" pad="42"/>
<contactref element="J15" pad="2"/>
<contactref element="R157" pad="1"/>
<contactref element="R205" pad="2"/>
<contactref element="R206" pad="2"/>
<contactref element="R207" pad="2"/>
<contactref element="R211" pad="2"/>
</signal>
<signal name="IO14">
<contactref element="U4" pad="1"/>
<contactref element="J14" pad="4"/>
<contactref element="J15" pad="1"/>
<contactref element="R143" pad="1"/>
<contactref element="U105" pad="11"/>
</signal>
<signal name="T1">
<contactref element="U4" pad="41"/>
<contactref element="R20" pad="1"/>
<contactref element="U6" pad="3"/>
<contactref element="U105" pad="13"/>
<contactref element="R38" pad="2"/>
</signal>
<signal name="C6">
<contactref element="U4" pad="25"/>
<contactref element="U102" pad="2"/>
</signal>
<signal name="ADC1">
<contactref element="R117" pad="2"/>
<contactref element="U4" pad="36"/>
<contactref element="J17" pad="2"/>
<contactref element="R122" pad="2"/>
</signal>
<signal name="ADC6">
<contactref element="U4" pad="31"/>
<contactref element="J17" pad="7"/>
<contactref element="R32" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="RX">
<contactref element="U4" pad="9"/>
<contactref element="J15" pad="3"/>
</signal>
<signal name="TX">
<contactref element="U4" pad="10"/>
<contactref element="J15" pad="4"/>
</signal>
<signal name="IO4">
<contactref element="U4" pad="40"/>
<contactref element="J15" pad="7"/>
<contactref element="R148" pad="2"/>
</signal>
<signal name="IO9">
<contactref element="U4" pad="14"/>
<contactref element="J16" pad="9"/>
<contactref element="U201" pad="3"/>
</signal>
<signal name="VIN">
<contactref element="C15" pad="1"/>
<contactref element="U5" pad="1"/>
<contactref element="Q2" pad="1(G)"/>
<contactref element="Q1" pad="3(D)"/>
<contactref element="R7" pad="1"/>
<contactref element="J18" pad="1"/>
<contactref element="R114" pad="2"/>
<contactref element="R115" pad="1"/>
<contactref element="Q109" pad="2(S)"/>
<contactref element="U6" pad="1"/>
<contactref element="U103" pad="3"/>
</signal>
<signal name="TDO">
<contactref element="U4" pad="23"/>
<contactref element="J13" pad="3"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="TMS">
<contactref element="R22" pad="1"/>
<contactref element="U4" pad="22"/>
<contactref element="J13" pad="5"/>
</signal>
<signal name="TDI">
<contactref element="U4" pad="24"/>
<contactref element="J13" pad="9"/>
<contactref element="U102" pad="3"/>
</signal>
<signal name="AREF">
<contactref element="C18" pad="1"/>
<contactref element="U4" pad="29"/>
<contactref element="R6" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="J16" pad="3"/>
</signal>
<signal name="ADC0">
<contactref element="U4" pad="37"/>
<contactref element="J17" pad="1"/>
<contactref element="R116" pad="2"/>
<contactref element="R121" pad="2"/>
</signal>
<signal name="ADC5">
<contactref element="U4" pad="32"/>
<contactref element="J17" pad="6"/>
<contactref element="R107" pad="2"/>
<contactref element="R108" pad="2"/>
<contactref element="C102" pad="1"/>
</signal>
<signal name="IO10">
<contactref element="U4" pad="13"/>
<contactref element="J16" pad="8"/>
<contactref element="U201" pad="1"/>
</signal>
<signal name="IO11">
<contactref element="U4" pad="16"/>
<contactref element="J16" pad="7"/>
<contactref element="U201" pad="5"/>
</signal>
<signal name="IO12">
<contactref element="J14" pad="1"/>
<contactref element="U4" pad="2"/>
<contactref element="J16" pad="6"/>
<contactref element="R214" pad="1"/>
<contactref element="U204" pad="2"/>
<contactref element="U204" pad="4"/>
<contactref element="U204" pad="6"/>
<contactref element="U204" pad="8"/>
<contactref element="U204" pad="10"/>
</signal>
<signal name="IO13">
<contactref element="J14" pad="3"/>
<contactref element="U4" pad="3"/>
<contactref element="J16" pad="5"/>
<contactref element="U201" pad="9"/>
</signal>
<signal name="SDA">
<contactref element="U4" pad="20"/>
<contactref element="J16" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="U4" pad="19"/>
<contactref element="J16" pad="1"/>
</signal>
<signal name="ADC7">
<contactref element="U4" pad="30"/>
<contactref element="J17" pad="8"/>
<contactref element="R37" pad="2"/>
<contactref element="R36" pad="1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$115">
<contactref element="C19" pad="2"/>
<contactref element="Y1" pad="3"/>
<contactref element="U4" pad="8"/>
</signal>
<signal name="N$116">
<contactref element="C20" pad="2"/>
<contactref element="Y1" pad="1"/>
<contactref element="U4" pad="7"/>
</signal>
<signal name="!RESET!">
<contactref element="J14" pad="5"/>
<contactref element="R35" pad="1"/>
<contactref element="D6" pad="A"/>
<contactref element="U4" pad="4"/>
<contactref element="J13" pad="6"/>
<contactref element="J18" pad="6"/>
</signal>
<signal name="TCK">
<contactref element="J13" pad="1"/>
<contactref element="U4" pad="21"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="SW">
<contactref element="U1" pad="12"/>
<contactref element="L1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="D4" pad="K"/>
</signal>
<signal name="SENSE">
<contactref element="R15" pad="2"/>
<contactref element="U1" pad="10"/>
<contactref element="R3" pad="2"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="7"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="TC+">
<contactref element="R29" pad="1"/>
<contactref element="R28" pad="2"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="TC-">
<contactref element="R29" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="D2" pad="C"/>
<contactref element="U1" pad="11"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="R14" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="Q3" pad="C"/>
</signal>
<signal name="NTC1">
<contactref element="U1" pad="8"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="D1" pad="A"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$46">
<contactref element="Q3" pad="B"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="5V88PL-DWN">
<contactref element="R16" pad="2"/>
<contactref element="D3" pad="C"/>
<contactref element="R25" pad="1"/>
<contactref element="Q5" pad="1(G)"/>
</signal>
<signal name="BAT">
<contactref element="R16" pad="1"/>
<contactref element="Q5" pad="2(S)"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="!FAULT">
<contactref element="U1" pad="5"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R11" pad="2"/>
<contactref element="Q4" pad="B"/>
</signal>
<signal name="N$7">
<contactref element="Q4" pad="C"/>
<contactref element="R34" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="Q2" pad="2(S)"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="R2" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="Q6" pad="2(S)"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="U3" pad="3"/>
<contactref element="R33" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="Q6" pad="1(G)"/>
<contactref element="R24" pad="2"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="6V58PL-DWN">
<contactref element="Q2" pad="3(D)"/>
<contactref element="R4" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="Q1" pad="1(G)"/>
</signal>
<signal name="N$17">
<contactref element="S2" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="D5" pad="C"/>
<contactref element="U3" pad="6"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="S1" pad="1"/>
<contactref element="Q6" pad="3(D)"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="F1" pad="2"/>
<contactref element="Q5" pad="3(D)"/>
</signal>
<signal name="N$103">
<contactref element="R8" pad="2"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$104">
<contactref element="U2" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$105">
<contactref element="R6" pad="2"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$106">
<contactref element="R18" pad="1"/>
<contactref element="R17" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="R116" pad="1"/>
<contactref element="R119" pad="2"/>
<contactref element="Q110" pad="C"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U101" pad="6"/>
<contactref element="C107" pad="+"/>
<contactref element="R113" pad="1"/>
<contactref element="Q108" pad="1(G)"/>
<contactref element="R114" pad="1"/>
<contactref element="Q109" pad="3(D)"/>
<contactref element="C106" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="Q105" pad="3(D)"/>
<contactref element="Q104" pad="3(D)"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="Q104" pad="1(G)"/>
<contactref element="R104" pad="1"/>
<contactref element="R105" pad="2"/>
</signal>
<signal name="SET-K1">
<contactref element="Q103" pad="1(G)"/>
<contactref element="R106" pad="1"/>
<contactref element="U102" pad="13"/>
</signal>
<signal name="N$28">
<contactref element="R105" pad="1"/>
<contactref element="Q106" pad="C"/>
</signal>
<signal name="N$29">
<contactref element="Q106" pad="B"/>
<contactref element="R106" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="Q103" pad="3(D)"/>
<contactref element="Q102" pad="3(D)"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="Q102" pad="1(G)"/>
<contactref element="R103" pad="1"/>
<contactref element="R102" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="R102" pad="1"/>
<contactref element="Q101" pad="C"/>
</signal>
<signal name="N$37">
<contactref element="Q101" pad="B"/>
<contactref element="R101" pad="2"/>
</signal>
<signal name="BOOST1">
<contactref element="Q104" pad="2(S)"/>
<contactref element="R104" pad="2"/>
<contactref element="Q102" pad="2(S)"/>
<contactref element="R103" pad="2"/>
<contactref element="C101" pad="+"/>
<contactref element="D101" pad="K"/>
</signal>
<signal name="RESET-K1">
<contactref element="Q105" pad="1(G)"/>
<contactref element="R101" pad="1"/>
<contactref element="U102" pad="12"/>
</signal>
<signal name="BOOST">
<contactref element="D101" pad="A"/>
<contactref element="D104" pad="A"/>
<contactref element="D105" pad="A"/>
<contactref element="R109" pad="1"/>
<contactref element="D102" pad="K"/>
<contactref element="R107" pad="1"/>
</signal>
<signal name="SMPS">
<contactref element="U102" pad="14"/>
<contactref element="Q119" pad="1(G)"/>
<contactref element="Q107" pad="1(G)"/>
</signal>
<signal name="SET-K2">
<contactref element="U102" pad="11"/>
<contactref element="Q115" pad="1(G)"/>
<contactref element="R129" pad="1"/>
</signal>
<signal name="RESET-K2">
<contactref element="U102" pad="10"/>
<contactref element="Q117" pad="1(G)"/>
<contactref element="R124" pad="1"/>
</signal>
<signal name="SET-K3">
<contactref element="U102" pad="9"/>
<contactref element="Q123" pad="1(G)"/>
<contactref element="R142" pad="1"/>
</signal>
<signal name="RESET-K3">
<contactref element="U102" pad="7"/>
<contactref element="Q125" pad="1(G)"/>
<contactref element="R137" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="Q117" pad="3(D)"/>
<contactref element="Q116" pad="3(D)"/>
<contactref element="J8" pad="4"/>
</signal>
<signal name="N$30">
<contactref element="Q116" pad="1(G)"/>
<contactref element="R127" pad="1"/>
<contactref element="R128" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="R128" pad="1"/>
<contactref element="Q118" pad="C"/>
</signal>
<signal name="N$32">
<contactref element="Q118" pad="B"/>
<contactref element="R129" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="Q115" pad="3(D)"/>
<contactref element="Q114" pad="3(D)"/>
<contactref element="J8" pad="3"/>
</signal>
<signal name="N$38">
<contactref element="Q114" pad="1(G)"/>
<contactref element="R126" pad="1"/>
<contactref element="R125" pad="2"/>
</signal>
<signal name="N$45">
<contactref element="R125" pad="1"/>
<contactref element="Q113" pad="C"/>
</signal>
<signal name="N$60">
<contactref element="Q113" pad="B"/>
<contactref element="R124" pad="2"/>
</signal>
<signal name="BOOST2">
<contactref element="Q116" pad="2(S)"/>
<contactref element="R127" pad="2"/>
<contactref element="Q114" pad="2(S)"/>
<contactref element="R126" pad="2"/>
<contactref element="C104" pad="+"/>
<contactref element="D104" pad="K"/>
</signal>
<signal name="N$67">
<contactref element="Q125" pad="3(D)"/>
<contactref element="Q124" pad="3(D)"/>
<contactref element="J8" pad="6"/>
</signal>
<signal name="N$83">
<contactref element="Q124" pad="1(G)"/>
<contactref element="R140" pad="1"/>
<contactref element="R141" pad="2"/>
</signal>
<signal name="N$84">
<contactref element="R141" pad="1"/>
<contactref element="Q126" pad="C"/>
</signal>
<signal name="N$85">
<contactref element="Q126" pad="B"/>
<contactref element="R142" pad="2"/>
</signal>
<signal name="N$86">
<contactref element="Q123" pad="3(D)"/>
<contactref element="Q122" pad="3(D)"/>
<contactref element="J8" pad="5"/>
</signal>
<signal name="N$89">
<contactref element="Q122" pad="1(G)"/>
<contactref element="R139" pad="1"/>
<contactref element="R138" pad="2"/>
</signal>
<signal name="N$90">
<contactref element="R138" pad="1"/>
<contactref element="Q121" pad="C"/>
</signal>
<signal name="N$91">
<contactref element="Q121" pad="B"/>
<contactref element="R137" pad="2"/>
</signal>
<signal name="BOOST3">
<contactref element="Q124" pad="2(S)"/>
<contactref element="R140" pad="2"/>
<contactref element="Q122" pad="2(S)"/>
<contactref element="R139" pad="2"/>
<contactref element="C108" pad="+"/>
<contactref element="D105" pad="K"/>
</signal>
<signal name="N$13">
<contactref element="U101" pad="5"/>
<contactref element="Q119" pad="3(D)"/>
<contactref element="R111" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="U101" pad="8"/>
<contactref element="R112" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="R112" pad="1"/>
<contactref element="U101" pad="7"/>
<contactref element="R113" pad="2"/>
<contactref element="L101" pad="2"/>
</signal>
<signal name="N$41">
<contactref element="U101" pad="1"/>
<contactref element="D102" pad="A"/>
<contactref element="L101" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="U101" pad="3"/>
<contactref element="C103" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="Q108" pad="3(D)"/>
<contactref element="Q107" pad="2(S)"/>
</signal>
<signal name="N$92">
<contactref element="R115" pad="2"/>
<contactref element="Q107" pad="3(D)"/>
<contactref element="Q109" pad="1(G)"/>
</signal>
<signal name="N$93">
<contactref element="R111" pad="1"/>
<contactref element="R109" pad="2"/>
<contactref element="R130" pad="2"/>
<contactref element="J19" pad="2"/>
</signal>
<signal name="N$120">
<contactref element="J19" pad="3"/>
<contactref element="R110" pad="1"/>
</signal>
<signal name="N$121">
<contactref element="J19" pad="1"/>
<contactref element="R131" pad="1"/>
</signal>
<signal name="N$94">
<contactref element="Q108" pad="2(S)"/>
<contactref element="D103" pad="A"/>
</signal>
<signal name="N$95">
<contactref element="U103" pad="1"/>
<contactref element="R132" pad="2"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="N$97">
<contactref element="R132" pad="1"/>
<contactref element="U103" pad="2"/>
</signal>
<signal name="N$55">
<contactref element="K101" pad="1"/>
<contactref element="D106" pad="C"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$96">
<contactref element="K102" pad="1"/>
<contactref element="D107" pad="C"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="3V3_S">
<contactref element="J18" pad="5"/>
<contactref element="C22" pad="+"/>
<contactref element="U6" pad="5"/>
<contactref element="U202" pad="16"/>
<contactref element="R202" pad="1"/>
<contactref element="R203" pad="1"/>
<contactref element="R201" pad="1"/>
<contactref element="R204" pad="2"/>
<contactref element="R144" pad="2"/>
<contactref element="C210" pad="1"/>
<contactref element="C216" pad="1"/>
<contactref element="U201" pad="14"/>
<contactref element="U202" pad="6"/>
<contactref element="U201" pad="11"/>
<contactref element="C232" pad="1"/>
<contactref element="U204" pad="14"/>
<contactref element="C110" pad="1"/>
<contactref element="U105" pad="14"/>
<contactref element="C201" pad="1"/>
<contactref element="U203" pad="12"/>
<contactref element="U203" pad="13"/>
<contactref element="C217" pad="1"/>
<contactref element="U205" pad="12"/>
<contactref element="U205" pad="13"/>
<contactref element="C233" pad="1"/>
<contactref element="U206" pad="12"/>
<contactref element="U206" pad="13"/>
<contactref element="C225" pad="1"/>
<contactref element="U207" pad="12"/>
<contactref element="U207" pad="13"/>
</signal>
<signal name="N$57">
<contactref element="C23" pad="1"/>
<contactref element="U6" pad="4"/>
</signal>
<signal name="N$98">
<contactref element="R155" pad="2"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="N$47">
<contactref element="K101" pad="2"/>
<contactref element="D106" pad="A"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$99">
<contactref element="K102" pad="2"/>
<contactref element="D107" pad="A"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="FT">
<contactref element="R156" pad="2"/>
<contactref element="K107" pad="4"/>
<contactref element="U108" pad="6"/>
<contactref element="Q129" pad="1(G)"/>
</signal>
<signal name="N$21">
<contactref element="Q131" pad="2(S)"/>
<contactref element="R154" pad="1"/>
</signal>
<signal name="N$88">
<contactref element="Q131" pad="3(D)"/>
<contactref element="D111" pad="K"/>
<contactref element="F104" pad="1"/>
</signal>
<signal name="N$133">
<contactref element="K107" pad="2"/>
<contactref element="D112" pad="A"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="N$139">
<contactref element="U202" pad="2"/>
<contactref element="U201" pad="4"/>
<contactref element="R202" pad="2"/>
</signal>
<signal name="N$140">
<contactref element="U202" pad="1"/>
<contactref element="U201" pad="2"/>
<contactref element="R203" pad="2"/>
</signal>
<signal name="SO1">
<contactref element="U204" pad="1"/>
<contactref element="U205" pad="15"/>
</signal>
<signal name="SO3">
<contactref element="U203" pad="15"/>
<contactref element="U204" pad="5"/>
</signal>
<signal name="N$108">
<contactref element="U202" pad="3"/>
<contactref element="R201" pad="2"/>
<contactref element="U201" pad="6"/>
</signal>
<signal name="IO4_">
<contactref element="F102" pad="2"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="!DRDY!2">
<contactref element="U105" pad="3"/>
<contactref element="U206" pad="14"/>
</signal>
<signal name="SO4">
<contactref element="U204" pad="9"/>
<contactref element="U207" pad="15"/>
</signal>
<signal name="SCK">
<contactref element="U201" pad="8"/>
<contactref element="R204" pad="1"/>
<contactref element="U203" pad="1"/>
<contactref element="U205" pad="1"/>
<contactref element="U206" pad="1"/>
<contactref element="U207" pad="1"/>
</signal>
<signal name="N$114">
<contactref element="U105" pad="2"/>
<contactref element="R205" pad="1"/>
</signal>
<signal name="!CS1">
<contactref element="U202" pad="14"/>
<contactref element="U205" pad="2"/>
</signal>
<signal name="!CS2">
<contactref element="U202" pad="13"/>
<contactref element="U206" pad="2"/>
</signal>
<signal name="!CS3">
<contactref element="U202" pad="12"/>
<contactref element="U203" pad="2"/>
</signal>
<signal name="!CS4">
<contactref element="U202" pad="11"/>
<contactref element="U207" pad="2"/>
</signal>
<signal name="!CS5">
<contactref element="U202" pad="10"/>
</signal>
<signal name="!CS6">
<contactref element="U202" pad="9"/>
</signal>
<signal name="!CS7">
<contactref element="U202" pad="7"/>
</signal>
<signal name="N$81">
<contactref element="U104" pad="4"/>
<contactref element="R143" pad="2"/>
</signal>
<signal name="SO5">
<contactref element="U204" pad="11"/>
</signal>
<signal name="MOSI">
<contactref element="R144" pad="1"/>
<contactref element="U105" pad="10"/>
<contactref element="U203" pad="16"/>
<contactref element="U205" pad="16"/>
<contactref element="U206" pad="16"/>
<contactref element="U207" pad="16"/>
</signal>
<signal name="N$82">
<contactref element="R121" pad="1"/>
<contactref element="Q110" pad="B"/>
</signal>
<signal name="N$122">
<contactref element="Q111" pad="B"/>
<contactref element="R122" pad="1"/>
</signal>
<signal name="N$141">
<contactref element="Q112" pad="B"/>
<contactref element="R123" pad="1"/>
</signal>
<signal name="N$146">
<contactref element="Q120" pad="B"/>
<contactref element="R136" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="K105" pad="2"/>
<contactref element="R151" pad="2"/>
</signal>
<signal name="!DRDY!1">
<contactref element="U105" pad="1"/>
<contactref element="U205" pad="14"/>
</signal>
<signal name="!DRDY!3">
<contactref element="U105" pad="5"/>
<contactref element="U203" pad="14"/>
</signal>
<signal name="N$12">
<contactref element="R152" pad="1"/>
<contactref element="J7" pad="8"/>
</signal>
<signal name="N$134">
<contactref element="C202" pad="1"/>
<contactref element="C205" pad="1"/>
<contactref element="R208" pad="1"/>
<contactref element="U203" pad="11"/>
<contactref element="C208" pad="1"/>
</signal>
<signal name="N$135">
<contactref element="R208" pad="2"/>
<contactref element="J11" pad="1"/>
</signal>
<signal name="N$136">
<contactref element="C203" pad="1"/>
<contactref element="R209" pad="1"/>
<contactref element="U203" pad="10"/>
<contactref element="C206" pad="1"/>
<contactref element="C209" pad="1"/>
</signal>
<signal name="N$137">
<contactref element="C204" pad="1"/>
<contactref element="C207" pad="1"/>
<contactref element="R210" pad="1"/>
<contactref element="U203" pad="7"/>
<contactref element="C209" pad="2"/>
</signal>
<signal name="N$151">
<contactref element="C214" pad="1"/>
<contactref element="C215" pad="1"/>
<contactref element="R213" pad="1"/>
<contactref element="U203" pad="6"/>
<contactref element="C208" pad="2"/>
</signal>
<signal name="N$152">
<contactref element="R209" pad="2"/>
<contactref element="J11" pad="2"/>
<contactref element="U203" pad="9"/>
</signal>
<signal name="N$153">
<contactref element="R210" pad="2"/>
<contactref element="J11" pad="3"/>
</signal>
<signal name="N$156">
<contactref element="R213" pad="2"/>
<contactref element="J11" pad="4"/>
</signal>
<signal name="N$158">
<contactref element="U203" pad="8"/>
<contactref element="J11" pad="6"/>
</signal>
<signal name="SO2">
<contactref element="U204" pad="3"/>
<contactref element="U206" pad="15"/>
</signal>
<signal name="N$157">
<contactref element="C211" pad="1"/>
<contactref element="C212" pad="1"/>
<contactref element="R212" pad="1"/>
<contactref element="C213" pad="1"/>
<contactref element="U205" pad="11"/>
</signal>
<signal name="N$159">
<contactref element="R212" pad="2"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="N$160">
<contactref element="C218" pad="1"/>
<contactref element="C221" pad="1"/>
<contactref element="R215" pad="1"/>
<contactref element="U205" pad="10"/>
<contactref element="C224" pad="1"/>
</signal>
<signal name="N$161">
<contactref element="C219" pad="1"/>
<contactref element="C222" pad="1"/>
<contactref element="R216" pad="1"/>
<contactref element="U205" pad="7"/>
<contactref element="C224" pad="2"/>
</signal>
<signal name="N$162">
<contactref element="C220" pad="1"/>
<contactref element="C223" pad="1"/>
<contactref element="R217" pad="1"/>
<contactref element="U205" pad="6"/>
<contactref element="C213" pad="2"/>
</signal>
<signal name="N$163">
<contactref element="R215" pad="2"/>
<contactref element="J9" pad="2"/>
<contactref element="U205" pad="9"/>
</signal>
<signal name="N$164">
<contactref element="U205" pad="8"/>
<contactref element="J9" pad="6"/>
</signal>
<signal name="N$165">
<contactref element="R217" pad="2"/>
<contactref element="J9" pad="4"/>
</signal>
<signal name="N$166">
<contactref element="R216" pad="2"/>
<contactref element="J9" pad="3"/>
</signal>
<signal name="N$87">
<contactref element="C234" pad="1"/>
<contactref element="C236" pad="1"/>
<contactref element="R220" pad="1"/>
<contactref element="C238" pad="1"/>
<contactref element="U206" pad="11"/>
</signal>
<signal name="N$100">
<contactref element="R220" pad="2"/>
<contactref element="J10" pad="1"/>
</signal>
<signal name="N$102">
<contactref element="C235" pad="1"/>
<contactref element="C237" pad="1"/>
<contactref element="R221" pad="1"/>
<contactref element="U206" pad="10"/>
<contactref element="C239" pad="1"/>
</signal>
<signal name="N$107">
<contactref element="C244" pad="1"/>
<contactref element="C246" pad="1"/>
<contactref element="R224" pad="1"/>
<contactref element="U206" pad="7"/>
<contactref element="C239" pad="2"/>
</signal>
<signal name="N$109">
<contactref element="C245" pad="1"/>
<contactref element="C247" pad="1"/>
<contactref element="R225" pad="1"/>
<contactref element="U206" pad="6"/>
<contactref element="C238" pad="2"/>
</signal>
<signal name="N$110">
<contactref element="R221" pad="2"/>
<contactref element="J10" pad="2"/>
<contactref element="U206" pad="9"/>
</signal>
<signal name="N$111">
<contactref element="U206" pad="8"/>
<contactref element="J10" pad="6"/>
</signal>
<signal name="N$112">
<contactref element="R225" pad="2"/>
<contactref element="J10" pad="4"/>
</signal>
<signal name="N$113">
<contactref element="J10" pad="3"/>
<contactref element="R224" pad="2"/>
</signal>
<signal name="N$119">
<contactref element="C226" pad="1"/>
<contactref element="C228" pad="1"/>
<contactref element="R218" pad="1"/>
<contactref element="C230" pad="1"/>
<contactref element="U207" pad="11"/>
</signal>
<signal name="N$123">
<contactref element="R218" pad="2"/>
<contactref element="J12" pad="1"/>
</signal>
<signal name="N$124">
<contactref element="C227" pad="1"/>
<contactref element="C229" pad="1"/>
<contactref element="R219" pad="1"/>
<contactref element="U207" pad="10"/>
<contactref element="C231" pad="1"/>
</signal>
<signal name="N$125">
<contactref element="C240" pad="1"/>
<contactref element="C242" pad="1"/>
<contactref element="R222" pad="1"/>
<contactref element="U207" pad="7"/>
<contactref element="C231" pad="2"/>
</signal>
<signal name="N$126">
<contactref element="C241" pad="1"/>
<contactref element="C243" pad="1"/>
<contactref element="R223" pad="1"/>
<contactref element="U207" pad="6"/>
<contactref element="C230" pad="2"/>
</signal>
<signal name="N$127">
<contactref element="R219" pad="2"/>
<contactref element="J12" pad="2"/>
<contactref element="U207" pad="9"/>
</signal>
<signal name="N$128">
<contactref element="U207" pad="8"/>
<contactref element="J12" pad="6"/>
</signal>
<signal name="N$129">
<contactref element="R223" pad="2"/>
<contactref element="J12" pad="4"/>
</signal>
<signal name="N$130">
<contactref element="J12" pad="3"/>
<contactref element="R222" pad="2"/>
</signal>
<signal name="!DRDY!4">
<contactref element="U207" pad="14"/>
<contactref element="U105" pad="9"/>
</signal>
<signal name="N$132">
<contactref element="U105" pad="8"/>
<contactref element="R211" pad="1"/>
</signal>
<signal name="N$147">
<contactref element="R206" pad="1"/>
<contactref element="U105" pad="4"/>
</signal>
<signal name="N$167">
<contactref element="U105" pad="6"/>
<contactref element="R207" pad="1"/>
</signal>
<signal name="TAB">
<contactref element="U103" pad="TAB"/>
</signal>
<signal name="N$20">
<contactref element="F101" pad="1"/>
<contactref element="J5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
