<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.404" y2="0" width="0" layer="20"/>
<wire x1="30.404" y1="0" x2="30.404" y2="50.79" width="0" layer="20"/>
<wire x1="30.404" y1="50.79" x2="0" y2="50.79" width="0" layer="20"/>
<wire x1="0" y1="50.79" x2="0" y2="0" width="0" layer="20"/>
<text>2.4SqIn</text>
<hole x="14.986" y="22.733" drill="2.54"/>
<text>Switch Side</text>
<text>VCC</text>
<text>Light</text>
<text>Motor</text>
<text>Motor</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>RV-Project.Com Waste Gate Switchboard  5/21/2020</text>
<text>Close
(DN)</text>
<text>Open
(UP)</text>
<text>2oz Copper (6A)</text>
<text>Keystone 3528</text>
<text>VCC</text>
</plain>
<libraries>
<library name="a-lib_Connectors">
<description>Thru-Hole Connectors (Connectors, Terminals)</description>
<packages>
<package name="KEYSTONE3528">
</package>
<package name="MO1-14AWG">
</package>
<package name="WAFER4PINVERTICAL">
<description>Pitch: 0.15" (3.81mm)</description>
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="RVPROJECT_NEWLOGO_XSMALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="2" library="a-lib_Connectors" package="KEYSTONE3528" value="">
<attribute name="NAME"/>
</element>
<element name="5" library="a-lib_Connectors" package="KEYSTONE3528" value="">
<attribute name="NAME"/>
</element>
<element name="1" library="a-lib_Connectors" package="KEYSTONE3528" value="">
<attribute name="NAME"/>
</element>
<element name="4" library="a-lib_Connectors" package="KEYSTONE3528" value="">
<attribute name="NAME"/>
</element>
<element name="GND" library="a-lib_Connectors" package="MO1-14AWG" value=""/>
<element name="J1" library="a-lib_Connectors" package="WAFER4PINVERTICAL" value="M4VERTICAL"/>
<element name="8" library="a-lib_Connectors" package="KEYSTONE3528" value="">
<attribute name="NAME"/>
</element>
<element name="7" library="a-lib_Connectors" package="KEYSTONE3528" value="">
<attribute name="NAME"/>
</element>
<element name="3" library="a-lib_Connectors" package="KEYSTONE3528" value="">
<attribute name="NAME"/>
</element>
<element name="6" library="a-lib_Connectors" package="KEYSTONE3528" value="">
<attribute name="NAME"/>
</element>
<element name="VCC" library="a-lib_Connectors" package="MO1-14AWG" value=""/>
<element name="VCC1" library="a-lib_Connectors" package="MO1-14AWG" value=""/>
<element name="VCC2" library="a-lib_Connectors" package="MO1-14AWG" value=""/>
<element name="GND1" library="a-lib_Connectors" package="MO1-14AWG" value=""/>
<element name="GND2" library="a-lib_Connectors" package="MO1-14AWG" value=""/>
<element name="U$1" library="a-lib_Asthetics" package="RVPROJECT_NEWLOGO_XSMALL" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="GND" pad="P$1"/>
<contactref element="6" pad="P$1"/>
<contactref element="6" pad="P$2"/>
<contactref element="1" pad="P$1"/>
<contactref element="1" pad="P$2"/>
<contactref element="8" pad="P$1"/>
<contactref element="8" pad="P$2"/>
<contactref element="GND2" pad="P$1"/>
<contactref element="GND1" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="3" pad="P$1"/>
<contactref element="3" pad="P$2"/>
<contactref element="VCC" pad="P$1"/>
<contactref element="J1" pad="P$4"/>
<contactref element="4" pad="P$1"/>
<contactref element="4" pad="P$2"/>
<contactref element="VCC2" pad="P$1"/>
<contactref element="VCC1" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="2" pad="P$1"/>
<contactref element="2" pad="P$2"/>
<contactref element="J1" pad="P$3"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="P$2"/>
<contactref element="5" pad="P$1"/>
<contactref element="5" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="P$1"/>
<contactref element="7" pad="P$1"/>
<contactref element="7" pad="P$2"/>
</signal>
<signal name="GND">
</signal>
</signals>
</board>
</drawing>
</eagle>
