(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 102)
    (no_connects 0)
    (area 93.521999 93.857999 200.622001 113.958001)
    (thickness 1.6)
    (drawings 19)
    (tracks 607)
    (zones 0)
    (modules 42)
    (nets 44)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.16)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.006)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.027)
    (via_min_drill 0.013)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin -8 216)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BLUE1-Pad2)")
  (net 2 GND)
  (net 3 "Net-(BLUE2-Pad2)")
  (net 4 "Net-(C1-Pad2)")
  (net 5 "Net-(C2-Pad2)")
  (net 6 VCC)
  (net 7 "Net-(C5-Pad1)")
  (net 8 DTR)
  (net 9 TX)
  (net 10 RX)
  (net 11 "Net-(P2-Pad3)")
  (net 12 "Net-(P2-Pad2)")
  (net 13 DIGITAL4)
  (net 14 DIGITAL7)
  (net 15 "Net-(R2-Pad1)")
  (net 16 DIGITAL8)
  (net 17 DIGITAL6)
  (net 18 "Net-(U1-Pad1)")
  (net 19 "Net-(U1-Pad9)")
  (net 20 DIGITAL9)
  (net 21 "Net-(U1-Pad14)")
  (net 22 "Net-(U1-Pad15)")
  (net 23 "Net-(U1-Pad16)")
  (net 24 "Net-(U1-Pad20)")
  (net 25 "Net-(U1-Pad23)")
  (net 26 "Net-(U1-Pad24)")
  (net 27 "Net-(U1-Pad25)")
  (net 28 "Net-(U1-Pad26)")
  (net 29 "Net-(U1-Pad27)")
  (net 30 "Net-(U1-Pad28)")
  (net 31 "Net-(U1-Pad32)")
  (net 32 "Net-(U2-Pad4)")
  (net 33 "Net-(U3-Pad4)")
  (net 34 "Net-(U4-Pad4)")
  (net 35 "Net-(U5-Pad4)")
  (net 36 "Net-(U6-Pad4)")
  (net 37 "Net-(U7-Pad4)")
  (net 38 "Net-(U8-Pad4)")
  (net 39 "Net-(U10-Pad2)")
  (net 40 "Net-(U10-Pad4)")
  (net 41 "Net-(P3-Pad2)")
  (net 42 "Net-(U1-Pad19)")
  (net 43 "Net-(U1-Pad22)")
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net DIGITAL4)
    (add_net DIGITAL6)
    (add_net DIGITAL7)
    (add_net DIGITAL8)
    (add_net DIGITAL9)
    (add_net DTR)
    (add_net GND)
    (add_net "Net-(BLUE1-Pad2)")
    (add_net "Net-(BLUE2-Pad2)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U10-Pad2)")
    (add_net "Net-(U10-Pad4)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U6-Pad4)")
    (add_net "Net-(U7-Pad4)")
    (add_net "Net-(U8-Pad4)")
    (add_net RX)
    (add_net TX)
    (add_net VCC)
  )
  (module "kicad modfiles:TQFP32-0.8-7X7MM" (layer F.Cu) (tedit 577A6EC5)
    (at 183.988145 102.794798 135)
    (descr "<B>Thin Plasic Quad Flat Package</B> Grid 0.8 mm")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference U1 (at -0.127 -5.5245 135) (layer F.SilkS))
    (fp_text value ATMEGA328P-AU (at 0.20997 0.081072 135) (layer F.SilkS))
    (pad 1 smd rect (at -4.2926 -2.8 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad1)") (solder_mask_margin 0.2))
    (pad 2 smd rect (at -4.2926 -2 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 13 DIGITAL4) (solder_mask_margin 0.2))
    (pad 3 smd rect (at -4.2926 -1.2 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 4 smd rect (at -4.2926 -0.4 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC) (solder_mask_margin 0.2))
    (pad 5 smd rect (at -4.2926 0.4 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 6 smd rect (at -4.2926 1.2 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC) (solder_mask_margin 0.2))
    (pad 7 smd rect (at -4.2926 2 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C1-Pad2)") (solder_mask_margin 0.2))
    (pad 8 smd rect (at -4.2926 2.8 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C2-Pad2)") (solder_mask_margin 0.2))
    (pad 9 smd rect (at -2.8 4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad9)") (solder_mask_margin 0.2))
    (pad 10 smd rect (at -2 4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 17 DIGITAL6) (solder_mask_margin 0.2))
    (pad 11 smd rect (at -1.2 4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 14 DIGITAL7) (solder_mask_margin 0.2))
    (pad 12 smd rect (at -0.4 4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 16 DIGITAL8) (solder_mask_margin 0.2))
    (pad 13 smd rect (at 0.4 4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 20 DIGITAL9) (solder_mask_margin 0.2))
    (pad 14 smd rect (at 1.2 4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad14)") (solder_mask_margin 0.2))
    (pad 15 smd rect (at 2 4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad15)") (solder_mask_margin 0.2))
    (pad 16 smd rect (at 2.8 4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad16)") (solder_mask_margin 0.2))
    (pad 17 smd rect (at 4.2926 2.8 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R2-Pad1)") (solder_mask_margin 0.2))
    (pad 18 smd rect (at 4.2926 2 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC) (solder_mask_margin 0.2))
    (pad 19 smd rect (at 4.2926 1.2 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad19)") (solder_mask_margin 0.2))
    (pad 20 smd rect (at 4.2926 0.4 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad20)") (solder_mask_margin 0.2))
    (pad 21 smd rect (at 4.2926 -0.4 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.2))
    (pad 22 smd rect (at 4.2926 -1.2 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad22)") (solder_mask_margin 0.2))
    (pad 23 smd rect (at 4.2926 -2 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad23)") (solder_mask_margin 0.2))
    (pad 24 smd rect (at 4.2926 -2.8 135) (size 1.27 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad24)") (solder_mask_margin 0.2))
    (pad 25 smd rect (at 2.8 -4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad25)") (solder_mask_margin 0.2))
    (pad 26 smd rect (at 2 -4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad26)") (solder_mask_margin 0.2))
    (pad 27 smd rect (at 1.2 -4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-Pad27)") (solder_mask_margin 0.2))
    (pad 28 smd rect (at 0.4 -4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-Pad28)") (solder_mask_margin 0.2))
    (pad 29 smd rect (at -0.4 -4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)") (solder_mask_margin 0.2))
    (pad 30 smd rect (at -1.2 -4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 RX) (solder_mask_margin 0.2))
    (pad 31 smd rect (at -2 -4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 TX) (solder_mask_margin 0.2))
    (pad 32 smd rect (at -2.8 -4.2926 135) (size 0.5588 1.27) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad32)") (solder_mask_margin 0.2))
  )
  (module "kicad modfiles:LED_WS2812B-PLCC4" (layer B.Cu) (tedit 577A68CA)
    (at 109.074 103.261356 180)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference U10 (at 22.84 0.291356 180) (layer B.SilkS) hide)
    (fp_text value WS2812B (at 21.062 -2.248644 180) (layer B.Fab) hide)
    (pad 3 smd rect (at 2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(U10-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(U10-Pad2)"))
    (pad 1 smd rect (at -2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module "kicad modfiles:LED_WS2812B-PLCC4" (layer B.Cu) (tedit 577A690D)
    (at 98.574 103.261356 180)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference U11 (at 11.959 2.450356 180) (layer B.SilkS) hide)
    (fp_text value WS2812B (at 11.705 -2.248644 180) (layer B.Fab) hide)
    (pad 3 smd rect (at 2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 20 DIGITAL9))
    (pad 2 smd rect (at -2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(U10-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module "kicad modfiles:LED_WS2812B-PLCC4" (layer B.Cu) (tedit 57792067)
    (at 172.074 103.314982 180)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference U4 (at 83.3 -10.323018 180) (layer B.SilkS) hide)
    (fp_text value WS2812B (at 85.967 -12.863018 180) (layer B.Fab) hide)
    (pad 3 smd rect (at 2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(U4-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(U3-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 57791F20)
    (at 119.532 107.796)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C14 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at 0 -2.3) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 577A4FFC)
    (at 164.31614 99.922)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference BLUE1 (at 2.68986 -8.382) (layer F.SilkS) hide)
    (fp_text value LED1 (at 0 2) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(BLUE1-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 577A4FF8)
    (at 164.31614 97.128)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference BLUE2 (at -3.15214 -5.588) (layer F.SilkS) hide)
    (fp_text value LED2 (at 0 2) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BLUE2-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 577A6E59)
    (at 172.672 100.66 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0.103 -1.983 90) (layer F.SilkS))
    (fp_text value <- (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 577A6E51)
    (at 175.872 100.66 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at -0.024 1.929 90) (layer F.SilkS))
    (fp_text value 18-24pF (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_4x4.5 (layer F.Cu) (tedit 577A6D93)
    (at 188.47286 110.808 180)
    (descr "SMT capacitor, aluminium electrolytic, 4x4.5")
    (attr smd)
    (fp_text reference C3 (at -1.13914 2.885 180) (layer F.SilkS))
    (fp_text value 47uF (at 0 3.175 180) (layer F.Fab))
    (pad 1 smd rect (at 1.80086 0 180) (size 2.60096 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC))
    (pad 2 smd rect (at -1.80086 0 180) (size 2.60096 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_4x4.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 577A6DD8)
    (at 198.472 96.908 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at -0.034 1.621 270) (layer B.SilkS))
    (fp_text value 1uF (at -0.034 -3.586 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 577A6E19)
    (at 156.972 112.008 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at -0.001 1.799 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 68.96 -10.393 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 DTR))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 577A6DE2)
    (at 192.176 96.112 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at -0.103 -1.651 180) (layer B.SilkS))
    (fp_text value 0.1uF (at -2.008 4.191 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 57791F37)
    (at 193.144 107.796)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at 0 -2.3) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 57791F34)
    (at 182.476 107.796)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C8 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at 0 -2.3) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 57791F31)
    (at 174.396 107.796)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at 0 -2.3) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 57791F2B)
    (at 162.204 109.574)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at 0 -2) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 57791F28)
    (at 151.172 107.796)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at 0 -2.3) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 57791F25)
    (at 140.487 107.796)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C12 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at 0 -2.3) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 57791F23)
    (at 130.2 107.796)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C13 (at -0.5 0) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at 0 -2.3) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 57791F1E)
    (at 108.864 107.796)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C15 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at 0 -2.3) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 57791F12)
    (at 98.196 107.796)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C16 (at -0.5 0) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at 0 -2.3) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 577A4FDF)
    (at 109.094 96.366 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 1.143 22.606 270) (layer F.SilkS) hide)
    (fp_text value SERIAL (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 DTR))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 TX))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 RX))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 VCC))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 577A695B)
    (at 174.88 109.574)
    (fp_text reference SW1 (at 1.016 8.509) (layer F.SilkS) hide)
    (fp_text value MODE (at 5.334 -2.921) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 VCC))
    (pad 2 thru_hole circle (at 3.81 2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 DIGITAL6))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 VCC))
    (pad 2 thru_hole circle (at -3.81 2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 DIGITAL6))
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 577A6962)
    (at 165.462 109.574)
    (fp_text reference SW2 (at -0.488 8.001) (layer F.SilkS) hide)
    (fp_text value RESET (at 0 1.016) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3.81 2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C5-Pad1)"))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C5-Pad1)"))
  )
  (module "kicad modfiles:LED_WS2812B-PLCC4" (layer B.Cu) (tedit 57792067)
    (at 193.074 103.314982 180)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference U2 (at 104.808 -14.133018 180) (layer B.SilkS) hide)
    (fp_text value WS2812B (at 105.443 -13.117018 180) (layer B.Fab) hide)
    (pad 3 smd rect (at 2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(U2-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(P3-Pad2)"))
    (pad 1 smd rect (at -2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module "kicad modfiles:LED_WS2812B-PLCC4" (layer B.Cu) (tedit 57792067)
    (at 182.574 103.314982 180)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference U3 (at 93.546 -16.927018 180) (layer B.SilkS) hide)
    (fp_text value WS2812B (at 96.594 -12.355018 180) (layer B.Fab) hide)
    (pad 3 smd rect (at 2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(U3-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(U2-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module "kicad modfiles:LED_WS2812B-PLCC4" (layer B.Cu) (tedit 57792067)
    (at 161.574 103.314982 180)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference U5 (at 73.308 -8.672018 180) (layer B.SilkS) hide)
    (fp_text value WS2812B (at 74.324 -8.545018 180) (layer B.Fab) hide)
    (pad 3 smd rect (at 2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(U5-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(U4-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module "kicad modfiles:LED_WS2812B-PLCC4" (layer B.Cu) (tedit 57792067)
    (at 151.074 103.314982 180)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference U6 (at 63.57 -7.148018 180) (layer B.SilkS) hide)
    (fp_text value WS2812B (at 64.84 -10.323018 180) (layer B.Fab) hide)
    (pad 3 smd rect (at 2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(U6-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(U5-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module "kicad modfiles:LED_WS2812B-PLCC4" (layer B.Cu) (tedit 57792067)
    (at 140.574 103.314982 180)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference U7 (at 52.816 -5.116018 180) (layer B.SilkS) hide)
    (fp_text value WS2812B (at 53.07 -6.386018 180) (layer B.Fab) hide)
    (pad 3 smd rect (at 2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(U7-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(U6-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module "kicad modfiles:LED_WS2812B-PLCC4" (layer B.Cu) (tedit 57792067)
    (at 130.074 103.314982 180)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference U8 (at 41.554 -2.957018 180) (layer B.SilkS) hide)
    (fp_text value WS2812B (at 45.745 -8.291018 180) (layer B.Fab) hide)
    (pad 3 smd rect (at 2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(U8-Pad4)"))
    (pad 2 smd rect (at -2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(U7-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module "kicad modfiles:LED_WS2812B-PLCC4" (layer B.Cu) (tedit 57792067)
    (at 119.574 103.314982 180)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference U9 (at 29.276 -1.560018 180) (layer B.SilkS) hide)
    (fp_text value WS2812B (at 33.975 -3.592018 180) (layer B.Fab) hide)
    (pad 3 smd rect (at 2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(U10-Pad2)"))
    (pad 2 smd rect (at -2.5 -1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(U8-Pad4)"))
    (pad 1 smd rect (at -2.5 1.6 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (model LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 180))
    )
  )
  (module "kicad modfiles:USB_A_bare-conn." (layer F.Cu) (tedit 577A6C9B)
    (at 198.756 100.303 270)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference P2 (at -1.90414 5.207 270) (layer F.SilkS) hide)
    (fp_text value USB_A (at 0 2 270) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.11286 -0.00212 180) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at 4.57286 -0.00212 180) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P2-Pad3)"))
    (pad 2 thru_hole circle (at 2.54086 -0.00212 180) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P2-Pad2)"))
    (pad 1 thru_hole circle (at 0.00086 -0.00212 180) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 VCC))
    (model Connect.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "kicad modfiles:CAP_SLIDER_SLIM" (layer F.Cu) (tedit 577A4FE9)
    (at 94.872 112.808)
    (fp_text reference M1 (at -5.082 2.989) (layer F.SilkS) hide)
    (fp_text value CAP_SLIDERSMD (at 6 -12) (layer F.Fab))
    (pad 1 smd rect (at 0 -5) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 14 DIGITAL7))
    (pad 2 smd rect (at 65 -5) (size 0.25 1) (layers F.Cu F.Paste F.Mask)
      (net 16 DIGITAL8))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 577A6E3B)
    (at 96.728 101.446 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1 180) (layer F.SilkS) hide)
    (fp_text value 1M (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 DIGITAL4))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 DIGITAL7))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 577F76FB)
    (at 182.072 95.858 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -0.047 -1.651 180) (layer B.SilkS))
    (fp_text value 300R (at 0.334 4.953 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(BLUE1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 577A6E34)
    (at 157.688 101.446 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -2.1 180) (layer F.SilkS) hide)
    (fp_text value 1M (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 DIGITAL4))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 DIGITAL8))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 577A6EDD)
    (at 188.522 95.808 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -0.836 -1.574 180) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 DIGITAL6))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 577A6ED8)
    (at 194.522 95.808 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -0.043 -1.701 180) (layer F.SilkS))
    (fp_text value 300R (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BLUE2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 577A6DB3)
    (at 182.022 110.808)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -0.03 1.56) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 577A6E63)
    (at 174.11294 96.408 180)
    (descr "Crystal Quarz HC49/U vertical stehend")
    (tags "Crystal Quarz HC49/U vertical stehend")
    (fp_text reference Y1 (at -0.25906 5.249 180) (layer F.SilkS) hide)
    (fp_text value 8MHZ (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.44094 0 180) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 2.44094 0 180) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C1-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 577A694D)
    (at 198.652 112.308 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value EXT (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "GND\n" (at 193.549 109.828 90) (layer F.SilkS))
  (gr_text DO (at 196.089 110.082 90) (layer F.SilkS))
  (gr_text VCC (at 198.629 109.574 90) (layer F.SilkS))
  (gr_text GND (at 96.394 98.144) (layer F.SilkS))
  (gr_text "MODE\n" (at 174.753 104.24) (layer F.SilkS))
  (gr_text "RESET\n" (at 165.355 104.367) (layer F.SilkS))
  (gr_line (start 93.572 113.908) (end 93.572 108.908) (layer Edge.Cuts) (width 0.1))
  (gr_text v2.4 (at 148.083 99.287) (layer F.SilkS))
  (gr_text "colourCTRL\n" (at 114.428 98.271) (layer F.SilkS))
  (gr_text "STATUS\n" (at 157.608 99.922) (layer F.SilkS))
  (gr_text "POWER\n" (at 157.608 97.128) (layer F.SilkS))
  (gr_line (start 200.572 113.908) (end 198.572 113.908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200.572 93.908) (end 200.572 113.908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 198.572 93.908) (end 200.572 93.908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 198.572 113.908) (end 193.572 113.908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 193.572 93.908) (end 198.572 93.908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 193.572 113.908) (end 93.572 113.908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 193.572 93.908) (end 93.572 93.908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.572 93.908) (end 93.572 108.908) (layer Edge.Cuts) (width 0.1))
  (zone (net 16) (net_name DIGITAL8) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.16)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.072 102.808) (xy 160.072 112.808) (xy 154.872 112.808) (xy 105.072 102.808)
      )
    )
  )
  (zone (net 14) (net_name DIGITAL7) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.16)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.672 102.808) (xy 99.872 102.808) (xy 152.072 112.808) (xy 94.872 112.808) (xy 94.672 112.808)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 93.473 113.892) (xy 93.6 101.192) (xy 93.473 93.953) (xy 200.534 93.953) (xy 200.534 113.892)
      )
    )
  )
)
