(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6)
    (drawings 39)
    (tracks 465)
    (zones 0)
    (modules 34)
    (nets 43)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu power)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (uvia_size 0.8)
    (uvia_drill 0.4)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 2.6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 Vdut)
  (net 3 Vprobe)
  (net 4 -XDP_PREQ)
  (net 5 -XDP_PRDY)
  (net 6 "Net-(J1-Pad23)")
  (net 7 "Net-(J1-Pad22)")
  (net 8 "Net-(J1-Pad20)")
  (net 9 "Net-(J1-Pad19)")
  (net 10 CORE_PWRGD)
  (net 11 "Net-(J1-Pad16)")
  (net 12 CFG0)
  (net 13 BPWRG)
  (net 14 -PLTRST)
  (net 15 -XDP_DBR)
  (net 16 XDP_TDO)
  (net 17 -XDP_TRST)
  (net 18 XDP_TDI)
  (net 19 XDP_TMS)
  (net 20 "Net-(J1-Pad3)")
  (net 21 XDP_TCK)
  (net 22 +1V8)
  (net 23 "Net-(D1-Pad1)")
  (net 24 "Net-(D2-Pad1)")
  (net 25 "Net-(D3-Pad1)")
  (net 26 Vdut_src)
  (net 27 /-XDP_PREQ_p)
  (net 28 /-XDP_PRDY_p)
  (net 29 /CORE_PWRGD_p)
  (net 30 /CFG0_p)
  (net 31 /BPWRG_p)
  (net 32 /-PLTRST_p)
  (net 33 /-XDP_DBR_p)
  (net 34 /XDP_TDO_p)
  (net 35 /-XDP_TRST_p)
  (net 36 /XDP_TDI_p)
  (net 37 /XDP_TMS_p)
  (net 38 /XDP_TCK_p)
  (net 39 Vprobe_src)
  (net 40 "Net-(U6-Pad4)")
  (net 41 XDP_CLK_100M_P)
  (net 42 XDP_CLK_100M_N)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.8)
    (uvia_drill 0.4)
    (add_net +1V8)
    (add_net -PLTRST)
    (add_net -XDP_DBR)
    (add_net -XDP_PRDY)
    (add_net -XDP_PREQ)
    (add_net -XDP_TRST)
    (add_net /-PLTRST_p)
    (add_net /-XDP_DBR_p)
    (add_net /-XDP_PRDY_p)
    (add_net /-XDP_PREQ_p)
    (add_net /-XDP_TRST_p)
    (add_net /BPWRG_p)
    (add_net /CFG0_p)
    (add_net /CORE_PWRGD_p)
    (add_net /XDP_TCK_p)
    (add_net /XDP_TDI_p)
    (add_net /XDP_TDO_p)
    (add_net /XDP_TMS_p)
    (add_net BPWRG)
    (add_net CFG0)
    (add_net CORE_PWRGD)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(U6-Pad4)")
    (add_net Vdut)
    (add_net Vdut_src)
    (add_net Vprobe)
    (add_net Vprobe_src)
    (add_net XDP_CLK_100M_N)
    (add_net XDP_CLK_100M_P)
    (add_net XDP_TCK)
    (add_net XDP_TDI)
    (add_net XDP_TDO)
    (add_net XDP_TMS)
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 60B9E1EF)
    (at 165.1 73.025)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U6 (at 0 -2.9) (layer F.SilkS))
    (fp_text value TPS73118DBV (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 +1V8))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U6-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 Vprobe))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 Vprobe))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 149.86 58.42 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value "0.1 ohm 1%" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 Vprobe_src))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 Vprobe))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 114.3 62.865 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value "0.1 ohm 1%" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 Vdut_src))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Vdut))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 164.465 86.995)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.5) (layer F.SilkS))
    (fp_text value DMN62D0U (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 29 /CORE_PWRGD_p))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 164.465 81.915)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value DMN62D0U (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 31 /BPWRG_p))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 164.465 64.135)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value DMN62D0U (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 38 /XDP_TCK_p))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_PLCC-2 (layer F.Cu) (tedit 59959404)
    (at 172.085 86.995)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (attr smd)
    (fp_text reference D3 (at 3.937 0) (layer F.SilkS))
    (fp_text value Yellow (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 22 +1V8))
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_PLCC-2 (layer F.Cu) (tedit 59959404)
    (at 172.085 81.915)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (attr smd)
    (fp_text reference D2 (at 3.937 0) (layer F.SilkS))
    (fp_text value Red (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 22 +1V8))
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_PLCC-2 (layer F.Cu) (tedit 59959404)
    (at 172.085 64.135)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (attr smd)
    (fp_text reference D1 (at 3.937 0) (layer F.SilkS))
    (fp_text value Green (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 22 +1V8))
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 172.72 75.415 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 +1V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 172.72 70.485 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 +1V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module x230-xdp:SOT65P210X110-5N (layer F.Cu) (tedit 60AFF80E)
    (at 130.81 99.06 180)
    (fp_text reference U13 (at 0.29 -2.008) (layer F.SilkS))
    (fp_text value NLSV1T34 (at 5.878 2.008) (layer F.Fab))
    (pad 1 smd rect (at -0.935 -0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 Vprobe))
    (pad 2 smd rect (at -0.935 0 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 27 /-XDP_PREQ_p))
    (pad 3 smd rect (at -0.935 0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.935 -0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 Vdut))
    (pad 4 smd rect (at 0.935 0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 4 -XDP_PREQ))
  )
  (module x230-xdp:SOT65P210X110-5N (layer F.Cu) (tedit 60AFF80E)
    (at 130.81 95.25)
    (fp_text reference U12 (at 0.29 -2.008) (layer F.SilkS))
    (fp_text value NLSV1T34 (at 5.878 2.008) (layer F.Fab))
    (pad 1 smd rect (at -0.935 -0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 Vdut))
    (pad 2 smd rect (at -0.935 0) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 5 -XDP_PRDY))
    (pad 3 smd rect (at -0.935 0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.935 -0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 Vprobe))
    (pad 4 smd rect (at 0.935 0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 28 /-XDP_PRDY_p))
  )
  (module x230-xdp:SOT65P210X110-5N (layer F.Cu) (tedit 60AFF80E)
    (at 130.81 91.44)
    (fp_text reference U11 (at 0.29 -2.008) (layer F.SilkS))
    (fp_text value NLSV1T34 (at 5.878 2.008) (layer F.Fab))
    (pad 1 smd rect (at -0.935 -0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 Vdut))
    (pad 2 smd rect (at -0.935 0) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 10 CORE_PWRGD))
    (pad 3 smd rect (at -0.935 0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.935 -0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 Vprobe))
    (pad 4 smd rect (at 0.935 0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 29 /CORE_PWRGD_p))
  )
  (module x230-xdp:SOT65P210X110-5N (layer F.Cu) (tedit 60AFF80E)
    (at 130.81 87.63 180)
    (fp_text reference U10 (at 0.29 -2.008) (layer F.SilkS))
    (fp_text value NLSV1T34 (at 5.878 2.008) (layer F.Fab))
    (pad 1 smd rect (at -0.935 -0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 Vprobe))
    (pad 2 smd rect (at -0.935 0 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 30 /CFG0_p))
    (pad 3 smd rect (at -0.935 0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.935 -0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 Vdut))
    (pad 4 smd rect (at 0.935 0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 12 CFG0))
  )
  (module x230-xdp:SOT65P210X110-5N (layer F.Cu) (tedit 60AFF80E)
    (at 130.81 83.82)
    (fp_text reference U9 (at 0.29 -2.008) (layer F.SilkS))
    (fp_text value NLSV1T34 (at 5.878 2.008) (layer F.Fab))
    (pad 1 smd rect (at -0.935 -0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 Vdut))
    (pad 2 smd rect (at -0.935 0) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 13 BPWRG))
    (pad 3 smd rect (at -0.935 0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.935 -0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 Vprobe))
    (pad 4 smd rect (at 0.935 0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 31 /BPWRG_p))
  )
  (module x230-xdp:SOT65P210X110-5N (layer F.Cu) (tedit 60AFF80E)
    (at 130.81 80.01)
    (fp_text reference U8 (at 0.29 -2.008) (layer F.SilkS))
    (fp_text value NLSV1T34 (at 5.878 2.008) (layer F.Fab))
    (pad 1 smd rect (at -0.935 -0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 Vdut))
    (pad 2 smd rect (at -0.935 0) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 14 -PLTRST))
    (pad 3 smd rect (at -0.935 0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.935 -0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 Vprobe))
    (pad 4 smd rect (at 0.935 0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 32 /-PLTRST_p))
  )
  (module x230-xdp:SOT65P210X110-5N (layer F.Cu) (tedit 60AFF80E)
    (at 130.81 76.2 180)
    (fp_text reference U7 (at 0.29 -2.008) (layer F.SilkS))
    (fp_text value NLSV1T34 (at 5.878 2.008) (layer F.Fab))
    (pad 1 smd rect (at -0.935 -0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 Vprobe))
    (pad 2 smd rect (at -0.935 0 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 33 /-XDP_DBR_p))
    (pad 3 smd rect (at -0.935 0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.935 -0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 Vdut))
    (pad 4 smd rect (at 0.935 0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 15 -XDP_DBR))
  )
  (module x230-xdp:SOT65P210X110-5N (layer F.Cu) (tedit 60AFF80E)
    (at 130.81 72.39)
    (fp_text reference U5 (at 0.29 -2.008) (layer F.SilkS))
    (fp_text value NLSV1T34 (at 5.878 2.008) (layer F.Fab))
    (pad 1 smd rect (at -0.935 -0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 Vdut))
    (pad 2 smd rect (at -0.935 0) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 16 XDP_TDO))
    (pad 3 smd rect (at -0.935 0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.935 -0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 Vprobe))
    (pad 4 smd rect (at 0.935 0.65) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 34 /XDP_TDO_p))
  )
  (module x230-xdp:SOT65P210X110-5N (layer F.Cu) (tedit 60AFF80E)
    (at 130.81 68.58 180)
    (fp_text reference U4 (at 0.29 -2.008) (layer F.SilkS))
    (fp_text value NLSV1T34 (at 5.878 2.008) (layer F.Fab))
    (pad 1 smd rect (at -0.935 -0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 Vprobe))
    (pad 2 smd rect (at -0.935 0 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 35 /-XDP_TRST_p))
    (pad 3 smd rect (at -0.935 0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.935 -0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 Vdut))
    (pad 4 smd rect (at 0.935 0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 17 -XDP_TRST))
  )
  (module x230-xdp:SOT65P210X110-5N (layer F.Cu) (tedit 60AFF80E)
    (at 130.81 64.77 180)
    (fp_text reference U3 (at 0.29 -2.008) (layer F.SilkS))
    (fp_text value NLSV1T34 (at 5.878 2.008) (layer F.Fab))
    (pad 1 smd rect (at -0.935 -0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 Vprobe))
    (pad 2 smd rect (at -0.935 0 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 36 /XDP_TDI_p))
    (pad 3 smd rect (at -0.935 0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.935 -0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 Vdut))
    (pad 4 smd rect (at 0.935 0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 18 XDP_TDI))
  )
  (module x230-xdp:SOT65P210X110-5N (layer F.Cu) (tedit 60AFF80E)
    (at 130.81 60.96 180)
    (fp_text reference U2 (at 0.29 -2.008) (layer F.SilkS))
    (fp_text value NLSV1T34 (at 5.878 2.008) (layer F.Fab))
    (pad 1 smd rect (at -0.935 -0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 Vprobe))
    (pad 2 smd rect (at -0.935 0 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 37 /XDP_TMS_p))
    (pad 3 smd rect (at -0.935 0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.935 -0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 Vdut))
    (pad 4 smd rect (at 0.935 0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 19 XDP_TMS))
  )
  (module x230-xdp:SOT65P210X110-5N (layer F.Cu) (tedit 60AFF80E)
    (at 130.81 57.15 180)
    (fp_text reference U1 (at 0.29 -2.008) (layer F.SilkS))
    (fp_text value NLSV1T34 (at 5.878 2.008) (layer F.Fab))
    (pad 1 smd rect (at -0.935 -0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 3 Vprobe))
    (pad 2 smd rect (at -0.935 0 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 38 /XDP_TCK_p))
    (pad 3 smd rect (at -0.935 0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.935 -0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 2 Vdut))
    (pad 4 smd rect (at 0.935 0.65 180) (size 1.06 0.39) (layers F.Cu F.Paste F.Mask)
      (net 21 XDP_TCK))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 60B59F80)
    (at 140.97 113.03 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "5x Male Header" (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Vprobe))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Vprobe))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Vprobe))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Vprobe))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Vprobe))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 60B59F88)
    (at 110.49 113.03 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "5x Male Header" (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 Vdut))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 Vdut))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 Vdut))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 Vdut))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 Vdut))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 60B59F79)
    (at 125.73 113.03 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "5x Male Header" (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole rect (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole rect (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole rect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 60B59F8E)
    (at 106.045 95.25 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "4x Male Header" (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 XDP_CLK_100M_P))
    (pad 3 thru_hole rect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 XDP_CLK_100M_N))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical (layer F.Cu) (tedit 60B9D40A)
    (at 142.875 61.595)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "14x Male Header" (at 0 35.35) (layer F.Fab))
    (fp_text user %R (at 0 16.51 90) (layer F.Fab))
    (pad 14 thru_hole rect (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /-XDP_PREQ_p))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /-XDP_PRDY_p))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /CORE_PWRGD_p))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /CFG0_p))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /BPWRG_p))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /-PLTRST_p))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /-XDP_DBR_p))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /XDP_TDO_p))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /-XDP_TRST_p))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /XDP_TDI_p))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /XDP_TMS_p))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /XDP_TCK_p))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Vprobe_src))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical (layer F.Cu) (tedit 60B9D411)
    (at 156.845 61.595)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "14x Male Header" (at 0 35.35) (layer F.Fab))
    (fp_text user %R (at 0 16.51 90) (layer F.Fab))
    (pad 14 thru_hole rect (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /-XDP_PREQ_p))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /-XDP_PRDY_p))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /CORE_PWRGD_p))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /CFG0_p))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /BPWRG_p))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /-PLTRST_p))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /-XDP_DBR_p))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /XDP_TDO_p))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /-XDP_TRST_p))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /XDP_TDI_p))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /XDP_TMS_p))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /XDP_TCK_p))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Vprobe_src))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module x230-xdp:Molex-52435-2671 (layer F.Cu) (tedit 5EF17B41)
    (at 118.745 78.105 270)
    (fp_text reference J1 (at -11 -2.337004 90) (layer F.SilkS))
    (fp_text value MLX-52435-2671 (at 0 0 90) (layer F.SilkS))
    (pad 26 smd rect (at 6.25 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 4 -XDP_PREQ))
    (pad 25 smd rect (at 5.749999 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 5 -XDP_PRDY))
    (pad 24 smd rect (at 5.25 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 23 smd rect (at 4.750001 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad23)"))
    (pad 22 smd rect (at 4.249999 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad22)"))
    (pad 21 smd rect (at 3.75 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at 3.249999 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad20)"))
    (pad 19 smd rect (at 2.75 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad19)"))
    (pad 18 smd rect (at 2.250001 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 1.749999 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 10 CORE_PWRGD))
    (pad 16 smd rect (at 1.25 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad16)"))
    (pad 15 smd rect (at 0.750001 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 12 CFG0))
    (pad 14 smd rect (at 0.249999 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 13 BPWRG))
    (pad 13 smd rect (at -0.249999 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 41 XDP_CLK_100M_P))
    (pad 12 smd rect (at -0.750001 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 42 XDP_CLK_100M_N))
    (pad 11 smd rect (at -1.25 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 26 Vdut_src))
    (pad 10 smd rect (at -1.749999 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 14 -PLTRST))
    (pad MP2 smd rect (at 8.727001 0.761997 90) (size 1.000001 1.000001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad MP1 smd rect (at -8.727001 0.761997 270) (size 1.000001 1.000001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -2.250001 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 15 -XDP_DBR))
    (pad 8 smd rect (at -2.75 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -3.250001 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 16 XDP_TDO))
    (pad 6 smd rect (at -3.75 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 17 -XDP_TRST))
    (pad 5 smd rect (at -4.250002 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 18 XDP_TDI))
    (pad 4 smd rect (at -4.750001 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 19 XDP_TMS))
    (pad 3 smd rect (at -5.25 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -5.750001 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -6.25 -0.762003 270) (size 0.299999 0.800001) (layers F.Cu F.Paste F.Mask)
      (net 21 XDP_TCK))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 134.62 108.585 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 Vprobe))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 134.62 104.775 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 Vprobe))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 127 108.585)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 Vdut))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 127 104.775)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 Vdut))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 170.18 113.792 180) (layer F.SilkS))
  (gr_text GND (at 109.22 52.832 90) (layer F.SilkS))
  (gr_text GND (at 168.148 55.88 180) (layer F.SilkS))
  (gr_text GND (at 158.115 102.87) (layer B.SilkS))
  (gr_text "XDP Adapter for ThinkPad X230 (LDB-2 11232-1)\nConnect to CN24 (CPU) or CN25 (PCH)\nInt80 Industries" (at 150.495 80.01 90) (layer B.SilkS))
  (gr_text "0.1 ohm" (at 112.522 61.468 90) (layer F.SilkS))
  (gr_text "0.1 ohm" (at 154.94 57.404) (layer F.SilkS))
  (gr_text XDP_TCK (at 171.958 66.929) (layer F.SilkS))
  (gr_text BPWRG (at 171.958 84.455) (layer F.SilkS))
  (gr_text CORE_PWRGD (at 172.212 90.043) (layer F.SilkS))
  (gr_text GND (at 111.252 96.774 90) (layer F.SilkS))
  (gr_text GND (at 108.712 96.774 90) (layer F.SilkS))
  (gr_text XDP_CLK_100M_P (at 113.792 96.774 90) (layer F.SilkS))
  (gr_text XDP_CLK_100M_N (at 106.172 96.774 90) (layer F.SilkS))
  (gr_text Vprobe (at 146.05 115.951) (layer F.SilkS))
  (gr_text GND (at 130.81 115.951) (layer F.SilkS))
  (gr_text Vdut (at 115.57 115.951) (layer F.SilkS))
  (gr_text GND (at 149.86 94.615) (layer F.SilkS))
  (gr_text -XDP_PREQ (at 149.86 92.075) (layer F.SilkS))
  (gr_text -XDP_PRDY (at 149.86 89.535) (layer F.SilkS))
  (gr_text CORE_PWRGD (at 149.86 86.995) (layer F.SilkS))
  (gr_text CFG0 (at 149.86 84.455) (layer F.SilkS))
  (gr_text BPWRG (at 149.86 81.915) (layer F.SilkS))
  (gr_text -PLTRST (at 149.86 79.375) (layer F.SilkS))
  (gr_text -XDP_DBR (at 149.86 76.835) (layer F.SilkS))
  (gr_text XDP_TDO (at 149.86 74.295) (layer F.SilkS))
  (gr_text -XDP_TRST (at 149.86 71.755) (layer F.SilkS))
  (gr_text XDP_TDI (at 149.86 69.215) (layer F.SilkS))
  (gr_text XDP_TMS (at 149.86 66.675) (layer F.SilkS))
  (gr_text XDP_TCK (at 149.86 64.135) (layer F.SilkS))
  (gr_text Vprobe (at 149.86 61.595) (layer F.SilkS))
  (gr_circle (center 105.41 53.975) (end 107.315 53.975) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 173.99 53.975) (end 175.895 53.975) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 173.99 116.205) (end 175.895 116.205) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 105.41 116.205) (end 107.315 116.205) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 177.8 50.165) (end 177.8 120.015) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.6 50.165) (end 177.8 50.165) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.6 120.015) (end 101.6 50.165) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.8 120.015) (end 101.6 120.015) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.38 85.09) (xy 119.38 85.725) (xy 118.11 85.725) (xy 118.745 84.455)
      )
    )
  )
  (zone (net 22) (net_name +1V8) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.26 88.9) (xy 172.085 88.9) (xy 172.085 80.01) (xy 165.735 80.01) (xy 165.735 66.04)
        (xy 172.085 66.04) (xy 172.085 62.23) (xy 175.26 62.23)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.165 119.38) (xy 102.235 119.38) (xy 102.235 50.8) (xy 177.165 50.8)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.715 55.88) (xy 131.445 55.88) (xy 131.445 100.33) (xy 134.62 100.33) (xy 134.62 109.855)
        (xy 137.795 111.125) (xy 137.795 119.38) (xy 123.825 119.38) (xy 123.825 111.125) (xy 127 109.855)
        (xy 127 100.33) (xy 130.175 100.33) (xy 130.175 55.88) (xy 128.905 55.88) (xy 128.905 52.705)
        (xy 132.715 52.705)
      )
    )
  )
  (zone (net 2) (net_name Vdut) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.175 100.33) (xy 125.73 100.33) (xy 125.73 109.855) (xy 122.555 109.855) (xy 122.555 115.57)
        (xy 108.585 115.57) (xy 108.585 110.49) (xy 103.124 110.6805) (xy 103.124 57.9755) (xy 106.68 56.515)
        (xy 108.585 55.88) (xy 130.175 55.88)
      )
    )
  )
  (zone (net 3) (net_name Vprobe) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.1 115.57) (xy 139.065 115.57) (xy 139.065 109.855) (xy 135.89 109.855) (xy 135.89 100.33)
        (xy 131.445 100.33) (xy 131.445 55.88) (xy 165.1 55.88)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.824 85.344) (xy 115.57 87.63) (xy 115.57 84.455) (xy 118.745 84.455)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.672 54.864) (xy 135.128 54.864) (xy 135.128 50.8) (xy 169.672 50.8)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 54.864) (xy 110.236 54.864) (xy 110.236 50.8) (xy 126.492 50.8)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.292 112.776) (xy 167.132 112.776) (xy 167.132 92.456) (xy 177.292 92.456)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.984 53.848) (xy 110.744 53.848) (xy 110.744 49.784) (xy 125.984 49.784)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.984 53.848) (xy 110.744 53.848) (xy 110.744 49.784) (xy 125.984 49.784)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.164 53.848) (xy 135.636 53.848) (xy 135.636 49.784) (xy 169.164 49.784)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.164 53.848) (xy 135.636 53.848) (xy 135.636 49.784) (xy 169.164 49.784)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.308 112.268) (xy 168.148 112.268) (xy 168.148 92.964) (xy 178.308 92.964)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.308 112.268) (xy 168.148 112.268) (xy 168.148 92.964) (xy 178.308 92.964)
      )
    )
  )
)
