(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
			(edge_connector bevelled)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/~{CE1}")
	(net 2 "/~{CE}")
	(net 3 "+5V")
	(net 4 "/A20")
	(net 5 "/D4")
	(net 6 "GND")
	(net 7 "/D2")
	(net 8 "/A6")
	(net 9 "/A8")
	(net 10 "/A2")
	(net 11 "/D11")
	(net 12 "/A13")
	(net 13 "/D9")
	(net 14 "/D15")
	(net 15 "/A10")
	(net 16 "/A5")
	(net 17 "/D5")
	(net 18 "/A19")
	(net 19 "/A11")
	(net 20 "/A18")
	(net 21 "/D13")
	(net 22 "/D0")
	(net 23 "/A1")
	(net 24 "/D7")
	(net 25 "/D12")
	(net 26 "/A4")
	(net 27 "/A0")
	(net 28 "/D8")
	(net 29 "/A16")
	(net 30 "/A9")
	(net 31 "/A12")
	(net 32 "/~{OE}")
	(net 33 "/D6")
	(net 34 "/D3")
	(net 35 "/D1")
	(net 36 "/A17")
	(net 37 "/D14")
	(net 38 "/D10")
	(net 39 "/A3")
	(net 40 "/A14")
	(net 41 "/A7")
	(net 42 "/A15")
	(net 43 "unconnected-(U2-NC-Pad14)")
	(net 44 "unconnected-(U2-R~{B}-Pad15)")
	(net 45 "unconnected-(U2-NC-Pad13)")
	(net 46 "unconnected-(U2-NC-Pad10)")
	(net 47 "unconnected-(U3-R~{B}-Pad15)")
	(net 48 "unconnected-(U3-NC-Pad14)")
	(net 49 "unconnected-(U3-NC-Pad13)")
	(net 50 "/~{CE2}")
	(net 51 "unconnected-(U3-NC-Pad10)")
	(net 52 "unconnected-(U4A-O2-Pad6)")
	(net 53 "unconnected-(U4B-O3-Pad9)")
	(net 54 "unconnected-(U4A-O3-Pad7)")
	(net 55 "unconnected-(U4B-O1-Pad11)")
	(net 56 "unconnected-(U4B-O0-Pad12)")
	(net 57 "unconnected-(U4B-O2-Pad10)")
	(net 58 "/~{BYTE}")
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 223.52 96.065 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 2.065 -0.52 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 270)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "29F160_to_27C322.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSOP-I-48_18.4x12mm_P0.5mm"
		(layer "F.Cu")
		(at 211.12 99.065)
		(descr "TSOP-I, 48 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation DD), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSOP-I SO")
		(property "Reference" "U2"
			(at -12.37 -5.065 360)
			(layer "F.SilkS")
		)
		(property "Value" "27C160"
			(at 0 6.95 360)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSOP-I-48_18.4x12mm_P0.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://pdf1.alldatasheet.com/datasheet-pdf/download/22894/STMICROELECTRONICS/M29F160BB.html"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "16 Mbit Flash"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W15.24mm* PLCC*")
		(sheetname "Root")
		(sheetfile "29F160_to_27C322.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -9.6875 -5.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "/A15")
			(pinfunction "A15")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -9.6875 -5.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "/A14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -9.6875 -4.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/A13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -9.6875 -4.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "/A12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -9.6875 -3.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "/A11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -9.6875 -3.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/A10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -9.6875 -2.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "/A9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -9.6875 -2.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "/A8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -9.6875 -1.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/A19")
			(pinfunction "A19")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -9.6875 -1.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "unconnected-(U2-NC-Pad10)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "11" smd roundrect
			(at -9.6875 -0.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at -9.6875 -0.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "~{RP}")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at -9.6875 0.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "unconnected-(U2-NC-Pad13)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "14" smd roundrect
			(at -9.6875 0.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "unconnected-(U2-NC-Pad14)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "15" smd roundrect
			(at -9.6875 1.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "unconnected-(U2-R~{B}-Pad15)")
			(pinfunction "R~{B}")
			(pintype "output")
		)
		(pad "16" smd roundrect
			(at -9.6875 1.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/A18")
			(pinfunction "A18")
			(pintype "input")
		)
		(pad "17" smd roundrect
			(at -9.6875 2.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "/A17")
			(pinfunction "A17")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at -9.6875 2.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "/A7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "19" smd roundrect
			(at -9.6875 3.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "/A6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at -9.6875 3.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/A5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at -9.6875 4.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "/A4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at -9.6875 4.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "/A3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at -9.6875 5.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "/A2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at -9.6875 5.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/A1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 9.6875 5.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "/A0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 9.6875 5.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/~{CE1}")
			(pinfunction "~{CE}")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 9.6875 4.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "28" smd roundrect
			(at 9.6875 4.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/~{OE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "29" smd roundrect
			(at 9.6875 3.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/D0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "30" smd roundrect
			(at 9.6875 3.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "/D8")
			(pinfunction "D8")
			(pintype "tri_state")
		)
		(pad "31" smd roundrect
			(at 9.6875 2.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "/D1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "32" smd roundrect
			(at 9.6875 2.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/D9")
			(pinfunction "D9")
			(pintype "tri_state")
		)
		(pad "33" smd roundrect
			(at 9.6875 1.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/D2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "34" smd roundrect
			(at 9.6875 1.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/D10")
			(pinfunction "D10")
			(pintype "tri_state")
		)
		(pad "35" smd roundrect
			(at 9.6875 0.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "/D3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "36" smd roundrect
			(at 9.6875 0.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/D11")
			(pinfunction "D11")
			(pintype "tri_state")
		)
		(pad "37" smd roundrect
			(at 9.6875 -0.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "38" smd roundrect
			(at 9.6875 -0.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "/D4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "39" smd roundrect
			(at 9.6875 -1.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/D12")
			(pinfunction "D12")
			(pintype "tri_state")
		)
		(pad "40" smd roundrect
			(at 9.6875 -1.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/D5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "41" smd roundrect
			(at 9.6875 -2.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/D13")
			(pinfunction "D13")
			(pintype "tri_state")
		)
		(pad "42" smd roundrect
			(at 9.6875 -2.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/D6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "43" smd roundrect
			(at 9.6875 -3.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/D14")
			(pinfunction "D14")
			(pintype "tri_state")
		)
		(pad "44" smd roundrect
			(at 9.6875 -3.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "/D7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "45" smd roundrect
			(at 9.6875 -4.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/D15")
			(pinfunction "D15A-1")
			(pintype "tri_state")
		)
		(pad "46" smd roundrect
			(at 9.6875 -4.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "47" smd roundrect
			(at 9.6875 -5.25)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "/~{BYTE}")
			(pinfunction "~{BYTE}")
			(pintype "input")
		)
		(pad "48" smd roundrect
			(at 9.6875 -5.75)
			(size 1.575 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "/A16")
			(pinfunction "A16")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSOP-I-48_18.4x12mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 196.5 101.75)
		(property "Reference" "G***"
			(at -5.75 -0.75 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
		(layer "F.Cu")
		(at 178.22 99.065 180)
		(descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U4"
			(at 0 -3.685 180)
			(layer "F.SilkS")
		)
		(property "Value" "74LS139"
			(at 0 3.45 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74ls139a.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual Decoder 1 of 4, Active low outputs"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?16*")
		(sheetname "Root")
		(sheetfile "29F160_to_27C322.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/~{CE}")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/A20")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "/~{CE1}")
			(pinfunction "O0")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "/~{CE2}")
			(pinfunction "O1")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "unconnected-(U4A-O2-Pad6)")
			(pinfunction "O2")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "unconnected-(U4A-O3-Pad7)")
			(pinfunction "O3")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at -2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "unconnected-(U4B-O3-Pad9)")
			(pinfunction "O3")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at 2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "unconnected-(U4B-O2-Pad10)")
			(pinfunction "O2")
			(pintype "output")
		)
		(pad "11" smd roundrect
			(at 2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "unconnected-(U4B-O1-Pad11)")
			(pinfunction "O1")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "unconnected-(U4B-O0-Pad12)")
			(pinfunction "O0")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at 2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-42_W15.24mm"
		(layer "F.Cu")
		(at 223.52 91.44 -90)
		(descr "42-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
		(property "Reference" "U1"
			(at 7.62 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "27C322"
			(at 7.62 53.13 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-42_W15.24mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://static1.squarespace.com/static/51f517f0e4b01da70d01ca2a/t/5575515de4b0888fee6170ec/1433751901367/27C322.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "32 Mbit UV EPROM"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W15.24mm* PLCC*")
		(sheetname "Root")
		(sheetfile "29F160_to_27C322.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 25.4 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/A18")
			(pinfunction "A18")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/A17")
			(pinfunction "A17")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/A7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/A6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/A5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/A4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/A3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/A2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/A1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/A0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/~{CE}")
			(pinfunction "~{CE}")
			(pintype "input")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/~{OE}")
			(pinfunction "~{G}VPP")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/D0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "15" thru_hole oval
			(at 0 35.56 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/D8")
			(pinfunction "D8")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 0 38.1 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/D1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "17" thru_hole oval
			(at 0 40.64 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/D9")
			(pinfunction "D9")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 0 43.18 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/D2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 0 45.72 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/D10")
			(pinfunction "D10")
			(pintype "tri_state")
		)
		(pad "20" thru_hole oval
			(at 0 48.26 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/D3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "21" thru_hole oval
			(at 0 50.8 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/D11")
			(pinfunction "D11")
			(pintype "tri_state")
		)
		(pad "22" thru_hole oval
			(at 15.24 50.8 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "23" thru_hole oval
			(at 15.24 48.26 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/D4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "24" thru_hole oval
			(at 15.24 45.72 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/D12")
			(pinfunction "D12")
			(pintype "tri_state")
		)
		(pad "25" thru_hole oval
			(at 15.24 43.18 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/D5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "26" thru_hole oval
			(at 15.24 40.64 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/D13")
			(pinfunction "D13")
			(pintype "tri_state")
		)
		(pad "27" thru_hole oval
			(at 15.24 38.1 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/D6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "28" thru_hole oval
			(at 15.24 35.56 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/D14")
			(pinfunction "D14")
			(pintype "tri_state")
		)
		(pad "29" thru_hole oval
			(at 15.24 33.02 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/D7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "30" thru_hole oval
			(at 15.24 30.48 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/D15")
			(pinfunction "D15")
			(pintype "tri_state")
		)
		(pad "31" thru_hole oval
			(at 15.24 27.94 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "32" thru_hole oval
			(at 15.24 25.4 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/A20")
			(pinfunction "A20")
			(pintype "input")
		)
		(pad "33" thru_hole oval
			(at 15.24 22.86 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/A16")
			(pinfunction "A16")
			(pintype "input")
		)
		(pad "34" thru_hole oval
			(at 15.24 20.32 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/A15")
			(pinfunction "A15")
			(pintype "input")
		)
		(pad "35" thru_hole oval
			(at 15.24 17.78 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/A14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "36" thru_hole oval
			(at 15.24 15.24 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/A13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "37" thru_hole oval
			(at 15.24 12.7 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/A12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "38" thru_hole oval
			(at 15.24 10.16 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/A11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "39" thru_hole oval
			(at 15.24 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/A10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "40" thru_hole oval
			(at 15.24 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/A9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "41" thru_hole oval
			(at 15.24 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/A8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "42" thru_hole oval
			(at 15.24 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/A19")
			(pinfunction "A19")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-42_W15.24mm.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 178.22 99.065 90)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP1"
			(at 2.065 0.03 180)
			(layer "F.SilkS")
		)
		(property "Value" "Jumper_2_Small_Open"
			(at 0 1.9 270)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 2-pole, small symbol, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(sheetname "Root")
		(sheetfile "29F160_to_27C322.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at -0.65 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "/~{CE}")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 1 "/~{CE1}")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 193.5 94.75)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 179.02 94.165 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 2.52 -0.085 180)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "29F160_to_27C322.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 185.62 101.965 90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at 0 -1.87 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Jumper_3_Open"
			(at 0 2 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 3-pole, both open"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*3Pads* TestPoint*Bridge*")
		(sheetname "Root")
		(sheetfile "29F160_to_27C322.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -1.3 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "+5V")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 58 "/~{BYTE}")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.3 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 6 "GND")
			(pinfunction "B")
			(pintype "passive")
		)
	)
	(footprint "Package_SO:TSOP-I-48_18.4x12mm_P0.5mm"
		(layer "B.Cu")
		(at 185.12 99.065 180)
		(descr "TSOP-I, 48 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation DD), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSOP-I SO")
		(property "Reference" "U3"
			(at -12.63 5.565 180)
			(layer "B.SilkS")
		)
		(property "Value" "27C160"
			(at 0 -6.95 180)
			(layer "B.Fab")
		)
		(property "Footprint" "Package_SO:TSOP-I-48_18.4x12mm_P0.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://pdf1.alldatasheet.com/datasheet-pdf/download/22894/STMICROELECTRONICS/M29F160BB.html"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "16 Mbit Flash"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W15.24mm* PLCC*")
		(sheetname "Root")
		(sheetfile "29F160_to_27C322.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 4 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -9.6875 5.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 42 "/A15")
			(pinfunction "A15")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -9.6875 5.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 40 "/A14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -9.6875 4.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/A13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -9.6875 4.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 31 "/A12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -9.6875 3.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 19 "/A11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -9.6875 3.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/A10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -9.6875 2.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 30 "/A9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -9.6875 2.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 9 "/A8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -9.6875 1.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/A19")
			(pinfunction "A19")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -9.6875 1.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 51 "unconnected-(U3-NC-Pad10)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "11" smd roundrect
			(at -9.6875 0.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at -9.6875 0.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "~{RP}")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at -9.6875 -0.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 49 "unconnected-(U3-NC-Pad13)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "14" smd roundrect
			(at -9.6875 -0.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 48 "unconnected-(U3-NC-Pad14)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "15" smd roundrect
			(at -9.6875 -1.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 47 "unconnected-(U3-R~{B}-Pad15)")
			(pinfunction "R~{B}")
			(pintype "output")
		)
		(pad "16" smd roundrect
			(at -9.6875 -1.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/A18")
			(pinfunction "A18")
			(pintype "input")
		)
		(pad "17" smd roundrect
			(at -9.6875 -2.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 36 "/A17")
			(pinfunction "A17")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at -9.6875 -2.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 41 "/A7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "19" smd roundrect
			(at -9.6875 -3.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "/A6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at -9.6875 -3.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/A5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at -9.6875 -4.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 26 "/A4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at -9.6875 -4.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 39 "/A3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at -9.6875 -5.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "/A2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at -9.6875 -5.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/A1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 9.6875 -5.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 27 "/A0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 9.6875 -5.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 50 "/~{CE2}")
			(pinfunction "~{CE}")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 9.6875 -4.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "28" smd roundrect
			(at 9.6875 -4.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/~{OE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "29" smd roundrect
			(at 9.6875 -3.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/D0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "30" smd roundrect
			(at 9.6875 -3.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 28 "/D8")
			(pinfunction "D8")
			(pintype "tri_state")
		)
		(pad "31" smd roundrect
			(at 9.6875 -2.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 35 "/D1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "32" smd roundrect
			(at 9.6875 -2.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/D9")
			(pinfunction "D9")
			(pintype "tri_state")
		)
		(pad "33" smd roundrect
			(at 9.6875 -1.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/D2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "34" smd roundrect
			(at 9.6875 -1.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/D10")
			(pinfunction "D10")
			(pintype "tri_state")
		)
		(pad "35" smd roundrect
			(at 9.6875 -0.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 34 "/D3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "36" smd roundrect
			(at 9.6875 -0.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/D11")
			(pinfunction "D11")
			(pintype "tri_state")
		)
		(pad "37" smd roundrect
			(at 9.6875 0.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "38" smd roundrect
			(at 9.6875 0.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "/D4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "39" smd roundrect
			(at 9.6875 1.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/D12")
			(pinfunction "D12")
			(pintype "tri_state")
		)
		(pad "40" smd roundrect
			(at 9.6875 1.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/D5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "41" smd roundrect
			(at 9.6875 2.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/D13")
			(pinfunction "D13")
			(pintype "tri_state")
		)
		(pad "42" smd roundrect
			(at 9.6875 2.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/D6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "43" smd roundrect
			(at 9.6875 3.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/D14")
			(pinfunction "D14")
			(pintype "tri_state")
		)
		(pad "44" smd roundrect
			(at 9.6875 3.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 24 "/D7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "45" smd roundrect
			(at 9.6875 4.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/D15")
			(pinfunction "D15A-1")
			(pintype "tri_state")
		)
		(pad "46" smd roundrect
			(at 9.6875 4.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "47" smd roundrect
			(at 9.6875 5.25 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 58 "/~{BYTE}")
			(pinfunction "~{BYTE}")
			(pintype "input")
		)
		(pad "48" smd roundrect
			(at 9.6875 5.75 180)
			(size 1.575 0.3)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 29 "/A16")
			(pinfunction "A16")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSOP-I-48_18.4x12mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 225.298 107.95)
		(end 225.298 90.17)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.942 90.17)
		(end 170.942 107.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.72 90.17)
		(end 170.942 90.17)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.942 107.95)
		(end 225.298 107.95)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 225.298 90.17)
		(end 172.72 90.17)
		(layer "Edge.Cuts")
	)
	(gr_text "29F160"
		(at 185.125 99.075 0)
		(layer "B.SilkS")
	)
	(gr_text "27C322: USE U2, U3, AND U4\n27C160: USE U2 ONLY"
		(at 221 100.5 0)
		(layer "B.SilkS")
	)
	(gr_text " 8-BIT"
		(at 186.75 101.25 0)
		(layer "F.SilkS")
	)
	(gr_text "U4:  4MB\nJP1: 2MB"
		(at 182.5 96.25 0)
		(layer "F.SilkS")
	)
	(gr_text "16-BIT"
		(at 187.25 103.75 0)
		(layer "F.SilkS")
	)
	(gr_text "29F160"
		(at 211.1 99.05 0)
		(layer "F.SilkS")
	)
	(gr_text "v1.0"
		(at 173.75 101.3 90)
		(layer "F.Mask")
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 186.25 102) (xy 186.5 102) (xy 187.25 101.25) (xy 191.5 101.25) (xy 196 96.75) (xy 213.15 96.5)
				(xy 213.1 95) (xy 212.65 94.1) (xy 215.2 93.5) (xy 216.65 93.35) (xy 217.25 94.4) (xy 217.75 95.75)
				(xy 218.75 97.25) (xy 219.25 98.25) (xy 221.25 98.25) (xy 221.25 96.5) (xy 223.75 96.5) (xy 223.75 97.75)
				(xy 222.75 97.75) (xy 222.5 99) (xy 221.75 100.25) (xy 217 100.25) (xy 216.5 100.75) (xy 193.5 100.75)
				(xy 191.75 102.5) (xy 191 103) (xy 188.25 103) (xy 187.5 103.5) (xy 186.25 103.5)
			)
		)
	)
	(zone
		(net 6)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 225.3 107.95) (xy 221.55 107.95) (xy 210.55 107.95) (xy 210.5 104.8) (xy 221.55 104.75) (xy 221.5 92.75)
				(xy 225.25 92.75)
			)
		)
	)
	(zone
		(net 6)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 180.5 97) (xy 182.75 97) (xy 182.75 95) (xy 185.5 92.5) (xy 185.5 89.75) (xy 170.25 89.75) (xy 170.25 104.5)
				(xy 174.75 104.5) (xy 174.75 96.75)
			)
		)
	)
	(zone
		(net 6)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 186.35 100.175) (xy 182.075 100.175) (xy 179.625 101.95) (xy 178.725 102) (xy 178.2 101.475)
				(xy 177.475 101.525) (xy 177.55 103.375) (xy 176.95 104.4) (xy 177.55 105) (xy 183.175 105) (xy 182.925 105)
				(xy 184.825 105) (xy 184.825 101.45) (xy 186.375 101.45)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 171 104.5) (xy 171 108) (xy 174 108) (xy 174 106.25) (xy 175 105.675) (xy 186.75 105.675) (xy 186.75 104.525)
				(xy 187.75 104.9) (xy 187.75 102.5) (xy 184 102.5) (xy 184 100.75) (xy 177.5 100.75) (xy 177 100.25)
				(xy 177 97.75) (xy 177.5 97.25) (xy 179 97.25) (xy 180.25 98.5) (xy 180.75 98.5) (xy 180.5 96.75)
				(xy 180.5 93.75) (xy 179 93.75) (xy 179 96.25) (xy 176.25 96.25) (xy 176.25 101.5) (xy 174.75 101.5)
				(xy 174.75 104.5)
			)
		)
	)
	(zone
		(net 6)
		(net_name "GND")
		(layers "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.75 90) (xy 225.5 90) (xy 225.5 108.25) (xy 170.75 108.25)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 175 98.5) (xy 179.5 98.5) (xy 179.5 102.25) (xy 175 102.25)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 186.37 104.315) (xy 187.37 104.315) (xy 188.87 102.815) (xy 191.62 102.815) (xy 193.62 100.815)
				(xy 195.37 100.815) (xy 195.37 99.065) (xy 205.87 99.065) (xy 205.87 97.315) (xy 194.12 97.315)
				(xy 194.12 98.065) (xy 189.12 98.065) (xy 186.37 100.565)
			)
		)
	)
)