(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 25)
    (no_connects 0)
    (area 88.871667 74.266666 195.608334 103.533333)
    (thickness 1.6)
    (drawings 13)
    (tracks 149)
    (zones 0)
    (modules 20)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.18)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.15)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(P1-Pad3)")
  (net 5 "Net-(P1-Pad4)")
  (net 6 "Net-(P5-Pad1)")
  (net 7 "Net-(P5-Pad2)")
  (net 8 "Net-(P5-Pad3)")
  (net 9 "Net-(P14-Pad6)")
  (net 10 "Net-(P14-Pad5)")
  (net 11 "Net-(P10-Pad1)")
  (net 12 "Net-(P11-Pad1)")
  (net 13 "Net-(P12-Pad1)")
  (net 14 "Net-(P13-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P11-Pad1)")
    (add_net "Net-(P12-Pad1)")
    (add_net "Net-(P13-Pad1)")
    (add_net "Net-(P14-Pad5)")
    (add_net "Net-(P14-Pad6)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class thin ""
    (clearance 0.2)
    (trace_width 0.18)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 106.68 80.01 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 1.25 -2.5 270) (layer F.SilkS))
    (fp_text value C_Small (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 58D7C4BE)
    (at 190.5 90.805)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -2.413) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 58D7126C)
    (at 139.7 96.52 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad3)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 58D71273)
    (at 139.7 81.28 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 58D7125E)
    (at 96.52 98.425 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 9.906 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 58D71253)
    (at 93.98 85.09)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 9.906) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P5-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 182.88 79.375 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P5-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58D7C824)
    (at 101.6 85.09 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 7.366 90) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 58D7C594)
    (at 190.5 83.82)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 0 -2.286) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P14-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 58D7C62F)
    (at 186.69 86.36)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 0 -2.286) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P14-Pad5)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 58D7C55D)
    (at 182.88 88.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P10 (at 0 -2.286) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P10-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 58D7C554)
    (at 157.48 88.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P11 (at 0 -2.286) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P11-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 58D7C566)
    (at 127 88.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P12 (at 0 -2.54) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P12-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 58D7D235)
    (at 101.6 88.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P13 (at 0 2.032) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P13-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 58D7123F)
    (at 114.3 79.375 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P14 (at 0.127 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P13-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P12-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P11-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P10-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P14-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P14-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 58D7127D)
    (at 160.02 79.375 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P15 (at -0.127 -2.286 90) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 58D71264)
    (at 114.3 98.425 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P16 (at -0.127 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 58D71287)
    (at 160.02 98.425 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P17 (at 0.127 -2.286 90) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58D71247)
    (at 99.06 81.28)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U1 (at 2.54 -1.524 180) (layer F.SilkS))
    (fp_text value XC6202 (at 0 3) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 58D7C83C)
    (at 98.298 83.82 270)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 4.572 -1.016 270) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (gr_text "Press.\nSensor" (at 186.69 94.234 90) (layer F.SilkS))
  (gr_text LED (at 93.98 81.28 90) (layer F.SilkS))
  (gr_text "MagicFlute Proto13" (at 123.19 94.234) (layer F.SilkS))
  (gr_circle (center 178.943 88.9) (end 178.943 90.805) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 161.29 88.9) (end 161.29 90.805) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 130.81 88.9) (end 130.81 90.805) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 105.41 88.9) (end 105.41 90.805) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.44 77.47) (end 91.44 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.04 77.47) (end 193.04 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.44 100.33) (end 193.04 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.04 77.47) (end 91.44 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 168 89) (end 169 89.5) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 116 89) (end 116.5 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.948 78.232) (xy 91.948 99.822) (xy 192.532 99.822) (xy 192.532 77.978) (xy 91.948 77.978)
        (xy 91.948 78.232)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.15)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 192.532 99.822) (xy 91.948 99.822) (xy 91.948 77.978) (xy 192.532 77.978) (xy 192.532 99.822)
      )
    )
  )
)
