(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 214)
    (zones 0)
    (modules 20)
    (nets 26)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.1524)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.381)
    (via_drill 0.254)
    (via_min_size 0.381)
    (via_min_drill 0.254)
    (user_via 0.381 0.254)
    (user_via 0.55 0.4)
    (user_via 0.75 0.6)
    (user_via 0.95 0.8)
    (user_via 1.3 1)
    (user_via 1.5 1.2)
    (user_via 1.7 1.4)
    (user_via 1.9 1.6)
    (uvia_size 0.381)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.381)
    (uvia_min_drill 0.254)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.1)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "LPC82X_JDH20_plots"))
  )
  (net 0 "")
  (net 1 VSS)
  (net 2 VDD)
  (net 3 /PIO0_9)
  (net 4 "Net-(C3-Pad1)")
  (net 5 /PIO0_8)
  (net 6 "Net-(FB1-Pad2)")
  (net 7 /PIO0_4)
  (net 8 /PIO0_3)
  (net 9 /PIO0_2)
  (net 10 /PIO0_11)
  (net 11 /PIO0_10)
  (net 12 /PIO0_15)
  (net 13 /PIO0_1)
  (net 14 "Net-(J2-Pad2)")
  (net 15 "Net-(J2-Pad4)")
  (net 16 "Net-(J2-Pad10)")
  (net 17 /RESET)
  (net 18 /PIO0_12)
  (net 19 /PIO0_13)
  (net 20 /PIO0_17)
  (net 21 /PIO0_14)
  (net 22 /PIO0_0)
  (net 23 /PIO0_16)
  (net 24 /PIO0_7)
  (net 25 /PIO0_6)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.381)
    (via_drill 0.254)
    (uvia_dia 0.381)
    (uvia_drill 0.254)
    (add_net /PIO0_0)
    (add_net /PIO0_1)
    (add_net /PIO0_10)
    (add_net /PIO0_11)
    (add_net /PIO0_12)
    (add_net /PIO0_13)
    (add_net /PIO0_14)
    (add_net /PIO0_15)
    (add_net /PIO0_16)
    (add_net /PIO0_17)
    (add_net /PIO0_2)
    (add_net /PIO0_3)
    (add_net /PIO0_4)
    (add_net /PIO0_6)
    (add_net /PIO0_7)
    (add_net /PIO0_8)
    (add_net /PIO0_9)
    (add_net /RESET)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(FB1-Pad2)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad4)")
    (add_net VDD)
    (add_net VSS)
  )
  (module SquantorSpecial:solder_jumper_2way_conn (layer F.Cu) (tedit 5BE55CFE)
    (at 135.4 109.8 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference SJ1 (at -2.2 0.8) (layer F.SilkS))
    (fp_text value SolderJumper_2way_1conn (at 0 1.8 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(FB1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0402_hand (layer F.Cu) (tedit 5921FEA0)
    (at 135.5 94.2 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at -2 0 180) (layer F.SilkS))
    (fp_text value 100k (at -2.9 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /PIO0_2))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorCrystal:Crystal_3225_4 (layer F.Cu) (tedit 5BF6F546)
    (at 130.6 110.25 180)
    (attr smd)
    (fp_text reference Y1 (at 1.7 2.55 270) (layer F.SilkS))
    (fp_text value 12MHz (at 1.7 2.65 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0.85 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 /PIO0_9))
    (pad 2 smd rect (at 1.1 0.85 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 VSS))
    (pad 3 smd rect (at 1.1 -0.85 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 /PIO0_8))
    (pad 4 smd rect (at -1.1 -0.85 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 VSS))
  )
  (module Symbols:OSHW-Symbol_6.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 134.5 101.3 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference N1 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OHWLOGO (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module SquantorLabels:Label_version (layer B.Cu) (tedit 5B5A1E49)
    (at 134.5 104.9)
    (fp_text reference N2 (at 0 -1.4) (layer B.Fab) hide)
    (fp_text value 20190310 (at -0.4 0.1) (layer B.SilkS))
    (fp_text user V: (at 4 0.1) (layer B.SilkS))
  )
  (module SquantorRcl:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 139.6 91 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -2.7 0 90) (layer F.SilkS))
    (fp_text value 10u (at -2.7 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VSS))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0402 (layer F.Cu) (tedit 58D18F8A)
    (at 130.6 107.95 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at -0.9 1.15) (layer F.SilkS))
    (fp_text value 18p (at -1 1.15 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VSS) (solder_mask_margin 0.1))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /PIO0_9) (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 134.3 107.6)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.4 0.1) (layer F.SilkS))
    (fp_text value 1u (at 2.4 0.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0402 (layer F.Cu) (tedit 58D18F8A)
    (at 130.7 112.55)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 2.1 0.05) (layer F.SilkS))
    (fp_text value 18p (at 2.2 0.05) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /PIO0_8) (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VSS) (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0402 (layer F.Cu) (tedit 58D18F8A)
    (at 134.6 106.2)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 2.1 0) (layer F.SilkS))
    (fp_text value 100n (at 2.9 0) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VSS) (solder_mask_margin 0.1))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)") (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0402 (layer F.Cu) (tedit 58D18F8A)
    (at 133.55 109.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference FB1 (at 2.3 -0.95 270) (layer F.SilkS))
    (fp_text value FB (at 2.4 -0.95 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)") (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(FB1-Pad2)") (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorConnectors:Header-0127-2X05-H006 (layer F.Cu) (tedit 5BE55D04)
    (at 133.2 90.6 180)
    (fp_text reference J2 (at -4.8 -0.4 270) (layer F.SilkS))
    (fp_text value JTAG_2X05 (at 0 2.5 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -2.54 0.635 180) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 VDD))
    (pad 2 thru_hole circle (at -2.54 -0.635 180) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at -1.27 0.635 180) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 VSS))
    (pad 4 thru_hole circle (at -1.27 -0.635 180) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at 0 0.635 180) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 VSS))
    (pad 6 thru_hole circle (at 0 -0.635 180) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 1.27 0.635 180) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 1.27 -0.635 180) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 2.54 0.635 180) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 VSS))
    (pad 10 thru_hole circle (at 2.54 -0.635 180) (size 0.75 0.75) (drill 0.6) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad10)"))
  )
  (module SquantorRcl:R_0402_hand (layer F.Cu) (tedit 5921FEA0)
    (at 130.9 94.2)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 1 1.5) (layer F.SilkS))
    (fp_text value 100K (at -0.2 1.5) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /RESET))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0402_hand (layer F.Cu) (tedit 5921FEA0)
    (at 133.2 94.2 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at -2.8 -1.5 180) (layer F.SilkS))
    (fp_text value 100k (at -2.1 -1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /PIO0_3))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VSS))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0402_hand (layer F.Cu) (tedit 5921FEA0)
    (at 135.5 92.9 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at -2 0 180) (layer F.SilkS))
    (fp_text value 33 (at -2.2 -0.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /PIO0_2))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0402_hand (layer F.Cu) (tedit 5921FEA0)
    (at 133.2 92.9 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at -0.8 -2.8 180) (layer F.SilkS))
    (fp_text value 33 (at -0.5 -2.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad4)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /PIO0_3))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0402_hand (layer F.Cu) (tedit 5921FEA0)
    (at 130.9 92.9)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at -1.3 2.8 180) (layer F.SilkS))
    (fp_text value 33 (at -1.2 2.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad10)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /RESET))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorIC:SOT360 (layer F.Cu) (tedit 5C853204)
    (at 134.6 101.6 180)
    (descr "<li><b>SOT360</b><hr>\n<ul><li>TSSOP20: plastic thin shrink small outline package; 20 leads; body width 4.4 mm\n<li><u>JEDEC</u>: MO-153\n<li><u>IEC</u>: </ul>")
    (fp_text reference U3 (at -4.6 -0.1 270) (layer F.SilkS))
    (fp_text value LPC812M101JDH20 (at 4.6 3.1 270) (layer F.Fab) hide)
    (pad 15 smd rect (at 0.325 -2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 16 smd rect (at -0.325 -2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 VSS))
    (pad 17 smd rect (at -0.975 -2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 24 /PIO0_7))
    (pad 18 smd rect (at -1.625 -2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 25 /PIO0_6))
    (pad 19 smd rect (at -2.275 -2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 22 /PIO0_0))
    (pad 20 smd rect (at -3.025 -2.925 180) (size 0.6 1.35) (layers F.Cu F.Paste F.Mask)
      (net 21 /PIO0_14))
    (pad 14 smd rect (at 0.975 -2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 5 /PIO0_8))
    (pad 13 smd rect (at 1.625 -2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 3 /PIO0_9))
    (pad 12 smd rect (at 2.275 -2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 13 /PIO0_1))
    (pad 11 smd rect (at 3.025 -2.925 180) (size 0.6 1.35) (layers F.Cu F.Paste F.Mask)
      (net 12 /PIO0_15))
    (pad 5 smd rect (at -0.325 2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 7 /PIO0_4))
    (pad 4 smd rect (at -0.975 2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 17 /RESET))
    (pad 3 smd rect (at -1.625 2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 18 /PIO0_12))
    (pad 2 smd rect (at -2.275 2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 19 /PIO0_13))
    (pad 1 smd rect (at -3.025 2.925 180) (size 0.6 1.35) (layers F.Cu F.Paste F.Mask)
      (net 20 /PIO0_17))
    (pad 6 smd rect (at 0.325 2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 8 /PIO0_3))
    (pad 7 smd rect (at 0.975 2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 9 /PIO0_2))
    (pad 8 smd rect (at 1.625 2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 10 /PIO0_11))
    (pad 9 smd rect (at 2.275 2.925 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 11 /PIO0_10))
    (pad 10 smd rect (at 3.025 2.925 180) (size 0.6 1.35) (layers F.Cu F.Paste F.Mask)
      (net 23 /PIO0_16))
  )
  (module SquantorConnectorsNamed:LPC81XJDH20_breakout_left (layer B.Cu) (tedit 5C85320D)
    (at 127 101.6 270)
    (descr "PIN HEADER")
    (tags "PIN HEADER")
    (attr virtual)
    (fp_text reference J1 (at -12 -2.3) (layer B.SilkS))
    (fp_text value LPC81XJDH20_breakout_left (at 0 -2.1 270) (layer B.Fab) hide)
    (fp_text user VSS (at -10.7 -2.3 180) (layer B.SilkS))
    (fp_text user PIO0_3 (at -8.9 -3 180) (layer B.SilkS))
    (fp_text user PIO0_2 (at -6.35 -3 180) (layer B.SilkS))
    (fp_text user PIO0_11 (at -3.8 -3.3 180) (layer B.SilkS))
    (fp_text user PIO0_10 (at -1.1 -3.3 180) (layer B.SilkS))
    (fp_text user PIO0_16 (at 1.2 -3.3 180) (layer B.SilkS))
    (fp_text user PIO0_15 (at 4.6 -3.3 180) (layer B.SilkS))
    (fp_text user PIO0_1 (at 6.3 -3 180) (layer B.SilkS))
    (fp_text user PIO0_9 (at 8.89 -3 180) (layer B.SilkS))
    (fp_text user PIO0_8 (at 11.4 -3 180) (layer B.SilkS))
    (pad 1 thru_hole rect (at -11.43 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 1 VSS))
    (pad 2 thru_hole circle (at -8.89 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 8 /PIO0_3))
    (pad 3 thru_hole circle (at -6.35 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 9 /PIO0_2))
    (pad 4 thru_hole circle (at -3.81 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 10 /PIO0_11))
    (pad 5 thru_hole circle (at -1.27 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 11 /PIO0_10))
    (pad 6 thru_hole circle (at 1.27 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 23 /PIO0_16))
    (pad 7 thru_hole circle (at 3.81 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 12 /PIO0_15))
    (pad 8 thru_hole circle (at 6.35 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 13 /PIO0_1))
    (pad 9 thru_hole circle (at 8.89 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 3 /PIO0_9))
    (pad 10 thru_hole circle (at 11.43 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 5 /PIO0_8))
  )
  (module SquantorConnectorsNamed:LPC81XJDH20_breakout_right (layer B.Cu) (tedit 5C853208)
    (at 142.24 101.6 270)
    (descr "PIN HEADER")
    (tags "PIN HEADER")
    (attr virtual)
    (fp_text reference J3 (at -12 2.34) (layer B.SilkS))
    (fp_text value LPC81XJDH20_breakout_right (at 0 -2.1 270) (layer B.Fab) hide)
    (fp_text user VDD (at -10.5 2.44 180) (layer B.SilkS))
    (fp_text user PIO0_4 (at -8.89 3.04 180) (layer B.SilkS))
    (fp_text user PIO0_5 (at -6.35 3.04 180) (layer B.SilkS))
    (fp_text user PIO0_12 (at -3.81 3.34 180) (layer B.SilkS))
    (fp_text user PIO0_13 (at -1.3 3.34 180) (layer B.SilkS))
    (fp_text user PIO0_17 (at 1.27 3.34 180) (layer B.SilkS))
    (fp_text user PIO0_14 (at 4.6 3.34 180) (layer B.SilkS))
    (fp_text user PIO0_0 (at 6.35 3.04 180) (layer B.SilkS))
    (fp_text user PIO0_6 (at 8.89 3.04 180) (layer B.SilkS))
    (fp_text user PIO0_7 (at 11.43 3.04 180) (layer B.SilkS))
    (pad 1 thru_hole rect (at 11.43 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 24 /PIO0_7))
    (pad 9 thru_hole circle (at -8.89 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 7 /PIO0_4))
    (pad 8 thru_hole circle (at -6.35 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 17 /RESET))
    (pad 7 thru_hole circle (at -3.81 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 18 /PIO0_12))
    (pad 6 thru_hole circle (at -1.27 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 19 /PIO0_13))
    (pad 5 thru_hole circle (at 1.27 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 20 /PIO0_17))
    (pad 4 thru_hole circle (at 3.81 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 21 /PIO0_14))
    (pad 3 thru_hole circle (at 6.35 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 22 /PIO0_0))
    (pad 2 thru_hole circle (at 8.89 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 25 /PIO0_6))
    (pad 10 thru_hole circle (at -11.43 0 90) (size 1.3 1.3) (drill 1) (layers *.Cu *.Mask)
      (net 2 VDD))
  )
  (gr_line (start 125.4 114.6) (end 125.4 88.6) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 143.8 114.6) (end 125.4 114.6) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 143.8 88.6) (end 143.8 114.6) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 125.4 88.6) (end 143.8 88.6) (layer Edge.Cuts) (width 0.2))
  (zone (net 1) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 125.3 88.5) (xy 143.9 88.5) (xy 143.9 114.7) (xy 125.3 114.7)
      )
    )
  )
  (zone (net 1) (net_name VSS) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 125.3 88.5) (xy 143.9 88.5) (xy 143.9 114.7) (xy 125.3 114.7)
      )
    )
  )
)
