<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="34.925" y1="0" x2="0.635" y2="0" width="0" layer="20"/>
<wire x1="0.635" y1="0" x2="0" y2="0.635" width="0" layer="20"/>
<wire x1="0" y1="0.635" x2="0" y2="17.145" width="0" layer="20"/>
<wire x1="0" y1="17.145" x2="0.635" y2="17.78" width="0" layer="20"/>
<wire x1="0.635" y1="17.78" x2="34.925" y2="17.78" width="0" layer="20"/>
<wire x1="34.925" y1="17.78" x2="35.56" y2="17.145" width="0" layer="20"/>
<wire x1="35.56" y1="17.145" x2="35.56" y2="0.635" width="0" layer="20"/>
<wire x1="35.56" y1="0.635" x2="34.925" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>VIN</text>
<text>GND</text>
<text>3V</text>
<text>GND</text>
<text>B</text>
<text>PWM</text>
<text>A</text>
<text>MAG</text>
<text>TAC</text>
<text>PSH</text>
<text>FIRE</text>
<text>ACC</text>
<text>SCL</text>
<text>SDA</text>
<text>3V</text>
<text>GND</text>
<text>5V</text>
<text>PWM</text>
<text>RapidShark
Breakout</text>
<text>by schizobovine &lt;sean@yak.net&gt;</text>
<text>&gt;VERSION</text>
<text>&gt;VERSION</text>
<text>BTN</text>
<text>&gt;VERSION</text>
<text>&gt;VERSION</text>
<text>GND</text>
<text>DRT</text>
<text>SN74LVC1T45</text>
<text>AP2204</text>
<text>2u2</text>
<text>1u</text>
</plain>
<libraries>
<library name="a_parts">
<packages>
<package name="DUMMY">
<description>NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.</description>
</package>
<package name="JST-3-PH-VERT-PTH">
<description>This 3-pin connector mates with the JST cable sold on SparkFun.</description>
</package>
<package name="JST-4-PH-VERT-PTH">
</package>
<package name="SMA-DIODE-TVS-BIDIR">
</package>
<package name="JST-6-PH-VERT-PTH">
</package>
<package name="PTC-1206">
</package>
<package name="R0603-TIGHTER">
</package>
<package name="TEENSY-3.1_OUTERONLY_NOSILK">
</package>
<package name="C0603-TIGHTER">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="JST-2-PH-VERT-PTH">
</package>
<package name="SOT23-6">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="VERSION" value="v1.i"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="a_parts" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="VERSION" value="v1.i"/>
<attribute name="DESIGNER" value="sean@yak.net"/>
</element>
<element name="TRIG" library="a_parts" package="JST-4-PH-VERT-PTH" value="M04JST-PTH-VERT"/>
<element name="PSH" library="a_parts" package="JST-6-PH-VERT-PTH" value="M06JST-PH-PTH-VERT"/>
<element name="TVS" library="a_parts" package="SMA-DIODE-TVS-BIDIR" value="15V">
<attribute name="NAME"/>
</element>
<element name="F1" library="a_parts" package="PTC-1206" value="500mA">
<attribute name="PROD_ID" value="RES-11150"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="a_parts" package="R0603-TIGHTER" value="4K7">
<attribute name="NAME"/>
</element>
<element name="R2" library="a_parts" package="R0603-TIGHTER" value="4K7">
<attribute name="NAME"/>
</element>
<element name="DISP" library="a_parts" package="JST-4-PH-VERT-PTH" value="M04JST-PTH-VERT"/>
<element name="U1" library="a_parts" package="TEENSY-3.1_OUTERONLY_NOSILK" value="TEENSY-3.1-OUTERPTH-NS"/>
<element name="C1" library="a_parts" package="C0603-TIGHTER" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="a_parts" package="C0603-TIGHTER" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="RST" library="a_parts" package="JST-2-PH-VERT-PTH" value="M02JST-PTH-VERT">
<attribute name="NAME"/>
</element>
<element name="U3" library="a_parts" package="SOT23-6" value="SN74LVC1T45">
<attribute name="NAME"/>
</element>
<element name="U4" library="a_parts" package="SOT23-5" value="AP2204">
<attribute name="NAME"/>
</element>
<element name="ACCL" library="a_parts" package="JST-3-PH-VERT-PTH" value="M03JST-PTH-VERT"/>
<element name="FWDIO" library="a_parts" package="JST-4-PH-VERT-PTH" value="M04JST-PTH-VERT"/>
</elements>
<signals>
<signal name="GND">
<contactref element="TRIG" pad="1"/>
<contactref element="PSH" pad="5"/>
<contactref element="DISP" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="AGND"/>
<contactref element="U1" pad="GND1"/>
<contactref element="U1" pad="GND"/>
<contactref element="TVS" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="RST" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="5"/>
<contactref element="U4" pad="2"/>
<contactref element="ACCL" pad="1"/>
</signal>
<signal name="5V">
<contactref element="U1" pad="VIN"/>
<contactref element="C2" pad="1"/>
<contactref element="U3" pad="1"/>
<contactref element="U4" pad="5"/>
<contactref element="ACCL" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="R1" pad="1"/>
<contactref element="DISP" pad="3"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="SCL">
<contactref element="R2" pad="1"/>
<contactref element="DISP" pad="4"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="CLIP">
<contactref element="FWDIO" pad="2"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="PUSH">
<contactref element="TRIG" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="FIRE">
<contactref element="TRIG" pad="3"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="ACCEL">
<contactref element="TRIG" pad="4"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="PUSH_A">
<contactref element="PSH" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="PUSH_PWM">
<contactref element="PSH" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="PUSH_B">
<contactref element="PSH" pad="3"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="ACCEL_PWM_5V">
<contactref element="U3" pad="3"/>
<contactref element="ACCL" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="3.3V"/>
<contactref element="U1" pad="3V"/>
<contactref element="PSH" pad="4"/>
<contactref element="DISP" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="VIN">
<contactref element="F1" pad="2"/>
<contactref element="TVS" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="BUTT">
<contactref element="U1" pad="23"/>
<contactref element="FWDIO" pad="4"/>
</signal>
<signal name="PROG">
<contactref element="U1" pad="PROG"/>
<contactref element="RST" pad="2"/>
</signal>
<signal name="VRAW">
<contactref element="PSH" pad="6"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="TACH">
<contactref element="U1" pad="16"/>
<contactref element="FWDIO" pad="1"/>
</signal>
<signal name="ACCEL_PWM_3V">
<contactref element="U3" pad="4"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="DART">
<contactref element="FWDIO" pad="3"/>
<contactref element="U1" pad="22"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
