(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 33)
    (zones 0)
    (modules 3)
    (nets 11)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.127)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 3)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "../"))
  )
  (net 0 "")
  (net 1 "Net-(JP2-Pad5)")
  (net 2 "Net-(JP2-Pad4)")
  (net 3 "Net-(JP2-Pad3)")
  (net 4 "Net-(JP2-Pad2)")
  (net 5 "Net-(JP2-Pad1)")
  (net 6 "Net-(U$1-PadTCK)")
  (net 7 "Net-(U$1-PadTMS)")
  (net 8 "Net-(U$1-PadTDO)")
  (net 9 "Net-(U$1-PadTDI)")
  (net 10 "Net-(H1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(H1-Pad1)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(JP2-Pad3)")
    (add_net "Net-(JP2-Pad4)")
    (add_net "Net-(JP2-Pad5)")
    (add_net "Net-(U$1-PadTCK)")
    (add_net "Net-(U$1-PadTDI)")
    (add_net "Net-(U$1-PadTDO)")
    (add_net "Net-(U$1-PadTMS)")
  )
  (net_class power ""
    (clearance 0.1524)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(JP2-Pad2)")
  )
  (module srxe:SMARTRESPONSEXEPOGO (layer Top) (tedit 5E313C6B)
    (at 135.6989 100)
    (fp_text reference U$1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value SMARTRESPONSEXE (at 0 0) (layer F.SilkS) hide)
    (fp_text user MISO (at 19.685 -2.5426) (layer F.SilkS) hide)
    (fp_text user RST (at 19.685 2.5374) (layer F.SilkS) hide)
    (fp_text user SCK (at 19.685 -0.0026) (layer F.SilkS) hide)
    (fp_text user GND (at 33.02 2.5374) (layer F.SilkS) hide)
    (fp_text user VCC (at 33.655 -2.5426) (layer F.SilkS) hide)
    (fp_text user MOSI (at 34.29 -0.0026) (layer F.SilkS) hide)
    (fp_text user TDI (at 7.2 -3.6) (layer F.SilkS) hide)
    (fp_text user TDO (at 2.4 -3.6) (layer F.SilkS) hide)
    (fp_text user TMS (at -2.4 -3.6) (layer F.SilkS) hide)
    (fp_text user TCK (at -7.2 -3.6) (layer F.SilkS) hide)
    (pad GND thru_hole circle (at -2.3989 2.2) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(H1-Pad1)") (solder_mask_margin 0.1016))
    (pad SCK thru_hole circle (at -7.1989 2.2) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(JP2-Pad3)") (solder_mask_margin 0.1016))
    (pad TCK thru_hole circle (at -7.1989 -2.2) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(U$1-PadTCK)") (solder_mask_margin 0.1016))
    (pad TMS thru_hole circle (at -2.3989 -2.2) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(U$1-PadTMS)") (solder_mask_margin 0.1016))
    (pad TDO thru_hole circle (at 2.4011 -2.2) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(U$1-PadTDO)") (solder_mask_margin 0.1016))
    (pad TDI thru_hole circle (at 7.2011 -2.2) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(U$1-PadTDI)") (solder_mask_margin 0.1016))
    (pad MOSI thru_hole circle (at 7.2011 2.2) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(JP2-Pad4)") (solder_mask_margin 0.1016))
    (pad VCC thru_hole circle (at 2.4011 2.2) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(JP2-Pad2)") (solder_mask_margin 0.1016))
    (pad MISO thru_hole circle (at 4.8011 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(JP2-Pad1)") (solder_mask_margin 0.1016))
    (pad RST thru_hole circle (at 0.0011 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(JP2-Pad5)") (solder_mask_margin 0.1016))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer Top) (tedit 5E313C8A)
    (at 149.6689 99.9974)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0.3311 0.0026) (size 4 4) (drill 3) (layers *.Cu *.Mask)
      (net 10 "Net-(H1-Pad1)"))
  )
  (module srxe:2X3_SMD (layer Top) (tedit 5E0720D5)
    (at 162.5 100 270)
    (fp_text reference JP2 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value M03X2FEMALE_SMD (at 0 0 270) (layer F.SilkS) hide)
    (fp_text user >Value (at -3.502 0.408 270) (layer F.Fab))
    (fp_text user >Name (at -3.502 -0.1 270) (layer F.SilkS) hide)
    (pad 6 smd rect (at 2.54 -2.85 270) (size 1.02 1.9) (layers Top F.Paste F.Mask)
      (net 10 "Net-(H1-Pad1)") (solder_mask_margin 0.1016))
    (pad 5 smd rect (at 2.54 2.85 270) (size 1.02 1.9) (layers Top F.Paste F.Mask)
      (net 1 "Net-(JP2-Pad5)") (solder_mask_margin 0.1016))
    (pad 4 smd rect (at 0 -2.85 270) (size 1.02 1.9) (layers Top F.Paste F.Mask)
      (net 2 "Net-(JP2-Pad4)") (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 0 2.85 270) (size 1.02 1.9) (layers Top F.Paste F.Mask)
      (net 3 "Net-(JP2-Pad3)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -2.54 -2.85 270) (size 1.02 1.9) (layers Top F.Paste F.Mask)
      (net 4 "Net-(JP2-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -2.54 2.85 270) (size 1.02 1.9) (layers Top F.Paste F.Mask)
      (net 5 "Net-(JP2-Pad1)") (solder_mask_margin 0.1016))
  )
  (gr_arc (start 172.75 96.25) (end 174 96.25) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 172.75 103.75) (end 172.75 105) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 127.25 103.75) (end 126 103.75) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 127.25 96.25) (end 127.25 95) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Smart Response Hacking Group\ngithub.com/srhg\nv0.2\nRemix of git.io/SRXE\nThanks securelyfitz!" (at 172.5289 99.9974) (layer B.SilkS))
  (gr_line (start 126 103.75) (end 126 96.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.75 105) (end 127.25 105) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174 96.25) (end 174 103.75) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.25 95) (end 172.75 95) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 166.8139 102.5374) (layer F.SilkS))
  (gr_text MOSI (at 166.8139 99.9974) (layer F.SilkS))
  (gr_text VCC (at 166.8139 97.4574) (layer F.SilkS))
  (gr_text RST (at 157.9239 102.5374) (layer F.SilkS))
  (gr_text SCK (at 157.9239 99.9974) (layer F.SilkS))
  (gr_text MISO (at 157.9239 97.4574) (layer F.SilkS))
  (zone (net 10) (net_name "Net-(H1-Pad1)") (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.127))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.2024) (thermal_bridge_width 0.2024))
    (polygon
      (pts
        (xy 126 105) (xy 126 95) (xy 174 95) (xy 174 105)
      )
    )
  )
  (zone (net 10) (net_name "Net-(H1-Pad1)") (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.127))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.2024) (thermal_bridge_width 0.2024))
    (polygon
      (pts
        (xy 126 105) (xy 126 95) (xy 174 95) (xy 174 105)
      )
    )
  )
)
