(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "1")
  (net 2 "2")
  (net 3 "3")
  (net 4 "4")
  (net 5 "5")
  (net 6 "6")
  (net 7 "7")
  (net 8 "8")
  (net 9 "9")
  (net 10 "10")
  (net 11 "11")
  (net 12 "12")
  (net 13 "13")
  (net 14 "14")
  (net 15 "15")
  (net 16 "16")
  (net 17 "17")
  (net 18 "18")
  (net 19 "19")
  (net 20 "20")
  (net 21 "21")
  (net 22 "22")
  (net 23 "23")
  (net 24 "24")
  (net 25 "25")
  (net 26 "26")
  (net 27 "27")
  (net 28 "28")
  (net 29 "29")
  (net 30 "30")
  (net 31 "31")
  (net 32 "32")
  (net 33 "33")
  (net 34 "34")
  (net 35 "35")
  (net 36 "36")
  (net 37 "37")
  (net 38 "38")
  (net 39 "39")
  (net 40 "40")
  (net 41 "41")
  (net 42 "42")
  (net 43 "43")
  (net 44 "44")
  (footprint "Package_SO:TSOP-II-44_10.16x18.41mm_P0.8mm" (layer "F.Cu")
    (tedit 5D9F72B2)
    (at 137.16 80.01)
    (descr "TSOP-II, 44 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSOP-II SO")
    (property "Sheetfile" "tsop-ii-44-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 16.764 -10.16) (layer "F.SilkS"))
    (fp_text value "LY62W51216" (at 0 10.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -5.5875 -8.4) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "1") (pinfunction "A4") (pintype "input"))
    (pad "2" smd roundrect (at -5.5875 -7.6) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "2") (pinfunction "A3") (pintype "input"))
    (pad "3" smd roundrect (at -5.5875 -6.8) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "3") (pinfunction "A2") (pintype "input"))
    (pad "4" smd roundrect (at -5.5875 -6) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "4") (pinfunction "A1") (pintype "input"))
    (pad "5" smd roundrect (at -5.5875 -5.2) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "5") (pinfunction "A0") (pintype "input"))
    (pad "6" smd roundrect (at -5.5875 -4.4) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "6") (pinfunction "CE#") (pintype "input"))
    (pad "7" smd roundrect (at -5.5875 -3.6) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "7") (pinfunction "DQ0") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -5.5875 -2.8) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "8") (pinfunction "DQ1") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -5.5875 -2) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "9") (pinfunction "DQ2") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -5.5875 -1.2) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "10") (pinfunction "DQ3") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -5.5875 -0.4) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "11") (pinfunction "Vcc") (pintype "power_in"))
    (pad "12" smd roundrect (at -5.5875 0.4) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "12") (pinfunction "Vss") (pintype "output"))
    (pad "13" smd roundrect (at -5.5875 1.2) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "13") (pinfunction "DQ4") (pintype "bidirectional"))
    (pad "14" smd roundrect (at -5.5875 2) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "14") (pinfunction "DQ5") (pintype "bidirectional"))
    (pad "15" smd roundrect (at -5.5875 2.8) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "15") (pinfunction "DQ6") (pintype "bidirectional"))
    (pad "16" smd roundrect (at -5.5875 3.6) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "16") (pinfunction "DQ7") (pintype "bidirectional"))
    (pad "17" smd roundrect (at -5.5875 4.4) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "17") (pinfunction "WE#") (pintype "input"))
    (pad "18" smd roundrect (at -5.5875 5.2) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "18") (pinfunction "A18") (pintype "input"))
    (pad "19" smd roundrect (at -5.5875 6) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "19") (pinfunction "A17") (pintype "input"))
    (pad "20" smd roundrect (at -5.5875 6.8) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "20") (pinfunction "A16") (pintype "input"))
    (pad "21" smd roundrect (at -5.5875 7.6) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "21") (pinfunction "A15") (pintype "input"))
    (pad "22" smd roundrect (at -5.5875 8.4) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "22") (pinfunction "A14") (pintype "input"))
    (pad "23" smd roundrect (at 5.5875 8.4) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "23") (pinfunction "A13") (pintype "input"))
    (pad "24" smd roundrect (at 5.5875 7.6) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "24") (pinfunction "A12") (pintype "input"))
    (pad "25" smd roundrect (at 5.5875 6.8) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "25") (pinfunction "A11") (pintype "input"))
    (pad "26" smd roundrect (at 5.5875 6) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "26") (pinfunction "A10") (pintype "input"))
    (pad "27" smd roundrect (at 5.5875 5.2) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "27") (pinfunction "A9") (pintype "input"))
    (pad "28" smd roundrect (at 5.5875 4.4) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "28") (pinfunction "A8") (pintype "input"))
    (pad "29" smd roundrect (at 5.5875 3.6) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "29") (pinfunction "DQ8") (pintype "bidirectional"))
    (pad "30" smd roundrect (at 5.5875 2.8) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "30") (pinfunction "DQ9") (pintype "bidirectional"))
    (pad "31" smd roundrect (at 5.5875 2) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "31") (pinfunction "DQ10") (pintype "bidirectional"))
    (pad "32" smd roundrect (at 5.5875 1.2) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "32") (pinfunction "DQ11") (pintype "bidirectional"))
    (pad "33" smd roundrect (at 5.5875 0.4) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "33") (pinfunction "Vcc") (pintype "power_in"))
    (pad "34" smd roundrect (at 5.5875 -0.4) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "34") (pinfunction "Vss") (pintype "output"))
    (pad "35" smd roundrect (at 5.5875 -1.2) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "35") (pinfunction "DQ12") (pintype "bidirectional"))
    (pad "36" smd roundrect (at 5.5875 -2) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "36") (pinfunction "DQ13") (pintype "bidirectional"))
    (pad "37" smd roundrect (at 5.5875 -2.8) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "37") (pinfunction "DQ14") (pintype "bidirectional"))
    (pad "38" smd roundrect (at 5.5875 -3.6) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "38") (pinfunction "DQ15") (pintype "bidirectional"))
    (pad "39" smd roundrect (at 5.5875 -4.4) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "39") (pinfunction "LB#") (pintype "input"))
    (pad "40" smd roundrect (at 5.5875 -5.2) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "40") (pinfunction "UB#") (pintype "input"))
    (pad "41" smd roundrect (at 5.5875 -6) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "41") (pinfunction "OE#") (pintype "input"))
    (pad "42" smd roundrect (at 5.5875 -6.8) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "42") (pinfunction "A7") (pintype "input"))
    (pad "43" smd roundrect (at 5.5875 -7.6) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "43") (pinfunction "A6") (pintype "input"))
    (pad "44" smd roundrect (at 5.5875 -8.4) (size 1.525 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "44") (pinfunction "A5") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSOP-II-44_10.16x18.41mm_P0.8mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x22_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 147.32 53.34 180)
    (descr "Through hole straight pin header, 1x22, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x22 2.54mm single row")
    (property "Sheetfile" "tsop-ii-44-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 3.556) (layer "B.SilkS"))
    (fp_text value "Conn_01x22_Male" (at 0 -55.67) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -26.67 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "44") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "43") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "42") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "41") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "40") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "39") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "38") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "37") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "36") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "35") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "34") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "33") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "32") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "31") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "30") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "29") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "28") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "27") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "26") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "25") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 -50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "24") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at 0 -53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "23") (pinfunction "Pin_22") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x22_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x22_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 127 53.34 180)
    (descr "Through hole straight pin header, 1x22, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x22 2.54mm single row")
    (property "Sheetfile" "tsop-ii-44-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 3.556) (layer "B.SilkS"))
    (fp_text value "Conn_01x22_Male" (at 0 -55.67) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -26.67 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "4") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "5") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "6") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "7") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "8") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "9") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "10") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "11") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "12") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "13") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "14") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "15") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "16") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "17") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "18") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "19") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "20") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 -50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "21") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at 0 -53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "22") (pinfunction "Pin_22") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x22_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 148.09 51.3) (mid 148.982724 51.680977) (end 149.350974 52.579026) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 149.350974 107.45) (end 149.350974 52.579026) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 126.239026 108.72) (mid 125.337266 108.342734) (end 124.96 107.440974) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 124.96 52.579026) (mid 125.337266 51.677266) (end 126.239026 51.3) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 126.239026 108.72) (end 148.09 108.72) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 124.96 52.579026) (end 124.96 107.440974) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 148.09 51.3) (end 126.239026 51.3) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 149.350974 107.45) (mid 148.98484 108.347474) (end 148.09 108.72) (layer "Edge.Cuts") (width 0.1))
  (gr_text "CC BY-NC-SA 4.0" (at 137.16 80.01) (layer "B.Cu"))
  (gr_text "44" (at 144.78 53.34) (layer "B.SilkS"))
  (gr_text "1" (at 129.032 53.34) (layer "B.SilkS"))
  (gr_text "TSOP-44 Type II\nBreakouT" (at 137.16 104.394) (layer "B.SilkS"))
  (gr_text "by @xunker" (at 137.16 107.188) (layer "B.SilkS"))
  (gr_text "1" (at 130.556 70.104) (layer "F.SilkS"))
  (gr_text "44" (at 144.78 53.34) (layer "F.SilkS"))
  (gr_text "TSOP-48\nTYPE II\nBREAKOUT" (at 137.16 103.505) (layer "F.SilkS"))
  (gr_text "1" (at 129.032 53.34) (layer "F.SilkS"))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.4 111.76)
        (xy 121.92 111.76)
        (xy 121.92 48.26)
        (xy 152.4 48.26)
      )
    )
  )
)
