(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 5)
    (no_connects 0)
    (area 152.324999 88.824999 177.875001 114.375001)
    (thickness 1.6)
    (drawings 17)
    (tracks 22)
    (zones 0)
    (modules 6)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4064)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 "Net-(BT1-Pad2)")
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(BT1-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5AF6C5DD)
    (at 165.1 92.075)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_2mmDrill (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2) (layers *.Cu *.Mask))
  )
  (module Symbols:KiCad-Logo_6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 165.1 103.505 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo_6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module footprints:Keystone_3001_1x12mm-CoinCell (layer F.Cu) (tedit 5AF636BE)
    (at 165.090481 108.035)
    (descr http://www.keyelco.com/product-pdf.cfm?p=778)
    (tags "Keystone type 3001 coin cell retainer")
    (fp_text reference BT1 (at 0.009519 -5.165) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 7.5) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.6 0) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 1 thru_hole circle (at 6.6 0) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask)
      (net 2 "Net-(BT1-Pad2)"))
    (model Battery_Holders.3dshapes/Keystone_3001_1x12mm-CoinCell.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm (layer F.Cu) (tedit 5AF636B5)
    (at 166.37 99.695 180)
    (descr "LED, diameter 3.0mm z-position of LED center 2.0mm, 2 pins")
    (tags "LED diameter 3.0mm z-position of LED center 2.0mm 2 pins")
    (fp_text reference D1 (at 1.27 1.905 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 7.63 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AF63732)
    (at 170.815 101.6 45)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 -2.31 45) (layer F.SilkS) hide)
    (fp_text value R (at 3.592102 0 45) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 45) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 45) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AF63732)
    (at 159.385 101.6 135)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.81 -2.31 135) (layer F.SilkS) hide)
    (fp_text value R (at 3.592102 0 135) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 135) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 135) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text + (at 162.56 98.425) (layer F.SilkS))
  (gr_text www.Makersbox.us (at 165.1 97.79) (layer B.SilkS))
  (gr_text "Hello     World" (at 165.1 92.075) (layer F.SilkS))
  (gr_line (start 154.94 88.9) (end 175.26 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 111.76) (end 152.4 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.26 114.3) (end 154.94 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 111.76) (end 177.8 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 175.26 91.44) (end 175.26 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 154.94 91.44) (end 152.4 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 154.94 111.76) (end 154.94 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 175.26 111.76) (end 177.8 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 26.67 (width 0.3) (layer Dwgs.User)
    (gr_text "1.0500 in" (at 165.735 118.19) (layer Dwgs.User))
    (feature1 (pts (xy 179.07 114.3) (xy 179.07 119.54)))
    (feature2 (pts (xy 152.4 114.3) (xy 152.4 119.54)))
    (crossbar (pts (xy 152.4 116.84) (xy 179.07 116.84)))
    (arrow1a (pts (xy 179.07 116.84) (xy 177.943496 117.426421)))
    (arrow1b (pts (xy 179.07 116.84) (xy 177.943496 116.253579)))
    (arrow2a (pts (xy 152.4 116.84) (xy 153.526504 117.426421)))
    (arrow2b (pts (xy 152.4 116.84) (xy 153.526504 116.253579)))
  )
  (dimension 24.13 (width 0.3) (layer Dwgs.User)
    (gr_text "0.9500 in" (at 148.51 102.235 270) (layer Dwgs.User))
    (feature1 (pts (xy 152.4 114.3) (xy 147.16 114.3)))
    (feature2 (pts (xy 152.4 90.17) (xy 147.16 90.17)))
    (crossbar (pts (xy 149.86 90.17) (xy 149.86 114.3)))
    (arrow1a (pts (xy 149.86 114.3) (xy 149.273579 113.173496)))
    (arrow1b (pts (xy 149.86 114.3) (xy 150.446421 113.173496)))
    (arrow2a (pts (xy 149.86 90.17) (xy 149.273579 91.296504)))
    (arrow2b (pts (xy 149.86 90.17) (xy 150.446421 91.296504)))
  )
)
