(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 168)
    (zones 0)
    (modules 4)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.304)
    (user_trace_width 2.74)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.25 0.51)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J2-Pad1)")
  (net 4 "Net-(J3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
  )
  (module Connectors_Molex:Molex_SMA_Jack_Edge_Mount (layer F.Cu) (tedit 587D2992)
    (at 134.62 76.2 180)
    (descr "Molex SMA Jack, Edge Mount, http://www.molex.com/pdm_docs/sd/732511150_sd.pdf")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J1 (at -1.905 -7.62 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -1.72 -7.11 180) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.89 0.46) (layers B.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.89 0.46) (layers B.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.89 0.46) (layers F.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.89 0.46) (layers F.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_SMA_Jack_Edge_Mount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_SMA_Jack_Edge_Mount (layer F.Cu) (tedit 587D2992)
    (at 111.76 83.82)
    (descr "Molex SMA Jack, Edge Mount, http://www.molex.com/pdm_docs/sd/732511150_sd.pdf")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J2 (at -1.72 7.11) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -1.72 -7.11) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38) (size 0.89 0.46) (layers B.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 1.27 -4.38) (size 0.89 0.46) (layers B.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 1.27 4.38) (size 0.89 0.46) (layers F.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 1.27 -4.38) (size 0.89 0.46) (layers F.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.72 4.38) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.72 0) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_SMA_Jack_Edge_Mount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_SMA_Jack_Edge_Mount (layer F.Cu) (tedit 587D2992)
    (at 134.62 93.98 180)
    (descr "Molex SMA Jack, Edge Mount, http://www.molex.com/pdm_docs/sd/732511150_sd.pdf")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J3 (at -1.72 7.11 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -1.72 -7.11 180) (layer F.Fab))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.89 0.46) (layers F.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.89 0.46) (layers F.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.89 0.46) (layers B.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.89 0.46) (layers B.Cu)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_SMA_Jack_Edge_Mount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "all the parts:DQ1225" (layer F.Cu) (tedit 5CCD028A)
    (at 123.105 84.33)
    (fp_text reference U1 (at 0 -2.56) (layer F.Fab))
    (fp_text value GP2X+ (at 0 2.56) (layer F.Fab))
    (pad 1 smd rect (at -1.355 -0.51) (size 0.51 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.355 0) (size 0.51 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at -1.355 0.51) (size 0.51 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.51 1.355) (size 0.25 0.51) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0 1.355) (size 0.25 0.51) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.51 1.355) (size 0.25 0.51) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 1.355 0.51) (size 0.51 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J3-Pad1)"))
    (pad 8 smd rect (at 1.355 0) (size 0.51 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 1.355 -0.51) (size 0.51 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 10 smd rect (at 0.51 -1.355) (size 0.25 0.51) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0 -1.355) (size 0.25 0.51) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -0.51 -1.355) (size 0.25 0.51) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad EP smd rect (at 0 0) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.001) (solder_paste_margin 0.001))
  )
  (gr_text "2800-7200MHz\nMax Input: 30dBm" (at 127 97.79 -45) (layer B.SilkS))
  (gr_text "GP2X1+ Power Splitter\nBy: Ethanleep" (at 120.65 72.39) (layer B.SilkS))
  (gr_text "Out 2\n" (at 127 96.52) (layer F.SilkS))
  (gr_text "Out 1" (at 128.27 72.39) (layer F.SilkS))
  (gr_text In (at 110.49 76.2) (layer F.SilkS))
  (gr_line (start 107.315 89.916) (end 107.315 80.645) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 118.237 100.838) (end 107.315 89.916) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 138.176 100.838) (end 118.237 100.838) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 139.192 99.822) (end 138.176 100.838) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 139.192 69.469) (end 139.192 99.822) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 138.684 68.961) (end 139.192 69.469) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 110.49 68.961) (end 138.684 68.961) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 107.315 72.136) (end 110.49 68.961) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 107.315 80.645) (end 107.315 72.136) (layer Edge.Cuts) (width 0.2))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.315 89.916) (xy 118.237 100.838) (xy 138.176 100.838) (xy 139.192 99.822) (xy 139.192 69.469)
        (xy 138.684 68.961) (xy 110.49 68.961) (xy 107.315 72.136)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.315 89.916) (xy 118.237 100.838) (xy 138.176 100.838) (xy 139.192 99.822) (xy 139.192 69.469)
        (xy 138.684 68.961) (xy 110.49 68.961) (xy 107.315 72.136)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.315 72.136) (xy 107.315 89.916) (xy 118.237 100.838) (xy 138.176 100.838) (xy 139.192 99.822)
        (xy 139.192 69.469) (xy 138.684 68.961) (xy 110.49 68.961)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.315 72.136) (xy 107.315 89.916) (xy 118.237 100.838) (xy 138.176 100.838) (xy 139.192 99.822)
        (xy 139.192 69.469) (xy 138.684 68.961) (xy 110.49 68.961)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.95 85.471) (xy 112.5855 85.471) (xy 112.776 85.4075) (xy 112.903 85.344) (xy 112.9665 85.2805)
        (xy 113.03 85.1535) (xy 113.0935 84.963) (xy 113.157 84.963) (xy 113.2205 84.963) (xy 121.92 84.963)
        (xy 122.174 84.8995) (xy 122.3645 84.7725) (xy 122.428 84.6455) (xy 122.428 84.0105) (xy 122.3645 83.8835)
        (xy 122.174 83.7565) (xy 121.92 83.693) (xy 113.665 83.693) (xy 113.3475 83.3755) (xy 113.0935 83.185)
        (xy 113.0935 82.7405) (xy 113.03 82.4865) (xy 112.776 82.2325) (xy 112.522 82.169) (xy 107.95 82.169)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.557 95.631) (xy 133.858 95.631) (xy 133.604 95.5675) (xy 133.4135 95.4405) (xy 133.2865 95.123)
        (xy 133.2865 94.4245) (xy 133.2865 94.361) (xy 133.096 94.234) (xy 127.6985 88.8365) (xy 127.508 88.8365)
        (xy 127.3175 88.773) (xy 127.127 88.7095) (xy 126.746 88.3285) (xy 126.619 88.138) (xy 126.5555 87.9475)
        (xy 126.5555 87.6935) (xy 124.333 85.471) (xy 124.206 85.471) (xy 124.0155 85.4075) (xy 123.8885 85.2805)
        (xy 123.7615 85.0265) (xy 123.7615 84.5185) (xy 125.095 84.5185) (xy 125.1585 84.5185) (xy 127.6985 87.0585)
        (xy 127.762 87.1855) (xy 127.8255 87.3125) (xy 127.889 87.4395) (xy 128.016 87.503) (xy 128.2065 87.5665)
        (xy 128.397 87.757) (xy 133.1595 92.5195) (xy 133.2865 92.583) (xy 133.35 92.583) (xy 133.4135 92.5195)
        (xy 133.477 92.456) (xy 133.604 92.3925) (xy 133.7945 92.329) (xy 138.557 92.329)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.557 77.851) (xy 133.858 77.851) (xy 133.604 77.7875) (xy 133.4135 77.6605) (xy 133.35 77.5335)
        (xy 133.2865 77.2795) (xy 133.2865 76.962) (xy 133.2865 76.8985) (xy 133.223 76.835) (xy 132.461 76.835)
        (xy 131.0005 78.2955) (xy 130.8735 78.4225) (xy 130.7465 78.486) (xy 130.4925 78.5495) (xy 130.3655 78.5495)
        (xy 130.2385 78.5495) (xy 129.7305 79.0575) (xy 129.7305 79.1845) (xy 129.794 79.3115) (xy 129.8575 79.5655)
        (xy 129.794 79.9465) (xy 129.6035 80.264) (xy 128.524 81.3435) (xy 128.3335 81.4705) (xy 128.2065 81.534)
        (xy 128.016 81.5975) (xy 127.8255 81.5975) (xy 127.762 81.5975) (xy 127.635 81.661) (xy 125.1585 84.1375)
        (xy 123.7615 84.1375) (xy 123.7615 83.693) (xy 123.698 83.693) (xy 123.7615 83.5025) (xy 123.825 83.3755)
        (xy 124.0155 83.2485) (xy 124.206 83.185) (xy 124.333 83.185) (xy 127.0635 80.4545) (xy 127.1905 80.3275)
        (xy 127.381 80.264) (xy 127.5715 80.2005) (xy 127.6985 80.2005) (xy 127.8255 80.2005) (xy 128.3335 79.6925)
        (xy 128.397 79.629) (xy 128.3335 79.502) (xy 128.27 79.375) (xy 128.2065 79.1845) (xy 128.2065 78.994)
        (xy 128.27 78.8035) (xy 128.3335 78.6765) (xy 128.4605 78.486) (xy 129.6035 77.343) (xy 129.7305 77.2795)
        (xy 129.8575 77.216) (xy 130.048 77.1525) (xy 130.2385 77.1525) (xy 130.3655 77.1525) (xy 131.7625 75.7555)
        (xy 131.953 75.6285) (xy 132.207 75.565) (xy 133.1595 75.565) (xy 133.2865 75.5015) (xy 133.2865 75.1205)
        (xy 133.35 74.8665) (xy 133.477 74.676) (xy 133.604 74.6125) (xy 133.7945 74.549) (xy 138.557 74.549)
      )
    )
  )
)
