(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "free_DFM_out_AIRCOILS_final")
		)
	)
	(net 0 "")
	(net 1 "positive_terminal")
	(net 2 "negative_terminal")
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 151.003 104.013)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J3"
			(at -2.921 0.002 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Solder Pad Positive Out"
			(at 0 2.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "PCB_for_aircoils.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 1 "positive_terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(footprint "G125-FV10605F3P:HARWIN_G125-FV10605F3P"
		(layer "F.Cu")
		(at 145 109)
		(property "Reference" "J1"
			(at -4.325 -3.635 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G125-FV10605F3P"
			(at 5.97 3.615 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "G125-FV10605F3P:HARWIN_G125-FV10605F3P"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Harwin"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "\n                        \n                            Gecko-SL DIL Female Vertical Throughboard Connector, Reverse fix with 5mm board mount studs, gold, pick & place (cut tape packing), 3+3 contacts\n                        \n"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/G125-FV10605F3P/Harwin/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/G125-FV10605F3P/Harwin/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "G125-FV10605F3P"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "HARWIN"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "PCB_for_aircoils.kicad_sch")
		(zone_connect 0)
		(attr through_hole)
		(pad "" thru_hole circle
			(at -5.15 0)
			(size 3 3)
			(drill 2.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "negative_terminal")
			(zone_connect 2)
		)
		(pad "" thru_hole circle
			(at 5.15 0)
			(size 3 3)
			(drill 2.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "negative_terminal")
			(zone_connect 2)
		)
		(pad "1" thru_hole rect
			(at 1.25 0.625)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "negative_terminal")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 0 0.625)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "negative_terminal")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -1.25 0.625)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "negative_terminal")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 1.25 -0.625)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "positive_terminal")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 0 -0.625)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "positive_terminal")
			(pinfunction "5")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at -1.25 -0.625)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "positive_terminal")
			(pinfunction "6")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "*.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 2.31)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 142.16 109) (xy 142.148877 109.22642) (xy 142.115614 109.450659) (xy 142.060532 109.670558)
					(xy 141.984162 109.883999) (xy 141.887238 110.088926) (xy 141.770695 110.283367) (xy 141.635654 110.465448)
					(xy 141.483417 110.633417) (xy 141.315448 110.785654) (xy 141.133367 110.920695) (xy 140.938926 111.037238)
					(xy 140.733999 111.134162) (xy 140.520558 111.210532) (xy 140.300659 111.265614) (xy 140.07642 111.298877)
					(xy 139.85 111.31) (xy 139.62358 111.298877) (xy 139.399341 111.265614) (xy 139.179442 111.210532)
					(xy 138.966001 111.134162) (xy 138.761074 111.037238) (xy 138.566633 110.920695) (xy 138.384552 110.785654)
					(xy 138.216583 110.633417) (xy 138.064346 110.465448) (xy 137.929305 110.283367) (xy 137.812762 110.088926)
					(xy 137.715838 109.883999) (xy 137.639468 109.670558) (xy 137.584386 109.450659) (xy 137.551123 109.22642)
					(xy 137.54 109) (xy 137.551123 108.77358) (xy 137.584386 108.549341) (xy 137.639468 108.329442)
					(xy 137.715838 108.116001) (xy 137.812762 107.911074) (xy 137.929305 107.716633) (xy 138.064346 107.534552)
					(xy 138.216583 107.366583) (xy 138.384552 107.214346) (xy 138.566633 107.079305) (xy 138.761074 106.962762)
					(xy 138.966001 106.865838) (xy 139.179442 106.789468) (xy 139.399341 106.734386) (xy 139.62358 106.701123)
					(xy 139.85 106.69) (xy 140.07642 106.701123) (xy 140.300659 106.734386) (xy 140.520558 106.789468)
					(xy 140.733999 106.865838) (xy 140.938926 106.962762) (xy 141.133367 107.079305) (xy 141.315448 107.214346)
					(xy 141.483417 107.366583) (xy 141.635654 107.534552) (xy 141.770695 107.716633) (xy 141.887238 107.911074)
					(xy 141.984162 108.116001) (xy 142.060532 108.329442) (xy 142.115614 108.549341) (xy 142.148877 108.77358)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "*.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 2.31)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 152.46 109) (xy 152.448877 109.22642) (xy 152.415614 109.450659) (xy 152.360532 109.670558)
					(xy 152.284162 109.883999) (xy 152.187238 110.088926) (xy 152.070695 110.283367) (xy 151.935654 110.465448)
					(xy 151.783417 110.633417) (xy 151.615448 110.785654) (xy 151.433367 110.920695) (xy 151.238926 111.037238)
					(xy 151.033999 111.134162) (xy 150.820558 111.210532) (xy 150.600659 111.265614) (xy 150.37642 111.298877)
					(xy 150.15 111.31) (xy 149.92358 111.298877) (xy 149.699341 111.265614) (xy 149.479442 111.210532)
					(xy 149.266001 111.134162) (xy 149.061074 111.037238) (xy 148.866633 110.920695) (xy 148.684552 110.785654)
					(xy 148.516583 110.633417) (xy 148.364346 110.465448) (xy 148.229305 110.283367) (xy 148.112762 110.088926)
					(xy 148.015838 109.883999) (xy 147.939468 109.670558) (xy 147.884386 109.450659) (xy 147.851123 109.22642)
					(xy 147.84 109) (xy 147.851123 108.77358) (xy 147.884386 108.549341) (xy 147.939468 108.329442)
					(xy 148.015838 108.116001) (xy 148.112762 107.911074) (xy 148.229305 107.716633) (xy 148.364346 107.534552)
					(xy 148.516583 107.366583) (xy 148.684552 107.214346) (xy 148.866633 107.079305) (xy 149.061074 106.962762)
					(xy 149.266001 106.865838) (xy 149.479442 106.789468) (xy 149.699341 106.734386) (xy 149.92358 106.701123)
					(xy 150.15 106.69) (xy 150.37642 106.701123) (xy 150.600659 106.734386) (xy 150.820558 106.789468)
					(xy 151.033999 106.865838) (xy 151.238926 106.962762) (xy 151.433367 107.079305) (xy 151.615448 107.214346)
					(xy 151.783417 107.366583) (xy 151.935654 107.534552) (xy 152.070695 107.716633) (xy 152.187238 107.911074)
					(xy 152.284162 108.116001) (xy 152.360532 108.329442) (xy 152.415614 108.549341) (xy 152.448877 108.77358)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 2.31)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 142.16 109) (xy 142.148877 109.22642) (xy 142.115614 109.450659) (xy 142.060532 109.670558)
					(xy 141.984162 109.883999) (xy 141.887238 110.088926) (xy 141.770695 110.283367) (xy 141.635654 110.465448)
					(xy 141.483417 110.633417) (xy 141.315448 110.785654) (xy 141.133367 110.920695) (xy 140.938926 111.037238)
					(xy 140.733999 111.134162) (xy 140.520558 111.210532) (xy 140.300659 111.265614) (xy 140.07642 111.298877)
					(xy 139.85 111.31) (xy 139.62358 111.298877) (xy 139.399341 111.265614) (xy 139.179442 111.210532)
					(xy 138.966001 111.134162) (xy 138.761074 111.037238) (xy 138.566633 110.920695) (xy 138.384552 110.785654)
					(xy 138.216583 110.633417) (xy 138.064346 110.465448) (xy 137.929305 110.283367) (xy 137.812762 110.088926)
					(xy 137.715838 109.883999) (xy 137.639468 109.670558) (xy 137.584386 109.450659) (xy 137.551123 109.22642)
					(xy 137.54 109) (xy 137.551123 108.77358) (xy 137.584386 108.549341) (xy 137.639468 108.329442)
					(xy 137.715838 108.116001) (xy 137.812762 107.911074) (xy 137.929305 107.716633) (xy 138.064346 107.534552)
					(xy 138.216583 107.366583) (xy 138.384552 107.214346) (xy 138.566633 107.079305) (xy 138.761074 106.962762)
					(xy 138.966001 106.865838) (xy 139.179442 106.789468) (xy 139.399341 106.734386) (xy 139.62358 106.701123)
					(xy 139.85 106.69) (xy 140.07642 106.701123) (xy 140.300659 106.734386) (xy 140.520558 106.789468)
					(xy 140.733999 106.865838) (xy 140.938926 106.962762) (xy 141.133367 107.079305) (xy 141.315448 107.214346)
					(xy 141.483417 107.366583) (xy 141.635654 107.534552) (xy 141.770695 107.716633) (xy 141.887238 107.911074)
					(xy 141.984162 108.116001) (xy 142.060532 108.329442) (xy 142.115614 108.549341) (xy 142.148877 108.77358)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 2.31)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 152.46 109) (xy 152.448877 109.22642) (xy 152.415614 109.450659) (xy 152.360532 109.670558)
					(xy 152.284162 109.883999) (xy 152.187238 110.088926) (xy 152.070695 110.283367) (xy 151.935654 110.465448)
					(xy 151.783417 110.633417) (xy 151.615448 110.785654) (xy 151.433367 110.920695) (xy 151.238926 111.037238)
					(xy 151.033999 111.134162) (xy 150.820558 111.210532) (xy 150.600659 111.265614) (xy 150.37642 111.298877)
					(xy 150.15 111.31) (xy 149.92358 111.298877) (xy 149.699341 111.265614) (xy 149.479442 111.210532)
					(xy 149.266001 111.134162) (xy 149.061074 111.037238) (xy 148.866633 110.920695) (xy 148.684552 110.785654)
					(xy 148.516583 110.633417) (xy 148.364346 110.465448) (xy 148.229305 110.283367) (xy 148.112762 110.088926)
					(xy 148.015838 109.883999) (xy 147.939468 109.670558) (xy 147.884386 109.450659) (xy 147.851123 109.22642)
					(xy 147.84 109) (xy 147.851123 108.77358) (xy 147.884386 108.549341) (xy 147.939468 108.329442)
					(xy 148.015838 108.116001) (xy 148.112762 107.911074) (xy 148.229305 107.716633) (xy 148.364346 107.534552)
					(xy 148.516583 107.366583) (xy 148.684552 107.214346) (xy 148.866633 107.079305) (xy 149.061074 106.962762)
					(xy 149.266001 106.865838) (xy 149.479442 106.789468) (xy 149.699341 106.734386) (xy 149.92358 106.701123)
					(xy 150.15 106.69) (xy 150.37642 106.701123) (xy 150.600659 106.734386) (xy 150.820558 106.789468)
					(xy 151.033999 106.865838) (xy 151.238926 106.962762) (xy 151.433367 107.079305) (xy 151.615448 107.214346)
					(xy 151.783417 107.366583) (xy 151.935654 107.534552) (xy 152.070695 107.716633) (xy 152.187238 107.911074)
					(xy 152.284162 108.116001) (xy 152.360532 108.329442) (xy 152.415614 108.549341) (xy 152.448877 108.77358)
				)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 139.065 104.013)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J2"
			(at 0 -1.998 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Solder Pad Negative Out"
			(at 0 2.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_2.0x2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "PCB_for_aircoils.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 2 "negative_terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
	)
	(gr_rect
		(start 137 102)
		(end 153 113)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "Go Jackets!"
		(at 149.479 106.299 0)
		(layer "B.SilkS")
	)
	(gr_text "BGRG"
		(at 143.256 105.41 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 147.32 105.156 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 140.208 105.156 0)
		(layer "F.SilkS")
	)
	(gr_text "SSDL"
		(at 143.383 103.759 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "negative_terminal")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1)
		)
		(polygon
			(pts
				(xy 137.033 113.03) (xy 152.908 112.903) (xy 152.908 102.108) (xy 137.033 102.108)
			)
		)
	)
)
