(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 94)
    (no_connects 0)
    (area 95.174999 59.614999 179.145001 133.425001)
    (thickness 1.6002)
    (drawings 30)
    (tracks 245)
    (zones 0)
    (modules 43)
    (nets 51)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 1.016)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 0.889)
    (user_trace_width 1.016)
    (trace_clearance 0)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFE7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(1N5819-Pad1)")
  (net 3 "Net-(C5-Pad1)")
  (net 4 "Net-(C7-Pad1)")
  (net 5 "Net-(C8-Pad2)")
  (net 6 "Net-(CT1-Pad1)")
  (net 7 STATUS0)
  (net 8 "Net-(D2-Pad2)")
  (net 9 STATUS1)
  (net 10 "Net-(D3-Pad2)")
  (net 11 STATUS2)
  (net 12 "Net-(D4-Pad2)")
  (net 13 XBEE_TX)
  (net 14 XBEE_RX)
  (net 15 MODE)
  (net 16 STATUS5)
  (net 17 STATUS6)
  (net 18 STATUS7)
  (net 19 "Net-(IC1-Pad12)")
  (net 20 "Net-(IC1-Pad13)")
  (net 21 BALLAST)
  (net 22 CSB)
  (net 23 MOSI)
  (net 24 MISO)
  (net 25 SCK)
  (net 26 "Net-(IC1-Pad21)")
  (net 27 STATUS3)
  (net 28 STATUS4)
  (net 29 "Net-(R1-Pad1)")
  (net 30 "Net-(U2-Pad4)")
  (net 31 "Net-(U2-Pad6)")
  (net 32 "Net-(U2-Pad7)")
  (net 33 "Net-(U2-Pad8)")
  (net 34 "Net-(U2-Pad9)")
  (net 35 "Net-(U2-Pad11)")
  (net 36 "Net-(U2-Pad12)")
  (net 37 "Net-(U2-Pad13)")
  (net 38 "Net-(U2-Pad14)")
  (net 39 "Net-(U2-Pad15)")
  (net 40 "Net-(U2-Pad16)")
  (net 41 "Net-(U2-Pad17)")
  (net 42 "Net-(U2-Pad18)")
  (net 43 "Net-(U2-Pad19)")
  (net 44 "Net-(U2-Pad20)")
  (net 45 3.3V)
  (net 46 "Net-(IC1-Pad11)")
  (net 47 RESET)
  (net 48 "Net-(IC1-Pad4)")
  (net 49 VDD)
  (net 50 "Net-(D1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net 3.3V)
    (add_net BALLAST)
    (add_net CSB)
    (add_net GND)
    (add_net MISO)
    (add_net MODE)
    (add_net MOSI)
    (add_net "Net-(1N5819-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(CT1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad21)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
    (add_net RESET)
    (add_net SCK)
    (add_net STATUS0)
    (add_net STATUS1)
    (add_net STATUS2)
    (add_net STATUS3)
    (add_net STATUS4)
    (add_net STATUS5)
    (add_net STATUS6)
    (add_net STATUS7)
    (add_net VDD)
    (add_net XBEE_RX)
    (add_net XBEE_TX)
  )
  (module payload:MS5607_Module (layer F.Cu) (tedit 5822AAA8)
    (at 151.13 108.204 270)
    (fp_text reference J1 (at -1.27 -7.62 360) (layer F.SilkS))
    (fp_text value MS5607_Module (at 0 -2.54 270) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at -7.62 0 270) (size 1.524 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at -5.08 0 270) (size 1.524 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 3.3V))
    (pad 3 thru_hole oval (at -2.54 0 270) (size 1.524 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 0 270) (size 1.524 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 SCK))
    (pad 5 thru_hole oval (at 2.54 0 270) (size 1.524 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 MOSI))
    (pad 6 thru_hole oval (at 5.08 0 270) (size 1.524 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 MISO))
    (pad 7 thru_hole oval (at 7.62 0 270) (size 1.524 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 CSB))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5821F357)
    (at 174.625 128.905)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5821F339)
    (at 174.625 64.135)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9 90) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5821F31E)
    (at 99.695 64.135)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5821F2F5)
    (at 99.695 128.905)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 5821F3A6)
    (at 124.587 118.7958)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C6 (at 1.651 4.445) (layer F.SilkS))
    (fp_text value "100 uF" (at 1.25 4.4) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 VDD))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm_LongPads (layer F.Cu) (tedit 5820FBB3)
    (at 137.16 86.36)
    (descr "28-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference IC1 (at 3.81 15.748) (layer F.SilkS))
    (fp_text value ATMEGA328-P (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 47 RESET))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 XBEE_TX))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 XBEE_RX))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(IC1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 STATUS7))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 STATUS6))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 3.3V))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C7-Pad1)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C8-Pad2)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(IC1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(IC1-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(IC1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 MODE))
    (pad 15 thru_hole oval (at 7.62 33.02) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 BALLAST))
    (pad 16 thru_hole oval (at 7.62 30.48) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 CSB))
    (pad 17 thru_hole oval (at 7.62 27.94) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 MOSI))
    (pad 18 thru_hole oval (at 7.62 25.4) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 MISO))
    (pad 19 thru_hole oval (at 7.62 22.86) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 SCK))
    (pad 20 thru_hole oval (at 7.62 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 3.3V))
    (pad 21 thru_hole oval (at 7.62 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(IC1-Pad21)"))
    (pad 22 thru_hole oval (at 7.62 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 23 thru_hole oval (at 7.62 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 STATUS0))
    (pad 24 thru_hole oval (at 7.62 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 STATUS1))
    (pad 25 thru_hole oval (at 7.62 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 STATUS2))
    (pad 26 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 STATUS3))
    (pad 27 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 STATUS4))
    (pad 28 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 STATUS5))
    (model Housings_DIP.3dshapes/DIP-28_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 582290BB)
    (at 135.255 129.413)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D1 (at 5.461 -0.127) (layer F.SilkS))
    (fp_text value D (at 4.37134 -3.55854) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254 180) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 -0.00254 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 49 VDD))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 58213B04)
    (at 105.156 117.348 270)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference 1N5819 (at 5.08 2.286 270) (layer F.SilkS))
    (fp_text value D5 (at 4.37134 -3.55854 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254 90) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 -0.00254 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(1N5819-Pad1)"))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58213981)
    (at 111.1504 89.9668)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -3.302 0) (layer F.SilkS))
    (fp_text value CP1 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 45 3.3V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5821397C)
    (at 111.1504 92.1512)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 3.302 0) (layer F.SilkS))
    (fp_text value CP1 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 45 3.3V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5820F78B)
    (at 137.16 81.026 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.254 1.778 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 47 RESET))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 134.5184 100.076 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value CP1 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 45 3.3V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5821F397)
    (at 127 106.68 90)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 22p (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5821F39E)
    (at 127 111.76 90)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value 22p (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C8-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 58229168)
    (at 124.8664 94.107)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C9 (at 5.6388 0.2032) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 4.4) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 3.3V))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 5821F6D2)
    (at 151.13 94.234)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D2 (at 1.27 1.7145) (layer F.SilkS))
    (fp_text value Green (at 1.524 -3.937) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 7 STATUS0))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 5821F69D)
    (at 151.13 87.884)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D3 (at 1.27 1.778) (layer F.SilkS))
    (fp_text value Yellow (at 1.524 -3.937) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 9 STATUS1))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 5821F6C2)
    (at 151.13 81.534)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D4 (at 1.27 1.7145) (layer F.SilkS))
    (fp_text value Red (at 1.524 -3.937) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 11 STATUS2))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Choke_Axial_ThroughHole:Choke_Horizontal_RM25mm (layer F.Cu) (tedit 582290B2)
    (at 102.489 102.9335 90)
    (descr "Choke, Axial, RM 25mm,")
    (tags "Choke, Axial, RM 25mm,")
    (fp_text reference L1 (at 0.5715 0.127 90) (layer F.SilkS))
    (fp_text value "50 uH" (at 0 5.4991 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -12.49934 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(1N5819-Pad1)"))
    (pad 2 thru_hole circle (at 12.50188 0 90) (size 2.30124 2.30124) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C5-Pad1)"))
  )
  (module Choke_Axial_ThroughHole:Choke_Horizontal_RM15mm (layer F.Cu) (tedit 5821F38E)
    (at 121.412 100.838 180)
    (descr "Choke, Axial, 15mm")
    (tags "Choke, Axial, 15mm")
    (fp_text reference L2 (at 0.254 -0.127 180) (layer F.SilkS))
    (fp_text value "1 uH" (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -7.50062 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 45 3.3V))
    (pad 2 thru_hole circle (at 7.73938 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C5-Pad1)"))
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Horizontal (layer F.Cu) (tedit 0)
    (at 151.638 124.968 270)
    (descr "TO-220, Neutral, Horizontal,")
    (tags "TO-220, Neutral, Horizontal,")
    (fp_text reference Q1 (at 0 -22.3012 270) (layer F.SilkS))
    (fp_text value Q1 (at -0.29972 3.44932 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(D1-Pad2)"))
    (pad 1 thru_hole oval (at -2.54 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 21 BALLAST))
    (pad 3 thru_hole oval (at 2.54 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 0 -16.764) (size 3.79984 3.79984) (drill 3.79984) (layers *.Cu *.Mask F.SilkS))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 5820FB7B)
    (at 119.38 119.38 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 22k (at 3.81 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 29 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 122.936 113.538 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at 4.05892 -3.50012 90) (layer F.SilkS))
    (fp_text value 36k (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 29 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C5-Pad1)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 582290C7)
    (at 147.955 122.174 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R3 (at 4.318 -0.127 270) (layer F.SilkS))
    (fp_text value 4.7k (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 21 BALLAST))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 58213AB0)
    (at 156.972 81.534)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R4 (at 4.572 0) (layer F.SilkS))
    (fp_text value 270 (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 "Net-(D4-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 45 3.3V))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 58213AB7)
    (at 156.972 87.884)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R5 (at 4.572 0) (layer F.SilkS))
    (fp_text value 270 (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(D3-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 45 3.3V))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 58213ABB)
    (at 156.972 94.234)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R6 (at 4.572 0) (layer F.SilkS))
    (fp_text value 270 (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 45 3.3V))
  )
  (module Housings_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 5821F38B)
    (at 111.76 106.68)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 3.81 2.54) (layer F.SilkS))
    (fp_text value MC33063A (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 VDD))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(1N5819-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(CT1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(R1-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 VDD))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 VDD))
    (pad 8 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 VDD))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module payload:XBee_S3B (layer F.Cu) (tedit 5822C498)
    (at 121.92 76.2 90)
    (fp_text reference U2 (at -9.271 -13.843 180) (layer F.SilkS))
    (fp_text value XBee_S3B (at 0 -15.24 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -11 -12 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 45 3.3V))
    (pad 2 thru_hole circle (at -11 -10 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 14 XBEE_RX))
    (pad 3 thru_hole circle (at -11 -8 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 13 XBEE_TX))
    (pad 4 thru_hole circle (at -11 -6 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 30 "Net-(U2-Pad4)"))
    (pad 5 thru_hole circle (at -11 -4 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 45 3.3V))
    (pad 6 thru_hole circle (at -11 -2 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 31 "Net-(U2-Pad6)"))
    (pad 7 thru_hole circle (at -11 0 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 32 "Net-(U2-Pad7)"))
    (pad 8 thru_hole circle (at -11 2 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 33 "Net-(U2-Pad8)"))
    (pad 9 thru_hole circle (at -11 4 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 34 "Net-(U2-Pad9)"))
    (pad 10 thru_hole circle (at -11 6 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole circle (at 11 6 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 35 "Net-(U2-Pad11)"))
    (pad 12 thru_hole circle (at 11 4 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 36 "Net-(U2-Pad12)"))
    (pad 13 thru_hole circle (at 11 2 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 37 "Net-(U2-Pad13)"))
    (pad 14 thru_hole circle (at 11 0 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 38 "Net-(U2-Pad14)"))
    (pad 15 thru_hole circle (at 11 -2 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 39 "Net-(U2-Pad15)"))
    (pad 16 thru_hole circle (at 11 -4 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 40 "Net-(U2-Pad16)"))
    (pad 17 thru_hole circle (at 11 -6 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 41 "Net-(U2-Pad17)"))
    (pad 18 thru_hole circle (at 11 -8 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 42 "Net-(U2-Pad18)"))
    (pad 19 thru_hole circle (at 11 -10 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 43 "Net-(U2-Pad19)"))
    (pad 20 thru_hole circle (at 11 -12 90) (size 1.524 1.524) (drill 0.6) (layers *.Cu *.Mask)
      (net 44 "Net-(U2-Pad20)"))
  )
  (module Crystals:Crystal_HC50-U_Vertical (layer F.Cu) (tedit 5820FB99)
    (at 132.08 107.95 270)
    (descr "Crystal, Quarz, HC50/U, vertical, stehend,")
    (tags "Crystal Quarz HC50/U vertical stehend")
    (fp_text reference Y1 (at 0 0 360) (layer F.SilkS))
    (fp_text value Crystal (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole oval (at -2.44094 0 270) (size 1.99898 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C7-Pad1)"))
    (pad 2 thru_hole oval (at 2.44094 0 270) (size 1.99898 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C8-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 5822C475)
    (at 137.16 69.596 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R7 (at 3.81 -0.127 270) (layer F.SilkS))
    (fp_text value 4.7k (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 45 3.3V))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 47 RESET))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 582290D7)
    (at 148.082 103.124 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at -3.556 -0.254 360) (layer F.SilkS))
    (fp_text value CP1 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 45 3.3V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module payload:BACON_LOGO (layer F.Cu) (tedit 58214A16)
    (at 170.18 80.01 270)
    (fp_text reference G*** (at 0.4 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (module Pin_Headers:Pin_Header_Straight_1x07 (layer F.Cu) (tedit 5822C3FF)
    (at 172.974 101.854)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN_01X07 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 RESET))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 MOSI))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 SCK))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 3.3V))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 MISO))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 BALLAST))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x07.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 582290BF)
    (at 143.764 124.079 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R8 (at 3.81 -0.127 180) (layer F.SilkS))
    (fp_text value 4.7K (at 3.81 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 45 3.3V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 MODE))
  )
  (module Connectors_JST:JST_EH_B02B-EH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5822C3F4)
    (at 128.27 127)
    (descr "JST EH series connector, B02B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference P5 (at 1.524 3.683) (layer F.SilkS) hide)
    (fp_text value VALVE (at 0 5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 49 VDD))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 "Net-(D1-Pad2)"))
    (model Connectors_JST.3dshapes/JST_EH_B02B-EH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x10 (layer F.Cu) (tedit 5822C2BB)
    (at 162.814 65.024 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -2.54 360) (layer F.SilkS) hide)
    (fp_text value CONN_01X10 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 STATUS0))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 STATUS1))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 STATUS2))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 STATUS3))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 STATUS4))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 STATUS5))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 STATUS6))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 STATUS7))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 XBEE_TX))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 XBEE_RX))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x10.wrl
      (at (xyz 0 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 582294EF)
    (at 108.204 117.602 270)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference CT1 (at 1.524 -1.778 270) (layer F.SilkS))
    (fp_text value "160 pF" (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(CT1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module payload:XT60 (layer F.Cu) (tedit 5822C42D)
    (at 116.332 126.238)
    (fp_text reference P1 (at -0.2 4.4) (layer F.SilkS) hide)
    (fp_text value BAT_TERMINALS (at -0.4 -3.8) (layer F.Fab) hide)
    (fp_text user - (at -3.556 5.461) (layer F.SilkS))
    (fp_text user + (at 3.556 5.461) (layer F.SilkS))
    (pad 1 thru_hole oval (at -3.6 0) (size 6.3 8.89) (drill 4.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 3.6 0) (size 6.3 8.89) (drill 4.6) (layers *.Cu *.Mask)
      (net 49 VDD))
  )
  (module payload:MAINE_BB_SMALL (layer B.Cu) (tedit 0)
    (at 119.126 75.946 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5822C3E5)
    (at 133.096 120.65 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 MODE))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 0)
    (at 116.9416 94.615)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C5 (at 1.25 -3.8) (layer F.SilkS))
    (fp_text value 22uF (at 1.25 3.8) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text BLST (at 176.657 117.094) (layer F.SilkS))
  (gr_text MISO (at 176.784 114.554) (layer F.SilkS))
  (gr_text 3.3V (at 176.657 112.014) (layer F.SilkS))
  (gr_text SCK (at 176.403 109.474) (layer F.SilkS))
  (gr_text MOSI (at 176.784 106.934) (layer F.SilkS))
  (gr_text RST (at 176.276 104.394) (layer F.SilkS))
  (gr_text GND (at 176.657 101.854) (layer F.SilkS))
  (gr_text S0 (at 162.814 61.849 90) (layer F.SilkS))
  (gr_text S1 (at 160.274 61.849 90) (layer F.SilkS))
  (gr_text S2 (at 157.734 61.849 90) (layer F.SilkS))
  (gr_text S3 (at 155.194 61.849 90) (layer F.SilkS))
  (gr_text S4 (at 152.654 61.849 90) (layer F.SilkS))
  (gr_text S5 (at 150.114 61.849 90) (layer F.SilkS))
  (gr_text S6 (at 147.574 61.849 90) (layer F.SilkS))
  (gr_text S7 (at 145.034 61.849 90) (layer F.SilkS))
  (gr_text "TX\n" (at 142.494 61.849 90) (layer F.SilkS))
  (gr_text RX (at 139.954 61.976 90) (layer F.SilkS))
  (gr_text SIM (at 130.175 119.38 90) (layer F.SilkS))
  (gr_arc (start 97.79 62.23) (end 95.25 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 97.79 130.81) (end 97.79 133.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 176.53 130.81) (end 179.07 130.81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 176.53 62.23) (end 176.53 59.69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.79 59.69) (end 176.53 59.69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.25 130.81) (end 95.25 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.53 133.35) (end 97.79 133.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.07 62.23) (end 179.07 130.81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Nick Levesque\nConrad Ege" (at 164.338 69.596) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 176.53 130.81) (xy 97.79 130.81) (xy 97.79 62.23) (xy 176.53 62.23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.188 113.03) (xy 97.79 113.03) (xy 97.79 92.71) (xy 107.188 92.71)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.746 102.9208) (xy 115.824 102.9208) (xy 115.824 98.8568) (xy 126.746 98.8568)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.746 102.9208) (xy 115.824 102.9208) (xy 115.824 98.8568) (xy 126.746 98.8568)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.188 113.03) (xy 97.79 113.03) (xy 97.79 92.71) (xy 107.188 92.71)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 164.084 79.248) (xy 141.732 79.248) (xy 141.732 72.644) (xy 164.084 72.644)
      )
    )
  )
)
