<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="69" y1="25" x2="37" y2="25" width="0.1524" layer="20"/>
<wire x1="37" y1="25" x2="36" y2="26" width="0.1524" layer="20" curve="-90"/>
<wire x1="36" y1="26" x2="36" y2="37" width="0.1524" layer="20"/>
<wire x1="36" y1="37" x2="35" y2="38" width="0.1524" layer="20" curve="90"/>
<wire x1="35" y1="38" x2="33" y2="38" width="0.1524" layer="20"/>
<wire x1="33" y1="38" x2="32" y2="39" width="0.1524" layer="20" curve="-90"/>
<wire x1="32" y1="39" x2="32" y2="53" width="0.1524" layer="20"/>
<wire x1="32" y1="53" x2="33" y2="54" width="0.1524" layer="20" curve="-90"/>
<wire x1="33" y1="54" x2="73" y2="54" width="0.1524" layer="20"/>
<wire x1="73" y1="54" x2="74" y2="53" width="0.1524" layer="20" curve="-90"/>
<wire x1="74" y1="53" x2="74" y2="39" width="0.1524" layer="20"/>
<wire x1="74" y1="39" x2="73" y2="38" width="0.1524" layer="20" curve="-90"/>
<wire x1="73" y1="38" x2="71" y2="38" width="0.1524" layer="20"/>
<wire x1="71" y1="38" x2="70" y2="37" width="0.1524" layer="20" curve="90"/>
<wire x1="70" y1="37" x2="70" y2="26" width="0.1524" layer="20"/>
<wire x1="70" y1="26" x2="69" y2="25" width="0.1524" layer="20" curve="-90"/>
<text>Extensometer Adapter</text>
<text>Rev 1</text>
</plain>
<libraries>
<library name="Kycon">
<packages>
<package name="K85X-ED-9P">
</package>
<package name="K85X-AD-15S-BRJ">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Kycon" package="K85X-ED-9P" value="K85X-ED-9P"/>
<element name="U$2" library="Kycon" package="K85X-AD-15S-BRJ" value="K85X-AD-15S-BRJ"/>
</elements>
<signals>
<signal name="A">
<contactref element="U$2" pad="P$1"/>
<contactref element="U$1" pad="P$4"/>
</signal>
<signal name="A'">
<contactref element="U$2" pad="P$9"/>
<contactref element="U$1" pad="P$8"/>
</signal>
<signal name="B">
<contactref element="U$2" pad="P$3"/>
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="B'">
<contactref element="U$2" pad="P$11"/>
<contactref element="U$1" pad="P$7"/>
</signal>
<signal name="R">
<contactref element="U$2" pad="P$14"/>
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="R'">
<contactref element="U$2" pad="P$7"/>
<contactref element="U$1" pad="P$6"/>
</signal>
<signal name="+5V">
<contactref element="U$2" pad="P$4"/>
<contactref element="U$1" pad="P$5"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="P$2"/>
<contactref element="U$2" pad="P$16"/>
<contactref element="U$2" pad="P$17"/>
<contactref element="U$1" pad="P$9"/>
<contactref element="U$1" pad="P$11"/>
<contactref element="U$1" pad="P$10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
