(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 25)
    (no_connects 2)
    (area 148 102.25 206.250001 125.000001)
    (thickness 1.6)
    (drawings 9)
    (tracks 99)
    (zones 0)
    (modules 6)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 2.5)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad2)")
  (net 2 "Net-(P1-Pad3)")
  (net 3 "Net-(P3-Pad5)")
  (net 4 "Net-(P3-Pad7)")
  (net 5 /vcc)
  (net 6 /gnd)
  (net 7 "Net-(D1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad7)")
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /gnd)
    (add_net /vcc)
  )
  (module Socket_Strips:Socket_Strip_Straight_2x04_Pitch2.54mm (layer B.Cu) (tedit 5BF1F1D6)
    (at 156 115.08)
    (descr "Through hole straight socket strip, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x04 2.54mm double row")
    (fp_text reference P4 (at -1.2 2.72 180) (layer F.SilkS))
    (fp_text value CONN_02X04 (at -1.27 -9.95) (layer B.Fab))
    (fp_text user %R (at -1.27 2.33) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad3)"))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /gnd))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad2)"))
    (pad 4 thru_hole oval (at -2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /gnd))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(P3-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /gnd))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(P3-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /gnd))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Connect:USB_A (layer F.Cu) (tedit 5BF1E279)
    (at 163.56 107.33)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference P2 (at -5.26 11.97) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 3.84 7.44) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.11 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 /gnd))
    (pad 3 thru_hole circle (at 4.57 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 /vcc))
    (pad 4 thru_hole circle (at 10.16 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 6 /gnd))
    (pad 4 thru_hole circle (at -3.56 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 6 /gnd))
    (model ${KISYS3DMOD}/Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "KiCad Libraries:USB_MOLEX_48037-2200" (layer F.Cu) (tedit 5BF1E27E)
    (at 191.2 113 90)
    (fp_text reference P1 (at 0 -8 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 1.3 90) (layer F.Fab))
    (pad 1 smd rect (at 3.5 -5.35 90) (size 1.2 2) (layers F.Cu F.Paste F.Mask)
      (net 5 /vcc))
    (pad 2 smd rect (at 1 -5.35 90) (size 1.2 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at -1 -5.35 90) (size 1.2 2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at -3.5 -5.35 90) (size 1.2 2) (layers F.Cu F.Paste F.Mask)
      (net 6 /gnd))
    (pad 4 thru_hole circle (at 5.85 -2.75 90) (size 3.2 3.2) (drill 2.5) (layers *.Cu *.Mask)
      (net 6 /gnd))
    (pad 4 thru_hole circle (at -5.85 -2.75 90) (size 3.2 3.2) (drill 2.5) (layers *.Cu *.Mask)
      (net 6 /gnd))
    (pad "" np_thru_hole circle (at -2.25 -2.75 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.25 -2.75 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_2x04_Pitch2.54mm (layer F.Cu) (tedit 58CD5448)
    (at 178.46 116.54 180)
    (descr "Through hole straight socket strip, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x04 2.54mm double row")
    (fp_text reference P3 (at 2.56 2.24 270) (layer F.SilkS))
    (fp_text value CONN_02X04 (at -1.27 9.95 180) (layer F.Fab))
    (fp_text user %R (at -1.27 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad3)"))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /gnd))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad2)"))
    (pad 4 thru_hole oval (at -2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /gnd))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(P3-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /gnd))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(P3-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /gnd))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Diodes_SMD:D_0603 (layer F.Cu) (tedit 590CE922)
    (at 178 119.2)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D1 (at -2.1 -2 90) (layer F.SilkS))
    (fp_text value LED_Small (at 0 1.4) (layer F.Fab))
    (fp_text user %R (at 0 -1.4) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 /gnd))
    (pad 2 smd rect (at 0.85 0) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 182.15 119.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.15 1.8 270) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 /vcc))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 190.2 119.5) (end 191.2 119.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 190.2 106.5) (end 190.2 105.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 154.8 117.2) (end 154.8 120.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Nick Boers\n2018-11-18" (at 159.6 117.9) (layer F.Cu))
  (gr_text "USB-LOGIC\nINTERROGATOR\nSolution17 2018-11" (at 176.5 115.9) (layer B.SilkS))
  (gr_line (start 151.5 117.2) (end 151.5 105.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190.2 120.5) (end 154.8 120.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.2 106.5) (end 191.2 119.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.5 105.5) (end 190.2 105.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name /gnd) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.75 104.25) (xy 204.75 102.25) (xy 206.25 125) (xy 148 124)
      )
    )
  )
)
