(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.8348)
  )
  (paper "A4")
  (title_block
    (comment 1 "Board keepout approximately 18mil")
    (comment 2 "Board width approximately .4in")
    (comment 3 "Board length approximately 1.0047in")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.1524))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.1524))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad1)")
  (net 2 "Net-(U1-Pad2)")
  (net 3 "3")
  (net 4 "Net-(U1-Pad4)")
  (net 5 "5")
  (net 6 "Net-(U1-Pad6)")
  (net 7 "7")
  (net 8 "Net-(U1-Pad8)")
  (net 9 "Net-(U1-Pad9)")
  (net 10 "11")
  (net 11 "Net-(U1-Pad12)")
  (net 12 "13")
  (net 13 "Net-(U1-Pad14)")
  (net 14 "15")
  (net 15 "Net-(U1-Pad16)")
  (net 16 "Net-(U1-Pad17)")
  (net 17 "18")
  (net 18 "Net-(U1-Pad20)")
  (net 19 "21")
  (net 20 "23")
  (net 21 "GND")
  (net 22 "Net-(U1-Pad10)")
  (net 23 "19")
  (footprint "calorimeter_fp:custom DIP 20" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 147.8 108.2)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (property "Sheetfile" "File: Calorimeter_circuit_designs[1].kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -0.3 -0.15 90) (layer "F.SilkS") hide)
    (fp_text value "DIP20_custom" (at -0.075 -0.075 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at -3.9 8.88) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad1)") (pintype "input"))
    (pad "2" thru_hole oval (at -3.9 6.34) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad2)") (pintype "input"))
    (pad "3" thru_hole oval (at -3.9 3.8) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "3") (pintype "input"))
    (pad "4" thru_hole oval (at -3.9 1.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad4)") (pintype "input"))
    (pad "5" thru_hole oval (at -3.9 -1.28) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "5") (pintype "input"))
    (pad "6" thru_hole oval (at -3.9 -3.82) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad6)") (pintype "input"))
    (pad "7" thru_hole oval (at -3.9 -6.36) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "7") (pintype "input"))
    (pad "8" thru_hole rect (at -3.9 -8.9) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad8)") (pintype "input"))
    (pad "9" thru_hole oval (at 3.72 8.88) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad9)") (pintype "input"))
    (pad "10" thru_hole oval (at 3.72 6.34) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad10)") (pintype "input"))
    (pad "11" thru_hole oval (at 3.72 3.8) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "11") (pintype "input"))
    (pad "12" thru_hole oval (at 3.72 1.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad12)") (pintype "input"))
    (pad "13" thru_hole oval (at 3.72 -1.28) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "13") (pintype "input"))
    (pad "14" thru_hole oval (at 3.72 -3.82) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad14)") (pintype "input"))
    (pad "15" thru_hole oval (at 3.72 -6.36) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "15") (pintype "input"))
    (pad "16" thru_hole oval (at 3.72 -8.9) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad16)") (pintype "input"))
    (pad "17" thru_hole oval (at -3.905 14.0364) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad17)") (pintype "input"))
    (pad "18" thru_hole oval (at -1.365 14.0364) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "18") (pintype "input"))
    (pad "19" thru_hole oval (at 1.175 14.0364) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "19") (pintype "input"))
    (pad "20" thru_hole oval (at 3.715 14.0364) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad20)") (pintype "input"))
    (pad "21" smd rect (at -2.1 0.675) (size 0.87376 0.87376) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "21") (pintype "input"))
    (pad "22" smd rect (at -2.1 -0.7) (size 0.87376 0.87376) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "21") (pintype "input"))
    (pad "23" smd rect (at 1.9 0.675) (size 0.87376 0.87376) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "23") (pintype "input"))
    (pad "24" smd rect (at 1.9 -0.7) (size 0.87376 0.87376) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "23") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm_Socket.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "calorimeter_fp:rb_rotator" (layer "F.Cu")
    (tedit 0)
    (at 147.725 119.65)
    (descr "503320-2560-3")
    (tags "Connector")
    (property "Sheetfile" "File: Calorimeter_circuit_designs[1].kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0.02 2.06) (layer "F.Fab"))
    (fp_text value "rb_rotator" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.75 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(U1-Pad1)") (pintype "input"))
    (pad "2" smd rect (at -3 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(U1-Pad2)") (pintype "input"))
    (pad "3" smd rect (at -2.25 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "3") (pintype "input"))
    (pad "4" smd rect (at -2.5 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(U1-Pad4)") (pintype "input"))
    (pad "5" smd rect (at -1.25 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "5") (pintype "input"))
    (pad "6" smd rect (at -1.5 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(U1-Pad6)") (pintype "input"))
    (pad "7" smd rect (at -0.75 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "7") (pintype "input"))
    (pad "8" smd rect (at -1 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(U1-Pad8)") (pintype "input"))
    (pad "9" smd rect (at 2.75 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(U1-Pad9)") (pintype "input"))
    (pad "10" smd rect (at 3 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(U1-Pad10)") (pintype "input"))
    (pad "11" smd rect (at 2.25 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "11") (pintype "input"))
    (pad "12" smd rect (at 2.5 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(U1-Pad12)") (pintype "input"))
    (pad "13" smd rect (at 1.25 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "13") (pintype "input"))
    (pad "14" smd rect (at 1.5 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(U1-Pad14)") (pintype "input"))
    (pad "15" smd rect (at 0.75 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "15") (pintype "input"))
    (pad "16" smd rect (at 1 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(U1-Pad16)") (pintype "input"))
    (pad "17" smd rect (at -0.25 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(U1-Pad17)") (pintype "input"))
    (pad "18" smd rect (at -0.5 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "18") (pintype "input"))
    (pad "19" smd rect (at 0.5 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "19") (pintype "input"))
    (pad "20" smd rect (at 0.25 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(U1-Pad20)") (pintype "input"))
    (pad "21" smd rect (at -1.75 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "21") (pintype "input"))
    (pad "22" smd rect (at -2 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "21") (pintype "input"))
    (pad "23" smd rect (at 1.75 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "23") (pintype "input"))
    (pad "24" smd rect (at 2 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "23") (pintype "input"))
    (pad "25" smd rect (at 0 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "GND") (pintype "input"))
    (pad "MP1" smd rect (at 3.67 0.9) (size 0.4 0.95) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "MP2" smd rect (at -3.67 0.9) (size 0.4 0.95) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "503320-2560.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 142.64 97.98062) (end 152.8 123.5) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "11" (at 150.4 112) (layer "B.SilkS"))
  (gr_text "13" (at 150.375 106.925) (layer "B.SilkS"))
  (gr_text "SH" (at 145.7 106.675) (layer "B.SilkS"))
  (gr_text "18" (at 145.475 123.1) (layer "B.SilkS"))
  (gr_text "7" (at 145.025 101.825) (layer "B.SilkS"))
  (gr_text "9" (at 150.4 117.125) (layer "B.SilkS"))
  (gr_text "12" (at 150.375 109.45) (layer "B.SilkS"))
  (gr_text "6" (at 145.025 104.375) (layer "B.SilkS"))
  (gr_text "17" (at 144.85 123.1) (layer "B.SilkS"))
  (gr_text "20" (at 150.55 123.1) (layer "B.SilkS"))
  (gr_text "1" (at 145 117.125) (layer "B.SilkS"))
  (gr_text "8" (at 145.025 99.3) (layer "B.SilkS"))
  (gr_text "15" (at 150.375 101.825) (layer "B.SilkS"))
  (gr_text "14" (at 150.375 104.375) (layer "B.SilkS"))
  (gr_text "GND" (at 147.725 102.85) (layer "B.SilkS"))
  (gr_text "3" (at 145 112.025) (layer "B.SilkS"))
  (gr_text "10" (at 150.4 114.525) (layer "B.SilkS"))
  (gr_text "19" (at 149.925 123.1) (layer "B.SilkS"))
  (gr_text "16" (at 150.375 99.275) (layer "B.SilkS"))
  (gr_text "5" (at 145.025 106.9) (layer "B.SilkS"))
  (gr_text "4" (at 145.025 109.45) (layer "B.SilkS"))
  (gr_text "SH" (at 149.7 106.675) (layer "B.SilkS"))
  (gr_text "2" (at 145 114.575) (layer "B.SilkS"))
  (gr_text "13" (at 150.375 106.925) (layer "F.SilkS"))
  (gr_text "18" (at 145.475 123.1) (layer "F.SilkS"))
  (gr_text "15" (at 148.475 117.875) (layer "F.SilkS"))
  (gr_text "8" (at 145.025 99.3) (layer "F.SilkS"))
  (gr_text "25" (at 147.725 120.225) (layer "F.SilkS"))
  (gr_text "23" (at 149.475 117.875) (layer "F.SilkS"))
  (gr_text "4" (at 145.025 109.45) (layer "F.SilkS"))
  (gr_text "10" (at 150.4 114.525) (layer "F.SilkS"))
  (gr_text "21" (at 145.725 120.2) (layer "F.SilkS"))
  (gr_text "5" (at 146.475 117.875) (layer "F.SilkS"))
  (gr_text "GND" (at 147.725 102.85) (layer "F.SilkS"))
  (gr_text "20" (at 150.55 123.1) (layer "F.SilkS"))
  (gr_text "9" (at 150.4 117.125) (layer "F.SilkS"))
  (gr_text "12" (at 150.375 109.45) (layer "F.SilkS"))
  (gr_text "14" (at 150.375 104.375) (layer "F.SilkS"))
  (gr_text "13" (at 148.975 117.875) (layer "F.SilkS"))
  (gr_text "18" (at 147.225 121.35) (layer "F.SilkS"))
  (gr_text "24" (at 149.725 120.225) (layer "F.SilkS"))
  (gr_text "7" (at 146.975 117.875) (layer "F.SilkS"))
  (gr_text "1" (at 145 117.125) (layer "F.SilkS"))
  (gr_text "19" (at 149.925 123.1) (layer "F.SilkS"))
  (gr_text "8" (at 146.725 120.2) (layer "F.SilkS"))
  (gr_text "5" (at 145.025 106.9) (layer "F.SilkS"))
  (gr_text "16" (at 150.375 99.275) (layer "F.SilkS"))
  (gr_text "4" (at 145.225 120.2) (layer "F.SilkS"))
  (gr_text "9" (at 150.475 117.875) (layer "F.SilkS"))
  (gr_text "15" (at 150.375 101.825) (layer "F.SilkS"))
  (gr_text "11" (at 150.4 112) (layer "F.SilkS"))
  (gr_text "6" (at 146.225 120.2) (layer "F.SilkS"))
  (gr_text "3" (at 145.475 117.875) (layer "F.SilkS"))
  (gr_text "19" (at 148.25 121.35) (layer "F.SilkS"))
  (gr_text "17" (at 144.85 123.1) (layer "F.SilkS"))
  (gr_text "20" (at 147.975 117.875) (layer "F.SilkS"))
  (gr_text "1" (at 144.975 117.875) (layer "F.SilkS"))
  (gr_text "21" (at 145.975 117.875) (layer "F.SilkS"))
  (gr_text "12" (at 150.225 120.225) (layer "F.SilkS"))
  (gr_text "10" (at 150.725 120.225) (layer "F.SilkS"))
  (gr_text "3" (at 145 112.025) (layer "F.SilkS"))
  (gr_text "16" (at 148.725 120.225) (layer "F.SilkS"))
  (gr_text "14" (at 149.225 120.225) (layer "F.SilkS"))
  (gr_text "6" (at 145.025 104.375) (layer "F.SilkS"))
  (gr_text "11" (at 149.975 117.875) (layer "F.SilkS"))
  (gr_text "2" (at 145 114.575) (layer "F.SilkS"))
  (gr_text "2" (at 144.725 120.2) (layer "F.SilkS"))
  (gr_text "7" (at 145.025 101.825) (layer "F.SilkS"))
  (gr_text "17" (at 147.475 117.875) (layer "F.SilkS"))
)
