(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 0)
    (no_connects 0)
    (area 115.99522 73.0726 143.204781 89.9274)
    (thickness 1.6)
    (drawings 4)
    (tracks 111)
    (zones 0)
    (modules 2)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.01)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.73 0.3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 126.825 83.175)
    (grid_origin 126.825 83.175)
    (visible_elements 7FFCD609)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (module Housings_DFN_QFN:QFN-20-1EP_5x5mm_Pitch0.65mm (layer F.Cu) (tedit 5AD845BC)
    (at 130 80)
    (descr "20-Lead Plastic Quad Flat, No Lead Package (MQ) - 5x5x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.65")
    (attr smd)
    (fp_text reference REF** (at -2 -6) (layer F.SilkS) hide)
    (fp_text value QFN-20-1EP_5x5mm_Pitch0.65mm (at -0.4 8.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.25 -1.3) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.25 -0.65) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -2.25 0) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -2.25 0.65) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.25 1.3) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -1.3 2.25 90) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -0.65 2.25 90) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 0 2.25 90) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 0.65 2.25 90) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 1.3 2.25 90) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 2.25 1.3) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 2.25 0.65) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 2.25 0) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 2.25 -0.65) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 2.25 -1.3) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 1.3 -2.25 90) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 0.65 -2.25 90) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 0 -2.25 90) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at -0.65 -2.25 90) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at -1.3 -2.25 90) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 0 0) (size 1.675 1.675) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-20-1EP_5x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-20-1EP_4x4mm_Pitch0.5mm (layer B.Cu) (tedit 5AD845C7)
    (at 130 80 270)
    (descr "20-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference REF** (at -6 -3.8 360) (layer B.SilkS) hide)
    (fp_text value QFN-20-1EP_4x4mm_Pitch0.5mm (at 6.8 0 360) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.965 1 270) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -1.965 0.5 270) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -1.965 0 270) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -1.965 -0.5 270) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -1.965 -1 270) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -1 -1.965 180) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -0.5 -1.965 180) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 0 -1.965 180) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 0.5 -1.965 180) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at 1 -1.965 180) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at 1.965 -1 270) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at 1.965 -0.5 270) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at 1.965 0 270) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd rect (at 1.965 0.5 270) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at 1.965 1 270) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 16 smd rect (at 1 1.965 180) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 17 smd rect (at 0.5 1.965 180) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 18 smd rect (at 0 1.965 180) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 19 smd rect (at -0.5 1.965 180) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd rect (at -1 1.965 180) (size 0.73 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 21 smd rect (at 0 0 270) (size 1.25 1.25) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
  )
  (gr_line (start 126.825 83.175) (end 126.825 76.825) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 133.17754 83.175) (end 126.825 83.175) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 133.17754 76.825) (end 133.17754 83.175) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 126.825 76.825) (end 133.17754 76.825) (layer Edge.Cuts) (width 0.01))
)
