(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 146.25 103.96 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 148.2 108.535 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 148.2 99.395 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 144.3 87.98 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 146.25 92.535 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 146.25 94.82 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 148.2 90.255 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 146.25 87.965 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 146.25 85.68 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 146.25 101.675 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 146.25 108.53)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 144.3 90.265 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 148.2 92.54 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 148.2 85.685 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 146.25 99.39 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 142.425 85.675)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "PinHeader_1x10_P2.54mm_Vertical" (at 0 25.19) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 11.43 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 144.3 106.26 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 144.3 97.12 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 146.25 90.25 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 146.25 97.105 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 146.25 106.245 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 148.2 106.25 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 144.3 103.975 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 148.2 103.965 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 150.05 85.7)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "PinHeader_1x10_P2.54mm_Vertical" (at 0 25.19) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 11.43 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 144.3 99.405 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 144.3 108.545)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 144.3 94.835 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 144.3 92.55 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 148.2 97.11 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 144.3 101.69 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 144.3 85.695 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 148.2 87.97 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 148.2 94.825 90)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75 90) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 90) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6812_EC15_1.5x1.5mm" (layer "F.Cu")
    (tedit 5DA624A9)
    (at 148.2 101.68 180)
    (descr "http://www.newstar-ledstrip.com/product/20181119172602110.pdf")
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.75) (layer "F.SilkS") hide)
    (fp_text value "LED_SK6812_EC15_1.5x1.5mm" (at 0 1.75) (layer "F.Fab") hide)
    (pad "D" smd rect (at -0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "G" smd rect (at 0.45 -0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "O" smd rect (at 0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "V" smd rect (at -0.45 0.45 180) (size 0.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812_EC15_1.5x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 146.3 106.6 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 1.43 -270) (layer "B.SilkS") hide)
    (fp_text value "C_0603_1608Metric" (at 0 -1.43 -270) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 5.7 0.025 -270) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 141.55 110.1) (mid 141.408579 110.041421) (end 141.35 109.9) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 141.55 110.1) (end 150.925 110.1) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 141.35 84.35) (mid 141.408579 84.208579) (end 141.55 84.15) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 151.125 109.9) (mid 151.066421 110.041421) (end 150.925 110.1) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 141.35 84.35) (end 141.35 109.9) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 150.925 84.15) (mid 151.066421 84.208579) (end 151.125 84.35) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 151.125 109.9) (end 151.125 84.35) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 150.925 84.15) (end 141.55 84.15) (layer "Edge.Cuts") (width 0.1))
  (gr_text "DI" (at 142.325 109.75) (layer "B.SilkS"))
  (gr_text "GND" (at 144 97.8 -90) (layer "B.SilkS"))
  (gr_text "DO" (at 150.05 86.85) (layer "B.SilkS"))
  (gr_text "POS" (at 148.5 99.7 90) (layer "B.SilkS"))
)
