(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 4)
    (no_connects 0)
    (area 133.274999 100.254999 150.570001 114.375001)
    (thickness 1.6)
    (drawings 13)
    (tracks 8)
    (zones 0)
    (modules 3)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(P1-Pad3)")
  (net 4 "Net-(P1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class thic ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5B089B6E)
    (at 148.336 102.616)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference "" (at 0 -2.33) (layer F.SilkS))
    (fp_text value "" (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_FFC-FPC:TE_84952-4_1x04-1MP_P1.0mm_Horizontal (layer F.Cu) (tedit 5B089B7E)
    (at 140.97 107.315 270)
    (descr "TE FPC connector, 04 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4")
    (tags "te fpc 84952")
    (attr smd)
    (fp_text reference "" (at 0 -4 270) (layer F.SilkS))
    (fp_text value "" (at 0 7.7 270) (layer F.Fab))
    (fp_text user "" (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -1.8 270) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at -0.5 -1.8 270) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at 0.5 -1.8 270) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at 1.5 -1.8 270) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(P1-Pad4)"))
    (pad MP smd rect (at -4.49 1 270) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
    (pad MP smd rect (at 4.49 1 270) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/TE_84952-4_1x04-1MP_P1.0mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cutekicad:cutelab_1cm (layer B.Cu) (tedit 5B07AD3E)
    (at 140.462 105.918 180)
    (descr "Imported from cutelab_inverti_path.svg")
    (tags svg2mod)
    (attr smd)
    (fp_text reference svg2mod (at 0 7.477367 180) (layer B.SilkS) hide)
    (fp_text value G*** (at 0 -7.477367 180) (layer B.SilkS) hide)
  )
  (gr_text "IKA pad\nHX711 Ribbon 1.0" (at 135.128 112.268) (layer B.SilkS))
  (gr_arc (start 134.62 113.03) (end 134.62 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 134.62 101.6) (end 133.35 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 149.225 113.03) (end 150.495 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 149.225 101.6) (end 149.225 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.35 113.03) (end 133.35 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.225 114.3) (end 134.62 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.495 101.6) (end 150.495 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 100.33) (end 149.225 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text A+ (at 145.4785 110.1725) (layer F.SilkS))
  (gr_text "A-\n" (at 145.4785 107.6325) (layer F.SilkS))
  (gr_text E- (at 145.415 105.0925) (layer F.SilkS))
  (gr_text "E+\n" (at 145.415 102.5525) (layer F.SilkS))
)
