(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 32)
    (tracks 211)
    (zones 0)
    (modules 29)
    (nets 38)
  )
  (page A4)
  (title_block
    (title "DMX Demonstrator - DMX-512 IO Module (DMX-IO1)")
    (date 2023-12-19)
    (rev 1.6)
    (company "Sparky Bobo Designs")
    (comment 2 "Designed by: SparkyBobo")
    (comment 3 https://creativecommons.org/licenses/by-sa/4.0/)
    (comment 4 "Released under the Creative Commons Attribution Share-Alike 4.0m License")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "grb"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 GNDD)
  (net 4 "Net-(J2-Pad2A)")
  (net 5 "Net-(J2-Pad3)")
  (net 6 "Net-(J3-Pad4B)")
  (net 7 "Net-(J3-Pad5B)")
  (net 8 "Net-(J2-Pad4B)")
  (net 9 "Net-(J2-Pad5B)")
  (net 10 VDD)
  (net 11 "Net-(U4-Pad1)")
  (net 12 "Net-(U4-Pad7)")
  (net 13 "Net-(U4-Pad4)")
  (net 14 "Net-(U3-Pad4)")
  (net 15 "Net-(U3-Pad7)")
  (net 16 "Net-(U3-Pad1)")
  (net 17 "Net-(U2-Pad1)")
  (net 18 "Net-(U2-Pad7)")
  (net 19 "Net-(U2-Pad4)")
  (net 20 "Net-(R6-Pad1)")
  (net 21 "Net-(R4-Pad1)")
  (net 22 "Net-(J1-Pad12)")
  (net 23 "Net-(R3-Pad2)")
  (net 24 "Net-(J1-Pad3)")
  (net 25 "Net-(J1-Pad4)")
  (net 26 "Net-(J1-Pad5)")
  (net 27 "Net-(J1-Pad6)")
  (net 28 "Net-(J1-Pad7)")
  (net 29 "Net-(J1-Pad8)")
  (net 30 /DMX-RX)
  (net 31 /DMX-DIR)
  (net 32 /DMX-TX)
  (net 33 "Net-(JP3-Pad2)")
  (net 34 "Net-(JP2-Pad2)")
  (net 35 "Net-(JP1-Pad2)")
  (net 36 "Net-(R1-Pad2)")
  (net 37 "Net-(SW1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net /DMX-DIR)
    (add_net /DMX-RX)
    (add_net /DMX-TX)
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad2A)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4B)")
    (add_net "Net-(J2-Pad5B)")
    (add_net "Net-(J3-Pad4B)")
    (add_net "Net-(J3-Pad5B)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(JP3-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad7)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 1.27)
    (via_drill 0.635)
    (uvia_dia 1.27)
    (uvia_drill 0.635)
    (diff_pair_width 0.3048)
    (diff_pair_gap 0.3048)
    (add_net +5V)
    (add_net GND)
    (add_net GNDD)
    (add_net VDD)
  )
  (module footprints:Converter_DCDC_Recom_RFM0505S_THT_Bypass (layer F.Cu) (tedit 6625C79A)
    (at 116.459 104.394 180)
    (descr "Recom RFB0505S footprint based on SIP7, https://recom-power.com/pdf/Econoline/RFB.pdf")
    (tags "Recom RFB0505S DCDC-Converter")
    (fp_text reference U1 (at -3 -3) (layer F.SilkS))
    (fp_text value RFM-0505S (at -1 19) (layer F.Fab))
    (fp_text user %R (at -2.25 6 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 GNDD))
    (pad 4 thru_hole circle (at -3.54 5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 VDD))
    (pad 1 thru_hole circle (at -3.54 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 VDD))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_muRata_NMAxxxxSC_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 144.526 79.375 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -2.2225 0 90) (layer F.SilkS))
    (fp_text value 120 (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2A)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:ESWITCH_1218_SPDT (layer F.Cu) (tedit 661C9A2B)
    (at 171.577 82.042 180)
    (descr "Breadboard-friendly SPDT Slide Switch")
    (tags "EG1218 SPDT Slide Switch")
    (fp_text reference SW1 (at 0.127 -2.2225 180) (layer F.SilkS))
    (fp_text value TERM (at 0 10.16) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(SW1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5A3EABFC)
    (at 168.26 91.313)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0.015 1.905) (layer F.SilkS))
    (fp_text value "Bypass Iso" (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 30 /DMX-RX))
    (pad 2 smd rect (at 0.65 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 35 "Net-(JP1-Pad2)"))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5A3EABFC)
    (at 155.336 91.313 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 -1.8 180) (layer F.SilkS))
    (fp_text value "Bypass Iso" (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 31 /DMX-DIR))
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 34 "Net-(JP2-Pad2)"))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5A3EABFC)
    (at 142.352 91.313 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP3 (at 0 -1.8 180) (layer F.SilkS))
    (fp_text value "Bypass Iso" (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 32 /DMX-TX))
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 33 "Net-(JP3-Pad2)"))
  )
  (module footprints:NEUTRIK-NC3MAH-NC5MAH (layer F.Cu) (tedit 661C9E3B)
    (at 156.070793 66.11216)
    (fp_text reference J3 (at 0 1.19784) (layer F.SilkS))
    (fp_text value NC3MAH/NC5MAH (at 0 -0.5) (layer F.Fab))
    (fp_text user "23mm on center" (at 0 -1.85) (layer Dwgs.User))
    (pad 1A thru_hole oval (at 3.81 17.78) (size 2.8 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 GNDD))
    (pad 2A thru_hole oval (at -3.81 17.78) (size 2.8 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2A)"))
    (pad 0 thru_hole circle (at 0 12.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.81 8.89) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 3.81) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad 5B thru_hole oval (at -6.98 17.78) (size 2.8 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad5B)"))
    (pad 4B thru_hole circle (at -3.81 12.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad4B)"))
    (pad 3 thru_hole circle (at 0 17.78) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 2B thru_hole circle (at 3.81 12.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2A)"))
    (pad 1B thru_hole oval (at 6.98 17.78) (size 2.8 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 GNDD))
  )
  (module Capacitor_THT:C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02 (layer F.Cu) (tedit 5AE50EF0)
    (at 161.798 96.52 90)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (fp_text reference C2 (at 4.7625 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02 (layer F.Cu) (tedit 5AE50EF0)
    (at 148.844 99.06 90)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (fp_text reference C3 (at 4.7625 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 GNDD))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 VDD))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02 (layer F.Cu) (tedit 5AE50EF0)
    (at 135.8265 99.06 90)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (fp_text reference C4 (at 4.7625 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 GNDD))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 VDD))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02 (layer F.Cu) (tedit 5AE50EF0)
    (at 122.809 99.06 90)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (fp_text reference C5 (at 4.7625 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 GNDD))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 VDD))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:NEUTRIK-NC3FAH-NC5FAH (layer F.Cu) (tedit 661C9E87)
    (at 132.702793 66.11216)
    (fp_text reference J2 (at 0 1.07084) (layer F.SilkS))
    (fp_text value NC3FAH/NC5FAH (at 0 -0.5) (layer F.Fab))
    (fp_text user "23mm on center" (at 0 -1.9) (layer Dwgs.User))
    (pad 2A thru_hole circle (at 3.81 13.335) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2A)"))
    (pad 1A thru_hole circle (at -3.81 12.7) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 GNDD))
    (pad 0 thru_hole circle (at -8.25 6.98) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.81 8.89) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 3.81) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad 5B thru_hole circle (at 3.81 17.15) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad5B)"))
    (pad 4B thru_hole circle (at 6.98 13.34) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad4B)"))
    (pad 3 thru_hole circle (at 0 17.15) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 2B thru_hole circle (at 0 13.4) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2A)"))
    (pad 1B thru_hole circle (at -3.81 17.15) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 GNDD))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 118.745 64.77)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 170.053 64.77)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 118.618 116.586)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 170.053 116.586)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connector_IDC:IDC-Header_2x07_P2.54mm_Horizontal (layer F.Cu) (tedit 5EAC9A08)
    (at 152.019 104.394 270)
    (descr "Through hole IDC box header, 2x07, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole horizontal IDC box header THT 2x07 2.54mm double row")
    (fp_text reference J1 (at -0.508 -2.413) (layer F.SilkS))
    (fp_text value "IO EXTENSION" (at 6.105 21.844 270) (layer F.Fab))
    (fp_text user %R (at 8.805 7.62) (layer F.Fab))
    (pad 14 thru_hole circle (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole circle (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad12)"))
    (pad 10 thru_hole circle (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /DMX-DIR))
    (pad 8 thru_hole circle (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad8)"))
    (pad 6 thru_hole circle (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad6)"))
    (pad 4 thru_hole circle (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad4)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 13 thru_hole circle (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole circle (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /DMX-TX))
    (pad 9 thru_hole circle (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /DMX-RX))
    (pad 7 thru_hole circle (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad7)"))
    (pad 5 thru_hole circle (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad5)"))
    (pad 3 thru_hole circle (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad3)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235294118)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x07_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm_Socket (layer F.Cu) (tedit 5A02E8C5)
    (at 146.177 99.06 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U4 (at 0 -2.413) (layer F.SilkS))
    (fp_text value 6N137 (at 3.81 9.95 180) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 180) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 VDD))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(U4-Pad4)"))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(U4-Pad7)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R6-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(JP3-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 5 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GNDD))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(U4-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 159.512 104.267 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 12.446 0 270) (layer F.SilkS))
    (fp_text value 470 (at 5.08 -0.635 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /DMX-TX))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm_Socket (layer F.Cu) (tedit 5A02E8C5)
    (at 133.096 99.06 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U5 (at 0 -2.413 180) (layer F.SilkS))
    (fp_text value MAX485 (at 3.81 9.95 180) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 180) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 VDD))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(JP3-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2A)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(JP2-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(JP2-Pad2)"))
    (pad 5 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GNDD))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(JP1-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm_Socket (layer F.Cu) (tedit 5A02E8C5)
    (at 172.085 99.06 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U2 (at 0 -2.413) (layer F.SilkS))
    (fp_text value 6N137 (at 3.81 9.95 180) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 180) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(U2-Pad4)"))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(U2-Pad7)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R3-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /DMX-RX))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 VDD))
    (pad 5 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U2-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm_Socket (layer F.Cu) (tedit 5A02E8C5)
    (at 159.131 99.06 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U3 (at 0 -2.413) (layer F.SilkS))
    (fp_text value 6N137 (at 3.81 9.95 180) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 180) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 VDD))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(U3-Pad4)"))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U3-Pad7)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R4-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(JP2-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 5 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GNDD))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(U3-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 156.6545 87.757)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at -1.905 0 90) (layer F.SilkS))
    (fp_text value 470 (at 5.08 -0.508) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /DMX-RX))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 165.608 104.267 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 12.319 0 270) (layer F.SilkS))
    (fp_text value 470 (at 5.08 0.635 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(JP1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 162.56 104.267 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 12.446 0 270) (layer F.SilkS))
    (fp_text value 470 (at 5.08 0.635 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /DMX-DIR))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 152.5905 87.757 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 12.065 0 270) (layer F.SilkS))
    (fp_text value 470 (at 5.08 0.635 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 VDD))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(JP2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:OSHW-LOGO-S locked (layer F.Cu) (tedit 200000)
    (at 127.381 116.332)
    (descr "OPEN-SOURCE HARDWARE (OSHW) LOGO - SMALL - SILKSCREEN")
    (tags "OPEN-SOURCE HARDWARE (OSHW) LOGO - SMALL - SILKSCREEN")
    (attr virtual)
    (fp_text reference "" (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 0) (layer F.SilkS))
  )
  (module footprints:logo_cr_5x5 locked (layer B.Cu) (tedit 0)
    (at 133.858 116.586 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 138.557 87.757 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 12.065 0 270) (layer F.SilkS))
    (fp_text value 470 (at 5.08 -0.508 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 VDD))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(JP3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 120 (at 144.5895 74.295 90) (layer F.SilkS))
  (gr_text On (at 171.6405 72.3265 90) (layer F.SilkS))
  (gr_text Off (at 171.6405 86.868 90) (layer F.SilkS))
  (gr_text 470 (at 165.5445 109.4105 90) (layer F.SilkS))
  (gr_text 470 (at 162.4965 109.4105 90) (layer F.SilkS))
  (gr_text 470 (at 159.4485 109.4105 90) (layer F.SilkS))
  (gr_text 470 (at 161.798 87.884) (layer F.SilkS))
  (gr_text 470 (at 147.574 87.884) (layer F.SilkS))
  (gr_text 470 (at 133.5405 87.884) (layer F.SilkS))
  (gr_text "RFB\n0505S" (at 119.38 96.8375) (layer F.SilkS))
  (gr_text 6N137 (at 168.275 96.52 90) (layer F.SilkS))
  (gr_text 6N137 (at 155.321 96.52 90) (layer F.SilkS))
  (gr_text 6N137 (at 142.367 96.52 90) (layer F.SilkS))
  (gr_text MAX485E (at 129.159 94.869 90) (layer F.SilkS))
  (gr_text 1 (at 118.745 101.9175) (layer F.SilkS))
  (gr_text 4 (at 118.745 99.3775) (layer F.SilkS))
  (gr_text 3 (at 117.729 99.3775) (layer F.SilkS))
  (gr_text 2 (at 117.729 101.854) (layer F.SilkS))
  (gr_text Termination (at 168.2115 79.5655 90) (layer F.SilkS))
  (gr_arc (start 173.609 61.397) (end 174.427 61.397) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.609 119.761) (end 173.609 120.579) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 115.189 119.817) (end 114.427 119.817) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 115.189 61.341) (end 115.189 60.579) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.427 119.817) (end 114.427 61.341) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.189 120.579) (end 173.609 120.579) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.427 61.397) (end 174.427 119.761) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.189 60.579) (end 173.609 60.579) (layer Edge.Cuts) (width 0.15))
  (gr_text "DMX-IO1, Rev 1.6\nSparky Bobo Designs" (at 144.399 117.221) (layer B.SilkS))
  (gr_text DMX-IO1 (at 127.127 119.253) (layer F.SilkS))
  (gr_text "IO EXPANSION" (at 144.018 119.253) (layer F.SilkS))
  (zone (net 3) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.33925 110.4265) (xy 164.49675 110.4265) (xy 164.49675 101.6) (xy 168.62425 101.6) (xy 168.529 86.2965)
        (xy 155.067 86.2965) (xy 155.067 100.33) (xy 147.828 100.33) (xy 147.828 90.043) (xy 142.113 90.043)
        (xy 142.113 100.33) (xy 134.747 100.33) (xy 129.032 100.33) (xy 114.554 100.33) (xy 114.554 61.214)
        (xy 115.062 60.706) (xy 173.736 60.706) (xy 174.244 61.087)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.33925 110.998) (xy 163.98875 110.998) (xy 163.8935 101.092) (xy 168.021 101.092) (xy 168.021 86.8045)
        (xy 155.575 86.8045) (xy 155.575 100.838) (xy 147.32 100.838) (xy 147.32 90.551) (xy 142.621 90.551)
        (xy 142.621 100.838) (xy 134.239 100.838) (xy 129.54 100.838) (xy 114.554 100.838) (xy 114.554 120.015)
        (xy 114.935 120.396) (xy 173.863 120.396) (xy 174.244 120.015)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.33925 110.998) (xy 163.98875 110.998) (xy 163.8935 101.092) (xy 168.021 101.092) (xy 168.021 86.8045)
        (xy 155.575 86.8045) (xy 155.575 100.838) (xy 147.32 100.838) (xy 147.32 90.551) (xy 142.621 90.551)
        (xy 142.621 100.838) (xy 134.239 100.838) (xy 129.54 100.838) (xy 114.554 100.838) (xy 114.554 120.015)
        (xy 114.935 120.396) (xy 173.863 120.396) (xy 174.244 120.015)
      )
    )
  )
  (zone (net 10) (net_name VDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.33925 110.4265) (xy 164.49675 110.4265) (xy 164.49675 101.6) (xy 168.62425 101.6) (xy 168.529 86.2965)
        (xy 155.067 86.2965) (xy 155.067 100.203) (xy 147.828 100.203) (xy 147.828 90.043) (xy 142.113 90.043)
        (xy 142.113 100.203) (xy 134.747 100.203) (xy 129.032 100.33) (xy 114.554 100.33) (xy 114.554 61.214)
        (xy 115.062 60.706) (xy 173.736 60.706) (xy 174.244 61.087)
      )
    )
  )
)
