(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~84~ubuntu18.04.1)
  (general
    (thickness 0.8)
    (drawings 10)
    (tracks 137)
    (zones 0)
    (modules 24)
    (nets 15)
  )
  (page A4)
  (title_block
    (title ProMicro_Boost)
    (date 2020-02-07)
    (rev v1.3)
    (company https://twitter.com/nerdyscout84)
    (comment 1 "CERN Open Hardware Licence v1.2")
    (comment 2 http://github.com/nerdyscout/ProMicro_Boost)
  )
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.15)
    (zone_45_only yes)
    (trace_min 0.1)
    (via_size 0.5)
    (via_drill 0.2)
    (via_min_size 0.45)
    (via_min_drill 0.2)
    (user_via 0.45 0.2)
    (user_via 0.5 0.2)
    (user_via 0.6 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.9 0.9)
    (mod_text_width 0.15)
    (pad_size 2.7 2.7)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 127 99.695)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x3d3ff_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(L1-Pad2)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(R3-Pad2)")
  (net 5 "Net-(R5-Pad2)")
  (net 6 /BAT)
  (net 7 +5V)
  (net 8 VBUS)
  (net 9 D4)
  (net 10 "Net-(R7-Pad2)")
  (net 11 "Net-(JP2-Pad1)")
  (net 12 +3V3)
  (net 13 /PowerBoost/LBO)
  (net 14 /PowerBoost/EN)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.5)
    (via_drill 0.2)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /BAT)
    (add_net /PowerBoost/EN)
    (add_net /PowerBoost/LBO)
    (add_net D4)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net VBUS)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class small ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.2)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class tiny ""
    (clearance 0.1)
    (trace_width 0.1)
    (via_dia 0.45)
    (via_drill 0.2)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Symbol:OSHW-Logo2_9.8x8mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 133.35 85.725 270)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference LOGO1 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value Logo_Open_Hardware_Small (at 0.75 0 90) (layer B.Fab) hide)
  )
  (module Module:Sparkfun_Pro_Micro (layer B.Cu) (tedit 5D5AC4F8)
    (at 127 99.695)
    (descr "Sparkfun Pro Micro, https://www.sparkfun.com/products/12587")
    (tags "Sparkfun Pro Micro")
    (fp_text reference A1 (at 2.54 0 90) (layer B.SilkS) hide)
    (fp_text value Sparkfun_Pro_Micro_3V3 (at 8.89 -13.97 -90) (layer B.Fab))
    (fp_text user %R (at 6.096 -13.97 -90) (layer B.Fab))
    (pad 24 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 VBUS))
    (pad 23 thru_hole oval (at 15.24 -2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 22 thru_hole oval (at 15.24 -5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 -27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 15.24 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 +3V3))
    (pad 11 thru_hole oval (at 0 -25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 15.24 -10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 -22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 15.24 -12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 -20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 15.24 -15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 15.24 -17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 D4))
    (pad 16 thru_hole oval (at 15.24 -20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 15.24 -22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 15.24 -25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 15.24 -27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Module.3dshapes/Sparkfun_Pro_Micro.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391EB7)
    (at 129.54 93.345 270)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value SolderJumper_3_Open (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 9 D4))
    (pad 3 smd custom (at 1.3 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 13 /PowerBoost/LBO) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -1.3 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 11 "Net-(JP2-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
      ))
  )
  (module Inductor_SMD:L_Bourns_SRN6045TA (layer F.Cu) (tedit 5B61DEEA)
    (at 136.525 75.565 270)
    (descr http://www.bourns.com/docs/product-datasheets/srn6045ta.pdf)
    (tags "Semi-shielded Power Inductor")
    (attr smd)
    (fp_text reference L1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 6.8µ/2A (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2.075 0 270) (size 2.35 5.1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(L1-Pad2)"))
    (pad 1 smd rect (at -2.075 0 270) (size 2.35 5.1) (layers F.Cu F.Paste F.Mask)
      (net 6 /BAT))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns_SRN6045TA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 134.62 95.885)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value JST (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.5) (layer F.Fab) hide)
    (pad MP smd roundrect (at 3.35 2.9) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at -3.35 2.9) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad 2 smd roundrect (at 1 -2.85) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 -2.85) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /BAT))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 128.905 88.9 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 200k (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(JP2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.81 88.9 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 1.1M (at 0.127 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(JP2-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /BAT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.175 80.645 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 4.7µ (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /BAT))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 139.065 80.645)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 1µ (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 139.065 82.55)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 4.7µ (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 132.715 88.9 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /BAT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.175 82.55 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 10µ (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /BAT))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 138.43 88.9 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 10µ (at 0 0 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 134.62 88.9 90)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 500mA (at 0 0 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 VBUS))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 139.065 86.36)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 200k (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 139.065 84.455 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 1.1M (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.175 84.455)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 390k (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.175 86.36 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 2.4M (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /BAT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 134.62 86.36 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 200k (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /BAT))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /PowerBoost/EN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.81 74.295)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 2k (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 136.525 88.9 90)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value D (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 140.335 88.9 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +5V))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N16_EP2.7x2.7mm_ThermalVias (layer F.Cu) (tedit 5E4032CC)
    (at 134.62 82.55 270)
    (descr "QFN, 16 Pin (http://www.ti.com/lit/ds/symlink/msp430g2001.pdf#page=43), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (clearance 0.2)
    (zone_connect 1)
    (attr smd)
    (fp_text reference U2 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value TPS61090 (at 0 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 16 smd roundrect (at -0.975 -1.9625 270) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +3V3) (zone_connect 1))
    (pad 15 smd roundrect (at -0.325 -1.9625 270) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +3V3) (zone_connect 1))
    (pad 14 smd roundrect (at 0.325 -1.9625 270) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(R7-Pad2)") (zone_connect 1))
    (pad 13 smd roundrect (at 0.975 -1.9625 270) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 1))
    (pad 12 smd roundrect (at 1.9625 -0.975 270) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /PowerBoost/LBO) (zone_connect 1))
    (pad 11 smd roundrect (at 1.9625 -0.325 270) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /PowerBoost/EN) (zone_connect 1))
    (pad 10 smd roundrect (at 1.9625 0.325 270) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 1))
    (pad 9 smd roundrect (at 1.9625 0.975 270) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(R5-Pad2)") (zone_connect 1))
    (pad 8 smd roundrect (at 0.975 1.9625 270) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /BAT) (zone_connect 1))
    (pad 7 smd roundrect (at 0.325 1.9625 270) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 1))
    (pad 6 smd roundrect (at -0.325 1.9625 270) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 1))
    (pad 5 smd roundrect (at -0.975 1.9625 270) (size 0.35 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND) (zone_connect 1))
    (pad 4 smd roundrect (at -1.9625 0.975 270) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(L1-Pad2)") (zone_connect 1))
    (pad 3 smd roundrect (at -1.9625 0.325 270) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(L1-Pad2)") (zone_connect 1))
    (pad 2 smd roundrect (at -1.9625 -0.325 270) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (zone_connect 1))
    (pad 1 smd roundrect (at -1.9625 -0.975 270) (size 0.825 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +3V3) (zone_connect 1))
    (pad "" smd roundrect (at 0.55 0.55 270) (size 0.954594 0.954594) (layers F.Paste) (roundrect_rratio 0.25)
      (zone_connect 1))
    (pad "" smd roundrect (at 0.55 -0.55 270) (size 0.954594 0.954594) (layers F.Paste) (roundrect_rratio 0.25)
      (zone_connect 1))
    (pad "" smd roundrect (at -0.55 0.55 270) (size 0.954594 0.954594) (layers F.Paste) (roundrect_rratio 0.25)
      (zone_connect 1))
    (pad "" smd roundrect (at -0.55 -0.55 270) (size 0.954594 0.954594) (layers F.Paste) (roundrect_rratio 0.25)
      (zone_connect 1))
    (pad 17 smd roundrect (at 0 0 270) (size 2.7 2.7) (layers B.Cu) (roundrect_rratio 0.09300000000000001)
      (net 1 GND) (zone_connect 2))
    (pad 17 thru_hole circle (at 1.1 1.1 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 1))
    (pad 17 thru_hole circle (at 0 1.1 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 1))
    (pad 17 thru_hole circle (at -1.1 1.1 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 1))
    (pad 17 thru_hole circle (at 1.1 0 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 1))
    (pad 17 thru_hole circle (at 0 0 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 1))
    (pad 17 thru_hole circle (at -1.1 0 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 1))
    (pad 17 thru_hole circle (at 1.1 -1.1 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 1))
    (pad 17 thru_hole circle (at 0 -1.1 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 1))
    (pad 17 thru_hole circle (at -1.1 -1.1 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND) (zone_connect 1))
    (pad 17 smd roundrect (at 0 0 270) (size 2.7 2.7) (layers F.Cu F.Mask) (roundrect_rratio 0.09259299999999999)
      (net 1 GND) (zone_connect 1))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N16_EP2.7x2.7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 130.81 77.47)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value MCP73831-2-OT (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R3-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 /BAT))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text v1.3 (at 137.795 85.725 90) (layer B.SilkS))
  (gr_arc (start 142.875 100.33) (end 142.875 100.965) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 126.365 100.33) (end 125.73 100.33) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 126.365 71.12) (end 126.365 70.485) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 142.875 71.12) (end 143.51 71.12) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_text github.com/nerdyscout/ProMicro_Boost (at 139.7 85.725 90) (layer B.SilkS))
  (gr_line (start 143.51 71.12) (end 143.51 100.33) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.875 70.485) (end 126.365 70.485) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.73 100.33) (end 125.73 71.12) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.365 100.965) (end 142.875 100.965) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 125.73 70.485) (xy 143.51 70.485) (xy 143.51 100.965) (xy 125.73 100.965)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.15) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 125.73 100.965) (xy 143.51 100.965) (xy 143.51 70.485) (xy 125.73 70.485)
      )
    )
  )
  (zone (net 12) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 139.192 82.931) (xy 140.335 84.074) (xy 140.335 84.582) (xy 138.303 84.582) (xy 137.287 83.693)
        (xy 137.287 82.931) (xy 136.906 82.55) (xy 136.017 82.55) (xy 135.255 82.55) (xy 135.255 79.629)
        (xy 138.811 79.629) (xy 139.192 80.01)
      )
    )
  )
  (zone (net 2) (net_name "Net-(L1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.125))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.125) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 133.477 80.899) (xy 135.255 80.899) (xy 135.255 79.502) (xy 136.652 79.502) (xy 136.652 77.47)
        (xy 133.477 77.47)
      )
    )
  )
  (zone (net 6) (net_name /BAT) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 129.032 85.979) (xy 130.175 87.122) (xy 130.175 88.392) (xy 134.239 88.392) (xy 134.239 86.233)
        (xy 133.096 85.09) (xy 133.096 83.185) (xy 132.334 83.185) (xy 132.08 83.439) (xy 132.08 84.201)
        (xy 131.445 84.836) (xy 130.81 84.836) (xy 130.429 84.455) (xy 130.429 77.978) (xy 129.032 77.978)
      )
    )
  )
  (zone (net 6) (net_name /BAT) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.125))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.985 76.2) (xy 132.08 78.134307) (xy 132.08 83.185) (xy 133.223 84.328) (xy 133.223 89.789)
        (xy 134.112 90.678) (xy 134.112 94.488) (xy 133.096 94.488) (xy 133.096 91.059) (xy 128.905 86.868)
        (xy 128.905 77.47) (xy 132.715 73.66) (xy 133.35 73.66) (xy 133.985 74.295)
      )
    )
  )
)
