(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 0.06)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.01))
      (layer "dielectric 1" (type "core") (color "Polyimide") (thickness 0.02) (material "Kapton") (epsilon_r 3.2) (loss_tangent 0.004))
      (layer "B.Cu" (type "copper") (thickness 0.01))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010c0_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerber")
    )
  )
  (net 0 "")
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "F.Cu")
    (at 100 56.25)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 -4.75) (layer "F.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.75) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 117 100)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "hvc" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.204082))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.204082))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:resistor_chain_connector_1" (layer "F.Cu")
    (at 158 100 180)
    (attr smd)
    (fp_text reference "connector" (at -1 4 180 unlocked) (layer "Dwgs.User") hide)
    (fp_text value "resistor_chain_connector_1" (at 5.25 5.25 180 unlocked) (layer "Dwgs.User") hide)
    (pad "2" thru_hole circle (at 3 -2 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 2 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 7 0 180) (size 2.54 2.54) (drill 2.1844) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 0 0 180) (size 3.556 3.556) (drill 1.7526) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "F.Cu")
    (at 168 56.25)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 -4.75) (layer "F.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.75) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "F.Cu")
    (at 168 76.45)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 -4.75) (layer "F.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.75) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 83 100)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "hvc" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.204082))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.204082))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "F.Cu")
    (at 100 76.45)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 -4.75) (layer "F.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.75) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "F.Cu")
    (at 100 143.75)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 -4.75) (layer "F.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.75) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:resistor_chain_connector_hook" (layer "F.Cu")
    (at 130 100)
    (attr smd)
    (fp_text reference "connector" (at -1 4 unlocked) (layer "Dwgs.User") hide)
    (fp_text value "resistor_chain_connector_hook" (at 5.25 5.25 unlocked) (layer "Dwgs.User") hide)
    (pad "2" thru_hole circle (at 3 -2) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 2) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 0 0) (size 3.556 3.556) (drill 1.7526) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "F.Cu")
    (at 100 123.55)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 -4.75) (layer "F.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.75) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "F.Cu")
    (at 184 100 90)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 -4.75 90) (layer "F.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.75 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 90) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 90) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "F.Cu")
    (at 72 100 90)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 -4.75 90) (layer "F.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.75 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 90) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 90) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "F.Cu")
    (at 168 143.75)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 -4.75) (layer "F.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.75) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "F.Cu")
    (at 168 123.55)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 -4.75) (layer "F.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.75) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:Resistor-link-loop-flwr-v3.3" (layer "B.Cu")
    (at 168 100)
    (attr smd)
    (fp_text reference "flwr2" (at 0 0.5 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Resistor-link-loop-flwr-v3.3" (at -2.54 5.08 90 unlocked) (layer "B.Fab") hide)
    (pad "1" connect roundrect (at 0 14.0875) (size 1 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
    (pad "2" smd roundrect (at 11.5 0) (size 2.5 1) (layers "*.Mask" "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "3" connect roundrect (at 0 -14.0875) (size 1 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
    (pad "4" smd roundrect (at -6.25 0) (size 2.5 1) (layers "*.Mask" "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
  )
  (footprint "Library:Resistor-link-loop-flwr-v3" (layer "B.Cu")
    (at 100 100 180)
    (attr smd)
    (fp_text reference "flwr1" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Resistor-link-loop-flwr-v3" (at -2.54 5.08 270 unlocked) (layer "B.Fab") hide)
    (pad "1" connect roundrect (at 0 14.0875 180) (size 1 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
    (pad "2" smd roundrect (at 11.5 0 180) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "3" connect roundrect (at 0 -14.0875 180) (size 1 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
    (pad "4" smd roundrect (at -11.5 0 180) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
  )
  (gr_line (start 173.770225 102.753632) (end 176.652367 105.232558)
    (layer "Edge.Cuts"))
  (gr_arc (start 166.75 85.417729) (mid 166.660192 85.831887) (end 166.406934 86.171677)
    (layer "Edge.Cuts"))
  (gr_arc (start 102.420259 111.848437) (mid 102.237561 112.934849) (end 101.593066 113.828323)
    (layer "Edge.Cuts"))
  (gr_arc (start 176.652367 105.232558) (mid 176.785836 108.785836) (end 173.232558 108.652367)
    (layer "Edge.Cuts"))
  (gr_line (start 159.347633 94.767442) (end 162.229775 97.246368)
    (layer "Edge.Cuts"))
  (gr_line (start 170.614827 105.608842) (end 173.232558 108.652367)
    (layer "Edge.Cuts"))
  (gr_arc (start 103.884725 95.483396) (mid 101.614652 96.031749) (end 100.372338 94.054231)
    (layer "Edge.Cuts"))
  (gr_line (start 171.884725 104.516604) (end 174.502457 107.560129)
    (layer "Edge.Cuts"))
  (gr_line (start 161.990765 97.816636) (end 160.186422 97.665749)
    (layer "Edge.Cuts"))
  (gr_arc (start 100.372338 105.945769) (mid 101.614652 103.968251) (end 103.884725 104.516604)
    (layer "Edge.Cuts"))
  (gr_line (start 163.322013 104.02353) (end 160.439871 106.502457)
    (layer "Edge.Cuts"))
  (gr_arc (start 99.627662 94.054231) (mid 98.385348 96.031749) (end 96.115275 95.483396)
    (layer "Edge.Cuts"))
  (gr_arc (start 90 97) (mid 90.842327 97.12068) (end 91.616886 97.47301)
    (layer "Edge.Cuts"))
  (gr_arc (start 77.196152 97) (mid 75.30633 96.819805) (end 73.484615 96.285714)
    (layer "Edge.Cuts"))
  (gr_line (start 178 103) (end 178.803848 103)
    (layer "Edge.Cuts"))
  (gr_line (start 96.115275 104.516604) (end 93.497543 107.560129)
    (layer "Edge.Cuts"))
  (gr_arc (start 178 103) (mid 177.157673 102.87932) (end 176.383114 102.52699)
    (layer "Edge.Cuts"))
  (gr_arc (start 73.484615 103.714286) (mid 75.30633 103.180195) (end 77.196152 103)
    (layer "Edge.Cuts"))
  (gr_line (start 102.420259 88.151562) (end 102.044064 94.158919)
    (layer "Edge.Cuts"))
  (gr_arc (start 94.767442 108.652367) (mid 91.214198 108.785802) (end 91.347633 105.232558)
    (layer "Edge.Cuts"))
  (gr_line (start 131.542466 103.242315) (end 133.421672 103.53753)
    (layer "Edge.Cuts"))
  (gr_arc (start 98.75 85.417729) (mid 98.660202 85.831895) (end 98.406934 86.171677)
    (layer "Edge.Cuts"))
  (gr_arc (start 138.244593 103.854022) (mid 137.49734 103.683886) (end 137.289668 102.9462)
    (layer "Edge.Cuts"))
  (gr_arc (start 101.593066 86.171677) (mid 101.339799 85.831894) (end 101.25 85.417729)
    (layer "Edge.Cuts"))
  (gr_line (start 171.884725 95.483396) (end 174.502457 92.439871)
    (layer "Edge.Cuts"))
  (gr_line (start 164 56.25) (end 164 76.45)
    (layer "Edge.Cuts"))
  (gr_arc (start 133.932281 103.293588) (mid 133.714807 103.494735) (end 133.421672 103.53753)
    (layer "Edge.Cuts"))
  (gr_line (start 106.009235 102.183364) (end 107.813578 102.334251)
    (layer "Edge.Cuts"))
  (gr_arc (start 176.383114 97.47301) (mid 177.157673 97.12068) (end 178 97)
    (layer "Edge.Cuts"))
  (gr_line (start 151.6075 104.004178) (end 158.45 102.966058)
    (layer "Edge.Cuts"))
  (gr_line (start 101.25 80.915143) (end 101.25 85.417729)
    (layer "Edge.Cuts"))
  (gr_line (start 103.884725 95.483396) (end 106.502457 92.439871)
    (layer "Edge.Cuts"))
  (gr_line (start 99.251466 88.046875) (end 99.627662 94.054231)
    (layer "Edge.Cuts"))
  (gr_line (start 170.420259 88.151562) (end 170.044064 94.158919)
    (layer "Edge.Cuts"))
  (gr_arc (start 91.0625 100.747391) (mid 90.25 100) (end 91.0625 99.252609)
    (layer "Edge.Cuts"))
  (gr_arc (start 159.616886 102.52699) (mid 159.056503 102.80781) (end 158.45 102.966058)
    (layer "Edge.Cuts"))
  (gr_line (start 102.420259 111.848438) (end 102.044064 105.841081)
    (layer "Edge.Cuts"))
  (gr_arc (start 98.2 80.022114) (mid 98.601469 80.390738) (end 98.75 80.915143)
    (layer "Edge.Cuts"))
  (gr_arc (start 169.593066 86.171677) (mid 169.339788 85.831896) (end 169.25 85.417729)
    (layer "Edge.Cuts"))
  (gr_arc (start 102.044064 105.841081) (mid 102.245941 105.519735) (end 102.614827 105.608842)
    (layer "Edge.Cuts"))
  (gr_circle (center 109 100) (end 109.01 100)
    (fill solid) (layer "Edge.Cuts"))
  (gr_arc (start 169.25 80.915143) (mid 169.398514 80.390722) (end 169.8 80.022114)
    (layer "Edge.Cuts"))
  (gr_arc (start 169.8 119.977886) (mid 169.398547 119.609258) (end 169.25 119.084857)
    (layer "Edge.Cuts"))
  (gr_line (start 106.009235 97.816636) (end 107.813578 97.665749)
    (layer "Edge.Cuts"))
  (gr_arc (start 168.372338 105.945769) (mid 169.614646 103.968305) (end 171.884725 104.516604)
    (layer "Edge.Cuts"))
  (gr_arc (start 104 143.75) (mid 100 147.75) (end 96 143.75)
    (layer "Edge.Cuts"))
  (gr_arc (start 101.593066 86.171677) (mid 102.237561 87.065151) (end 102.420259 88.151563)
    (layer "Edge.Cuts"))
  (gr_arc (start 166.406934 113.828323) (mid 166.660212 114.168104) (end 166.75 114.582271)
    (layer "Edge.Cuts"))
  (gr_line (start 93.851182 100.51419) (end 91.0625 100.747391)
    (layer "Edge.Cuts"))
  (gr_arc (start 169.8 119.977886) (mid 171.405877 121.452382) (end 172 123.55)
    (layer "Edge.Cuts"))
  (gr_arc (start 166.2 80.022114) (mid 164.594123 78.547618) (end 164 76.45)
    (layer "Edge.Cuts"))
  (gr_arc (start 169.593066 86.171677) (mid 170.237561 87.065151) (end 170.420259 88.151563)
    (layer "Edge.Cuts"))
  (gr_arc (start 173.232558 91.347633) (mid 176.785804 91.214196) (end 176.652367 94.767442)
    (layer "Edge.Cuts"))
  (gr_arc (start 170.614827 94.391158) (mid 170.245907 94.480278) (end 170.044064 94.158919)
    (layer "Edge.Cuts"))
  (gr_arc (start 172 76.45) (mid 171.405877 78.547618) (end 169.8 80.022114)
    (layer "Edge.Cuts"))
  (gr_line (start 104 56.25) (end 104 76.45)
    (layer "Edge.Cuts"))
  (gr_arc (start 159.347633 94.767442) (mid 159.214164 91.214164) (end 162.767442 91.347633)
    (layer "Edge.Cuts"))
  (gr_arc (start 160.186422 97.665749) (mid 159.889894 97.604131) (end 159.616886 97.47301)
    (layer "Edge.Cuts"))
  (gr_arc (start 165.579741 88.151563) (mid 165.762438 87.065151) (end 166.406934 86.171677)
    (layer "Edge.Cuts"))
  (gr_line (start 135.917443 99.855187) (end 133.932281 103.293588)
    (layer "Edge.Cuts"))
  (gr_line (start 100.372338 94.054231) (end 100.748534 88.046875)
    (layer "Edge.Cuts"))
  (gr_line (start 104.677987 104.02353) (end 107.560129 106.502457)
    (layer "Edge.Cuts"))
  (gr_arc (start 105.770225 102.753632) (mid 105.68241 102.381604) (end 106.009235 102.183364)
    (layer "Edge.Cuts"))
  (gr_arc (start 182.515385 96.285714) (mid 180.693671 96.819813) (end 178.803848 97)
    (layer "Edge.Cuts"))
  (gr_line (start 96 76.45) (end 96 56.25)
    (layer "Edge.Cuts"))
  (gr_line (start 94.229775 97.246368) (end 91.347633 94.767442)
    (layer "Edge.Cuts"))
  (gr_arc (start 94.229775 97.246368) (mid 94.317588 97.618393) (end 93.990765 97.816636)
    (layer "Edge.Cuts"))
  (gr_arc (start 136.371471 95.999069) (mid 140.939537 99.060563) (end 138.244593 103.854022)
    (layer "Edge.Cuts"))
  (gr_arc (start 101.25 80.915143) (mid 101.39853 80.390737) (end 101.8 80.022114)
    (layer "Edge.Cuts"))
  (gr_line (start 94.229775 102.753632) (end 91.347633 105.232558)
    (layer "Edge.Cuts"))
  (gr_arc (start 166.2 80.022114) (mid 166.601453 80.390742) (end 166.75 80.915143)
    (layer "Edge.Cuts"))
  (gr_arc (start 161.497543 107.560129) (mid 160.398568 107.601432) (end 160.439871 106.502457)
    (layer "Edge.Cuts"))
  (gr_arc (start 95.322013 95.97647) (mid 95.862392 98.265849) (end 93.851182 99.48581)
    (layer "Edge.Cuts"))
  (gr_arc (start 92.439871 93.497543) (mid 92.398602 92.398602) (end 93.497543 92.439871)
    (layer "Edge.Cuts"))
  (gr_arc (start 104 76.45) (mid 103.405877 78.547618) (end 101.8 80.022114)
    (layer "Edge.Cuts"))
  (gr_arc (start 175.813578 102.334251) (mid 176.110106 102.395869) (end 176.383114 102.52699)
    (layer "Edge.Cuts"))
  (gr_arc (start 175.560129 106.502457) (mid 175.601432 107.601432) (end 174.502457 107.560129)
    (layer "Edge.Cuts"))
  (gr_arc (start 168.748534 111.953125) (mid 168 112.75) (end 167.251466 111.953125)
    (layer "Edge.Cuts"))
  (gr_arc (start 164.115275 104.516604) (mid 166.385346 103.968253) (end 167.627662 105.945769)
    (layer "Edge.Cuts"))
  (gr_arc (start 96 123.55) (mid 96.594123 121.452382) (end 98.2 119.977886)
    (layer "Edge.Cuts"))
  (gr_arc (start 73.484615 103.714286) (mid 68 100) (end 73.484615 96.285714)
    (layer "Edge.Cuts"))
  (gr_line (start 93.851182 99.48581) (end 91.0625 99.252609)
    (layer "Edge.Cuts"))
  (gr_arc (start 174.502457 92.439871) (mid 175.601432 92.398568) (end 175.560129 93.497543)
    (layer "Edge.Cuts"))
  (gr_line (start 108.652367 94.767442) (end 105.770225 97.246368)
    (layer "Edge.Cuts"))
  (gr_line (start 165.579741 88.151562) (end 165.955936 94.158919)
    (layer "Edge.Cuts"))
  (gr_line (start 159.347633 105.232558) (end 162.229775 102.753632)
    (layer "Edge.Cuts"))
  (gr_line (start 174.148818 100.51419) (end 176.9375 100.747391)
    (layer "Edge.Cuts"))
  (gr_arc (start 164 123.55) (mid 164.594123 121.452382) (end 166.2 119.977886)
    (layer "Edge.Cuts"))
  (gr_line (start 95.322013 95.97647) (end 92.439871 93.497543)
    (layer "Edge.Cuts"))
  (gr_arc (start 172 143.75) (mid 168 147.75) (end 164 143.75)
    (layer "Edge.Cuts"))
  (gr_line (start 90 103) (end 77.196152 103)
    (layer "Edge.Cuts"))
  (gr_arc (start 182.515385 96.285714) (mid 188 100) (end 182.515385 103.714286)
    (layer "Edge.Cuts"))
  (gr_arc (start 101.8 119.977886) (mid 101.398532 119.609261) (end 101.25 119.084857)
    (layer "Edge.Cuts"))
  (gr_line (start 164.115275 104.516604) (end 161.497543 107.560129)
    (layer "Edge.Cuts"))
  (gr_arc (start 100.748534 111.953125) (mid 100 112.75) (end 99.251466 111.953125)
    (layer "Edge.Cuts"))
  (gr_line (start 97.385173 94.391158) (end 94.767442 91.347633)
    (layer "Edge.Cuts"))
  (gr_arc (start 167.627662 94.054231) (mid 166.385354 96.031695) (end 164.115275 95.483396)
    (layer "Edge.Cuts"))
  (gr_line (start 104 143.75) (end 104 123.55)
    (layer "Edge.Cuts"))
  (gr_line (start 101.25 119.084857) (end 101.25 114.582271)
    (layer "Edge.Cuts"))
  (gr_circle (center 158 100) (end 158.01 100)
    (fill solid) (layer "Edge.Cuts"))
  (gr_line (start 164.115275 95.483396) (end 161.497543 92.439871)
    (layer "Edge.Cuts"))
  (gr_arc (start 97.579741 88.151563) (mid 97.762438 87.065151) (end 98.406934 86.171677)
    (layer "Edge.Cuts"))
  (gr_arc (start 91.616886 102.52699) (mid 91.889893 102.395866) (end 92.186422 102.334251)
    (layer "Edge.Cuts"))
  (gr_arc (start 166.75 119.084857) (mid 166.601486 119.609278) (end 166.2 119.977886)
    (layer "Edge.Cuts"))
  (gr_line (start 100.372338 105.945769) (end 100.748534 111.953125)
    (layer "Edge.Cuts"))
  (gr_arc (start 92.186422 97.665749) (mid 91.889893 97.604134) (end 91.616886 97.47301)
    (layer "Edge.Cuts"))
  (gr_arc (start 102.614827 94.391158) (mid 102.245941 94.480264) (end 102.044064 94.158919)
    (layer "Edge.Cuts"))
  (gr_arc (start 96.115275 104.516604) (mid 98.385348 103.968251) (end 99.627662 105.945769)
    (layer "Edge.Cuts"))
  (gr_line (start 170.614827 94.391158) (end 173.232558 91.347633)
    (layer "Edge.Cuts"))
  (gr_arc (start 99.251466 88.046875) (mid 100 87.25) (end 100.748534 88.046875)
    (layer "Edge.Cuts"))
  (gr_line (start 97.385173 105.608842) (end 94.767442 108.652367)
    (layer "Edge.Cuts"))
  (gr_arc (start 108.383114 97.47301) (mid 108.110108 97.604137) (end 107.813578 97.665749)
    (layer "Edge.Cuts"))
  (gr_arc (start 106.148818 99.48581) (mid 104.137608 98.26585) (end 104.677987 95.97647)
    (layer "Edge.Cuts"))
  (gr_line (start 110 103) (end 128.438617 103)
    (layer "Edge.Cuts"))
  (gr_line (start 166.75 119.084857) (end 166.75 114.582271)
    (layer "Edge.Cuts"))
  (gr_arc (start 166.406934 113.828323) (mid 165.762439 112.934849) (end 165.579741 111.848437)
    (layer "Edge.Cuts"))
  (gr_line (start 131.542466 96.757685) (end 136.371471 95.999069)
    (layer "Edge.Cuts"))
  (gr_arc (start 106.009235 97.816636) (mid 105.682414 97.618394) (end 105.770225 97.246368)
    (layer "Edge.Cuts"))
  (gr_line (start 173.770225 97.246368) (end 176.652367 94.767442)
    (layer "Edge.Cuts"))
  (gr_line (start 106.148818 99.48581) (end 108.9375 99.252609)
    (layer "Edge.Cuts"))
  (gr_line (start 163.322013 95.97647) (end 160.439871 93.497543)
    (layer "Edge.Cuts"))
  (gr_arc (start 170.420259 111.848437) (mid 170.237562 112.934849) (end 169.593066 113.828323)
    (layer "Edge.Cuts"))
  (gr_line (start 164.017849 97.492767) (end 164.017849 102.507233)
    (layer "Edge.Cuts"))
  (gr_arc (start 96 56.25) (mid 100 52.25) (end 104 56.25)
    (layer "Edge.Cuts"))
  (gr_line (start 172.677987 104.02353) (end 175.560129 106.502457)
    (layer "Edge.Cuts"))
  (gr_line (start 168.748534 88.046875) (end 168.372338 94.054231)
    (layer "Edge.Cuts"))
  (gr_arc (start 93.851182 100.51419) (mid 95.862392 101.73415) (end 95.322013 104.02353)
    (layer "Edge.Cuts"))
  (gr_line (start 98.75 80.915143) (end 98.75 85.417729)
    (layer "Edge.Cuts"))
  (gr_line (start 104.677987 95.97647) (end 107.560129 93.497543)
    (layer "Edge.Cuts"))
  (gr_arc (start 97.385173 105.608842) (mid 97.75406 105.519735) (end 97.955936 105.841081)
    (layer "Edge.Cuts"))
  (gr_line (start 172.677987 95.97647) (end 175.560129 93.497543)
    (layer "Edge.Cuts"))
  (gr_arc (start 158.45 97.033942) (mid 159.056504 97.192189) (end 159.616886 97.47301)
    (layer "Edge.Cuts"))
  (gr_arc (start 106.502457 92.439871) (mid 107.6014 92.3986) (end 107.560129 93.497543)
    (layer "Edge.Cuts"))
  (gr_arc (start 91.347633 94.767442) (mid 91.214198 91.214198) (end 94.767442 91.347633)
    (layer "Edge.Cuts"))
  (gr_line (start 167.627662 105.945769) (end 167.251466 111.953125)
    (layer "Edge.Cuts"))
  (gr_arc (start 171.884725 95.483396) (mid 169.614654 96.031747) (end 168.372338 94.054231)
    (layer "Edge.Cuts"))
  (gr_line (start 174.148818 99.48581) (end 176.9375 99.252609)
    (layer "Edge.Cuts"))
  (gr_arc (start 162.229775 97.246368) (mid 162.317597 97.618434) (end 161.990765 97.816636)
    (layer "Edge.Cuts"))
  (gr_line (start 96 123.55) (end 96 143.75)
    (layer "Edge.Cuts"))
  (gr_arc (start 174.009235 97.816636) (mid 173.68249 97.618397) (end 173.770225 97.246368)
    (layer "Edge.Cuts"))
  (gr_arc (start 101.8 119.977886) (mid 103.405877 121.452382) (end 104 123.55)
    (layer "Edge.Cuts"))
  (gr_arc (start 101.25 114.582271) (mid 101.339798 114.168105) (end 101.593066 113.828323)
    (layer "Edge.Cuts"))
  (gr_line (start 164 143.75) (end 164 123.55)
    (layer "Edge.Cuts"))
  (gr_arc (start 172.677987 104.02353) (mid 172.137598 101.734109) (end 174.148818 100.51419)
    (layer "Edge.Cuts"))
  (gr_arc (start 176.383114 97.47301) (mid 176.110108 97.604137) (end 175.813578 97.665749)
    (layer "Edge.Cuts"))
  (gr_line (start 92.186422 97.665749) (end 93.990765 97.816636)
    (layer "Edge.Cuts"))
  (gr_arc (start 98.2 80.022114) (mid 96.594123 78.547618) (end 96 76.45)
    (layer "Edge.Cuts"))
  (gr_line (start 169.25 119.084857) (end 169.25 114.582271)
    (layer "Edge.Cuts"))
  (gr_line (start 95.322013 104.02353) (end 92.439871 106.502457)
    (layer "Edge.Cuts"))
  (gr_line (start 103.884725 104.516604) (end 106.502457 107.560129)
    (layer "Edge.Cuts"))
  (gr_arc (start 107.560129 106.502457) (mid 107.601432 107.601432) (end 106.502457 107.560129)
    (layer "Edge.Cuts"))
  (gr_arc (start 105.232558 91.347633) (mid 108.785802 91.214198) (end 108.652367 94.767442)
    (layer "Edge.Cuts"))
  (gr_line (start 92.186422 102.334251) (end 93.990765 102.183364)
    (layer "Edge.Cuts"))
  (gr_line (start 97.579741 88.151562) (end 97.955936 94.158919)
    (layer "Edge.Cuts"))
  (gr_arc (start 167.251466 88.046875) (mid 168 87.25) (end 168.748534 88.046875)
    (layer "Edge.Cuts"))
  (gr_line (start 102.614827 105.608842) (end 105.232558 108.652367)
    (layer "Edge.Cuts"))
  (gr_line (start 166.75 80.915143) (end 166.75 85.417729)
    (layer "Edge.Cuts"))
  (gr_line (start 175.813578 102.334251) (end 174.009235 102.183364)
    (layer "Edge.Cuts"))
  (gr_line (start 96.115275 95.483396) (end 93.497543 92.439871)
    (layer "Edge.Cuts"))
  (gr_line (start 169.25 80.915143) (end 169.25 85.417729)
    (layer "Edge.Cuts"))
  (gr_circle (center 130 100) (end 130.01 100)
    (fill solid) (layer "Edge.Cuts"))
  (gr_line (start 170.420259 111.848438) (end 170.044064 105.841081)
    (layer "Edge.Cuts"))
  (gr_arc (start 151.6075 104.004178) (mid 146.95 100) (end 151.6075 95.995822)
    (layer "Edge.Cuts"))
  (gr_arc (start 110 103) (mid 109.157673 102.87932) (end 108.383114 102.52699)
    (layer "Edge.Cuts"))
  (gr_arc (start 93.497543 107.560129) (mid 92.398602 107.601398) (end 92.439871 106.502457)
    (layer "Edge.Cuts"))
  (gr_circle (center 134 100) (end 134.01 100)
    (fill solid) (layer "Edge.Cuts"))
  (gr_arc (start 98.406934 113.828323) (mid 97.762439 112.934849) (end 97.579741 111.848437)
    (layer "Edge.Cuts"))
  (gr_line (start 161.990765 102.183364) (end 160.186422 102.334251)
    (layer "Edge.Cuts"))
  (gr_line (start 110 97) (end 128.438617 97)
    (layer "Edge.Cuts"))
  (gr_line (start 172 76.45) (end 172 56.25)
    (layer "Edge.Cuts"))
  (gr_arc (start 104.677987 104.02353) (mid 104.137604 101.734147) (end 106.148818 100.51419)
    (layer "Edge.Cuts"))
  (gr_line (start 172 123.55) (end 172 143.75)
    (layer "Edge.Cuts"))
  (gr_arc (start 162.767442 108.652367) (mid 159.214196 108.785804) (end 159.347633 105.232558)
    (layer "Edge.Cuts"))
  (gr_arc (start 165.385173 105.608842) (mid 165.754093 105.519722) (end 165.955936 105.841081)
    (layer "Edge.Cuts"))
  (gr_arc (start 169.25 114.582271) (mid 169.339808 114.168113) (end 169.593066 113.828323)
    (layer "Edge.Cuts"))
  (gr_line (start 175.813578 97.665749) (end 174.009235 97.816636)
    (layer "Edge.Cuts"))
  (gr_arc (start 173.770225 102.753632) (mid 173.682403 102.381566) (end 174.009235 102.183364)
    (layer "Edge.Cuts"))
  (gr_line (start 102.614827 94.391158) (end 105.232558 91.347633)
    (layer "Edge.Cuts"))
  (gr_arc (start 128.438617 103) (mid 129.995264 103.060672) (end 131.542466 103.242315)
    (layer "Edge.Cuts"))
  (gr_arc (start 135.917443 99.855187) (mid 137.373554 98.973668) (end 137.922371 100.584921)
    (layer "Edge.Cuts"))
  (gr_arc (start 98.75 119.084857) (mid 98.601469 119.609262) (end 98.2 119.977886)
    (layer "Edge.Cuts"))
  (gr_arc (start 93.990765 102.183364) (mid 94.317587 102.381607) (end 94.229775 102.753632)
    (layer "Edge.Cuts"))
  (gr_arc (start 108.9375 99.252609) (mid 109.75 100) (end 108.9375 100.747391)
    (layer "Edge.Cuts"))
  (gr_arc (start 176.9375 99.252609) (mid 177.75 100) (end 176.9375 100.747391)
    (layer "Edge.Cuts"))
  (gr_line (start 167.627662 94.054231) (end 167.251466 88.046875)
    (layer "Edge.Cuts"))
  (gr_line (start 137.922371 100.584921) (end 137.289668 102.9462)
    (layer "Edge.Cuts"))
  (gr_line (start 168.748534 111.953125) (end 168.372338 105.945769)
    (layer "Edge.Cuts"))
  (gr_line (start 151.6075 95.995822) (end 158.45 97.033942)
    (layer "Edge.Cuts"))
  (gr_arc (start 170.044064 105.841081) (mid 170.245934 105.519789) (end 170.614827 105.608842)
    (layer "Edge.Cuts"))
  (gr_arc (start 107.813578 102.334251) (mid 108.110106 102.395869) (end 108.383114 102.52699)
    (layer "Edge.Cuts"))
  (gr_line (start 108.652367 105.232558) (end 105.770225 102.753632)
    (layer "Edge.Cuts"))
  (gr_arc (start 174.148818 99.48581) (mid 172.137609 98.265851) (end 172.677987 95.97647)
    (layer "Edge.Cuts"))
  (gr_line (start 97.579741 111.848438) (end 97.955936 105.841081)
    (layer "Edge.Cuts"))
  (gr_arc (start 161.990765 102.183364) (mid 162.31751 102.381603) (end 162.229775 102.753632)
    (layer "Edge.Cuts"))
  (gr_line (start 165.579741 111.848438) (end 165.955936 105.841081)
    (layer "Edge.Cuts"))
  (gr_arc (start 108.383114 97.47301) (mid 109.157673 97.12068) (end 110 97)
    (layer "Edge.Cuts"))
  (gr_arc (start 91.616886 102.52699) (mid 90.842327 102.87932) (end 90 103)
    (layer "Edge.Cuts"))
  (gr_line (start 99.251466 111.953125) (end 99.627662 105.945769)
    (layer "Edge.Cuts"))
  (gr_arc (start 98.406934 113.828323) (mid 98.660202 114.168106) (end 98.75 114.582271)
    (layer "Edge.Cuts"))
  (gr_arc (start 164.017849 102.507233) (mid 163.835577 103.341396) (end 163.322013 104.02353)
    (layer "Edge.Cuts"))
  (gr_line (start 165.385173 94.391158) (end 162.767442 91.347633)
    (layer "Edge.Cuts"))
  (gr_arc (start 163.322013 95.97647) (mid 163.835584 96.6586) (end 164.017849 97.492767)
    (layer "Edge.Cuts"))
  (gr_line (start 98.75 119.084857) (end 98.75 114.582271)
    (layer "Edge.Cuts"))
  (gr_arc (start 178.803848 103) (mid 180.693668 103.180204) (end 182.515385 103.714286)
    (layer "Edge.Cuts"))
  (gr_line (start 165.385173 105.608842) (end 162.767442 108.652367)
    (layer "Edge.Cuts"))
  (gr_arc (start 131.542466 96.757685) (mid 129.995264 96.93933) (end 128.438617 97)
    (layer "Edge.Cuts"))
  (gr_line (start 106.148818 100.51419) (end 108.9375 100.747391)
    (layer "Edge.Cuts"))
  (gr_arc (start 160.439871 93.497543) (mid 160.398568 92.398568) (end 161.497543 92.439871)
    (layer "Edge.Cuts"))
  (gr_arc (start 165.955936 94.158919) (mid 165.754066 94.480211) (end 165.385173 94.391158)
    (layer "Edge.Cuts"))
  (gr_arc (start 108.652367 105.232558) (mid 108.785836 108.785836) (end 105.232558 108.652367)
    (layer "Edge.Cuts"))
  (gr_line (start 90 97) (end 77.196152 97)
    (layer "Edge.Cuts"))
  (gr_arc (start 159.616886 102.52699) (mid 159.889892 102.395863) (end 160.186422 102.334251)
    (layer "Edge.Cuts"))
  (gr_arc (start 97.955936 94.158919) (mid 97.75406 94.480265) (end 97.385173 94.391158)
    (layer "Edge.Cuts"))
  (gr_line (start 178 97) (end 178.803848 97)
    (layer "Edge.Cuts"))
  (gr_arc (start 164 56.25) (mid 168 52.25) (end 172 56.25)
    (layer "Edge.Cuts"))
  (zone (net 0) (net_name "") (layers "*.Mask") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 94 31)
        (xy 238 30)
        (xy 221 158)
        (xy 56 170)
        (xy 35 48)
        (xy 95 31)
      )
    )
  )
)
