(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 237)
    (zones 0)
    (modules 77)
    (nets 41)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.508)
    (user_trace_width 0.6096)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 0.889 0.889)
    (mod_text_width 0.1397)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BI1-Pad1)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C4-Pad1)")
  (net 4 "Net-(C4-Pad2)")
  (net 5 "Net-(C22-Pad1)")
  (net 6 GND)
  (net 7 "Net-(C6-Pad2)")
  (net 8 "Net-(C6-Pad1)")
  (net 9 "Net-(C22-Pad2)")
  (net 10 "Net-(F2-Pad1)")
  (net 11 "Net-(Q1-Pad3)")
  (net 12 +9V)
  (net 13 "Net-(C7-Pad2)")
  (net 14 "Net-(C10-Pad1)")
  (net 15 "Net-(C9-Pad1)")
  (net 16 "Net-(C10-Pad2)")
  (net 17 "Net-(C13-Pad2)")
  (net 18 "Net-(C13-Pad1)")
  (net 19 "Net-(Q5-Pad3)")
  (net 20 "Net-(C7-Pad1)")
  (net 21 "Net-(BO1-Pad1)")
  (net 22 "Net-(C3-Pad2)")
  (net 23 "Net-(C3-Pad1)")
  (net 24 "Net-(C17-Pad1)")
  (net 25 "Net-(C8-Pad1)")
  (net 26 "Net-(C11-Pad1)")
  (net 27 "Net-(C12-Pad2)")
  (net 28 "Net-(C12-Pad1)")
  (net 29 "Net-(C14-Pad2)")
  (net 30 "Net-(C14-Pad1)")
  (net 31 "Net-(C15-Pad2)")
  (net 32 "Net-(C16-Pad1)")
  (net 33 "Net-(C17-Pad2)")
  (net 34 "Net-(C18-Pad2)")
  (net 35 "Net-(Q6-Pad1)")
  (net 36 "Net-(Q7-Pad1)")
  (net 37 "Net-(Q8-Pad1)")
  (net 38 "Net-(C20-Pad1)")
  (net 39 "Net-(C20-Pad2)")
  (net 40 +9VA)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +9V)
    (add_net +9VA)
    (add_net GND)
    (add_net "Net-(BI1-Pad1)")
    (add_net "Net-(BO1-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(F2-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q5-Pad3)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(Q7-Pad1)")
    (add_net "Net-(Q8-Pad1)")
  )
  (module Connector_Wire:SolderWire-0.75sqmm_1x03_P4.8mm_D1.25mm_OD2.3mm (layer F.Cu) (tedit 60A2C39F)
    (at 134.3025 53.975 180)
    (descr "Soldered wire connection, for 3 times 0.75 mm² wires, basic insulation, conductor diameter 1.25mm, outer diameter 2.3mm, size source Multi-Contact FLEXI-E 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (attr virtual)
    (fp_text reference VOL (at 2.413 0 90) (layer F.SilkS))
    (fp_text value A100K (at 4.8 2.47) (layer F.Fab))
    (fp_text user %R (at 4.8 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 9.6 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 38 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 4.8 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 21 "Net-(BO1-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.098039)
      (net 6 GND))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x03_P4.8mm_D1.25mm_OD2.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWire-0.75sqmm_1x03_P4.8mm_D1.25mm_OD2.3mm (layer F.Cu) (tedit 60A2C39F)
    (at 119.6975 53.975 180)
    (descr "Soldered wire connection, for 3 times 0.75 mm² wires, basic insulation, conductor diameter 1.25mm, outer diameter 2.3mm, size source Multi-Contact FLEXI-E 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (attr virtual)
    (fp_text reference HI (at 2.413 0 90) (layer F.SilkS))
    (fp_text value B100K (at 4.8 2.47) (layer F.Fab))
    (fp_text user %R (at 4.8 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 9.6 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 25 "Net-(C8-Pad1)"))
    (pad 2 thru_hole circle (at 4.8 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 22 "Net-(C3-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.098039)
      (net 26 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x03_P4.8mm_D1.25mm_OD2.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWire-0.75sqmm_1x03_P4.8mm_D1.25mm_OD2.3mm (layer F.Cu) (tedit 60A2C39F)
    (at 88.9 53.975 180)
    (descr "Soldered wire connection, for 3 times 0.75 mm² wires, basic insulation, conductor diameter 1.25mm, outer diameter 2.3mm, size source Multi-Contact FLEXI-E 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (attr virtual)
    (fp_text reference LO (at 2.413 0 90) (layer F.SilkS))
    (fp_text value A1M (at 4.8 2.47) (layer F.Fab))
    (fp_text user %R (at 4.8 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 9.6 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 15 "Net-(C9-Pad1)"))
    (pad 2 thru_hole circle (at 4.8 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 14 "Net-(C10-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.098039)
      (net 16 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x03_P4.8mm_D1.25mm_OD2.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWire-0.75sqmm_1x03_P4.8mm_D1.25mm_OD2.3mm (layer F.Cu) (tedit 60A2C39F)
    (at 74.6125 53.975 180)
    (descr "Soldered wire connection, for 3 times 0.75 mm² wires, basic insulation, conductor diameter 1.25mm, outer diameter 2.3mm, size source Multi-Contact FLEXI-E 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (attr virtual)
    (fp_text reference GAIN (at 2.413 0 90) (layer F.SilkS))
    (fp_text value A100K (at 4.8 2.47) (layer F.Fab))
    (fp_text user %R (at 4.8 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 9.6 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 10 "Net-(F2-Pad1)"))
    (pad 2 thru_hole circle (at 4.8 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 9 "Net-(C22-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.098039)
      (net 6 GND))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x03_P4.8mm_D1.25mm_OD2.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Device_VN:TO-92_Inline_Wide (layer F.Cu) (tedit 60A261F8)
    (at 122.2375 81.915 90)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q8 (at 2.54 -1.905 90) (layer F.SilkS))
    (fp_text value 2n5089 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.599946 2.199894) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(Q8-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 39 "Net-(C20-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 23 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Device_VN:TO-92_Inline_Wide (layer F.Cu) (tedit 60A261F8)
    (at 113.3475 82.55 90)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q7 (at 2.54 -1.905 90) (layer F.SilkS))
    (fp_text value 2n5089 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.599946 2.199894) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(Q7-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 24 "Net-(C17-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 34 "Net-(C18-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Device_VN:TO-92_Inline_Wide (layer F.Cu) (tedit 60A261F8)
    (at 101.6 81.28 90)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q6 (at 2.54 -1.905 90) (layer F.SilkS))
    (fp_text value 2n5089 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.599946 2.199894) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(Q6-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 30 "Net-(C14-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 31 "Net-(C15-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Device_VN:TO-92_Inline_Wide (layer F.Cu) (tedit 60A261F8)
    (at 89.535 76.835 270)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q5 (at 2.54 -1.905 90) (layer F.SilkS))
    (fp_text value BS170 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.599946 2.199894) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(C12-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 19 "Net-(Q5-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 17 "Net-(C13-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Device_VN:TO-92_Inline_Wide (layer F.Cu) (tedit 60A261F8)
    (at 74.295 67.945 270)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at 2.54 -1.905 90) (layer F.SilkS))
    (fp_text value 2n3904 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.599946 2.199894) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(C7-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 40 +9VA))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Device_VN:TO-92_Inline_Wide (layer F.Cu) (tedit 60A261F8)
    (at 59.3725 57.785 270)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 2.54 -1.905 90) (layer F.SilkS))
    (fp_text value BS170 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.599946 2.199894) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Device_VN:TO-92_Inline_Wide (layer F.Cu) (tedit 60A261F8)
    (at 69.215 65.405 90)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 2.54 -1.905 90) (layer F.SilkS))
    (fp_text value 2n5458 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.599946 2.199894) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 9 "Net-(C22-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Device_VN:TO-92_Inline_Wide (layer F.Cu) (tedit 60A261F8)
    (at 69.215 69.215 270)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 2.54 -1.905 90) (layer F.SilkS))
    (fp_text value 2n5458 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.599946 2.199894) (drill 1) (layers *.Cu *.Mask)
      (net 40 +9VA))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 2.2) (drill oval 0.8 1) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W3.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5FFE8EC9)
    (at 129.54 58.1025 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.5mm Capacitor")
    (fp_text reference C20 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 1µF (at 2.5 3 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(C20-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W3.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W3.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5FFE8EC9)
    (at 53.975 57.785 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.5mm Capacitor")
    (fp_text reference C4 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 1µF (at 2.5 3 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W3.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W3.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5FFE8EC9)
    (at 124.7775 63.1825 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.5mm Capacitor")
    (fp_text reference C3 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 1µF (at 2.5 3 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W3.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 124.7775 73.9775 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R27 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 470k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 +9VA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5FFDD768)
    (at 133.6675 78.74 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 1.27 1.905 90) (layer F.SilkS))
    (fp_text value 100µF (at 1.25 4.4 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 +9VA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal (layer F.Cu) (tedit 608D6521)
    (at 117.475 82.8675 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D4 (at 4.318 0.127 90) (layer F.SilkS))
    (fp_text value 1n4148 (at 3.81 0.127 90) (layer F.Fab))
    (fp_text user K (at -1.905 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(C18-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(C17-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp (layer F.Cu) (tedit 5AE50CD5)
    (at 123.19 86.0425 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D3 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 1n4148 (at 1.27 3.639635) (layer F.Fab))
    (fp_text user A (at 4.64 0) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.750635) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "Net-(C17-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 "Net-(C18-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 120.015 58.1025 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R32 (at 3.81 0) (layer F.SilkS))
    (fp_text value 39k (at 3.81 0) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(C8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 112.395 61.595)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R31 (at 3.81 0) (layer F.SilkS))
    (fp_text value 39k (at 3.81 0) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(C11-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 128.5875 73.9775 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R30 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(C20-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 +9VA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 128.5875 78.105 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R29 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 2k2 (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(Q8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 121.285 73.9775 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R28 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 100k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 113.3475 67.31 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R26 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 15k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C17-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 +9VA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 108.9025 85.725)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R25 (at 3.81 0) (layer F.SilkS))
    (fp_text value 100R (at 3.81 0) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(Q7-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 108.9025 82.55 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R24 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 470k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C17-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C18-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 104.775 85.725 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R23 (at 3.81 0) (layer F.SilkS))
    (fp_text value 100k (at 3.81 0) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C18-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 105.7275 74.93 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R22 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 27k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C18-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 105.7275 53.975 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R21 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 15k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(C14-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 +9VA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 97.155 74.295 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R20 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 100R (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(Q6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 99.06 61.595 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R19 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 470k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(C14-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(C15-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 95.885 61.595 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R18 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 100k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(C15-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 92.71 61.595 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R17 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 27k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(C15-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 93.98 81.915 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R15 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(C12-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 +9VA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal (layer F.Cu) (tedit 608D6521)
    (at 102.235 71.755 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 4.318 0.127 90) (layer F.SilkS))
    (fp_text value 1n4148 (at 3.81 0.127 90) (layer F.Fab))
    (fp_text user K (at -1.905 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(C15-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(C14-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal (layer F.Cu) (tedit 608D6521)
    (at 98.7425 64.135 270)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 4.318 0.127 90) (layer F.SilkS))
    (fp_text value 1n4148 (at 3.81 0.127 90) (layer F.Fab))
    (fp_text user K (at -1.905 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(C14-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(C15-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 60095440)
    (at 108.9025 66.675 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (fp_text reference C18 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 470pF (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C18-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 60A0E717)
    (at 117.475 67.31 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C17 (at 2.413 0 90) (layer F.SilkS))
    (fp_text value 100n (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(C17-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 60A0E717)
    (at 105.7275 71.755 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C16 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 100n (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(C14-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 60095440)
    (at 102.235 54.2925 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (fp_text reference C15 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 470pF (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(C15-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 60A0E717)
    (at 95.25 66.04 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C14 (at 2.413 0 90) (layer F.SilkS))
    (fp_text value 100n (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C14-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 60A0E717)
    (at 92.3925 66.04 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C12 (at 2.413 0 90) (layer F.SilkS))
    (fp_text value 100n (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(C12-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 60A0E717)
    (at 118.4275 64.77 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C11 (at 2.413 0) (layer F.SilkS))
    (fp_text value 6n8 (at 2.5 2.2) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 60A0E717)
    (at 108.9025 58.1025 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C8 (at 2.413 0 90) (layer F.SilkS))
    (fp_text value 6n8 (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C17-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Device_VN:SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm (layer F.Cu) (tedit 5EB70B43)
    (at 133.6675 85.725 90)
    (descr "Soldered wire connection, for a single 0.75 mm² wire, basic insulation, conductor diameter 1.25mm, outer diameter 2.3mm, size source Multi-Contact FLEXI-E 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (attr virtual)
    (fp_text reference BO (at 0 2.54 90) (layer F.SilkS))
    (fp_text value pad (at 0 2.47 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.098039)
      (net 21 "Net-(BO1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 85.725 81.915 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R16 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 10M (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C13-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 86.36 85.725)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R14 (at 3.81 0) (layer F.SilkS))
    (fp_text value 2k2 (at 3.81 0) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(Q5-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 82.2325 78.105 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 10M (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C13-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 82.55 66.675 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 100k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C13-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 89.2175 58.42 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 27k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 78.74 58.42 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 100k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 60A0E717)
    (at 89.2175 74.215 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C24 (at 2.413 0 90) (layer F.SilkS))
    (fp_text value 330pF (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C13-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 60A0E717)
    (at 85.725 66.675 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C13 (at 2.413 0 90) (layer F.SilkS))
    (fp_text value 100n (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C13-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 60A0E717)
    (at 86.0425 63.5 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C10 (at 2.413 0 90) (layer F.SilkS))
    (fp_text value 10n (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C10-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 60A0E717)
    (at 82.8675 63.5 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C9 (at 2.413 0 90) (layer F.SilkS))
    (fp_text value 2n2 (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C10-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 60A0E18A)
    (at 79.0575 74.295 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.0mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.0mm Capacitor")
    (fp_text reference C7 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 220n (at 2.5 2.75 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 60A0E717)
    (at 64.4525 85.725 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C21 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 100pF (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BI1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 60A0E18A)
    (at 53.975 76.835 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*3.0mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 3.0mm Capacitor")
    (fp_text reference C1 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 220n (at 2.5 2.75 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BI1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W3.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Device_VN:SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm (layer F.Cu) (tedit 5EB70B43)
    (at 53.975 85.725 90)
    (descr "Soldered wire connection, for a single 0.75 mm² wire, basic insulation, conductor diameter 1.25mm, outer diameter 2.3mm, size source Multi-Contact FLEXI-E 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (attr virtual)
    (fp_text reference BI (at -2.2225 0 180) (layer F.SilkS))
    (fp_text value pad (at 0 2.47 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.098039)
      (net 1 "Net-(BI1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5FFDEF2B)
    (at 74.6125 83.185 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C5 (at 1.3208 1.7272 90) (layer F.SilkS))
    (fp_text value 47µF (at 1.1938 1.7272 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C22-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5FFDEF2B)
    (at 74.6125 76.835 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C6 (at 1.3208 1.7272 90) (layer F.SilkS))
    (fp_text value 10µF (at 1.1938 1.7272 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 60095440)
    (at 74.6125 64.135 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (fp_text reference C22 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 470pF (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C22-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Device_VN:SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm (layer F.Cu) (tedit 5EB70B43)
    (at 53.975 53.975)
    (descr "Soldered wire connection, for a single 0.75 mm² wire, basic insulation, conductor diameter 1.25mm, outer diameter 2.3mm, size source Multi-Contact FLEXI-E 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (attr virtual)
    (fp_text reference F1 (at 0 -2.2225) (layer F.SilkS))
    (fp_text value pad (at 0 2.47) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.098039)
      (net 3 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Device_VN:SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm (layer F.Cu) (tedit 5EB70B43)
    (at 59.69 53.975)
    (descr "Soldered wire connection, for a single 0.75 mm² wire, basic insulation, conductor diameter 1.25mm, outer diameter 2.3mm, size source Multi-Contact FLEXI-E 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (attr virtual)
    (fp_text reference F2 (at 0 -2.2225) (layer F.SilkS))
    (fp_text value pad (at 0 2.47) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.098039)
      (net 10 "Net-(F2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Device_VN:SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm (layer F.Cu) (tedit 5EB70B43)
    (at 134.3025 58.7375 180)
    (descr "Soldered wire connection, for a single 0.75 mm² wire, basic insulation, conductor diameter 1.25mm, outer diameter 2.3mm, size source Multi-Contact FLEXI-E 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (attr virtual)
    (fp_text reference GND (at -2.2225 0 90) (layer F.SilkS))
    (fp_text value pad (at 0 2.47) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.098039)
      (net 6 GND))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 53.975 74.295 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 10M (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 60.96 78.105 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 2k2 (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 60.96 74.295 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 +9VA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 57.4675 66.675 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 10M (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 57.4675 78.105 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 1M (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BI1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 69.215 78.105 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 1k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C22-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 79.0575 78.105 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 64.4525 59.055 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 1M (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 +9VA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 64.4525 70.485 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 1M (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 600953E3)
    (at 134.3025 62.23 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R33 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 100R (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 +9VA))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 +9V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Device_VN:SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm (layer F.Cu) (tedit 5EB70B43)
    (at 134.3025 73.3425 90)
    (descr "Soldered wire connection, for a single 0.75 mm² wire, basic insulation, conductor diameter 1.25mm, outer diameter 2.3mm, size source Multi-Contact FLEXI-E 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (attr virtual)
    (fp_text reference V+ (at 0 2.2225 90) (layer F.SilkS))
    (fp_text value pad (at 0 2.47 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.098039)
      (net 12 +9V))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x01_D1.25mm_OD2.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Wizard Fuzz" (at 66.675 83.5025 90) (layer F.SilkS))
  (gr_line (start 50.8 88.9) (end 50.8 50.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.4775 88.9) (end 50.8 88.9) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.4775 50.8) (end 137.4775 88.9) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 50.8 50.8) (end 137.4775 50.8) (layer Edge.Cuts) (width 0.05))
  (zone (net 40) (net_name +9VA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.127))
    (polygon
      (pts
        (xy 137.16 88.265) (xy 51.435 88.265) (xy 51.435 51.435) (xy 137.16 51.435)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.127))
    (polygon
      (pts
        (xy 137.16 88.265) (xy 51.435 88.265) (xy 51.435 51.435) (xy 137.16 51.435)
      )
    )
  )
)
