(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(A1-Pad1)")
  (net 2 "unconnected-(A1-Pad2)")
  (net 3 "unconnected-(A1-Pad3)")
  (net 4 "GND")
  (net 5 "Net-(A1-Pad5)")
  (net 6 "Net-(A1-Pad6)")
  (net 7 "Net-(A1-Pad7)")
  (net 8 "Net-(A1-Pad8)")
  (net 9 "Net-(A1-Pad9)")
  (net 10 "unconnected-(A1-Pad11)")
  (net 11 "unconnected-(A1-Pad12)")
  (net 12 "unconnected-(A1-Pad13)")
  (net 13 "unconnected-(A1-Pad15)")
  (net 14 "unconnected-(A1-Pad16)")
  (net 15 "unconnected-(A1-Pad17)")
  (net 16 "unconnected-(A1-Pad18)")
  (net 17 "unconnected-(A1-Pad19)")
  (net 18 "unconnected-(A1-Pad20)")
  (net 19 "unconnected-(A1-Pad21)")
  (net 20 "Net-(A1-Pad22)")
  (net 21 "Net-(A1-Pad23)")
  (net 22 "Net-(A1-Pad24)")
  (net 23 "Net-(A1-Pad25)")
  (net 24 "unconnected-(A1-Pad28)")
  (net 25 "Net-(A1-Pad30)")
  (net 26 "Net-(C1-Pad2)")
  (net 27 "Net-(R3-Pad2)")
  (net 28 "unconnected-(U3-Pad9)")
  (net 29 "unconnected-(U3-Pad10)")
  (net 30 "unconnected-(U3-Pad15)")
  (net 31 "unconnected-(U3-Pad16)")
  (net 32 "Net-(R4-Pad1)")
  (net 33 "unconnected-(U4-Pad4)")
  (net 34 "unconnected-(U5-Pad4)")
  (net 35 "unconnected-(U6-Pad4)")
  (net 36 "unconnected-(J2-Pad0)")
  (net 37 "Net-(R5-Pad1)")
  (net 38 "Net-(R6-Pad1)")
  (net 39 "Net-(A1-Pad14)")
  (net 40 "Net-(R15-Pad2)")
  (net 41 "Net-(R16-Pad2)")
  (net 42 "Net-(R17-Pad2)")
  (net 43 "Net-(R18-Pad2)")
  (net 44 "Net-(R19-Pad2)")
  (net 45 "Net-(R20-Pad1)")
  (net 46 "Net-(R21-Pad1)")
  (net 47 "Net-(R22-Pad1)")
  (net 48 "Net-(R23-Pad1)")
  (net 49 "Net-(R24-Pad1)")
  (net 50 "Net-(R25-Pad1)")
  (net 51 "Net-(R26-Pad1)")
  (net 52 "Net-(R27-Pad1)")
  (net 53 "Net-(R28-Pad1)")
  (net 54 "Net-(R29-Pad1)")
  (net 55 "Net-(R30-Pad1)")
  (net 56 "Net-(R31-Pad1)")
  (net 57 "Net-(R32-Pad1)")
  (net 58 "Net-(R33-Pad1)")
  (net 59 "Net-(R34-Pad1)")
  (net 60 "Net-(R35-Pad1)")
  (net 61 "Net-(R36-Pad1)")
  (net 62 "Net-(R37-Pad1)")
  (net 63 "Net-(U13-Pad2)")
  (net 64 "Net-(U3-Pad7)")
  (net 65 "Net-(U14-Pad2)")
  (net 66 "Net-(U15-Pad2)")
  (net 67 "Net-(U17-Pad2)")
  (net 68 "Net-(U16-Pad2)")
  (net 69 "unconnected-(U8-Pad9)")
  (net 70 "unconnected-(U8-Pad10)")
  (net 71 "unconnected-(U8-Pad15)")
  (net 72 "unconnected-(U8-Pad16)")
  (net 73 "Net-(U18-Pad2)")
  (net 74 "Net-(U19-Pad2)")
  (net 75 "Net-(U21-Pad2)")
  (net 76 "Net-(U20-Pad2)")
  (net 77 "unconnected-(U9-Pad9)")
  (net 78 "unconnected-(U9-Pad10)")
  (net 79 "unconnected-(U9-Pad15)")
  (net 80 "unconnected-(U9-Pad16)")
  (net 81 "Net-(U10-Pad2)")
  (net 82 "Net-(U10-Pad4)")
  (net 83 "Net-(U10-Pad7)")
  (net 84 "unconnected-(U10-Pad9)")
  (net 85 "unconnected-(U10-Pad10)")
  (net 86 "unconnected-(U10-Pad15)")
  (net 87 "unconnected-(U10-Pad16)")
  (net 88 "unconnected-(U11-Pad9)")
  (net 89 "unconnected-(U11-Pad10)")
  (net 90 "unconnected-(U11-Pad15)")
  (net 91 "unconnected-(U11-Pad16)")
  (net 92 "Net-(U12-Pad2)")
  (net 93 "Net-(J2-Pad2)")
  (net 94 "Net-(J2-Pad12)")
  (net 95 "Net-(J2-Pad24)")
  (net 96 "unconnected-(U12-Pad9)")
  (net 97 "unconnected-(U12-Pad10)")
  (net 98 "unconnected-(U12-Pad15)")
  (net 99 "unconnected-(U12-Pad16)")
  (net 100 "unconnected-(U13-Pad4)")
  (net 101 "unconnected-(U15-Pad4)")
  (net 102 "unconnected-(U16-Pad4)")
  (net 103 "unconnected-(U17-Pad4)")
  (net 104 "unconnected-(U18-Pad4)")
  (net 105 "unconnected-(U19-Pad4)")
  (net 106 "unconnected-(U20-Pad4)")
  (net 107 "unconnected-(U21-Pad4)")
  (net 108 "unconnected-(U22-Pad4)")
  (net 109 "unconnected-(U23-Pad4)")
  (net 110 "unconnected-(U24-Pad4)")
  (net 111 "unconnected-(U25-Pad4)")
  (net 112 "unconnected-(U26-Pad4)")
  (net 113 "unconnected-(U27-Pad4)")
  (net 114 "unconnected-(U28-Pad4)")
  (net 115 "unconnected-(U29-Pad4)")
  (net 116 "unconnected-(U30-Pad4)")
  (net 117 "Net-(A1-Pad27)")
  (net 118 "Net-(J2-Pad1)")
  (net 119 "Net-(J2-Pad25)")
  (net 120 "Net-(J2-Pad3)")
  (net 121 "Net-(J2-Pad4)")
  (net 122 "Net-(J2-Pad5)")
  (net 123 "Net-(J2-Pad6)")
  (net 124 "Net-(J2-Pad7)")
  (net 125 "Net-(J2-Pad8)")
  (net 126 "Net-(J2-Pad9)")
  (net 127 "Net-(J2-Pad10)")
  (net 128 "Net-(R38-Pad1)")
  (net 129 "unconnected-(J2-Pad13)")
  (net 130 "Net-(J2-Pad11)")
  (net 131 "Net-(J2-Pad14)")
  (net 132 "Net-(J2-Pad15)")
  (net 133 "Net-(J2-Pad16)")
  (net 134 "Net-(J2-Pad17)")
  (net 135 "Net-(J2-Pad18)")
  (net 136 "Net-(J2-Pad19)")
  (net 137 "Net-(J2-Pad20)")
  (net 138 "Net-(J2-Pad21)")
  (net 139 "Net-(J2-Pad22)")
  (net 140 "Net-(R39-Pad1)")
  (net 141 "Net-(R40-Pad1)")
  (net 142 "Net-(J2-Pad23)")
  (net 143 "Net-(J3-Pad1)")
  (net 144 "Net-(R8-Pad1)")
  (net 145 "Net-(A1-Pad26)")
  (net 146 "Net-(R7-Pad1)")
  (net 147 "Net-(A1-Pad10)")
  (net 148 "unconnected-(U14-Pad4)")
  (net 149 "Net-(U3-Pad4)")
  (net 150 "Net-(U3-Pad5)")
  (net 151 "Net-(U10-Pad5)")
  (net 152 "Net-(U11-Pad2)")
  (net 153 "Net-(U11-Pad4)")
  (net 154 "Net-(U11-Pad5)")
  (net 155 "Net-(U11-Pad7)")
  (net 156 "Net-(U12-Pad5)")
  (net 157 "unconnected-(U2-Pad4)")
  (net 158 "Net-(U12-Pad4)")
  (net 159 "Net-(U12-Pad7)")
  (net 160 "unconnected-(U31-Pad4)")
  (net 161 "unconnected-(U32-Pad4)")
  (net 162 "Net-(C9-Pad1)")
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.25 85.725 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at 0 -1.905 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(R19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 85.725 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U32" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "Net-(R40-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "Net-(U12-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "Net-(J2-Pad25)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 161 "unconnected-(U32-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "Net-(U12-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 104.14 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R36" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(R36-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 142 "Net-(J2-Pad23)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.785 119.38 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(A1-Pad27)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 169.545 83.185 90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U8" (at 0 -3.45 90) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(U17-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(R15-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(U16-Pad2)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(U14-Pad2)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(R15-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(U15-Pad2)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(A1-Pad9)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "unconnected-(U8-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "unconnected-(U8-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "unconnected-(U8-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "unconnected-(U8-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.325 119.38 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(A1-Pad27)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.25 80.645 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 1.905 270) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 185.42 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U13" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(R20-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(U13-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "Net-(J2-Pad15)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "unconnected-(U13-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(U13-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 128.905 83.185 90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U10" (at 0 -3.45 90) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(U10-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(R17-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "Net-(U10-Pad4)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 151 "Net-(U10-Pad5)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(R17-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(U10-Pad7)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(A1-Pad7)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "unconnected-(U10-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "unconnected-(U10-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "unconnected-(U10-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "unconnected-(U10-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 172.72 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(R22-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "Net-(J2-Pad16)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 152.4 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U19" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(R26-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Net-(U19-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "Net-(J2-Pad18)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "unconnected-(U19-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Net-(U19-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.665 80.645 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0.14058 1.905 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 190.119 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V3" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "Net-(J2-Pad2)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "Net-(J2-Pad15)") (pintype "bidirectional"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 115.57 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U26" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "Net-(R33-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "Net-(U11-Pad5)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "Net-(J2-Pad9)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "unconnected-(U26-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "Net-(U11-Pad5)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 165.1 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R24" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(R24-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "Net-(J2-Pad17)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 185.42 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(R20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "Net-(J2-Pad15)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.14 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R35" (at 1.715 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(R35-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "Net-(J2-Pad10)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 153.67 78.105 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at -2.54 0.635 270) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(A1-Pad8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 92.075 135.325)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0.14058 -1.34) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 196.85 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(R4-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "Net-(U3-Pad5)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "Net-(J2-Pad1)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "unconnected-(U4-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "Net-(U3-Pad5)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 200.279 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V1" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "Net-(J2-Pad1)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "Net-(J2-Pad14)") (pintype "bidirectional"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.155 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R37" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(R37-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 130 "Net-(J2-Pad11)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-223_ST_LIT:SOT-223_ST_LIT" (layer "F.Cu")
    (tedit 0)
    (at 93.98 129.61 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -0.07 -5.08 -90) (layer "F.SilkS"))
    (fp_text value "LT3088EST-PBF" (at -5.785 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0 0 -90) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 -90) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.2987 3.4925 270) (size 0.889 1.016) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "Net-(C9-Pad1)") (pinfunction "SET") (pintype "input"))
    (pad "2" smd rect (at 0 3.4925 270) (size 0.889 1.016) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(A1-Pad25)") (pinfunction "OUT") (pintype "output"))
    (pad "3" smd rect (at 2.2987 3.4925 270) (size 0.889 1.016) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "Net-(A1-Pad27)") (pinfunction "IN") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.505 138.505001 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at -0.559999 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0.1" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 144 "Net-(R8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 129.159 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V15" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "Net-(J2-Pad8)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "Net-(J2-Pad21)") (pintype "bidirectional"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 133.35 78.105 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at -2.54 0.635 270) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(A1-Pad7)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 139.319 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V13" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "Net-(J2-Pad7)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "Net-(J2-Pad20)") (pintype "bidirectional"))
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 195.199 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V2" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "Net-(J2-Pad14)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "Net-(J2-Pad2)") (pintype "bidirectional"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 173.99 78.105 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at -2.54 0.635 270) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(A1-Pad9)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.665 85.725 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at 0 -1.905 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(R18-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm" (layer "F.Cu")
    (tedit 59FEDEE2)
    (at 204.659669 98.945 90)
    (descr "25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -16.62 -3.7 90) (layer "F.SilkS"))
    (fp_text value "DB25_Female_MountingHoles" (at -16.62 15.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -16.62 11.265 90) (layer "F.Fab"))
    (pad "0" thru_hole circle (at 6.93 0.3 90) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 36 "unconnected-(J2-Pad0)") (pinfunction "PAD") (pintype "passive"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 118 "Net-(J2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.77 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(J2-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.54 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 120 "Net-(J2-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -8.31 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 121 "Net-(J2-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -11.08 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 122 "Net-(J2-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -13.85 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 123 "Net-(J2-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at -16.62 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 "Net-(J2-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at -19.39 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 125 "Net-(J2-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at -22.16 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 126 "Net-(J2-Pad9)") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole circle (at -24.93 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 127 "Net-(J2-Pad10)") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole circle (at -27.7 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 130 "Net-(J2-Pad11)") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole circle (at -30.47 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(J2-Pad12)") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole circle (at -33.24 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 129 "unconnected-(J2-Pad13)") (pinfunction "13") (pintype "passive"))
    (pad "14" thru_hole circle (at -1.385 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 131 "Net-(J2-Pad14)") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole circle (at -4.155 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 132 "Net-(J2-Pad15)") (pinfunction "P15") (pintype "passive"))
    (pad "16" thru_hole circle (at -6.925 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 133 "Net-(J2-Pad16)") (pinfunction "P16") (pintype "passive"))
    (pad "17" thru_hole circle (at -9.695 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 134 "Net-(J2-Pad17)") (pinfunction "P17") (pintype "passive"))
    (pad "18" thru_hole circle (at -12.465 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 135 "Net-(J2-Pad18)") (pinfunction "P18") (pintype "passive"))
    (pad "19" thru_hole circle (at -15.235 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 136 "Net-(J2-Pad19)") (pinfunction "P19") (pintype "passive"))
    (pad "20" thru_hole circle (at -18.005 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 137 "Net-(J2-Pad20)") (pinfunction "P20") (pintype "passive"))
    (pad "21" thru_hole circle (at -20.775 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 138 "Net-(J2-Pad21)") (pinfunction "P21") (pintype "passive"))
    (pad "22" thru_hole circle (at -23.545 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 139 "Net-(J2-Pad22)") (pinfunction "P22") (pintype "passive"))
    (pad "23" thru_hole circle (at -26.315 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 142 "Net-(J2-Pad23)") (pinfunction "P23") (pintype "passive"))
    (pad "24" thru_hole circle (at -29.085 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(J2-Pad24)") (pinfunction "P24") (pintype "passive"))
    (pad "25" thru_hole circle (at -31.855 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 119 "Net-(J2-Pad25)") (pinfunction "P25") (pintype "passive"))
    (pad "26" thru_hole circle (at -40.17 0.3 90) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 172.72 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U15" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "Net-(R22-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(U15-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "Net-(J2-Pad16)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "unconnected-(U15-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(U15-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 194.945 85.725 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.905 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 174.625 80.645 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 1.905 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 128.27 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U24" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "Net-(R31-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "Net-(U10-Pad4)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "Net-(J2-Pad8)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "unconnected-(U24-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "Net-(U10-Pad4)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 135.89 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R29" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(R29-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(J2-Pad7)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 103.759 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V20" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "Net-(J2-Pad23)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "Net-(J2-Pad11)") (pintype "bidirectional"))
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 113.919 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V18" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "Net-(J2-Pad22)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "Net-(J2-Pad10)") (pintype "bidirectional"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 174.625 85.725 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.905 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(R15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 134.239 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V14" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "Net-(J2-Pad20)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "Net-(J2-Pad8)") (pintype "bidirectional"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 89.535 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U31" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "Net-(R39-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "Net-(U12-Pad4)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "Net-(J2-Pad12)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "unconnected-(U31-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "Net-(U12-Pad4)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 189.865 83.185 90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 -3.45 90) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(U13-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(R3-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 149 "Net-(U3-Pad4)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 150 "Net-(U3-Pad5)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(R3-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(U3-Pad7)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 147 "Net-(A1-Pad10)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "unconnected-(U3-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "unconnected-(U3-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "unconnected-(U3-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "unconnected-(U3-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 174.879 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V6" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "Net-(J2-Pad16)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "Net-(J2-Pad4)") (pintype "bidirectional"))
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 88.519 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V23" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "Net-(J2-Pad12)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "Net-(J2-Pad25)") (pintype "bidirectional"))
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 144.399 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V12" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "Net-(J2-Pad19)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "Net-(J2-Pad7)") (pintype "bidirectional"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 96.52 135.325 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0 1.34 180) (layer "F.SilkS"))
    (fp_text value "100u" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 162 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 85.725 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R40" (at 1.705 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 141 "Net-(R40-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "Net-(J2-Pad25)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 164.719 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V8" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "Net-(J2-Pad17)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "Net-(J2-Pad5)") (pintype "bidirectional"))
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 169.799 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V7" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "Net-(J2-Pad4)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "Net-(J2-Pad17)") (pintype "bidirectional"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 93.345 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R38" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "Net-(R38-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "Net-(J2-Pad24)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 104.14 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U29" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(R36-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "Net-(U11-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "Net-(J2-Pad23)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "unconnected-(U29-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "Net-(U11-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 154.559 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V10" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "Net-(J2-Pad18)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "Net-(J2-Pad6)") (pintype "bidirectional"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.315 134.55 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -0.14058 1.759999) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(A1-Pad27)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 196.85 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "Net-(J2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 93.345 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U30" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "Net-(R38-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "Net-(U12-Pad7)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "Net-(J2-Pad24)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "unconnected-(U30-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "Net-(U12-Pad7)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 144.78 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U21" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(R28-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "Net-(U21-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "Net-(J2-Pad19)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "unconnected-(U21-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "Net-(U21-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 89.535 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R39" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 140 "Net-(R39-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(J2-Pad12)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 148.59 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U20" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(R27-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "Net-(U20-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "Net-(J2-Pad6)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "unconnected-(U20-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "Net-(U20-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 168.91 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R23" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(R23-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(J2-Pad4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 132.08 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U23" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(R30-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(U10-Pad7)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "Net-(J2-Pad20)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "unconnected-(U23-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(U10-Pad7)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Module:Arduino_Nano" (layer "F.Cu")
    (tedit 58ACAF70)
    (at 75.565 95.25 -90)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "A1" (at 0 -5.08) (layer "F.SilkS"))
    (fp_text value "Arduino_Nano_v3.x" (at 8.89 19.05) (layer "F.Fab"))
    (fp_text user "USB" (at 7.62 35.56 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.35 19.05) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "unconnected-(A1-Pad1)") (pinfunction "D1/TX") (pintype "bidirectional"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "unconnected-(A1-Pad2)") (pinfunction "D0/RX") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "unconnected-(A1-Pad3)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad5)") (pinfunction "D2") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad6)") (pinfunction "D3") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad7)") (pinfunction "D4") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad8)") (pinfunction "D5") (pintype "bidirectional"))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad9)") (pinfunction "D6") (pintype "bidirectional"))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 147 "Net-(A1-Pad10)") (pinfunction "D7") (pintype "bidirectional"))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "unconnected-(A1-Pad11)") (pinfunction "D8") (pintype "bidirectional"))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "unconnected-(A1-Pad12)") (pinfunction "D9") (pintype "bidirectional"))
    (pad "13" thru_hole oval (at 0 30.48 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "unconnected-(A1-Pad13)") (pinfunction "D10") (pintype "bidirectional"))
    (pad "14" thru_hole oval (at 0 33.02 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(A1-Pad14)") (pinfunction "D11") (pintype "bidirectional"))
    (pad "15" thru_hole oval (at 0 35.56 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(A1-Pad15)") (pinfunction "D12") (pintype "bidirectional"))
    (pad "16" thru_hole oval (at 15.24 35.56 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "unconnected-(A1-Pad16)") (pinfunction "D13") (pintype "bidirectional"))
    (pad "17" thru_hole oval (at 15.24 33.02 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "unconnected-(A1-Pad17)") (pinfunction "3V3") (pintype "power_out"))
    (pad "18" thru_hole oval (at 15.24 30.48 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "unconnected-(A1-Pad18)") (pinfunction "AREF") (pintype "input"))
    (pad "19" thru_hole oval (at 15.24 27.94 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "unconnected-(A1-Pad19)") (pinfunction "A0") (pintype "bidirectional"))
    (pad "20" thru_hole oval (at 15.24 25.4 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "unconnected-(A1-Pad20)") (pinfunction "A1") (pintype "bidirectional"))
    (pad "21" thru_hole oval (at 15.24 22.86 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "unconnected-(A1-Pad21)") (pinfunction "A2") (pintype "bidirectional"))
    (pad "22" thru_hole oval (at 15.24 20.32 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad22)") (pinfunction "A3") (pintype "bidirectional"))
    (pad "23" thru_hole oval (at 15.24 17.78 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad23)") (pinfunction "A4") (pintype "bidirectional"))
    (pad "24" thru_hole oval (at 15.24 15.24 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad24)") (pinfunction "A5") (pintype "bidirectional"))
    (pad "25" thru_hole oval (at 15.24 12.7 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad25)") (pinfunction "A6") (pintype "bidirectional"))
    (pad "26" thru_hole oval (at 15.24 10.16 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 145 "Net-(A1-Pad26)") (pinfunction "A7") (pintype "bidirectional"))
    (pad "27" thru_hole oval (at 15.24 7.62 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 117 "Net-(A1-Pad27)") (pinfunction "+5V") (pintype "power_out"))
    (pad "28" thru_hole oval (at 15.24 5.08 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 24 "unconnected-(A1-Pad28)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "29" thru_hole oval (at 15.24 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "30" thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad30)") (pinfunction "VIN") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Module.3dshapes/Arduino_Nano_WithMountingHoles.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 189.23 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U6" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(R6-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "Net-(U3-Pad4)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "Net-(J2-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "unconnected-(U6-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "Net-(U3-Pad4)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 111.76 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U27" (at 0 -0.635) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.508 -0.127) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "Net-(R34-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "Net-(U11-Pad7)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "Net-(J2-Pad22)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "unconnected-(U27-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "Net-(U11-Pad7)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 94.615 78.105 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at -2.54 0.635 270) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(A1-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 176.53 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(R21-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "Net-(J2-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 124.079 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V16" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "Net-(J2-Pad21)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "Net-(J2-Pad9)") (pintype "bidirectional"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.76 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R34" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(R34-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 139 "Net-(J2-Pad22)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.46 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R32" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(R32-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "Net-(J2-Pad21)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 149.225 83.185 90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U9" (at 0 -3.45 90) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(U21-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(R16-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(U20-Pad2)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(U18-Pad2)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(R16-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(U19-Pad2)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(A1-Pad8)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "unconnected-(U9-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "unconnected-(U9-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "unconnected-(U9-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "unconnected-(U9-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 149.479 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V11" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "Net-(J2-Pad6)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "Net-(J2-Pad19)") (pintype "bidirectional"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 65.405 120.015 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at -2.54 0 180) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 146 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 145 "Net-(A1-Pad26)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 156.21 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R25" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(R25-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 122 "Net-(J2-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.03 78.105 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at -2.54 0.635 270) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(A1-Pad6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 135.89 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U22" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(R29-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "Net-(U10-Pad5)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "Net-(J2-Pad7)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "unconnected-(U22-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "Net-(U10-Pad5)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 176.53 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U14" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(R21-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "Net-(U14-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "Net-(J2-Pad3)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "unconnected-(U14-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "Net-(U14-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 107.95 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U28" (at 0 -0.635) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.635 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Net-(R35-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "Net-(U11-Pad4)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "Net-(J2-Pad10)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "unconnected-(U28-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "Net-(U11-Pad4)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 152.4 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R26" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(R26-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 135 "Net-(J2-Pad18)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 97.155 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "Net-(R37-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "Net-(U12-Pad5)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "Net-(J2-Pad11)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "unconnected-(U2-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "Net-(U12-Pad5)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 108.839 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V19" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "Net-(J2-Pad10)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "Net-(J2-Pad23)") (pintype "bidirectional"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 165.1 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U17" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(R24-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(U17-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "Net-(J2-Pad17)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "unconnected-(U17-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(U17-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "D22012_B_NKK:D22012_B_NKK" (layer "F.Cu")
    (tedit 0)
    (at 74.93 129.54 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 12.065 -4.421774 180) (layer "F.SilkS"))
    (fp_text value "D22018B" (at 0 -4.421774 180) (layer "F.SilkS"))
    (fp_text user "*" (at -0.635 -1.905 180) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 180) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad25)") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 5.08 0 180) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask)
      (net 144 "Net-(R8-Pad1)") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 10.16 0 180) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask)
      (net 143 "Net-(J3-Pad1)") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at -2.54 -2.54 180) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "5" thru_hole circle (at 12.7 -2.54 180) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "6" thru_hole circle (at -2.54 2.54 180) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "7" thru_hole circle (at 12.7 2.54 180) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 90.17 83.185 90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U12" (at 0 -3.45 90) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(U12-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(R19-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 158 "Net-(U12-Pad4)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 156 "Net-(U12-Pad5)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(R19-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 159 "Net-(U12-Pad7)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(A1-Pad5)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "unconnected-(U12-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "unconnected-(U12-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "unconnected-(U12-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "unconnected-(U12-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 189.23 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(R6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(J2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 193.04 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(R5-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "Net-(U3-Pad7)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "Net-(J2-Pad14)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "unconnected-(U5-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "Net-(U3-Pad7)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 118.999 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V17" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "Net-(J2-Pad9)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "Net-(J2-Pad22)") (pintype "bidirectional"))
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 108.585 83.185 90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U11" (at 0 -3.81 270) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 152 "Net-(U11-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(R18-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 153 "Net-(U11-Pad4)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 154 "Net-(U11-Pad5)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(R18-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 155 "Net-(U11-Pad7)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(A1-Pad6)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "unconnected-(U11-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "unconnected-(U11-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "unconnected-(U11-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "unconnected-(U11-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 98.679 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V21" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "Net-(J2-Pad11)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "Net-(J2-Pad24)") (pintype "bidirectional"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 154.305 80.645 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 1.905 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 194.31 78.105 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at -2.54 0 270) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 147 "Net-(A1-Pad10)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 168.91 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U16" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(R23-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(U16-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "Net-(J2-Pad4)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "unconnected-(U16-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(U16-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 93.599 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V22" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "Net-(J2-Pad24)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "Net-(J2-Pad12)") (pintype "bidirectional"))
  )
  (footprint "Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal" (layer "F.Cu")
    (tedit 5C13907B)
    (at 46.99 129.563226 90)
    (descr "http://www.farnell.com/datasheets/612848.pdf")
    (tags "BNC Amphenol Horizontal")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 4 90) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial_Power" (at 0 6 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 143 "Net-(J3-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 -5.08 90) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 90) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole oval (at -5.08 -5.08 90) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 154.305 85.915 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at -0.19 -1.905 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(R16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DCK0006A_N:DCK0006A_N" (layer "F.Cu")
    (tedit 0)
    (at 106.68 138.36 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U7" (at -0.565 -2.54 -90) (layer "F.SilkS"))
    (fp_text value "INA213AIDCKT" (at 3.048 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0 0 -90) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 -90) (layer "Cmts.User"))
    (fp_text user ".Designator" (at -0.0508 -0.6604 180) (layer "Cmts.User"))
    (fp_text user ".Designator" (at -0.0508 -0.6604 180) (layer "F.Fab"))
    (fp_text user "*" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.124999 -0.650001) (size 0.399999 0.850001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "REF") (pintype "input"))
    (pad "2" smd rect (at -1.124999 0) (size 0.399999 0.850001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -1.124999 0.649999) (size 0.399999 0.850001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "Net-(A1-Pad27)") (pinfunction "V+") (pintype "power_in"))
    (pad "4" smd rect (at 1.125002 0.649999) (size 0.399999 0.850001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "Net-(R8-Pad1)") (pinfunction "IN+") (pintype "input"))
    (pad "5" smd rect (at 1.125002 0) (size 0.399999 0.850001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(C1-Pad2)") (pinfunction "IN-") (pintype "input"))
    (pad "6" smd rect (at 1.125002 -0.650001) (size 0.399999 0.850001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "Net-(R7-Pad1)") (pinfunction "OUT") (pintype "output"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 133.985 85.915 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at -0.19 -1.905 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(R17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 159.639 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V9" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "Net-(J2-Pad5)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "Net-(J2-Pad18)") (pintype "bidirectional"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.27 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R31" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(R31-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(J2-Pad8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 148.59 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R27" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(R27-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "Net-(J2-Pad6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 194.945 80.645 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 1.905 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 124.46 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U25" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "Net-(R32-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "Net-(U10-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "Net-(J2-Pad21)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "unconnected-(U25-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "Net-(U10-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.57 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R33" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(R33-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "Net-(J2-Pad9)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 179.959 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V5" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "Net-(J2-Pad3)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "Net-(J2-Pad16)") (pintype "bidirectional"))
  )
  (footprint "myVaristor:AVX_0805" (layer "F.Cu")
    (tedit 0)
    (at 185.039 95.885 180)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V4" (at 2.032 -1.778 180 unlocked) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 1.524 1.778 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "Net-(J2-Pad15)") (pintype "bidirectional"))
    (pad "2" smd rect (at 3.048 0 180) (size 1.016 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "Net-(J2-Pad3)") (pintype "bidirectional"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 156.21 90.805 -90)
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U18" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 -90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(R25-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "Net-(U18-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "Net-(J2-Pad5)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "unconnected-(U18-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "Net-(U18-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 133.985 80.645 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at -0.14058 1.905 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 99.695 134.62 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R41" (at 0 1.905 270) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 162 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(A1-Pad14)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_BarrelJack:BarrelJack_CUI_PJ-063AH_Horizontal" (layer "F.Cu")
    (tedit 5B0886BD)
    (at 46.14 80.01 -90)
    (descr "Barrel Jack, 2.0mm ID, 5.5mm OD, 24V, 8A, no switch, https://www.cui.com/product/resource/pj-063ah.pdf")
    (tags "barrel jack cui dc power")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.755 90) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial_Power" (at 0 13 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.5 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 9 270) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 270) (size 4 2) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad30)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 6 270) (size 3.3 2) (drill oval 2.3 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "MP" thru_hole oval (at 4.5 7 270) (size 2 3.5) (drill oval 1 2.5) (layers *.Cu *.Mask))
    (pad "MP" thru_hole oval (at -4.5 7 270) (size 2 3.5) (drill oval 1 2.5) (layers *.Cu *.Mask))
    (model "${KICAD6_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-063AH_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 144.78 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R28" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(R28-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 136 "Net-(J2-Pad19)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.08 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R30" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(R30-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 137 "Net-(J2-Pad20)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 193.04 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "Net-(J2-Pad14)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 215.9 69.215) (end 32.385 147.32) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "SLAC National Accelerator Laboratory\nRF switch control board \nv2.0 - 02/23/2023\nTaj Dyson (tdyson@stanford.edu)" (at 158.115 138.43) (layer "F.SilkS"))
  (gr_text "CHECK SWITCH BEFORE \nCONNECTING POWER!" (at 71.755 142.24) (layer "F.SilkS"))
  (gr_text "ARD" (at 57.15 129.54) (layer "F.SilkS"))
  (gr_text "EXT" (at 82.55 129.54) (layer "F.SilkS"))
  (zone (net 4) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 214.631761 70.47558)
        (xy 214.630015 146.073313)
        (xy 33.655 146.073226)
        (xy 33.656746 70.498719)
      )
    )
  )
)
