(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 67)
    (no_connects 9)
    (area 94.687429 69.131 192.305715 135.415001)
    (thickness 1.6)
    (drawings 28)
    (tracks 121)
    (zones 0)
    (modules 28)
    (nets 28)
  )
  (page A4)
  (title_block
    (title "Teensy Base PCB")
    (rev 1a)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P_UART1-Pad3)")
  (net 2 "Net-(P_UART1-Pad4)")
  (net 3 NC)
  (net 4 "Net-(U3-Pad10)")
  (net 5 "Net-(U3-Pad11)")
  (net 6 "Net-(U3-Pad12)")
  (net 7 "Net-(U3-Pad13)")
  (net 8 "Net-(U3-Pad14)")
  (net 9 "Net-(P_DISP1-Pad1)")
  (net 10 "Net-(P_DISP1-Pad2)")
  (net 11 GND)
  (net 12 +9V)
  (net 13 +5V)
  (net 14 +3.3V)
  (net 15 "Net-(SW_DN1-Pad2)")
  (net 16 "Net-(SW_ENT1-Pad2)")
  (net 17 "Net-(SW_UP1-Pad2)")
  (net 18 "Net-(R1-Pad1)")
  (net 19 ACC2)
  (net 20 ACC1)
  (net 21 "Net-(P_PUMP1-Pad2)")
  (net 22 "Net-(P_PUMP1-Pad1)")
  (net 23 "Net-(U3-Pad20)")
  (net 24 "Net-(U3-Pad21)")
  (net 25 "Net-(U5-Pad6)")
  (net 26 "Net-(C7-Pad1)")
  (net 27 "Net-(P_SERVO1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.1)
    (add_net ACC1)
    (add_net ACC2)
    (add_net NC)
    (add_net "Net-(P_DISP1-Pad1)")
    (add_net "Net-(P_DISP1-Pad2)")
    (add_net "Net-(P_SERVO1-Pad3)")
    (add_net "Net-(P_UART1-Pad3)")
    (add_net "Net-(P_UART1-Pad4)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(SW_DN1-Pad2)")
    (add_net "Net-(SW_ENT1-Pad2)")
    (add_net "Net-(SW_UP1-Pad2)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad20)")
    (add_net "Net-(U3-Pad21)")
    (add_net "Net-(U5-Pad6)")
  )
  (net_class Current ""
    (clearance 0.254)
    (trace_width 1.0668)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.1)
    (add_net +9V)
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(P_PUMP1-Pad1)")
    (add_net "Net-(P_PUMP1-Pad2)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.6096)
    (via_dia 0.9398)
    (via_drill 0.5842)
    (uvia_dia 0.762)
    (uvia_drill 0.1)
    (add_net +3.3V)
    (add_net +5V)
    (add_net GND)
  )
  (module Connect:BARREL_JACK (layer F.Cu) (tedit 5817BD6B)
    (at 110.49 96.52)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference CON_9V1 (at -5.08 0 90) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -3.175) (layer F.Fab))
    (pad 1 thru_hole rect (at 6.20014 0) (size 3.50012 3.50012) (drill 2.99974) (layers *.Cu *.Mask F.SilkS)
      (net 12 +9V))
    (pad 2 thru_hole rect (at 0.20066 0) (size 3.50012 3.50012) (drill 2.99974) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 3 thru_hole rect (at 3.2004 4.699) (size 3.50012 3.50012) (drill 2.99974) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
  )
  (module Socket_Strips:Socket_Strip_Straight_2x04 (layer F.Cu) (tedit 58153747)
    (at 156.21 74.93 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference U4 (at 3.81 -2.54 180) (layer F.SilkS) hide)
    (fp_text value nRF24L01+ (at 3.175 4.445 180) (layer F.Fab))
    (pad 2 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 +3.3V))
    (pad 1 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 4 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(U3-Pad10)"))
    (pad 3 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(U3-Pad14)"))
    (pad 6 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(U3-Pad11)"))
    (pad 5 thru_hole oval (at 5.08 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(U3-Pad13)"))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 NC))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(U3-Pad12)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz 0.15 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module lib:Teensy-3.1 (layer F.Cu) (tedit 58153795)
    (at 139.7 102.87 90)
    (fp_text reference U3 (at 13.335 -7.62 180) (layer F.SilkS) hide)
    (fp_text value Teensy_3.2 (at 5.08 -2.54 90) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P_UART1-Pad3)"))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P_UART1-Pad4)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 NC))
    (pad 3 thru_hole circle (at 7.62 0 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P_SERVO1-Pad3)"))
    (pad 4 thru_hole circle (at 10.16 0 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 NC))
    (pad 5 thru_hole circle (at 12.7 0 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 NC))
    (pad 6 thru_hole circle (at 15.24 0 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(SW_ENT1-Pad2)"))
    (pad 7 thru_hole circle (at 17.78 0 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(SW_DN1-Pad2)"))
    (pad 8 thru_hole circle (at 20.32 0 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(SW_UP1-Pad2)"))
    (pad 9 thru_hole circle (at 22.86 0 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 ACC1))
    (pad 10 thru_hole circle (at 25.4 0 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(U3-Pad10)"))
    (pad 11 thru_hole circle (at 27.94 0 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(U3-Pad11)"))
    (pad 12 thru_hole circle (at 30.48 0 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(U3-Pad12)"))
    (pad 13 thru_hole circle (at 30.48 -15.24 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(U3-Pad13)"))
    (pad 14 thru_hole circle (at 27.94 -15.24 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(U3-Pad14)"))
    (pad 15 thru_hole circle (at 25.4 -15.24 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 NC))
    (pad 16 thru_hole circle (at 22.86 -15.24 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 ACC2))
    (pad 17 thru_hole circle (at 20.32 -15.24 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 NC))
    (pad 18 thru_hole circle (at 17.78 -15.24 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P_DISP1-Pad1)"))
    (pad 19 thru_hole circle (at 15.24 -15.24 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P_DISP1-Pad2)"))
    (pad 20 thru_hole circle (at 12.7 -15.24 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U3-Pad20)"))
    (pad 21 thru_hole circle (at 10.16 -15.24 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U3-Pad21)"))
    (pad 22 thru_hole circle (at 7.62 -15.24 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 NC))
    (pad 23 thru_hole circle (at 5.08 -15.24 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 NC))
    (pad 24 thru_hole circle (at 2.54 -15.24 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 +3.3V))
    (pad 25 thru_hole circle (at 0 -15.24 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 NC))
    (pad 26 thru_hole circle (at -2.54 -15.24 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 NC))
    (pad 27 thru_hole circle (at -2.54 0 90) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 5815377E)
    (at 168.91 118.11)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 3.175 3.175) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_2.5mm locked (layer F.Cu) (tedit 58153789)
    (at 168.91 73.66)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 1.905 -3.175) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 58153776)
    (at 106.68 118.11)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at -3.81 2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Angled_1x03 (layer F.Cu) (tedit 58153BD5)
    (at 162.56 110.49 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P_SERVO1 (at -2.54 3.175 360) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 4.445 -2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 +5V))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P_SERVO1-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x04 (layer F.Cu) (tedit 581536FD)
    (at 144.78 110.49)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P_UART1 (at 3.81 -2.54) (layer F.SilkS))
    (fp_text value CONN_01X04 (at -2.54 4.445 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 +5V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P_UART1-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P_UART1-Pad4)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_1x04.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm locked (layer F.Cu) (tedit 581536B8)
    (at 106.68 73.66)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at -3.175 -2.54) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical_LargePads (layer F.Cu) (tedit 58153691)
    (at 106.68 83.82 90)
    (descr "TO-220, Neutral, Vertical, Large Pads,")
    (tags "TO-220, Neutral, Vertical, Large Pads,")
    (fp_text reference U1 (at 6.35 -0.635 180) (layer F.SilkS))
    (fp_text value LM7805CT (at 0 -2.54 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 +9V))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 +5V))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical_LargePads (layer F.Cu) (tedit 5815369B)
    (at 116.84 73.66)
    (descr "TO-220, Neutral, Vertical, Large Pads,")
    (tags "TO-220, Neutral, Vertical, Large Pads,")
    (fp_text reference U2 (at -6.985 -2.54) (layer F.SilkS))
    (fp_text value LD1117V33 (at 0 -2.54) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 14 +3.3V))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 +5V))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04 (layer F.Cu) (tedit 581536F4)
    (at 135.89 110.49 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P_DISP1 (at -2.54 3.81 360) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 4.445 -1.905 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P_DISP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P_DISP1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 +3.3V))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 58153720)
    (at 161.29 86.36)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference SW_DN1 (at 6.985 1.27) (layer F.SilkS))
    (fp_text value SW_PUSH (at 6.985 -0.635) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(SW_DN1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 5815372C)
    (at 161.29 92.71)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference SW_ENT1 (at 6.985 1.27) (layer F.SilkS))
    (fp_text value SW_PUSH (at 6.985 -0.635) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(SW_ENT1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 58153726)
    (at 161.29 80.01)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference SW_UP1 (at 6.985 1.27) (layer F.SilkS))
    (fp_text value SW_PUSH (at 6.985 -0.635) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(SW_UP1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 58153735)
    (at 159.385 99.06)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5.334 0) (layer F.SilkS))
    (fp_text value 100 (at 5.08 -2.413) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 18 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer B.Cu) (tedit 580AC8BC)
    (at 155.575 100.33 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P_ACC1 (at 0 5.1 90) (layer B.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 3.1 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 14 +3.3V))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 13 +5V))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 11 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer B.Cu) (tedit 580AC8C8)
    (at 150.495 82.55 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P_ACC2 (at 0 5.1 270) (layer B.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 3.1 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 19 ACC2))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 20 ACC1))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 58140FB1)
    (at 115.57 88.9)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 2.54 0) (layer F.SilkS))
    (fp_text value 330nF (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 +9V))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 58140FB5)
    (at 120.65 78.74 270)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 +5V))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 581536C8)
    (at 111.76 85.09)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 2.54 0) (layer F.SilkS))
    (fp_text value 100nF (at 2.54 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 +5V))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
  )
  (module Capacitors_ThroughHole:C_Radial_D8_L13_P3.8 (layer F.Cu) (tedit 58153D10)
    (at 165.1 105.41)
    (descr "Radial Electrolytic Capacitor Diameter 8mm x Length 13mm, Pitch 3.8mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C5 (at -2.54 -3.175) (layer F.SilkS))
    (fp_text value 470uF (at 5.08 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 +5V))
    (pad 2 thru_hole circle (at 3.8 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D8_L13_P3.8.wrl
      (at (xyz 0.0748031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 5815375D)
    (at 161.925 74.93 90)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C6 (at 1.27 3.81 90) (layer F.SilkS))
    (fp_text value 100uF (at -1.27 -3.175 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 +3.3V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer F.Cu) (tedit 581537B4)
    (at 113.03 117.475)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P_PUMP1 (at 8.89 0) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 6.35 -0.635 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P_PUMP1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P_PUMP1-Pad1)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x07 (layer F.Cu) (tedit 5814D92A)
    (at 105.41 110.49)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference U5 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value TA8428K (at 1.905 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U3-Pad20)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U3-Pad21)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P_PUMP1-Pad1)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P_PUMP1-Pad2)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(U5-Pad6)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(C7-Pad1)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x07.wrl
      (at (xyz 0.3 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 58141CDF)
    (at 116.84 79.375 180)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C4 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 2.5 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 +3.3V))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 5814D6C8)
    (at 110.49 105.41 180)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 2.5 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
  )
  (module Fuse_Holders_and_Fuses:Fuse_TE5_Littlefuse-395Series (layer F.Cu) (tedit 581537A5)
    (at 117.475 105.41 180)
    (descr "Fuse, TE5, Littlefuse/Wickmann, No. 460, No560,")
    (tags "Fuse, TE5, Littlefuse/Wickmann, No. 460, No560,")
    (fp_text reference F1 (at 0 0 180) (layer F.SilkS))
    (fp_text value F_Small (at -1.905 3.175 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 +9V))
    (pad 2 thru_hole circle (at 2.54 0.01016 180) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(C7-Pad1)"))
  )
  (dimension 52.07 (width 0.3) (layer Dwgs.User)
    (gr_text "2.0500 in" (at 186.77 95.885 90) (layer Dwgs.User))
    (feature1 (pts (xy 176.53 69.85) (xy 188.12 69.85)))
    (feature2 (pts (xy 176.53 121.92) (xy 188.12 121.92)))
    (crossbar (pts (xy 185.42 121.92) (xy 185.42 69.85)))
    (arrow1a (pts (xy 185.42 69.85) (xy 186.006421 70.976504)))
    (arrow1b (pts (xy 185.42 69.85) (xy 184.833579 70.976504)))
    (arrow2a (pts (xy 185.42 121.92) (xy 186.006421 120.793496)))
    (arrow2b (pts (xy 185.42 121.92) (xy 184.833579 120.793496)))
  )
  (dimension 69.85 (width 0.3) (layer Dwgs.User)
    (gr_text "2.7500 in" (at 137.795 134.065) (layer Dwgs.User))
    (feature1 (pts (xy 172.72 123.825) (xy 172.72 135.415)))
    (feature2 (pts (xy 102.87 123.825) (xy 102.87 135.415)))
    (crossbar (pts (xy 102.87 132.715) (xy 172.72 132.715)))
    (arrow1a (pts (xy 172.72 132.715) (xy 171.593496 133.301421)))
    (arrow1b (pts (xy 172.72 132.715) (xy 171.593496 132.128579)))
    (arrow2a (pts (xy 102.87 132.715) (xy 103.996504 133.301421)))
    (arrow2b (pts (xy 102.87 132.715) (xy 103.996504 132.128579)))
  )
  (gr_text TA8428K (at 107.315 113.665) (layer F.SilkS))
  (dimension 62.23 (width 0.3) (layer Dwgs.User)
    (gr_text "2.4500 in" (at 137.795 128.985) (layer Dwgs.User))
    (feature1 (pts (xy 168.91 123.825) (xy 168.91 130.335)))
    (feature2 (pts (xy 106.68 123.825) (xy 106.68 130.335)))
    (crossbar (pts (xy 106.68 127.635) (xy 168.91 127.635)))
    (arrow1a (pts (xy 168.91 127.635) (xy 167.783496 128.221421)))
    (arrow1b (pts (xy 168.91 127.635) (xy 167.783496 127.048579)))
    (arrow2a (pts (xy 106.68 127.635) (xy 107.806504 128.221421)))
    (arrow2b (pts (xy 106.68 127.635) (xy 107.806504 127.048579)))
  )
  (dimension 44.45 (width 0.3) (layer Dwgs.User)
    (gr_text "1.7500 in" (at 181.69 95.885 270) (layer Dwgs.User))
    (feature1 (pts (xy 176.53 118.11) (xy 183.04 118.11)))
    (feature2 (pts (xy 176.53 73.66) (xy 183.04 73.66)))
    (crossbar (pts (xy 180.34 73.66) (xy 180.34 118.11)))
    (arrow1a (pts (xy 180.34 118.11) (xy 179.753579 116.983496)))
    (arrow1b (pts (xy 180.34 118.11) (xy 180.926421 116.983496)))
    (arrow2a (pts (xy 180.34 73.66) (xy 179.753579 74.786504)))
    (arrow2b (pts (xy 180.34 73.66) (xy 180.926421 74.786504)))
  )
  (gr_line (start 102.87 115.57) (end 102.87 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 115.57) (end 172.72 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text A2 (at 150.495 80.01 90) (layer B.SilkS))
  (gr_text D9 (at 153.035 80.01 90) (layer B.SilkS))
  (gr_text 3.3V (at 155.575 103.505 90) (layer B.SilkS))
  (gr_text 5V (at 153.035 103.505 90) (layer B.SilkS))
  (gr_text GND (at 150.495 103.505 90) (layer B.SilkS))
  (gr_text "Cat Trainer\nrev. 1a" (at 147.955 91.44 90) (layer B.SilkS))
  (gr_text "Cat Trainer\nrev. 1a" (at 147.955 91.44 90) (layer F.SilkS))
  (gr_text nRF24L01 (at 152.4 77.47) (layer F.SilkS))
  (gr_text "Teensy 3" (at 127.508 97.028 90) (layer F.SilkS))
  (gr_line (start 170.18 69.85) (end 105.41 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.41 121.92) (end 170.18 121.92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 72.39) (end 172.72 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.87 72.39) (end 102.87 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 105.41 119.38) (end 105.41 121.92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 105.41 72.39) (end 102.87 72.39) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 170.18 72.39) (end 170.18 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 170.18 119.38) (end 172.72 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 11) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 172.72 121.92) (xy 102.87 121.92) (xy 102.87 69.85) (xy 172.72 69.85)
      )
    )
  )
)
