(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "5V")
  (net 2 "3V3")
  (net 3 "GND")
  (net 4 "IO36")
  (net 5 "IO4")
  (net 6 "TP_INT")
  (net 7 "IO2")
  (net 8 "IO34")
  (net 9 "LCD_CS")
  (net 10 "I2C1_SCL")
  (net 11 "SPI2_MOSI")
  (net 12 "I2C1_SDA")
  (net 13 "ESP32_EN")
  (net 14 "LCD_DC")
  (net 15 "LCD_RST")
  (net 16 "TXD0")
  (net 17 "LCD_BKLT")
  (net 18 "SPI2_MISO")
  (net 19 "IO0")
  (net 20 "SPI2_CLK")
  (net 21 "IO5")
  (net 22 "IO27")
  (net 23 "IO25")
  (net 24 "IO32")
  (net 25 "IO26")
  (net 26 "IO33")
  (net 27 "IO35")
  (footprint "WT32-SC01:WT32-SC01_J6" locked (layer "F.Cu")
    (at 136.597446 97.324554)
    (property "Sheetfile" "WT32-SC01-Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "ESP32 Devboard with 320x480 touchscreen")
    (attr smd)
    (fp_text reference "U1" (at 33.274 -26.9 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WT32-SC01_J6" (at 33.274 -25.4 unlocked) (layer "F.Fab") hide)
    (fp_text user "J5" (at -40.132 22.606 unlocked) (layer "F.SilkS") hide)
    (fp_text user "J6" (at -20.066 25.146 90 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 33.274 -23.9 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at -41.086446 -25.026554) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle locked (at -41.086446 26.273446) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle locked (at 43.033554 -25.026554) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle locked (at 43.033554 26.273446) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect locked (at 19.973554 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "5V") (pinfunction "5V") (pintype "power_in"))
    (pad "2" thru_hole oval locked (at 19.973554 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "5V") (pinfunction "5V") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 17.973554 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "3V3") (pinfunction "3V3") (pintype "power_out"))
    (pad "4" thru_hole oval locked (at 17.973554 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "3V3") (pinfunction "3V3") (pintype "power_out"))
    (pad "5" thru_hole oval locked (at 15.973554 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" thru_hole oval locked (at 15.973554 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" thru_hole oval locked (at 13.973554 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval locked (at 13.973554 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval locked (at 11.973554 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "IO36") (pinfunction "IO36/SENSOR_VP/EM_INT") (pintype "bidirectional"))
    (pad "10" thru_hole oval locked (at 11.973554 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "IO4") (pinfunction "IO4") (pintype "bidirectional"))
    (pad "11" thru_hole oval locked (at 9.973554 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "TP_INT") (pinfunction "J_IO39/SENSOR_VN/TP_INT") (pintype "bidirectional"))
    (pad "12" thru_hole oval locked (at 9.973554 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "IO2") (pinfunction "IO2") (pintype "bidirectional"))
    (pad "13" thru_hole oval locked (at 7.973554 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "IO34") (pinfunction "IO34") (pintype "bidirectional"))
    (pad "14" thru_hole oval locked (at 7.973554 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "LCD_CS") (pinfunction "J_IO15/LCD_CS") (pintype "output"))
    (pad "15" thru_hole oval locked (at 5.973554 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "I2C1_SCL") (pinfunction "J_IO19/I2C1_SCL") (pintype "output"))
    (pad "16" thru_hole oval locked (at 5.973554 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "SPI2_MOSI") (pinfunction "J_IO13/SPI2_MOSI") (pintype "output"))
    (pad "17" thru_hole oval locked (at 3.973554 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "I2C1_SDA") (pinfunction "J_IO18/I2C1_SDA") (pintype "bidirectional"))
    (pad "18" thru_hole oval locked (at 3.973554 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "ESP32_EN") (pinfunction "ESP32_EN") (pintype "input"))
    (pad "19" thru_hole oval locked (at 1.973554 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "LCD_DC") (pinfunction "J_IO21/LCD_DC") (pintype "output"))
    (pad "20" thru_hole oval locked (at 1.973554 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "LCD_RST") (pinfunction "J_IO22/LCD_RESET") (pintype "output"))
    (pad "21" thru_hole oval locked (at -0.026446 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "TXD0") (pinfunction "TXD0") (pintype "output"))
    (pad "22" thru_hole oval locked (at -0.026446 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "LCD_BKLT") (pinfunction "J_IO23/LCD_BKLIGHT") (pintype "output"))
    (pad "23" thru_hole oval locked (at -2.026446 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "SPI2_MISO") (pinfunction "IO12/SPI2_MISO") (pintype "input"))
    (pad "24" thru_hole oval locked (at -2.026446 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "IO0") (pinfunction "IO0") (pintype "bidirectional"))
    (pad "25" thru_hole oval locked (at -4.026446 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "SPI2_CLK") (pinfunction "J_IO14/SPI2_CLK") (pintype "output"))
    (pad "26" thru_hole oval locked (at -4.026446 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "IO5") (pinfunction "IO5") (pintype "bidirectional"))
    (pad "27" thru_hole oval locked (at -6.026446 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "IO27") (pinfunction "IO27") (pintype "bidirectional"))
    (pad "28" thru_hole oval locked (at -6.026446 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "IO25") (pinfunction "IO25/DAC_CHAN1") (pintype "bidirectional"))
    (pad "29" thru_hole oval locked (at -8.026446 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "IO32") (pinfunction "IO32") (pintype "bidirectional"))
    (pad "30" thru_hole oval locked (at -8.026446 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "IO26") (pinfunction "IO26/DAC_CHAN2") (pintype "bidirectional"))
    (pad "31" thru_hole oval locked (at -10.026446 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "IO33") (pinfunction "IO33") (pintype "bidirectional"))
    (pad "32" thru_hole oval locked (at -10.026446 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "IO35") (pinfunction "IO35") (pintype "bidirectional"))
    (pad "33" thru_hole oval locked (at -12.026446 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "34" thru_hole oval locked (at -12.026446 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "35" thru_hole oval locked (at -14.026446 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "36" thru_hole oval locked (at -14.026446 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "37" thru_hole oval locked (at -16.026446 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "3V3") (pinfunction "3V3") (pintype "power_out"))
    (pad "38" thru_hole oval locked (at -16.026446 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "3V3") (pinfunction "3V3") (pintype "power_out"))
    (pad "39" thru_hole oval locked (at -18.026446 25.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "5V") (pinfunction "5V") (pintype "power_in"))
    (pad "40" thru_hole oval locked (at -18.026446 23.01 270) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "5V") (pinfunction "5V") (pintype "power_in"))
    (model "C:/Users/hmohamed/Documents/KiCad/7.0/3dmodels/WT32-SC01 ESP32 with 3.5in touch screen.step"
      (offset (xyz 4.36 28.5 7.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 -180))
    )
    (model ":KICAD6_3DMODEL_DIR:Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x20_P2.00mm_Vertical.step"
      (offset (xyz 20 -23 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical" (layer "B.Cu")
    (at 161.6672 111.523346 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (property "Sheetfile" "WT32-SC01-Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 2.33 90) (layer "B.SilkS") hide)
    (fp_text value "Conn_02x20_Odd_Even" (at 4.699 -41.602) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "3V3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "3V3") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "IO36") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 -10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "IO4") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "TP_INT") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 2.54 -12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "IO2") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "IO34") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 2.54 -15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "LCD_CS") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "I2C1_SCL") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 2.54 -17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "SPI2_MOSI") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "I2C1_SDA") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 2.54 -20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "ESP32_EN") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "LCD_DC") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 2.54 -22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "LCD_RST") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 -25.4 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "TXD0") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at 2.54 -25.4 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "LCD_BKLT") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 0 -27.94 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "SPI2_MISO") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at 2.54 -27.94 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "IO0") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval (at 0 -30.48 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "SPI2_CLK") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval (at 2.54 -30.48 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "IO5") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole oval (at 0 -33.02 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "IO27") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval (at 2.54 -33.02 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "IO25") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole oval (at 0 -35.56 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "IO32") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval (at 2.54 -35.56 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "IO26") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole oval (at 0 -38.1 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "IO33") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole oval (at 2.54 -38.1 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "IO35") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole oval (at 0 -40.64 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole oval (at 2.54 -40.64 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" thru_hole oval (at 0 -43.18 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" thru_hole oval (at 2.54 -43.18 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" thru_hole oval (at 0 -45.72 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "3V3") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" thru_hole oval (at 2.54 -45.72 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "3V3") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" thru_hole oval (at 0 -48.26 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "5V") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" thru_hole oval (at 2.54 -48.26 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "5V") (pinfunction "Pin_40") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "clipboard:579d114b-482e-4930-9728-e2bebf0b6204" (layer "B.Cu")
    (at 163.2712 122.6268 90)
    (fp_text reference "" (at 5.969 -18.288 90) (layer "B.SilkS"))
    (fp_text value "" (at 5.969 -18.288 90) (layer "B.SilkS"))
    (pad "" np_thru_hole circle (at 3.45 -51.3 90) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 3.45 0 90) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (gr_line (start 108.6447 121.022846) (end 108.6447 104.512846)
    (layer "Edge.Cuts"))
  (gr_arc (start 166.4297 121.022846) (mid 165.499764 123.26791) (end 163.2547 124.197846)
    (layer "Edge.Cuts"))
  (gr_arc (start 111.8197 124.197846) (mid 109.574636 123.26791) (end 108.6447 121.022846)
    (layer "Edge.Cuts"))
  (gr_line (start 163.2547 124.197846) (end 111.8197 124.197846)
    (layer "Edge.Cuts"))
  (gr_arc (start 108.6447 104.512846) (mid 109.574636 102.267782) (end 111.8197 101.337846)
    (layer "Edge.Cuts"))
  (gr_line (start 111.8197 101.337846) (end 163.2547 101.337846)
    (layer "Edge.Cuts"))
  (gr_arc (start 163.2547 101.337846) (mid 165.499764 102.267782) (end 166.4297 104.512846)
    (layer "Edge.Cuts"))
  (gr_line (start 166.4297 104.512846) (end 166.4297 121.022846)
    (layer "Edge.Cuts"))
  (gr_text "IO26" (at 127.0572 106.920847 90) (layer "B.SilkS"))
  (gr_text "LCD_BKL" (at 137.2172 102.108 90) (layer "B.SilkS" knockout))
  (gr_text "3V3" (at 116.8972 113.275845 90) (layer "B.SilkS"))
  (gr_text "IO0" (at 134.6772 106.920847 90) (layer "B.SilkS"))
  (gr_text "↓edge" (at 163.5722 123.689846) (layer "B.SilkS"))
  (gr_text "IO33" (at 124.5172 118.295845 90) (layer "B.SilkS"))
  (gr_text "GND" (at 121.9772 113.275845 90) (layer "B.SilkS"))
  (gr_text "3V3" (at 160.0772 106.920847 90) (layer "B.SilkS"))
  (gr_text " LCD_CS" (at 147.3772 102.108 90) (layer "B.SilkS" knockout))
  (gr_text "GND" (at 157.5372 117.762512 90) (layer "B.SilkS"))
  (gr_text "TP_INT" (at 149.9172 118.355846 90) (layer "B.SilkS" knockout))
  (gr_text "IO36" (at 152.4572 118.295845 90) (layer "B.SilkS"))
  (gr_text "SDA" (at 142.2972 117.429178 90) (layer "B.SilkS"))
  (gr_text "3V3" (at 116.8972 106.920847 90) (layer "B.SilkS"))
  (gr_text "IO34" (at 147.3772 118.295845 90) (layer "B.SilkS"))
  (gr_text "GND" (at 119.4372 113.275845 90) (layer "B.SilkS"))
  (gr_text "WT32-SC01 \nBreakout" (at 110.3376 110.2868 90) (layer "B.SilkS"))
  (gr_text "edge↓" (at 116.0742 123.689846) (layer "B.SilkS"))
  (gr_text "5V" (at 114.3572 113.275845 90) (layer "B.SilkS"))
  (gr_text "3V3" (at 160.0772 117.362511 90) (layer "B.SilkS"))
  (gr_text "MOSI" (at 144.8372 106.920847 90) (layer "B.SilkS"))
  (gr_text "IO4" (at 152.4572 106.920847 90) (layer "B.SilkS"))
  (gr_text "TXD0" (at 137.2172 118.629178 90) (layer "B.SilkS"))
  (gr_text "MISO" (at 134.6772 118.562512 90) (layer "B.SilkS"))
  (gr_text "5V" (at 162.6172 116.029178 90) (layer "B.SilkS"))
  (gr_text "IO5" (at 132.1372 106.920847 90) (layer "B.SilkS"))
  (gr_text " LCD_DC" (at 139.8232 118.355846 90) (layer "B.SilkS" knockout))
  (gr_text "IO27" (at 129.5972 118.295845 90) (layer "B.SilkS"))
  (gr_text "GND" (at 119.4372 106.920847 90) (layer "B.SilkS"))
  (gr_text "IO35" (at 124.5172 106.920847 90) (layer "B.SilkS"))
  (gr_text "SCL" (at 144.8372 117.362511 90) (layer "B.SilkS"))
  (gr_text "GND" (at 154.9972 106.920847 90) (layer "B.SilkS"))
  (gr_text "IO25" (at 129.5972 106.920847 90) (layer "B.SilkS"))
  (gr_text "IO2" (at 149.9172 106.920847 90) (layer "B.SilkS"))
  (gr_text "LCD_RST" (at 139.7508 102.108 90) (layer "B.SilkS" knockout))
  (gr_text "SCLK" (at 132.1372 118.762511 90) (layer "B.SilkS"))
  (gr_text "IO32" (at 127.0572 118.295845 90) (layer "B.SilkS"))
  (gr_text "5V" (at 114.3572 106.920847 90) (layer "B.SilkS"))
  (gr_text "GND" (at 157.5372 106.920847 90) (layer "B.SilkS"))
  (gr_text "5V" (at 162.6172 106.920847 90) (layer "B.SilkS"))
  (gr_text "GND" (at 154.9972 117.762512 90) (layer "B.SilkS"))
  (gr_text "EN" (at 142.2972 106.920847 90) (layer "B.SilkS"))
  (gr_text "GND" (at 121.9772 106.920847 90) (layer "B.SilkS"))
  (gr_text "GND" (at 117.4712 107.052846 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 120.0112 117.894511 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 153.0312 113.407844 -90) (layer "F.SilkS"))
  (gr_text " LCD_DC" (at 135.2512 118.355846 270) (layer "F.SilkS" knockout))
  (gr_text "IO2" (at 125.0912 107.052846 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 155.5712 107.052846 -90) (layer "F.SilkS"))
  (gr_text "IO5" (at 142.8712 107.052846 -90) (layer "F.SilkS"))
  (gr_text "v1.0" (at 110.2868 110.236 -90) (layer "F.SilkS"))
  (gr_text "MOSI" (at 130.1712 107.052846 -90) (layer "F.SilkS"))
  (gr_text "SDA" (at 132.7112 117.561177 -90) (layer "F.SilkS"))
  (gr_text "5V" (at 160.6512 107.052846 -90) (layer "F.SilkS"))
  (gr_text "IO26" (at 147.9512 107.052846 -90) (layer "F.SilkS"))
  (gr_text "IO27" (at 145.4112 118.427844 -90) (layer "F.SilkS"))
  (gr_text "IO32" (at 147.9512 118.427844 -90) (layer "F.SilkS"))
  (gr_text "| edge" (at 164.9984 115.4684 -90) (layer "F.SilkS"))
  (gr_text "IO25" (at 145.4112 107.052846 -90) (layer "F.SilkS"))
  (gr_text "MISO" (at 140.3312 118.694511 -90) (layer "F.SilkS"))
  (gr_text "3V3" (at 158.1112 113.407844 -90) (layer "F.SilkS"))
  (gr_text "3V3" (at 158.1112 107.052846 -90) (layer "F.SilkS"))
  (gr_text "3V3" (at 114.9312 117.49451 -90) (layer "F.SilkS"))
  (gr_text "LCD_RST" (at 135.2804 102.108 270) (layer "F.SilkS" knockout))
  (gr_text "5V" (at 112.3912 116.161177 -90) (layer "F.SilkS"))
  (gr_text "5V" (at 160.6512 113.407844 -90) (layer "F.SilkS"))
  (gr_text "EN" (at 132.7112 107.052846 -90) (layer "F.SilkS"))
  (gr_text "SCLK" (at 142.8712 118.89451 -90) (layer "F.SilkS"))
  (gr_text "LCD_BKL" (at 137.7912 102.108 270) (layer "F.SilkS" knockout))
  (gr_text "IO0" (at 140.3312 107.052846 -90) (layer "F.SilkS"))
  (gr_text "IO34" (at 127.6312 118.427844 -90) (layer "F.SilkS"))
  (gr_text "IO35" (at 150.4912 107.052846 -90) (layer "F.SilkS"))
  (gr_text "SCL" (at 130.1712 117.49451 -90) (layer "F.SilkS"))
  (gr_text "LCD_CS " (at 127.6312 102.108 270) (layer "F.SilkS" knockout))
  (gr_text "GND" (at 120.0112 107.052846 -90) (layer "F.SilkS"))
  (gr_text "IO4" (at 122.5512 107.052846 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 117.4712 117.894511 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 153.0312 107.052846 -90) (layer "F.SilkS"))
  (gr_text "3V3" (at 114.9312 107.052846 -90) (layer "F.SilkS"))
  (gr_text "IO33" (at 150.4912 118.427844 -90) (layer "F.SilkS"))
  (gr_text "TP_INT" (at 125.0912 118.355846 -90) (layer "F.SilkS" knockout))
  (gr_text "GND" (at 155.5712 113.407844 -90) (layer "F.SilkS"))
  (gr_text "5V" (at 112.3912 107.052846 -90) (layer "F.SilkS"))
  (gr_text "TXD0" (at 137.7912 118.761177 -90) (layer "F.SilkS"))
  (gr_text "| edge " (at 108.966 115.4684 -90) (layer "F.SilkS"))
  (gr_text "IO36" (at 122.5512 118.427844 -90) (layer "F.SilkS"))
)
