(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 31)
    (tracks 149)
    (zones 0)
    (modules 19)
    (nets 41)
  )
  (page A4)
  (title_block
    (date "lun. 30 mars 2015")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.35)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.15)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 110.998 126.365)
    (grid_origin 110.998 126.365)
    (visible_elements 7FFDFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /IOREF)
  (net 2 /Reset)
  (net 3 +5V)
  (net 4 GND)
  (net 5 /Vin)
  (net 6 /AREF)
  (net 7 "Net-(P5-Pad1)")
  (net 8 "Net-(P6-Pad1)")
  (net 9 "Net-(P7-Pad1)")
  (net 10 "Net-(P8-Pad1)")
  (net 11 "Net-(P1-Pad1)")
  (net 12 +3V3)
  (net 13 /SCL)
  (net 14 /SDA)
  (net 15 /READ)
  (net 16 /VCC_3V3)
  (net 17 /ADC_CS)
  (net 18 /ADC_DATA)
  (net 19 /ADC_CLK)
  (net 20 GNDA)
  (net 21 /VIDEO_N)
  (net 22 /VIDEO_P)
  (net 23 /CLR_PIX)
  (net 24 /SHUTTER)
  (net 25 /CLR_DATA)
  (net 26 /DATA_RDY)
  (net 27 /PWR_DOWN)
  (net 28 "Net-(P3-Pad7)")
  (net 29 "Net-(P3-Pad10)")
  (net 30 "Net-(P2-Pad3)")
  (net 31 "Net-(P2-Pad4)")
  (net 32 "Net-(P2-Pad5)")
  (net 33 "Net-(P2-Pad6)")
  (net 34 /VDD_OA)
  (net 35 /AVDD)
  (net 36 /AVSS)
  (net 37 "Net-(C2-Pad1)")
  (net 38 "Net-(P4-Pad1)")
  (net 39 "Net-(P4-Pad2)")
  (net 40 "Net-(P4-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.35)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /ADC_CLK)
    (add_net /ADC_CS)
    (add_net /ADC_DATA)
    (add_net /AREF)
    (add_net /AVDD)
    (add_net /AVSS)
    (add_net /CLR_DATA)
    (add_net /CLR_PIX)
    (add_net /DATA_RDY)
    (add_net /IOREF)
    (add_net /PWR_DOWN)
    (add_net /READ)
    (add_net /Reset)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SHUTTER)
    (add_net /VCC_3V3)
    (add_net /VDD_OA)
    (add_net /VIDEO_N)
    (add_net /VIDEO_P)
    (add_net /Vin)
    (add_net GND)
    (add_net GNDA)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P3-Pad10)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P8-Pad1)")
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5F82805D)
    (at 124.968 123.825)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P5 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 7 "Net-(P5-Pad1)"))
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5F82805D)
    (at 177.038 118.745)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P6 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 8 "Net-(P6-Pad1)"))
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5F82805D)
    (at 126.238 75.565)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P7 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 9 "Net-(P7-Pad1)"))
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5F82805D)
    (at 177.038 90.805)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P8 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 10 "Net-(P8-Pad1)"))
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x06 locked (layer F.Cu) (tedit 5F827FDE)
    (at 161.798 123.825)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at 6.604 -2.54) (layer F.SilkS) hide)
    (fp_text value Analog (at 6.604 -4.064) (layer F.Fab))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(P2-Pad6)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad5)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(P2-Pad4)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(P2-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /VIDEO_N))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /VIDEO_P))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x06.wrl
      (offset (xyz 6.349999904632568 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x08 locked (layer F.Cu) (tedit 5F828000)
    (at 138.938 123.825)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 8.89 -2.54) (layer F.SilkS) hide)
    (fp_text value Power (at 8.89 -4.064) (layer F.Fab))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /Vin))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 +3V3))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /Reset))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /IOREF))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(P1-Pad1)"))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x08.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x08 locked (layer F.Cu) (tedit 5F828000)
    (at 156.718 75.565)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 8.89 2.794) (layer F.SilkS) hide)
    (fp_text value Digital (at 8.89 4.318) (layer F.Fab))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /PWR_DOWN))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /DATA_RDY))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /CLR_DATA))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /SHUTTER))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /CLR_PIX))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "Net-(P4-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "Net-(P4-Pad2)"))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "Net-(P4-Pad1)"))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x08.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x10 locked (layer F.Cu) (tedit 5F828027)
    (at 129.794 75.565)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 11.43 2.794) (layer F.SilkS) hide)
    (fp_text value Digital (at 11.43 4.318) (layer F.Fab))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(P3-Pad10)"))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /READ))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /ADC_CS))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(P3-Pad7)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /ADC_DATA))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /ADC_CLK))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /AREF))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /SDA))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /SCL))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x10.wrl
      (offset (xyz 11.42999982833862 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 140.898 108.265 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 1.6) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 147.198 116.565 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 2.9 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5A02FF57)
    (at 141.898 114.365 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value AP1117-33 (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 3.15 0 90) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 156.718 78.105 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 0 2.77 270) (layer B.SilkS))
    (fp_text value Conn_01x05 (at 0 -12.93 270) (layer B.Fab))
    (fp_text user %R (at 0 -5.08) (layer B.Fab))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /VIDEO_N))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /VIDEO_P))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /AVSS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /AVDD))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 139.698 100.965 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at -0.1 8 90) (layer F.SilkS))
    (fp_text value Jumper (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /VCC_3V3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 144.798 106.265)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at 5.2 -0.1 90) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 3.75) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 150.698 117.465)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C3 (at 1.2 -4 90) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 3.75) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 159.298 84.865 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP4 (at 0 -3.3 90) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /AVSS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 GNDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 154.998 84.865 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP3 (at 0 -3.1 90) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /AVDD))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /VDD_OA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 159.298 114.865)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at 0 -3 90) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 GNDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x10_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A427)
    (at 162.498 96.465 270)
    (descr "Through hole straight socket strip, 2x10, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x10 2.54mm double row")
    (fp_text reference J1 (at -1.27 -2.77 90) (layer F.SilkS))
    (fp_text value Camera (at -1.27 25.63 90) (layer F.Fab))
    (fp_text user %R (at -1.27 11.43) (layer F.Fab))
    (pad 20 thru_hole oval (at -2.54 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /SCL))
    (pad 19 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /SDA))
    (pad 18 thru_hole oval (at -2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /READ))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 16 thru_hole oval (at -2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /VCC_3V3))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 14 thru_hole oval (at -2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /ADC_CS))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /ADC_DATA))
    (pad 12 thru_hole oval (at -2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /ADC_CLK))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 10 thru_hole oval (at -2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /VDD_OA))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /VIDEO_N))
    (pad 8 thru_hole oval (at -2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /VIDEO_P))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 GNDA))
    (pad 6 thru_hole oval (at -2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /CLR_PIX))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /SHUTTER))
    (pad 4 thru_hole oval (at -2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /CLR_DATA))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /DATA_RDY))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /PWR_DOWN))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Rev A" (at 140.598 115.165) (layer B.SilkS))
  (gr_text "EPC901 Breakout to Shield Adapter" (at 151.298 110.865) (layer B.SilkS))
  (gr_text FRONT (at 170.798 86.665) (layer F.SilkS))
  (gr_text FRONT (at 130.998 86.665) (layer F.SilkS))
  (gr_text LDO (at 127.398 107.365) (layer F.SilkS))
  (gr_text HOST (at 127.398 104.265) (layer F.SilkS))
  (gr_text "3.3V VCC" (at 130.698 100.965) (layer F.SilkS))
  (gr_text *GND (at 162.498 116.065 90) (layer F.SilkS))
  (gr_text AVDD (at 151.998 83.565 90) (layer F.SilkS))
  (gr_text AVSS (at 162.598 83.565 90) (layer F.SilkS))
  (gr_line (start 122.498 126.365) (end 122.498 73.025) (layer Edge.Cuts) (width 0.15))
  (gr_text 1 (at 138.938 121.285 90) (layer F.SilkS))
  (gr_line (start 177.038 74.549) (end 175.514 73.025) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 85.979) (end 177.038 74.549) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.578 88.519) (end 177.038 85.979) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.578 121.285) (end 179.578 88.519) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 123.825) (end 179.578 121.285) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 126.365) (end 177.038 123.825) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.498 126.365) (end 177.038 126.365) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.514 73.025) (end 122.498 73.025) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 180.498 127.365) (xy 121.498 127.365) (xy 121.498 71.865) (xy 180.498 71.865)
      )
    )
  )
  (zone (net 20) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 168.098 77.865) (xy 168.098 82.165) (xy 156.698 93.565) (xy 156.698 96.465) (xy 156.698 103.765)
        (xy 163.998 111.065) (xy 163.998 116.065) (xy 157.798 116.065) (xy 157.798 108.94) (xy 150.698 101.615)
        (xy 150.698 95.965) (xy 151.698 94.965) (xy 151.698 83.365) (xy 163.398 83.365) (xy 163.398 77.165)
        (xy 167.598 77.165)
      )
    )
  )
  (zone (net 16) (net_name /VCC_3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.198 95.665) (xy 143.898 95.665) (xy 143.898 101.365) (xy 141.398 101.365) (xy 141.398 100.265)
        (xy 142.898 98.965) (xy 142.898 93.265) (xy 145.198 93.265)
      )
    )
  )
)
