(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 28)
    (tracks 37)
    (zones 0)
    (modules 5)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.35 1.35)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (grid_origin 135.89 85.725)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /PP2)
  (net 2 /GP1)
  (net 3 /SCL)
  (net 4 /3V3)
  (net 5 /SDA)
  (net 6 /XVS)
  (net 7 /FSTB)
  (net 8 /GP0)
  (net 9 /GND)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3V3)
    (add_net /FSTB)
    (add_net /GND)
    (add_net /GP0)
    (add_net /GP1)
    (add_net /PP2)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /XVS)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 5F89D12F)
    (at 144.71 82.725 90)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (fp_text reference J2 (at 3 6.43) (layer F.SilkS))
    (fp_text value Header (at 3 10.18) (layer F.Fab))
    (fp_text user %R (at 0 10.16 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /PP2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GP1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /3V3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SDA))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /XVS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /FSTB))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /GP0))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x09_P2.00mm_Vertical (layer F.Cu) (tedit 5F89D10B)
    (at 146.89 87.725 90)
    (descr "Through hole straight pin header, 1x09, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.00mm single row")
    (fp_text reference J1 (at -2.5 2) (layer F.SilkS))
    (fp_text value Castellations (at -2.5 8) (layer F.Fab))
    (fp_text user %R (at -2.5 14.25 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /PP2))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /GP1))
    (pad 3 thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /SCL))
    (pad 4 thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /3V3))
    (pad 5 thru_hole oval (at 0 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /SDA))
    (pad 6 thru_hole oval (at 0 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /XVS))
    (pad 7 thru_hole oval (at 0 12 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /FSTB))
    (pad 8 thru_hole oval (at 0 14 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /GP0))
    (pad 9 thru_hole oval (at 0 16 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x09_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 139.89 89.725)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference H1 (at -6.25 3.5) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 169.89 89.725)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference H2 (at -6.4 3.5) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Connector_Coaxial:U.FL_Hirose_U.FL-R-SMT-1_Vertical (layer F.Cu) (tedit 5A1DBFC3)
    (at 170.14 83.225 90)
    (descr "Hirose U.FL Coaxial https://www.hirose.com/product/en/products/U.FL/U.FL-R-SMT-1%2810%29/")
    (tags "Hirose U.FL Coaxial")
    (attr smd)
    (fp_text reference J3 (at 3.5 0 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0.475 3.2 90) (layer F.Fab))
    (fp_text user %R (at 0.475 0) (layer F.Fab))
    (pad 2 smd rect (at 0.475 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 9 /GND))
    (pad 1 smd rect (at -1.05 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /XVS))
    (pad 2 smd rect (at 0.475 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 9 /GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/U.FL_Hirose_U.FL-R-SMT-1_Vertical.wrl
      (offset (xyz 0.4749999928262157 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text XVS (at 172.64 85.225) (layer F.SilkS))
  (gr_text "PI HQ\nBREAKOUT\n201016" (at 139.64 83.225) (layer F.SilkS))
  (gr_arc (start 165.14 89.725) (end 167.14 89.725) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 144.64 89.725) (end 144.64 87.725) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 137.89 90.475) (end 135.89 90.475) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 171.89 90.475) (end 171.89 92.475) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 171.89 82.725) (end 173.89 82.725) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 137.89 82.725) (end 137.89 80.725) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text GND (at 164.89 85.475 270) (layer F.SilkS))
  (gr_text GP0 (at 162.39 85.475 270) (layer F.SilkS))
  (gr_text FSTB (at 159.89 85.475 270) (layer F.SilkS))
  (gr_text XVS (at 157.39 85.475 270) (layer F.SilkS))
  (gr_text SDA (at 154.89 85.475 270) (layer F.SilkS))
  (gr_text 3V3 (at 152.39 85.475 270) (layer F.SilkS))
  (gr_text SCL (at 149.64 85.475 270) (layer F.SilkS))
  (gr_text GP1 (at 147.14 85.475 270) (layer F.SilkS))
  (gr_text PP2 (at 144.64 85.475 270) (layer F.SilkS))
  (gr_line (start 139.89 92.475) (end 137.89 92.475) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 169.89 92.475) (end 171.89 92.475) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 169.89 89.725) (end 167.14 89.725) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 139.89 89.725) (end 139.89 92.475) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 173.89 82.725) (end 173.89 90.475) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.89 82.725) (end 135.89 90.475) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.89 80.725) (end 171.89 80.725) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144.64 87.725) (end 165.14 87.725) (layer Edge.Cuts) (width 0.05))
)
