(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 33)
    (tracks 116)
    (zones 0)
    (modules 7)
    (nets 28)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 1)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad8)")
  (net 2 "Net-(J1-Pad7)")
  (net 3 "Net-(J1-Pad6)")
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J1-Pad4)")
  (net 6 "Net-(J1-Pad3)")
  (net 7 "Net-(J1-Pad2)")
  (net 8 "Net-(J1-Pad1)")
  (net 9 "Net-(OLD-HOLES1-Pad16)")
  (net 10 "Net-(OLD-HOLES1-Pad15)")
  (net 11 "Net-(OLD-HOLES1-Pad7)")
  (net 12 "Net-(OLD-HOLES1-Pad14)")
  (net 13 "Net-(OLD-HOLES1-Pad6)")
  (net 14 "Net-(OLD-HOLES1-Pad13)")
  (net 15 "Net-(OLD-HOLES1-Pad5)")
  (net 16 "Net-(OLD-HOLES1-Pad12)")
  (net 17 "Net-(OLD-HOLES1-Pad4)")
  (net 18 "Net-(OLD-HOLES1-Pad11)")
  (net 19 "Net-(OLD-HOLES1-Pad3)")
  (net 20 "Net-(OLD-HOLES1-Pad10)")
  (net 21 "Net-(OLD-HOLES1-Pad2)")
  (net 22 "Net-(OLD-HOLES1-Pad9)")
  (net 23 "Net-(OLD-HOLES1-Pad1)")
  (net 24 "Net-(R1-Pad2)")
  (net 25 "Net-(R2-Pad2)")
  (net 26 "Net-(R3-Pad2)")
  (net 27 "Net-(R4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(OLD-HOLES1-Pad1)")
    (add_net "Net-(OLD-HOLES1-Pad10)")
    (add_net "Net-(OLD-HOLES1-Pad11)")
    (add_net "Net-(OLD-HOLES1-Pad12)")
    (add_net "Net-(OLD-HOLES1-Pad13)")
    (add_net "Net-(OLD-HOLES1-Pad14)")
    (add_net "Net-(OLD-HOLES1-Pad15)")
    (add_net "Net-(OLD-HOLES1-Pad16)")
    (add_net "Net-(OLD-HOLES1-Pad2)")
    (add_net "Net-(OLD-HOLES1-Pad3)")
    (add_net "Net-(OLD-HOLES1-Pad4)")
    (add_net "Net-(OLD-HOLES1-Pad5)")
    (add_net "Net-(OLD-HOLES1-Pad6)")
    (add_net "Net-(OLD-HOLES1-Pad7)")
    (add_net "Net-(OLD-HOLES1-Pad9)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
  )
  (module "nes to pce:SolderWirePad_1x08_SMD_5x12mm" (layer F.Cu) (tedit 5E448D98)
    (at 123.063 73.152)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J1 (at 0 1.27 180 unlocked) (layer F.SilkS))
    (fp_text value Mini-DIN-8 (at 0 6.35) (layer F.Fab))
    (pad 8 smd rect (at 6.985 3.81) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad8)"))
    (pad 7 smd rect (at 5.08 3.81) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad7)"))
    (pad 6 smd rect (at 3.175 3.81) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 5 smd rect (at 1.27 3.81) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 4 smd rect (at -0.635 3.81) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at -2.54 3.81) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -4.445 3.81) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -6.35 3.81) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad1)"))
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 123.317 87.441 270)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at 2.7 -6.223 270 unlocked) (layer F.SilkS))
    (fp_text value 74LS157 (at 0 5.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 16 smd roundrect (at 2.475 -4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(J1-Pad1)"))
    (pad 15 smd roundrect (at 2.475 -3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J1-Pad7)"))
    (pad 14 smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(OLD-HOLES1-Pad13)"))
    (pad 13 smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(OLD-HOLES1-Pad6)"))
    (pad 12 smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(R4-Pad2)"))
    (pad 11 smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(OLD-HOLES1-Pad14)"))
    (pad 10 smd roundrect (at 2.475 3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(OLD-HOLES1-Pad5)"))
    (pad 9 smd roundrect (at 2.475 4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(R3-Pad2)"))
    (pad 8 smd roundrect (at -2.475 4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J1-Pad8)"))
    (pad 7 smd roundrect (at -2.475 3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(R2-Pad2)"))
    (pad 6 smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(OLD-HOLES1-Pad7)"))
    (pad 5 smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(OLD-HOLES1-Pad15)"))
    (pad 4 smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(R1-Pad2)"))
    (pad 3 smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(OLD-HOLES1-Pad4)"))
    (pad 2 smd roundrect (at -2.475 -3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(OLD-HOLES1-Pad1)"))
    (pad 1 smd roundrect (at -2.475 -4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad6)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 127.508 81.289 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 1.64 90) (layer F.SilkS) hide)
    (fp_text value 330 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 "Net-(J1-Pad5)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 27 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 124.714 81.271 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 330 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 26 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 121.92 81.28 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 330 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(J1-Pad3)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 25 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 119.126 81.271 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 330 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 24 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5E44924B)
    (at 119.38 93.98)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference OLD-HOLES1 (at 3.87 -0.255) (layer F.SilkS) hide)
    (fp_text value 4021 (at 3.9 18.415) (layer F.Fab))
    (fp_text user %R (at 3.81 8.834999 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(OLD-HOLES1-Pad16)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad8)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(OLD-HOLES1-Pad15)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(OLD-HOLES1-Pad7)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(OLD-HOLES1-Pad14)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(OLD-HOLES1-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(OLD-HOLES1-Pad13)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(OLD-HOLES1-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(OLD-HOLES1-Pad12)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(OLD-HOLES1-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(OLD-HOLES1-Pad11)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(OLD-HOLES1-Pad3)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(OLD-HOLES1-Pad10)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(OLD-HOLES1-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(OLD-HOLES1-Pad9)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(OLD-HOLES1-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "1 x 74LS157 - 16-SOIC\n(Digikey 296-14884-1-ND)\n4 x 330Ω resistor - 0805\n(Digikey CR0805-JW-331ELFCT-ND)" (at 123.19 74.422 90) (layer B.SilkS))
  (gr_text "NES to PCE Adapter V1.1" (at 116.84 85.598 -90) (layer F.SilkS))
  (gr_text 1 (at 117.602 93.98 -90) (layer F.SilkS))
  (gr_line (start 129.54 92.456) (end 130.81 92.456) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.54 114.3) (end 129.54 92.456) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 116.84 92.456) (end 116.84 114.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 115.57 92.456) (end 116.84 92.456) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 130.81 73.66) (end 130.81 92.456) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.57 73.66) (end 130.81 73.66) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.57 92.456) (end 115.57 73.66) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.54 114.3) (end 116.84 114.3) (layer Edge.Cuts) (width 0.1))
  (gr_text 1 (at 129.54 84.836 -90) (layer F.SilkS))
  (gr_text 8 (at 130.048 74.422 180) (layer F.SilkS))
  (gr_text 1 (at 116.586 74.422 180) (layer F.SilkS))
  (gr_text "Basic Gravis\nComputer\nTechnology" (at 123.19 106.426 270) (layer F.SilkS))
)
