(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(gr_arc
		(start 100.58 95.57)
		(mid 97.885923 94.454077)
		(end 96.77 91.76)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 199.77 91.76)
		(mid 198.654077 94.454077)
		(end 195.96 95.57)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 195.78 91.58)
		(end 197.8755 91.58)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 96.77 91.76)
		(end 96.77 68.88)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 96.77 68.88)
		(mid 97.885923 66.185923)
		(end 100.58 65.07)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 167.32 80.32)
		(end 172.0825 80.32)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 110.17 80.32)
		(end 114.9325 80.32)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 195.78 69.06)
		(end 197.8755 69.06)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 195.96 95.57)
		(end 100.58 95.57)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100.58 65.07)
		(end 195.96 65.07)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 195.96 65.07)
		(mid 198.654077 66.185923)
		(end 199.77 68.88)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 186.37 80.32)
		(end 191.1325 80.32)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 129.22 80.32)
		(end 133.9825 80.32)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 100.76 91.58)
		(end 102.8555 91.58)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.77 68.88)
		(end 199.77 91.76)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 148.27 80.32)
		(end 154.62 80.32)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 100.76 69.06)
		(end 102.8555 69.06)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "+/- 15vdc"
		(at 148.27 70 0)
		(layer "F.SilkS")
	)
	(gr_text "Input"
		(at 119.695 70 0)
		(layer "F.SilkS")
	)
	(gr_text "Output"
		(at 176.85 70 0)
		(layer "F.SilkS")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 96.5 64.76) (xy 200.11 64.72) (xy 200.12 95.92) (xy 96.42 95.92) (xy 96.4 64.76)
			)
		)
	)
)
