(kicad_pcb (version 20171130) (host pcbnew "(5.1.9-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 911)
    (zones 0)
    (modules 55)
    (nets 72)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1)
    (pad_drill 0.65)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(AC1-Pad24)")
  (net 4 "Net-(AC1-Pad23)")
  (net 5 "Net-(AC1-Pad22)")
  (net 6 "Net-(AC1-Pad21)")
  (net 7 /SDA)
  (net 8 /SCL)
  (net 9 "Net-(AC1-Pad18)")
  (net 10 "Net-(AC1-Pad16)")
  (net 11 "Net-(AC1-Pad15)")
  (net 12 /INT_MOTION)
  (net 13 "Net-(AC1-Pad13)")
  (net 14 "Net-(AC1-Pad12)")
  (net 15 /RST_MOTION)
  (net 16 "Net-(AC1-Pad9)")
  (net 17 "Net-(AC1-Pad8)")
  (net 18 "Net-(AC1-Pad7)")
  (net 19 "Net-(AC1-Pad4)")
  (net 20 "Net-(AC1-Pad1)")
  (net 21 "Net-(C5-Pad1)")
  (net 22 /EN_HAP)
  (net 23 /SCK)
  (net 24 /MISO)
  (net 25 /MOSI)
  (net 26 "Net-(C1-Pad2)")
  (net 27 VCC_UNREG)
  (net 28 +5V)
  (net 29 VBAT)
  (net 30 "Net-(C16-Pad2)")
  (net 31 "Net-(C16-Pad1)")
  (net 32 "Net-(C19-Pad2)")
  (net 33 "Net-(C19-Pad1)")
  (net 34 "Net-(C20-Pad2)")
  (net 35 /CHG_PMP_M_SEL_1)
  (net 36 /CHG_PMP_M_SEL_2)
  (net 37 /PIEZO_PWM)
  (net 38 /PIEZO_OUT_2)
  (net 39 /PIEZO_OUT_1)
  (net 40 /VIB-)
  (net 41 /VIB+)
  (net 42 /RESET)
  (net 43 /SWCLK)
  (net 44 /SWDIO)
  (net 45 "Net-(J2-Pad4)")
  (net 46 "Net-(R1-Pad2)")
  (net 47 "Net-(R8-Pad1)")
  (net 48 "Net-(R11-Pad2)")
  (net 49 "Net-(R16-Pad2)")
  (net 50 "Net-(U1-Pad27)")
  (net 51 "Net-(U1-Pad14)")
  (net 52 "Net-(U1-Pad13)")
  (net 53 "Net-(U1-Pad11)")
  (net 54 "Net-(U1-Pad5)")
  (net 55 "Net-(U1-Pad4)")
  (net 56 "Net-(U1-Pad3)")
  (net 57 "Net-(U1-Pad2)")
  (net 58 "Net-(U3-Pad6)")
  (net 59 "Net-(U5-Pad4)")
  (net 60 /CLK_32_768)
  (net 61 "Net-(D3-Pad1)")
  (net 62 /SD_PWR)
  (net 63 "Net-(J4-Pad1)")
  (net 64 /SD_CS)
  (net 65 "Net-(J4-Pad8)")
  (net 66 /CARD_DETECT)
  (net 67 /SD_PWR_EN)
  (net 68 "Net-(U2-Pad4)")
  (net 69 "Net-(J2-Pad3)")
  (net 70 "Net-(J2-Pad2)")
  (net 71 "Net-(U1-Pad23)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /CARD_DETECT)
    (add_net /CHG_PMP_M_SEL_1)
    (add_net /CHG_PMP_M_SEL_2)
    (add_net /CLK_32_768)
    (add_net /EN_HAP)
    (add_net /INT_MOTION)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /PIEZO_OUT_1)
    (add_net /PIEZO_OUT_2)
    (add_net /PIEZO_PWM)
    (add_net /RESET)
    (add_net /RST_MOTION)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SD_CS)
    (add_net /SD_PWR)
    (add_net /SD_PWR_EN)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /VIB+)
    (add_net /VIB-)
    (add_net GND)
    (add_net "Net-(AC1-Pad1)")
    (add_net "Net-(AC1-Pad12)")
    (add_net "Net-(AC1-Pad13)")
    (add_net "Net-(AC1-Pad15)")
    (add_net "Net-(AC1-Pad16)")
    (add_net "Net-(AC1-Pad18)")
    (add_net "Net-(AC1-Pad21)")
    (add_net "Net-(AC1-Pad22)")
    (add_net "Net-(AC1-Pad23)")
    (add_net "Net-(AC1-Pad24)")
    (add_net "Net-(AC1-Pad4)")
    (add_net "Net-(AC1-Pad7)")
    (add_net "Net-(AC1-Pad8)")
    (add_net "Net-(AC1-Pad9)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U5-Pad4)")
    (add_net VBAT)
    (add_net VCC_UNREG)
  )
  (module SmartwatchLibrary:QFN-12-1EP_3x3mm_P0.5mm_EP1.65x1.65mm_ThermalVias (layer F.Cu) (tedit 6015A99E)
    (at 217.2 50.3)
    (descr "QFN, 12 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_12_%2005-08-1855.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference IC2 (at -2.15 1.75) (layer F.SilkS))
    (fp_text value PAM8904EJPR (at 0 2.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd roundrect (at 0.41 0.41) (size 0.71 0.71) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.41 -0.41) (size 0.71 0.71) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.41 0.41) (size 0.71 0.71) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.41 -0.41) (size 0.71 0.71) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 13 smd rect (at 0 0) (size 1.65 1.65) (layers B.Cu)
      (net 2 GND))
    (pad 13 thru_hole circle (at 0.575 0.575) (size 0.5 0.5) (drill 0.254) (layers *.Cu)
      (net 2 GND))
    (pad 13 thru_hole circle (at -0.575 0.575) (size 0.5 0.5) (drill 0.254) (layers *.Cu)
      (net 2 GND))
    (pad 13 thru_hole circle (at 0.575 -0.575) (size 0.5 0.5) (drill 0.254) (layers *.Cu)
      (net 2 GND))
    (pad 13 thru_hole circle (at -0.575 -0.575) (size 0.5 0.5) (drill 0.254) (layers *.Cu)
      (net 2 GND))
    (pad 13 smd rect (at 0 0) (size 1.65 1.65) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 12 smd roundrect (at -0.5 -1.49) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 11 smd roundrect (at 0 -1.49) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C19-Pad2)"))
    (pad 10 smd roundrect (at 0.5 -1.49) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(C20-Pad2)"))
    (pad 9 smd roundrect (at 1.49 -0.5) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(C16-Pad2)"))
    (pad 8 smd roundrect (at 1.49 0) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(C19-Pad1)"))
    (pad 7 smd roundrect (at 1.49 0.5) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /PIEZO_OUT_1))
    (pad 6 smd roundrect (at 0.5 1.49) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /PIEZO_OUT_2))
    (pad 5 smd roundrect (at 0 1.49) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 4 smd roundrect (at -0.5 1.49) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(C16-Pad1)"))
    (pad 3 smd roundrect (at -1.49 0.5) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /PIEZO_PWM))
    (pad 2 smd roundrect (at -1.49 0) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /CHG_PMP_M_SEL_2))
    (pad 1 smd roundrect (at -1.49 -0.5) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /CHG_PMP_M_SEL_1))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-12-1EP_3x3mm_P0.5mm_EP1.65x1.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SmartwatchLibrary:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm_ThermalVias (layer F.Cu) (tedit 6015A21B)
    (at 212.4 66.1 180)
    (descr "QFN, 32 Pin (http://infocenter.nordicsemi.com/pdf/nRF52810_PS_v1.1.pdf#page=468), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U1 (at -4.2 -1.3) (layer F.SilkS))
    (fp_text value ATSAMD21E18A-M (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd custom (at 1.4 1.4 180) (size 0.554596 0.554596) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.232106 -0.157228) (xy -0.157228 -0.232106) (xy 0.232106 -0.232106) (xy 0.232106 0.232106) (xy -0.232106 0.232106)
) (width 0.180769))
      ))
    (pad "" smd custom (at 1.4 -1.4 180) (size 0.554596 0.554596) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.232106 -0.232106) (xy 0.232106 -0.232106) (xy 0.232106 0.232106) (xy -0.157228 0.232106) (xy -0.232106 0.157228)
) (width 0.180769))
      ))
    (pad "" smd custom (at -1.4 1.4 180) (size 0.554596 0.554596) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.232106 -0.232106) (xy 0.157228 -0.232106) (xy 0.232106 -0.157228) (xy 0.232106 0.232106) (xy -0.232106 0.232106)
) (width 0.180769))
      ))
    (pad "" smd custom (at -1.4 -1.4 180) (size 0.554596 0.554596) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.232106 -0.232106) (xy 0.232106 -0.232106) (xy 0.232106 0.157228) (xy 0.157228 0.232106) (xy -0.232106 0.232106)
) (width 0.180769))
      ))
    (pad "" smd custom (at 0.5 1.4 180) (size 0.568298 0.568298) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.32643 -0.182281) (xy -0.262904 -0.245807) (xy 0.262904 -0.245807) (xy 0.32643 -0.182281) (xy 0.32643 0.245807)
           (xy -0.32643 0.245807)) (width 0.153366))
      ))
    (pad "" smd custom (at -0.5 1.4 180) (size 0.568298 0.568298) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.32643 -0.182281) (xy -0.262904 -0.245807) (xy 0.262904 -0.245807) (xy 0.32643 -0.182281) (xy 0.32643 0.245807)
           (xy -0.32643 0.245807)) (width 0.153366))
      ))
    (pad "" smd custom (at 0.5 -1.4 180) (size 0.568298 0.568298) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.32643 -0.245807) (xy 0.32643 -0.245807) (xy 0.32643 0.182281) (xy 0.262904 0.245807) (xy -0.262904 0.245807)
           (xy -0.32643 0.182281)) (width 0.153366))
      ))
    (pad "" smd custom (at -0.5 -1.4 180) (size 0.568298 0.568298) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.32643 -0.245807) (xy 0.32643 -0.245807) (xy 0.32643 0.182281) (xy 0.262904 0.245807) (xy -0.262904 0.245807)
           (xy -0.32643 0.182281)) (width 0.153366))
      ))
    (pad "" smd custom (at 1.4 0.5 180) (size 0.568298 0.568298) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.245807 -0.262904) (xy -0.182281 -0.32643) (xy 0.245807 -0.32643) (xy 0.245807 0.32643) (xy -0.182281 0.32643)
           (xy -0.245807 0.262904)) (width 0.153366))
      ))
    (pad "" smd custom (at 1.4 -0.5 180) (size 0.568298 0.568298) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.245807 -0.262904) (xy -0.182281 -0.32643) (xy 0.245807 -0.32643) (xy 0.245807 0.32643) (xy -0.182281 0.32643)
           (xy -0.245807 0.262904)) (width 0.153366))
      ))
    (pad "" smd custom (at -1.4 0.5 180) (size 0.568298 0.568298) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.245807 -0.32643) (xy 0.182281 -0.32643) (xy 0.245807 -0.262904) (xy 0.245807 0.262904) (xy 0.182281 0.32643)
           (xy -0.245807 0.32643)) (width 0.153366))
      ))
    (pad "" smd custom (at -1.4 -0.5 180) (size 0.568298 0.568298) (layers F.Paste)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.245807 -0.32643) (xy 0.182281 -0.32643) (xy 0.245807 -0.262904) (xy 0.245807 0.262904) (xy 0.182281 0.32643)
           (xy -0.245807 0.32643)) (width 0.153366))
      ))
    (pad "" smd roundrect (at 0.5 0.5 180) (size 0.806226 0.806226) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.5 -0.5 180) (size 0.806226 0.806226) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.5 0.5 180) (size 0.806226 0.806226) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.5 -0.5 180) (size 0.806226 0.806226) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 33 smd rect (at 0 0 180) (size 2.5 2.5) (layers B.Cu)
      (net 2 GND))
    (pad 33 thru_hole circle (at 1 1 180) (size 0.5 0.5) (drill 0.254) (layers *.Cu)
      (net 2 GND))
    (pad 33 thru_hole circle (at 0 1 180) (size 0.5 0.5) (drill 0.254) (layers *.Cu)
      (net 2 GND))
    (pad 33 thru_hole circle (at -1 1 180) (size 0.5 0.5) (drill 0.254) (layers *.Cu)
      (net 2 GND))
    (pad 33 thru_hole circle (at 1 0 180) (size 0.5 0.5) (drill 0.254) (layers *.Cu)
      (net 2 GND))
    (pad 33 thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.254) (layers *.Cu)
      (net 2 GND))
    (pad 33 thru_hole circle (at -1 0 180) (size 0.5 0.5) (drill 0.254) (layers *.Cu)
      (net 2 GND))
    (pad 33 thru_hole circle (at 1 -1 180) (size 0.5 0.5) (drill 0.254) (layers *.Cu)
      (net 2 GND))
    (pad 33 thru_hole circle (at 0 -1 180) (size 0.5 0.5) (drill 0.254) (layers *.Cu)
      (net 2 GND))
    (pad 33 thru_hole circle (at -1 -1 180) (size 0.5 0.5) (drill 0.254) (layers *.Cu)
      (net 2 GND))
    (pad 33 smd rect (at 0 0 180) (size 3.6 3.6) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 32 smd roundrect (at -1.75 -2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /SWDIO))
    (pad 31 smd roundrect (at -1.25 -2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /SWCLK))
    (pad 30 smd roundrect (at -0.75 -2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 29 smd roundrect (at -0.25 -2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)"))
    (pad 28 smd roundrect (at 0.25 -2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 27 smd roundrect (at 0.75 -2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(U1-Pad27)"))
    (pad 26 smd roundrect (at 1.25 -2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /RESET))
    (pad 25 smd roundrect (at 1.75 -2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /SD_CS))
    (pad 24 smd roundrect (at 2.45 -1.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /SD_PWR_EN))
    (pad 23 smd roundrect (at 2.45 -1.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(U1-Pad23)"))
    (pad 22 smd roundrect (at 2.45 -0.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /SCL))
    (pad 21 smd roundrect (at 2.45 -0.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /SDA))
    (pad 20 smd roundrect (at 2.45 0.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /EN_HAP))
    (pad 19 smd roundrect (at 2.45 0.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /RST_MOTION))
    (pad 18 smd roundrect (at 2.45 1.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /INT_MOTION))
    (pad 17 smd roundrect (at 2.45 1.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /PIEZO_PWM))
    (pad 16 smd roundrect (at 1.75 2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /CHG_PMP_M_SEL_2))
    (pad 15 smd roundrect (at 1.25 2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /CHG_PMP_M_SEL_1))
    (pad 14 smd roundrect (at 0.75 2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(U1-Pad14)"))
    (pad 13 smd roundrect (at 0.25 2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(U1-Pad13)"))
    (pad 12 smd roundrect (at -0.25 2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /MISO))
    (pad 11 smd roundrect (at -0.75 2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(U1-Pad11)"))
    (pad 10 smd roundrect (at -1.25 2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at -1.75 2.45 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 8 smd roundrect (at -2.45 1.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /SCK))
    (pad 7 smd roundrect (at -2.45 1.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /MOSI))
    (pad 6 smd roundrect (at -2.45 0.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(R1-Pad2)"))
    (pad 5 smd roundrect (at -2.45 0.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(U1-Pad5)"))
    (pad 4 smd roundrect (at -2.45 -0.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(U1-Pad4)"))
    (pad 3 smd roundrect (at -2.45 -0.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(U1-Pad3)"))
    (pad 2 smd roundrect (at -2.45 -1.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(U1-Pad2)"))
    (pad 1 smd roundrect (at -2.45 -1.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /CLK_32_768))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SmartwatchLibrary:M50_3130545R (layer F.Cu) (tedit 6015DF52)
    (at 224.03 79.4 90)
    (descr "surface-mounted straight pin header, 1x05, 1.27mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x05 1.27mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference J5 (at 3.1 -0.03 180) (layer F.SilkS))
    (fp_text value Conn_01x05 (at 0 4.235 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 2.54 90) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 1.27 90) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -1.27 90) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -2.54 90) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad 4 smd rect (at 1.3 1.27 90) (size 1.6 0.74) (layers F.Cu F.Paste F.Mask)
      (net 44 /SWDIO))
    (pad 2 smd rect (at 1.3 -1.27 90) (size 1.6 0.74) (layers F.Cu F.Paste F.Mask)
      (net 42 /RESET))
    (pad 5 smd rect (at -1.3 2.54 90) (size 1.6 0.74) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.3 0 90) (size 1.6 0.74) (layers F.Cu F.Paste F.Mask)
      (net 43 /SWCLK))
    (pad 1 smd rect (at -1.3 -2.54 90) (size 1.6 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x04_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 201.5 81.7 90)
    (descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x04 1.27mm single row")
    (fp_text reference J1 (at 1.6 3.65 180) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 5.505 90) (layer F.Fab))
    (fp_text user %R (at 0 1.905) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 3.81 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 38 /PIEZO_OUT_2))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 39 /PIEZO_OUT_1))
    (pad 2 thru_hole oval (at 0 1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 40 /VIB-))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 41 /VIB+))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x04_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SmartwatchLibrary:UCLAMP_0571P (layer F.Cu) (tedit 60150E86)
    (at 203.65 61.7 180)
    (descr spg1610)
    (tags "TVS Diode (Uni-directional)")
    (attr smd)
    (fp_text reference D2 (at 2.65 0) (layer F.SilkS))
    (fp_text value UCLAMP0571P (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -2.54) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.9 1.1) (layers F.Cu F.Paste F.Mask)
      (net 28 +5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.9 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model UCLAMP0571P.TNT.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/LIB_UCLAMP0571P.TNT/UCLAMP0571P.TNT/3D/UCLAMP0571P.TNT.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 215.5 80.65)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 0 1.8) (layer F.SilkS))
    (fp_text value AP2112K-3.3 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 62 /SD_PWR))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U2-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 67 /SD_PWR_EN))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC_UNREG))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 209.9 80.775 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0.075 1 90) (layer F.SilkS))
    (fp_text value 47k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /SD_PWR_EN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 206.5 62.275 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at -1.325 -1 90) (layer F.SilkS))
    (fp_text value 47k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /CARD_DETECT))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /SD_PWR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 207.125 73.1)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at -0.825 1.1) (layer F.SilkS))
    (fp_text value 47k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /MISO))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /SD_PWR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 207.125 71.1)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at -1.725 -0.05 90) (layer F.SilkS))
    (fp_text value 47k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /MOSI))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /SD_PWR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 208.1 62.325 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0.425 1.1 90) (layer F.SilkS))
    (fp_text value 47k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(J4-Pad1)"))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /SD_PWR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 207.525 69.3)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -1.775 0 90) (layer F.SilkS))
    (fp_text value 47k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /SD_CS))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /SD_PWR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 216.3 58.975 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 1.925 -0.75 90) (layer F.SilkS))
    (fp_text value 47k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(J4-Pad8)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /SD_PWR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SmartwatchLibrary:Molex_MicroSD_503398-1892 (layer F.Cu) (tedit 6013A083)
    (at 200.2 59.99 90)
    (descr 503398-1892)
    (tags Connector)
    (attr smd)
    (fp_text reference J4 (at 7.19 4.9 90) (layer F.SilkS))
    (fp_text value Micro_SD_Card_Det (at 5.996 -5.08 90) (layer F.Fab) hide)
    (fp_text user %R (at 7.19 4.9 90) (layer F.Fab))
    (pad 1 smd rect (at 4.17 1.4 90) (size 0.7 1.1) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(J4-Pad1)"))
    (pad 2 smd rect (at 5.27 1.4 90) (size 0.7 1.1) (layers F.Cu F.Paste F.Mask)
      (net 64 /SD_CS))
    (pad 3 smd rect (at 6.37 1.4 90) (size 0.7 1.1) (layers F.Cu F.Paste F.Mask)
      (net 25 /MOSI))
    (pad 4 smd rect (at 7.47 1.4 90) (size 0.7 1.1) (layers F.Cu F.Paste F.Mask)
      (net 62 /SD_PWR))
    (pad 5 smd rect (at 8.57 1.4 90) (size 0.7 1.1) (layers F.Cu F.Paste F.Mask)
      (net 23 /SCK))
    (pad 6 smd rect (at 9.67 1.4 90) (size 0.7 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 10.77 1.4 90) (size 0.7 1.1) (layers F.Cu F.Paste F.Mask)
      (net 24 /MISO))
    (pad 8 smd rect (at 11.87 1.4 90) (size 0.7 1.1) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(J4-Pad8)"))
    (pad 9 smd rect (at 2.38 13.865 90) (size 0.9 0.93) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 6.645 13.94 180) (size 0.78 1.05) (layers F.Cu F.Paste F.Mask)
      (net 66 /CARD_DETECT))
    (pad 11 smd rect (at 13.03 12.665 90) (size 0.7 3.33) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 12.95 1.9 90) (size 0.86 2.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 0.29 1.415 90) (size 1.14 1.83) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 0.07 12.665 90) (size 0.7 3.33) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model 503398-1892.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /Users/kevin/Downloads/5033981892--3DModel-STEP-56544.STEP
      (offset (xyz 6.5 -7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 180))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 218.8 80.575 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at -1.225 -1.15 90) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /SD_PWR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 211.9 80.775 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at -0.425 -1.15 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 VCC_UNREG))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 216.3 55.8 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -0.6 -1.05 90) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /SD_PWR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SmartwatchLibrary:BNO085 (layer F.Cu) (tedit 5FF2636A)
    (at 222.849999 57.099999 180)
    (descr BNO085-1)
    (tags Accelerometer)
    (attr smd)
    (fp_text reference AC1 (at 1.199999 3.399999 180) (layer F.SilkS))
    (fp_text value BNO085 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text user %R (at 0.35 -5.08) (layer F.Fab))
    (pad 28 smd rect (at 1.563 -1.75 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 27 smd rect (at 1.563 -1.25 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 60 /CLK_32_768))
    (pad 26 smd rect (at 1.563 -0.75 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 25 smd rect (at 1.563 -0.25 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 1.563 0.25 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(AC1-Pad24)"))
    (pad 23 smd rect (at 1.563 0.75 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(AC1-Pad23)"))
    (pad 22 smd rect (at 1.563 1.25 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(AC1-Pad22)"))
    (pad 21 smd rect (at 1.563 1.75 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(AC1-Pad21)"))
    (pad 20 smd rect (at 1.563 2.25 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 7 /SDA))
    (pad 19 smd rect (at 0.75 2.313 180) (size 0.25 0.575) (layers F.Cu F.Paste F.Mask)
      (net 8 /SCL))
    (pad 18 smd rect (at 0.25 2.313 180) (size 0.25 0.575) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(AC1-Pad18)"))
    (pad 17 smd rect (at -0.25 2.313 180) (size 0.25 0.575) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -0.75 2.313 180) (size 0.25 0.575) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(AC1-Pad16)"))
    (pad 15 smd rect (at -1.563 2.25 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(AC1-Pad15)"))
    (pad 14 smd rect (at -1.563 1.75 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 12 /INT_MOTION))
    (pad 13 smd rect (at -1.563 1.25 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(AC1-Pad13)"))
    (pad 12 smd rect (at -1.563 0.75 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(AC1-Pad12)"))
    (pad 11 smd rect (at -1.563 0.25 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 15 /RST_MOTION))
    (pad 10 smd rect (at -1.563 -0.25 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 9 smd rect (at -1.563 -0.75 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(AC1-Pad9)"))
    (pad 8 smd rect (at -1.563 -1.25 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(AC1-Pad8)"))
    (pad 7 smd rect (at -1.563 -1.75 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(AC1-Pad7)"))
    (pad 6 smd rect (at -1.563 -2.25 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -0.75 -2.313 180) (size 0.25 0.575) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.25 -2.313 180) (size 0.25 0.575) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(AC1-Pad4)"))
    (pad 3 smd rect (at 0.25 -2.313 180) (size 0.25 0.575) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 -2.313 180) (size 0.25 0.575) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.563 -2.25 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(AC1-Pad1)"))
    (model BNO085.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/LIB_BNO085/BNO085/3D/BNO085.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SmartwatchLibrary:OM7604C732768kHz20PPMTAQC (layer F.Cu) (tedit 600477D5)
    (at 219.1 67.15 270)
    (descr OM-7604-C7-32.768kHz-20PPM-TA-QC-2)
    (tags "Crystal or Oscillator")
    (attr smd)
    (fp_text reference Y1 (at -2.85 -0.6) (layer F.SilkS))
    (fp_text value OM-7604-C7-32.768kHz-20PPM-TA-QC (at -0.275 -5.08 90) (layer F.SilkS) hide)
    (fp_text user %R (at -0.275 -2.54 90) (layer F.Fab))
    (pad 4 smd rect (at -1.35 -0.6) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 1.35 -0.6) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.35 0.6) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.35 0.6) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 60 /CLK_32_768))
    (model OM-7604-C7-32.768kHz-20PPM-TA-QC.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/LIB_OM-7604-C7-32.768kHz-20PPM-TA-QC/OM-7604-C7-32.768kHz-20PPM-TA-QC/3D/OM-7604-C7-32.768kHz-20PPM-TA-QC.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SmartwatchLibrary:DRV2605LDGS (layer F.Cu) (tedit 5D9F72B2)
    (at 224.4 49.8)
    (descr "VSSOP, 10 Pin (http://www.ti.com/lit/ds/symlink/ads1115.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "VSSOP SO")
    (attr smd)
    (fp_text reference U3 (at -0.15 1.6) (layer F.SilkS))
    (fp_text value DRV2605LDGS (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.2 -1) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at -2.2 -0.5) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /SCL))
    (pad 3 smd roundrect (at -2.2 0) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /SDA))
    (pad 4 smd roundrect (at -2.2 0.5) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 5 smd roundrect (at -2.2 1) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /EN_HAP))
    (pad 6 smd roundrect (at 2.2 1) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(U3-Pad6)"))
    (pad 7 smd roundrect (at 2.2 0.5) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /VIB+))
    (pad 8 smd roundrect (at 2.2 0) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 2.2 -0.5) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /VIB-))
    (pad 10 smd roundrect (at 2.2 -1) (size 1.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 VCC_UNREG))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/VSSOP-10_3x3mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 202.1 79.3)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D3 (at -0.75 1.25) (layer F.SilkS))
    (fp_text value "ORANGE LED" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 +5V))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 217.2 76.8)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U5 (at 2.85 0.4) (layer F.SilkS))
    (fp_text value AP2112K-3.3 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U5-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R16-Pad2)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC_UNREG))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 204.2 76.35)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at 0.7 2.5) (layer F.SilkS))
    (fp_text value MCP73831-2-OT (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R11-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 +5V))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 29 VBAT))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 214.4 76.7875 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 1.7625 -0.3 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(R16-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 VCC_UNREG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 226.6 53.3875 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -0.0375 -1 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(AC1-Pad15)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 224.3125 52.7 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 2.4125 -0.1) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(AC1-Pad16)"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 226.6 56.4875 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0.0875 -1 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /RST_MOTION))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 211.9875 78.4)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -1.7875 0.05 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 206.9 76.0125 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 1.1625 1.1 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(R11-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 224.175 61.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 2.525 0.85) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(AC1-Pad4)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 203.7875 73.7)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 1.1125 -1.1 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(D3-Pad1)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 207.125 67.6 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 1.725 0 90) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 207.125 65.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -1.725 0 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /SDA))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 220.1875 71.2)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 2.4625 0.15) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 220.125 72.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.475 -0.05) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 VBAT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 211.75 73.4 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 1.2 -1.85 180) (layer F.SilkS))
    (fp_text value DMP2035U (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 29 VBAT))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC_UNREG))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 28 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_Micro-B_Molex_47346-0001 (layer F.Cu) (tedit 5D8620A7)
    (at 202.7 67.75 270)
    (descr "Micro USB B receptable with flange, bottom-mount, SMD, right-angle (http://www.molex.com/pdm_docs/sd/473460001_sd.pdf)")
    (tags "Micro B USB SMD")
    (attr smd)
    (fp_text reference J2 (at 4.45 -0.4) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0 4.6 270) (layer F.Fab))
    (fp_text user %R (at 0 1.2 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.67 270) (layer Dwgs.User))
    (pad 6 smd rect (at 1.55 1.2 270) (size 1 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -1.15 1.2 270) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 3.375 1.2 270) (size 1.65 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -3.375 1.2 270) (size 1.65 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.4875 -1.375 270) (size 1.425 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.4875 -1.375 270) (size 1.425 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.3 -1.46 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.65 -1.46 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J2-Pad4)"))
    (pad 3 smd rect (at 0 -1.46 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at -0.65 -1.46 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at -1.3 -1.46 270) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 28 +5V))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123F (layer F.Cu) (tedit 587F7769)
    (at 211.3 76.4 180)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D1 (at 2.1 1.55 90) (layer F.SilkS))
    (fp_text value MBR120VLSFT3G (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.905) (layer F.Fab))
    (pad 2 smd rect (at 1.4 0 180) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 28 +5V))
    (pad 1 smd rect (at -1.4 0 180) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC_UNREG))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 219.6875 47.2 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0.5375 -1.1 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(C20-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 220.1 50.6875 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at -2.2125 -0.1 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C19-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 216.7875 74.1 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at -2.2625 -0.6) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 214.4 73.7125 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 1.7625 1.2 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 VCC_UNREG))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 217.1875 53.3)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0.4625 1.05) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(C16-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 201.5 76.7125 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 2.8125 0 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 VBAT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 226.6 59.5875 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0.1625 1.05 90) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(AC1-Pad9)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 216.4125 47.2)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at -1.5125 1.4 90) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 218.4 59.025 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -1.975 0.3 90) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 221.125 61.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -1.175 1.2) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 207.6875 78.3)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -0.7875 1.1) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 226.0125 47.2)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 1.5875 0.9 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 VCC_UNREG))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 222.7875 47.2)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 1.0625 1.6 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 213.8875 70.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 2.0125 -0.75) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 212.175 61.4 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -0.575 -1.05) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 210.8125 70.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 1.1875 0.95) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:SM02B-SRSS-TB (layer F.Cu) (tedit 60036C19)
    (at 222.7 68)
    (descr SM02B-SRSS-TB)
    (tags Connector)
    (attr smd)
    (fp_text reference J3 (at 3 1) (layer F.SilkS))
    (fp_text value SM02B-SRSS (at 1.654 -8.89) (layer F.Fab) hide)
    (fp_text user %R (at 1.654 -6.35) (layer F.Fab))
    (pad 1 smd rect (at 1.5 -4.575) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.5 -4.575) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 29 VBAT))
    (pad 3 smd rect (at 0.2 -0.7) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 3.8 -0.7) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (model ${KIPRJMOD}/SM02B-SRSS-TB-LF--SN---3DModel-STEP-56544.STEP
      (offset (xyz 2 2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 180))
    )
  )
  (gr_line (start 228 46) (end 228 70.085) (layer Edge.Cuts) (width 0.0001))
  (gr_line (start 227.405986 70.6) (end 225 70.6) (layer Edge.Cuts) (width 0.0001))
  (gr_arc (start 227.405986 70) (end 227.405986 70.6) (angle -81.9) (layer Edge.Cuts) (width 0.0001))
  (gr_line (start 228 75.6) (end 228 83) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 227.484541 75.005986) (end 225 75.006) (layer Edge.Cuts) (width 0.001))
  (gr_arc (start 227.4 75.6) (end 228 75.6) (angle -81.9) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 225 75.006) (end 225 70.6) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 228 46) (end 200 46) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 200 83) (end 228 83) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 200 46) (end 200 83) (layer Edge.Cuts) (width 0.001))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 214.6 52.7) (xy 213.7 52.7) (xy 213.7 54) (xy 214.6 54) (xy 214.6 57)
        (xy 213.5 57) (xy 213.5 58.2) (xy 214.6 58.2) (xy 214.6 59.4) (xy 211.1 59.4)
        (xy 211.1 60.4) (xy 203 60.3) (xy 203 47.6) (xy 203.6 47.6) (xy 203.6 46.5)
        (xy 211.175 46.5) (xy 211.2 47.4) (xy 214.6 47.4)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 228 83) (xy 200 83) (xy 200 46) (xy 228 46)
      )
    )
  )
  (zone (net 1) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 228 83) (xy 200 83) (xy 200 46) (xy 228 46)
      )
    )
  )
  (zone (net 0) (net_name "") (layers In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 220.6 69.5) (xy 217.5 69.5) (xy 217.5 64.4) (xy 220.6 64.4)
      )
    )
  )
)
