(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 88.9 93.98)
    (grid_origin 88.9 93.98)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "GND")
  (net 3 "+5V")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(J1-Pad3)")
  (net 6 "Net-(J1-Pad4)")
  (net 7 "Net-(Q1-Pad2)")
  (net 8 "Net-(R1-Pad1)")
  (net 9 "Net-(J1-Pad5)")
  (footprint "Relay_THT:Relay_StandexMeder_DIP_LowProfile" (layer "F.Cu")
    (tedit 5A54BF5F)
    (at 112.756 84.592 -90)
    (descr "package for Standex Meder DIP reed relay series, see https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_DIP.pdf")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil reed relay")
    (property "Sheetfile" "IRProbeRcvr.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K1" (at 7.61 7.346) (layer "F.SilkS"))
    (fp_text value "HE721C0510" (at 3.81 18.63 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.815 7.62 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.54 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "+5V") (pintype "passive"))
    (pad "6" thru_hole circle (at 0 12.8 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 15.24 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad4)") (pintype "passive"))
    (pad "8" thru_hole circle (at 7.62 15.24 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad "9" thru_hole circle (at 7.62 12.8 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad "13" thru_hole circle (at 7.62 2.54 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad "14" thru_hole circle (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_StandexMeder_DIP_LowProfile.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 100.912 81.46 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "IRProbeRcvr.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 9.98 0) (layer "F.SilkS"))
    (fp_text value "1K" (at 2.614 -0.074) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 93.292 78.92)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "IRProbeRcvr.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at -2.36 0.074) (layer "F.SilkS"))
    (fp_text value "39" (at 5.26 0.074) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.72 0.074) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(Q1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 112.522 78.735 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "IRProbeRcvr.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at -0.757 -2.794) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:TO-18-3" (layer "F.Cu")
    (tedit 5AFC2FDD)
    (at 107.2335 80.068 180)
    (property "Category" "Discrete Semiconductor Products")
    (property "DK_Datasheet_Link" "https://my.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=2N2906.PDF")
    (property "DK_Detail_Page" "/product-detail/en/central-semiconductor-corp/2N2907A/2N2907ACS-ND/4806853")
    (property "Description" "TRANS PNP 60V 0.6A TO-18")
    (property "Digi-Key_PN" "2N2907ACS-ND")
    (property "Family" "Transistors - Bipolar (BJT) - Single")
    (property "MPN" "2N2907A")
    (property "Manufacturer" "Central Semiconductor Corp")
    (property "Sheetfile" "IRProbeRcvr.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "Q1" (at -1.7325 2.344) (layer "F.SilkS"))
    (fp_text value "2N2907A" (at 1.3155 -3.244) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.27 -1.4) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.68) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 1.27 180) (size 1.46 1.46) (drill 0.68) (layers *.Cu *.Mask)
      (net 7 "Net-(Q1-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 2.54 0 180) (size 1.52 1.52) (drill 0.68) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-18-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 117.602 81.28)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheetfile" "IRProbeRcvr.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Male" (at 0 12.49) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "OptoDevice:Vishay_MINICAST-3Pin" (layer "F.Cu")
    (tedit 5B8886B7)
    (at 91.431 91.186 90)
    (descr "IR Receiver Vishay TSOP-xxxx, MINICAST package, see https://www.vishay.com/docs/82669/tsop32s40f.pdf")
    (tags "IR Receiver Vishay TSOP-xxxx MINICAST")
    (property "Category" "Sensors, Transducers")
    (property "DK_Datasheet_Link" "http://www.vishay.com/docs/82479/tssp58038.pdf")
    (property "DK_Detail_Page" "/product-detail/en/vishay-semiconductor-opto-division/TSSP58038/TSSP58038-ND/4695717")
    (property "Description" "SENSOR REMOTE REC 38.0KHZ 25M")
    (property "Digi-Key_PN" "TSSP58038-ND")
    (property "Family" "Optical Sensors - Photo Detectors - Remote Receiver")
    (property "MPN" "TSSP58038")
    (property "Manufacturer" "Vishay Semiconductor Opto Division")
    (property "Sheetfile" "IRProbeRcvr.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "U1" (at -1.524 2.295 180) (layer "F.SilkS"))
    (fp_text value "TSSP4038" (at 2.55 4.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.139)
      (net 8 "Net-(R1-Pad1)") (pinfunction "OUT") (pintype "output"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "+5V") (pinfunction "Vs") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/OptoDevice.3dshapes/Vishay_MINICAST-3Pin.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbols:OSHW-Logo2_7.3x6mm_SilkScreen" (layer "B.Cu")
    (tedit 0)
    (at 106.172 83.82)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "OSHW-Logo2_7.3x6mm_SilkScreen" (at 0.75 0) (layer "B.Fab") hide)
  )
  (gr_rect (start 88.9 93.98) (end 120.396 76.454) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "Wireless CNC Probe \nIR Rcvr\nDavid Wolfenbarger\nRev -" (at 105.664 88.9 180) (layer "B.SilkS"))
  (gr_text "NC to Mill" (at 115.824 87.884 90) (layer "F.SilkS"))
  (gr_text "GND" (at 115.57 81.28 90) (layer "F.SilkS"))
  (gr_text "NO" (at 115.824 91.694 90) (layer "F.SilkS"))
  (gr_text "+5V" (at 115.57 83.82 90) (layer "F.SilkS"))
  (zone (net 3) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.396 93.98)
        (xy 88.9 93.98)
        (xy 88.9 76.454)
        (xy 120.396 76.454)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.396 93.98)
        (xy 88.9 93.98)
        (xy 88.9 76.454)
        (xy 120.396 76.454)
      )
    )
  )
)
