<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="7.62" width="0" layer="20"/>
<wire x1="0" y1="7.62" x2="17.78" y2="7.62" width="0" layer="20"/>
<wire x1="17.78" y1="7.62" x2="17.78" y2="0" width="0" layer="20"/>
<wire x1="17.78" y1="0" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="talkbacksies">
<description>talkbacksies</description>
<packages>
<package name="SINGLE-100MIL-HOLE">
</package>
<package name="DEBUG-HEADER-20021121-00010C4LF">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TVCC" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="DIO" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="GND" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="CLK" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="RST" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="MLU" library="talkbacksies" package="DEBUG-HEADER-20021121-00010C4LF" value="DEBUG-HEADER-20021121-00010C4LF"/>
</elements>
<signals>
<signal name="TVCC">
<contactref element="TVCC" pad="P$1"/>
<contactref element="MLU" pad="1"/>
</signal>
<signal name="TMS/SWD_DIO">
<contactref element="DIO" pad="P$1"/>
<contactref element="MLU" pad="2"/>
</signal>
<signal name="GND">
<contactref element="GND" pad="P$1"/>
<contactref element="MLU" pad="3"/>
<contactref element="MLU" pad="5"/>
</signal>
<signal name="TCK/SWD_CLK">
<contactref element="CLK" pad="P$1"/>
<contactref element="MLU" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="MLU" pad="10"/>
<contactref element="RST" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
