<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<text>GND

DAT

CLK

C/S

VCC</text>
<wire x1="42" y1="0" x2="42" y2="68" width="0.4064" layer="20"/>
<wire x1="42" y1="68" x2="11.5" y2="68" width="0.4064" layer="20"/>
<wire x1="11.5" y1="68" x2="11.5" y2="56.5" width="0.4064" layer="20"/>
<wire x1="11.5" y1="56.5" x2="0" y2="56.5" width="0.4064" layer="20"/>
<wire x1="0" y1="56.5" x2="0" y2="0" width="0.4064" layer="20"/>
<wire x1="0" y1="0" x2="42" y2="0" width="0.4064" layer="20"/>
<hole x="16.41" y="63.57" drill="4.2"/>
<hole x="4.43" y="3.97" drill="4.5"/>
<text>RAW

GND

RST

VCC

F4

F5

F6

F7

B1

B2

B3

B6</text>
<text>D3

D2

GND

GND

D1

D0

D4

C6

D7

E6

B4

B5</text>
<text>VCC

C/S

CLK

DAT

GND</text>
<text>Debolestis</text>
<text>RESET</text>
<text>X-AXIS --&gt; F6

Y-AXIS --&gt; F7

C/S -----&gt; D0

DATA ----&gt; D1</text>
<text>X-AXIS --&gt; F6

Y-AXIS --&gt; F7

C/S -----&gt; D0

DATA ----&gt; D1</text>
<text>BROWN

RED

ORANGE

YELLOW

GREEN</text>
<text>-Y-

GND

VCC</text>
<text>-X-

GND

VCC</text>
<text>VCC

GND

-Y-</text>
<text>-X-

GND

VCC</text>
</plain>
<libraries>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA12-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C5B5.5">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 5.5 mm, grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="Switches_rev16a">
<description>&lt;BR&gt;Wurth Elektronik - Switches&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-405&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/eagle"&gt;http://www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Eagle Version 6, Library Revision 2015b, 08.04.2015&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="430156050926">
<description>WS-TST-6x6 mm THT Tact Switch,4 pins</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C-L" library="con-lstb" package="MA12-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="C-R" library="con-lstb" package="MA12-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="X-AXIS" library="pinhead" package="1X03/90" value="">
<attribute name="VALUE"/>
</element>
<element name="Y-AXIS" library="pinhead" package="1X03/90" value="">
<attribute name="VALUE"/>
</element>
<element name="SHIFT_REGISTER" library="pinhead" package="1X05/90" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="capacitor-wima" package="C5B5.5" value="1nF">
<attribute name="VALUE"/>
</element>
<element name="RESET" library="Switches_rev16a" package="430156050926" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="D3">
<contactref element="C-L" pad="1"/>
</signal>
<signal name="D2">
<contactref element="C-L" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C-L" pad="4"/>
<contactref element="C-L" pad="3"/>
<contactref element="C-R" pad="2"/>
<contactref element="X-AXIS" pad="2"/>
<contactref element="Y-AXIS" pad="2"/>
<contactref element="SHIFT_REGISTER" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="RESET" pad="4"/>
<contactref element="RESET" pad="2"/>
</signal>
<signal name="D1">
<contactref element="C-L" pad="5"/>
<contactref element="SHIFT_REGISTER" pad="2"/>
</signal>
<signal name="D0">
<contactref element="C-L" pad="6"/>
<contactref element="SHIFT_REGISTER" pad="4"/>
</signal>
<signal name="D4">
<contactref element="C-L" pad="7"/>
</signal>
<signal name="C6">
<contactref element="C-L" pad="8"/>
</signal>
<signal name="D7">
<contactref element="C-L" pad="9"/>
</signal>
<signal name="E6">
<contactref element="C-L" pad="10"/>
</signal>
<signal name="B4">
<contactref element="C-L" pad="11"/>
</signal>
<signal name="B5">
<contactref element="C-L" pad="12"/>
</signal>
<signal name="RAW">
<contactref element="C-R" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="C-R" pad="4"/>
<contactref element="X-AXIS" pad="3"/>
<contactref element="Y-AXIS" pad="3"/>
<contactref element="SHIFT_REGISTER" pad="5"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="RST">
<contactref element="C-R" pad="3"/>
<contactref element="RESET" pad="3"/>
</signal>
<signal name="F4">
<contactref element="C-R" pad="5"/>
</signal>
<signal name="F5">
<contactref element="C-R" pad="6"/>
</signal>
<signal name="F6">
<contactref element="C-R" pad="7"/>
<contactref element="X-AXIS" pad="1"/>
</signal>
<signal name="F7">
<contactref element="C-R" pad="8"/>
<contactref element="Y-AXIS" pad="1"/>
</signal>
<signal name="B1-SCK">
<contactref element="C-R" pad="9"/>
<contactref element="SHIFT_REGISTER" pad="3"/>
</signal>
<signal name="B2">
<contactref element="C-R" pad="10"/>
</signal>
<signal name="B3">
<contactref element="C-R" pad="11"/>
</signal>
<signal name="B6">
<contactref element="C-R" pad="12"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
