(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 2)
    (zones 0)
    (modules 3)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
  )
  (module "City Hub Battery Insert Footprints:TestPoint_Pad_3mm_x_8mm" (layer B.Cu) (tedit 5EA118D9)
    (at 104.5 95.2)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP2 (at 0.1 -5) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -5.08) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 3 8) (layers B.Cu B.Mask)
      (net 1 "Net-(J1-Pad2)"))
  )
  (module "City Hub Battery Insert Footprints:TestPoint_Pad_3mm_x_12mm" (layer B.Cu) (tedit 5EA118F8)
    (at 112.3 91.2)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP1 (at 0 -7.1) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -6.985) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 3 12) (layers B.Cu B.Mask)
      (net 2 "Net-(J1-Pad1)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 93.4 89.16)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 0.7 -3.7) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 112.3 84.3) (layer B.SilkS))
  (gr_text +9V (at 104.7 90.2) (layer B.SilkS))
  (gr_text GND (at 93.4 86.8) (layer F.SilkS))
  (gr_text +9V (at 93.5 94.1) (layer B.SilkS))
  (gr_text GND (at 93.4 86.8) (layer B.SilkS))
  (gr_text "2020-04-23\nv1.0" (at 118 94.9) (layer F.SilkS))
  (gr_text "Powered Up\n9V Battery Insert\nCity Hub (\"HUB NO. 4\")" (at 107.4 84.2) (layer F.SilkS))
  (gr_text +9V (at 93.3 94.1) (layer F.SilkS))
  (gr_line (start 106.5 99.4) (end 102.5 99.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 108.5 97.4) (end 106.5 99.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100.5 97.4) (end 102.5 99.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.8 97.4) (end 108.5 97.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 90.2 97.4) (end 100.5 97.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.8 81) (end 118.8 97.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 90.2 81) (end 90.2 97.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 90.2 81) (end 118.8 81) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.6 100.2) (xy 89.4 99.9) (xy 89.5 98.6) (xy 89.8 80.6) (xy 119.3 80.6)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121 101.3) (xy 87.6 101.3) (xy 87.9 98.6) (xy 89.3 80) (xy 120.2 79.7)
      )
    )
  )
)
