<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.0">
<drawing>
<board>
<plain>
<wire x1="23.038" y1="1.36966875" x2="23.038" y2="17.6858375" width="0" layer="20"/>
<wire x1="23.038" y1="17.6858375" x2="21.6838375" y2="19.04" width="0" layer="20" curve="90"/>
<wire x1="21.6838375" y1="19.04" x2="1.27" y2="19.04" width="0" layer="20"/>
<wire x1="1.27" y1="19.04" x2="0" y2="17.77" width="0" layer="20" curve="90"/>
<wire x1="0" y1="17.77" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="21.66833125" y2="0" width="0" layer="20"/>
<wire x1="21.66833125" y1="0" x2="23.038" y2="1.36966875" width="0" layer="20" curve="90"/>
<text>tiny dice </text>
<text>by marius_mym</text>
</plain>
<libraries>
<library name="SparkFun-Batteries">
<description>&lt;h3&gt;SparkFun Batteries&lt;/h3&gt;
This library contains battery clips, connectors, and appropriately sized silk outlines for LiPo batteries. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_12MM">
<description>&lt;h3&gt;12mm Coin Cell (CR1225) Battery Holder - SMD&lt;/h3&gt;
&lt;p&gt;Holds battery in place with friction. The metal housing connects to the positive side of the battery and the PCB pad underneath is connected to the negative side.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Prototyping/KEY-3000.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="homemade-hardware">
<packages>
<package name="KMR2">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="MSK-12C02 SMD Micro Slider Switch SPDT">
<packages>
<package name="MSK-12C02">
<description>Footprint of the VIMEX MSK-12C02 SPDT SMD Switch
Created by mzst on 17-Jan-2016</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CR1220" library="SparkFun-Batteries" package="BATTCON_12MM" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="BATT-08044"/>
<attribute name="SF_SKU" value="PRT-10592"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED5" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED6" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED7" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="10K" library="adafruit" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="homemade-hardware" package="KMR2" value="BUTTON_SPST-KMR2"/>
<element name="ATTINY85" library="homemade-hardware" package="SOIC8" value="ATTINY85-20SU">
<attribute name="NAME"/>
</element>
<element name="U$1" library="MSK-12C02 SMD Micro Slider Switch SPDT" package="MSK-12C02" value="MSK-12C02_SMD_SPDT_SWITCH"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="10K" pad="2"/>
<contactref element="SW1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="ATTINY85" pad="7"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="CR1220" pad="GND"/>
<contactref element="U$1" pad="COM"/>
</signal>
<signal name="VCC">
<contactref element="SW1" pad="4"/>
<contactref element="SW1" pad="2"/>
<contactref element="ATTINY85" pad="8"/>
<contactref element="CR1220" pad="PWR@1"/>
</signal>
<signal name="N$7">
<contactref element="ATTINY85" pad="5"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="ATTINY85" pad="2"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="ATTINY85" pad="6"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="ATTINY85" pad="3"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="BTM">
</signal>
<signal name="GND-BTN">
<contactref element="U$1" pad="L1"/>
<contactref element="ATTINY85" pad="4"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED5" pad="C"/>
<contactref element="LED6" pad="C"/>
<contactref element="LED7" pad="C"/>
<contactref element="10K" pad="1"/>
</signal>
<signal name="N$3">
</signal>
</signals>
</board>
</drawing>
</eagle>
